<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-HCI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCI_1365">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1365</description>
</package>
<package name="WE-HCI_1890_MINZN">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1890</description>
</package>
<package name="WE-HCI_1335">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1335</description>
</package>
<package name="WE-HCI_1890">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1890</description>
</package>
<package name="WE-HCI_7040">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7040</description>
</package>
<package name="WE-HCI_1350">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1350</description>
</package>
<package name="WE-HCI_2212">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;2212</description>
</package>
<package name="WE-HCI_7030">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7030</description>
</package>
<package name="WE-HCI_1030">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI  SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1030</description>
</package>
<package name="WE-HCI_1050">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1050</description>
</package>
<package name="WE-HCI_5040">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;5040</description>
</package>
<package name="WE-HCI_1040">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1040</description>
</package>
<package name="WE-HCI_7050">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;7050</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCI_1890" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_WE-PERM2" package="WE-HCI_1890">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443556082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556082.pdf"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="41.5A"/>
<attribute name="ISAT" value="65A"/>
<attribute name="LR" value="0.72uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556082 "/>
<attribute name="RDC" value="0.54mOhm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74435561100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435561100.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="ISAT" value="21.5A"/>
<attribute name="LR" value="8.2uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 74435561100 "/>
<attribute name="RDC" value="6.9mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7443556130">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556130.pdf"/>
<attribute name="FRES" value="78MHz"/>
<attribute name="IR" value="34.5A"/>
<attribute name="ISAT" value="62A"/>
<attribute name="LR" value="1.15uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556130 "/>
<attribute name="RDC" value="0.94mOhm"/>
<attribute name="VALUE" value="1.3uH"/>
</technology>
<technology name="_7443556190">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556190.pdf"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="32.5A"/>
<attribute name="ISAT" value="52A"/>
<attribute name="LR" value="1.6uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556190 "/>
<attribute name="RDC" value="1.2mOhm"/>
<attribute name="VALUE" value="1.9uH"/>
</technology>
<technology name="_7443556260">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556260.pdf"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="31.5A"/>
<attribute name="ISAT" value="50A"/>
<attribute name="LR" value="2.15uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556260 "/>
<attribute name="RDC" value="1.58mOhm"/>
<attribute name="VALUE" value="2.6uH"/>
</technology>
<technology name="_7443556350">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556350.pdf"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="22.5A"/>
<attribute name="ISAT" value="37A"/>
<attribute name="LR" value="3uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556350 "/>
<attribute name="RDC" value="3.1mOhm"/>
<attribute name="VALUE" value="3.5uH"/>
</technology>
<technology name="_7443556450">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556450.pdf"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="20.5A"/>
<attribute name="ISAT" value="37A"/>
<attribute name="LR" value="3.8uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556450 "/>
<attribute name="RDC" value="3.4mOhm"/>
<attribute name="VALUE" value="4.5uH"/>
</technology>
<technology name="_7443556560">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556560.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="33A"/>
<attribute name="LR" value="4.8uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556560 "/>
<attribute name="RDC" value="3.7mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_7443556680">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443556680.pdf"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="18.5A"/>
<attribute name="ISAT" value="27A"/>
<attribute name="LR" value="5.6uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 7443556680 "/>
<attribute name="RDC" value="4.1mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
<device name="_MNZN" package="WE-HCI_1890_MINZN">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74435571100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435571100.pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="16.5A"/>
<attribute name="ISAT" value="18.5A"/>
<attribute name="LR" value="8.2uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435571100 "/>
<attribute name="RDC" value="6.9mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74435571500">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435571500.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="LR" value="12uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435571500 "/>
<attribute name="RDC" value="9mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74435572200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435572200.pdf"/>
<attribute name="FRES" value="10.5MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="LR" value="15.5uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435572200 "/>
<attribute name="RDC" value="14.6mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74435573300">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435573300.pdf"/>
<attribute name="FRES" value="9.5MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="LR" value="26uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435573300 "/>
<attribute name="RDC" value="21.7mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74435574700">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435574700.pdf"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="LR" value="40uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435574700 "/>
<attribute name="RDC" value="33.5mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_7443557560">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443557560.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="27A"/>
<attribute name="LR" value="3.45uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 7443557560 "/>
<attribute name="RDC" value="2.82mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_7443557760">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443557760.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="20.5A"/>
<attribute name="LR" value="4.9uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 7443557760 "/>
<attribute name="RDC" value="3.75mOhm"/>
<attribute name="VALUE" value="7.6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1365" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1365">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443551111">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551111.pdf"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="LR" value="7.5uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551111 "/>
<attribute name="RDC" value="9.1mOhm"/>
<attribute name="VALUE" value="11.3uH"/>
</technology>
<technology name="_7443551130">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551130.pdf"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LR" value="0.9uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551130 "/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="VALUE" value="1.3uH"/>
</technology>
<technology name="_7443551131">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551131.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="LR" value="9uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551131 "/>
<attribute name="RDC" value="11.2mOhm"/>
<attribute name="VALUE" value="13uH"/>
</technology>
<technology name="_7443551151">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551151.pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="LR" value="10uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551151 "/>
<attribute name="RDC" value="14.8mOhm"/>
<attribute name="VALUE" value="15.4uH"/>
</technology>
<technology name="_7443551181">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551181.pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="LR" value="13uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551181 "/>
<attribute name="RDC" value="22mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7443551200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551200.pdf"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="23A"/>
<attribute name="ISAT" value="22A"/>
<attribute name="LR" value="1.4uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551200 "/>
<attribute name="RDC" value="2.6mOhm"/>
<attribute name="VALUE" value="2uH"/>
</technology>
<technology name="_744355122">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355122.pdf"/>
<attribute name="FRES" value="230MHz"/>
<attribute name="IR" value="32A"/>
<attribute name="ISAT" value="65A"/>
<attribute name="LR" value="0.17uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355122 "/>
<attribute name="RDC" value="0.35mOhm"/>
<attribute name="VALUE" value="0.2uH"/>
</technology>
<technology name="_7443551221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551221.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="LR" value="16uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551221 "/>
<attribute name="RDC" value="24.7mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7443551280">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551280.pdf"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="17.5A"/>
<attribute name="LR" value="1.85uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551280 "/>
<attribute name="RDC" value="3.3mOhm"/>
<attribute name="VALUE" value="2.8uH"/>
</technology>
<technology name="_7443551331">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551331.pdf"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="LR" value="23uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551331 "/>
<attribute name="RDC" value="30.5mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7443551370">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551370.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="17A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="LR" value="2.6uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551370 "/>
<attribute name="RDC" value="4.9mOhm"/>
<attribute name="VALUE" value="3.7uH"/>
</technology>
<technology name="_744355147">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355147.pdf"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="30A"/>
<attribute name="ISAT" value="50A"/>
<attribute name="LR" value="0.41uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355147 "/>
<attribute name="RDC" value="0.67mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_7443551470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551470.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="13A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="LR" value="3.4uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551470 "/>
<attribute name="RDC" value="7mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7443551600">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551600.pdf"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="LR" value="4.5uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551600 "/>
<attribute name="RDC" value="8.4mOhm"/>
<attribute name="VALUE" value="6uH"/>
</technology>
<technology name="_7443551730">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551730.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="13A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="LR" value="5uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551730 "/>
<attribute name="RDC" value="5.9mOhm"/>
<attribute name="VALUE" value="7.3uH"/>
</technology>
<technology name="_744355182">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355182.pdf"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT" value="35A"/>
<attribute name="LR" value="0.64uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355182 "/>
<attribute name="RDC" value="0.9mOhm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_7443551920">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443551920.pdf"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="LR" value="6.3uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443551920 "/>
<attribute name="RDC" value="7.8mOhm"/>
<attribute name="VALUE" value="9.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1335" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1335">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744313025">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744313025.pdf"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="60A"/>
<attribute name="LR" value="0.22uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744313025 "/>
<attribute name="RDC" value="0.75mOhm"/>
<attribute name="VALUE" value="0.25uH"/>
</technology>
<technology name="_744313068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744313068.pdf"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="40A"/>
<attribute name="LR" value="0.47uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744313068 "/>
<attribute name="RDC" value="1.58mOhm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744313120">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744313120.pdf"/>
<attribute name="FRES" value="58MHz"/>
<attribute name="IR" value="17A"/>
<attribute name="ISAT" value="28A"/>
<attribute name="LR" value="0.98uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744313120 "/>
<attribute name="RDC" value="2.85mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_744313180">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744313180.pdf"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="22A"/>
<attribute name="LR" value="1.45uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744313180 "/>
<attribute name="RDC" value="5.6mOhm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_744313220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744313220.pdf"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="LR" value="1.75uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744313220 "/>
<attribute name="RDC" value="5.7mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744313330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744313330.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="LR" value="2.45uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744313330 "/>
<attribute name="RDC" value="8.1mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7040" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744311022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311022.pdf"/>
<attribute name="FRES" value="290MHz"/>
<attribute name="IR" value="21A"/>
<attribute name="ISAT" value="32A"/>
<attribute name="LR" value="0.18mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311022 "/>
<attribute name="RDC" value="1.1mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744311047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311047.pdf"/>
<attribute name="FRES" value="250MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LR" value="0.32mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311047 "/>
<attribute name="RDC" value="1.85mOhm"/>
<attribute name="VALUE" value="0.4uH"/>
</technology>
<technology name="_744311068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311068.pdf"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="IR" value="17A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.52mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311068 "/>
<attribute name="RDC" value="3.1mOhm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744311100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311100.pdf"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="LR" value="0.78mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311100 "/>
<attribute name="RDC" value="4.6mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744311150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311150.pdf"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="LR" value="1.12mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311150 "/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744311220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311220.pdf"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LR" value="1.75mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311220 "/>
<attribute name="RDC" value="11.4mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744311330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311330.pdf"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="LR" value="2.75mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311330 "/>
<attribute name="RDC" value="17.2mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744311470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744311470.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="LR" value="3.5mOhm"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744311470 "/>
<attribute name="RDC" value="19.5mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1350" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1350">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443550101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443550101.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="LR" value="7.8uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443550101 "/>
<attribute name="RDC" value="14.1mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7443550140">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443550140.pdf"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="26A"/>
<attribute name="LR" value="1.05uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443550140 "/>
<attribute name="RDC" value="2.4mOhm"/>
<attribute name="VALUE" value="1.4uH"/>
</technology>
<technology name="_744355019">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355019.pdf"/>
<attribute name="FRES" value="225MHz"/>
<attribute name="IR" value="29A"/>
<attribute name="ISAT" value="60A"/>
<attribute name="LR" value="0.17uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355019 "/>
<attribute name="RDC" value="0.5mOhm"/>
<attribute name="VALUE" value="0.19uH"/>
</technology>
<technology name="_7443550230">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443550230.pdf"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="17.5A"/>
<attribute name="ISAT" value="17A"/>
<attribute name="LR" value="1.6uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443550230 "/>
<attribute name="RDC" value="3.7mOhm"/>
<attribute name="VALUE" value="2.3uH"/>
</technology>
<technology name="_7443550320">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443550320.pdf"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="LR" value="2.2uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443550320 "/>
<attribute name="RDC" value="5.3mOhm"/>
<attribute name="VALUE" value="3.2uH"/>
</technology>
<technology name="_744355047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355047.pdf"/>
<attribute name="FRES" value="95MHz"/>
<attribute name="IR" value="26A"/>
<attribute name="ISAT" value="50A"/>
<attribute name="LR" value="0.42uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355047 "/>
<attribute name="RDC" value="0.9mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_7443550480">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443550480.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LR" value="3.55uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443550480 "/>
<attribute name="RDC" value="10.5mOhm"/>
<attribute name="VALUE" value="4.8uH"/>
</technology>
<technology name="_7443550600">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443550600.pdf"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="LR" value="4.7uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443550600 "/>
<attribute name="RDC" value="13.5mOhm"/>
<attribute name="VALUE" value="6uH"/>
</technology>
<technology name="_7443550820">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443550820.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="LR" value="6.1uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443550820 "/>
<attribute name="RDC" value="11.6mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744355090">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355090.pdf"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="28A"/>
<attribute name="LR" value="0.66uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355090 "/>
<attribute name="RDC" value="1.6mOhm"/>
<attribute name="VALUE" value="0.9uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_2212" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_2212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74435580330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435580330.pdf"/>
<attribute name="FRES" value="26.5MHz"/>
<attribute name="IR" value="29A"/>
<attribute name="ISAT" value="45A"/>
<attribute name="LR" value="2.85uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435580330 "/>
<attribute name="RDC" value="1.7mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74435580680">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435580680.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="28.5A"/>
<attribute name="ISAT" value="31A"/>
<attribute name="LR" value="4.82uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435580680 "/>
<attribute name="RDC" value="2.1mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74435580820">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435580820.pdf"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="25.5A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="LR" value="5.98uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435580820 "/>
<attribute name="RDC" value="2.7mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74435581000">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435581000.pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="21A"/>
<attribute name="ISAT" value="26A"/>
<attribute name="LR" value="7.8uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435581000 "/>
<attribute name="RDC" value="3.4mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74435581200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435581200.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LR" value="8.9uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435581200 "/>
<attribute name="RDC" value="4.3mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_74435582200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435582200.pdf"/>
<attribute name="FRES" value="8.3MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="LR" value="17.7uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435582200 "/>
<attribute name="RDC" value="7mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74435583300">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435583300.pdf"/>
<attribute name="FRES" value="6.8MHz"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="LR" value="30.5uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435583300 "/>
<attribute name="RDC" value="13.2mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74435584700">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435584700.pdf"/>
<attribute name="FRES" value="6.1MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="LR" value="45.2uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435584700 "/>
<attribute name="RDC" value="19.2mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74435586800">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435586800.pdf"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="LR" value="66uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435586800 "/>
<attribute name="RDC" value="27.3mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_74435588200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74435588200.pdf"/>
<attribute name="FRES" value="4.4MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="LR" value="76uH"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="PART-NUMBER" value=" 74435588200 "/>
<attribute name="RDC" value="30.4mOhm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7030" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744310013">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744310013.pdf"/>
<attribute name="FRES" value="400MHz"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="48A"/>
<attribute name="LR" value="0.11uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744310013 "/>
<attribute name="RDC" value="0.91mOhm"/>
<attribute name="VALUE" value="0.13uH"/>
</technology>
<technology name="_744310024">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744310024.pdf"/>
<attribute name="FRES" value="220MHz"/>
<attribute name="IR" value="18A"/>
<attribute name="ISAT" value="40A"/>
<attribute name="LR" value="0.22uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744310024 "/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="VALUE" value="0.24uH"/>
</technology>
<technology name="_744310055">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744310055.pdf"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.43uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744310055 "/>
<attribute name="RDC" value="3.7mOhm"/>
<attribute name="VALUE" value="0.52uH"/>
</technology>
<technology name="_744310095">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744310095.pdf"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LR" value="0.71uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744310095 "/>
<attribute name="RDC" value="6.2mOhm"/>
<attribute name="VALUE" value="0.95uH"/>
</technology>
<technology name="_744310115">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744310115.pdf"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LR" value="1uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744310115 "/>
<attribute name="RDC" value="8.6mOhm"/>
<attribute name="VALUE" value="1.15uH"/>
</technology>
<technology name="_744310150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744310150.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="LR" value="1.25uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744310150 "/>
<attribute name="RDC" value="12.7mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744310200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744310200.pdf"/>
<attribute name="FRES" value="58MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="LR" value="1.55uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744310200 "/>
<attribute name="RDC" value="14.2mOhm"/>
<attribute name="VALUE" value="2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1030" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744323020">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323020.pdf"/>
<attribute name="FRES" value="216MHz"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="50A"/>
<attribute name="LR" value="0.18uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323020 "/>
<attribute name="RDC" value="0.82mOhm"/>
<attribute name="VALUE" value="0.2uH"/>
</technology>
<technology name="_744323033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323033.pdf"/>
<attribute name="FRES" value="119MHz"/>
<attribute name="IR" value="18A"/>
<attribute name="ISAT" value="36A"/>
<attribute name="LR" value="0.29uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323033 "/>
<attribute name="RDC" value="2.17mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744323056">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323056.pdf"/>
<attribute name="FRES" value="106MHz"/>
<attribute name="IR" value="18A"/>
<attribute name="ISAT" value="33A"/>
<attribute name="LR" value="0.48uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323056 "/>
<attribute name="RDC" value="2.17mOhm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744323068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323068.pdf"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="21A"/>
<attribute name="LR" value="0.55uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323068 "/>
<attribute name="RDC" value="4.79mOhm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744323100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323100.pdf"/>
<attribute name="FRES" value="69MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="21A"/>
<attribute name="LR" value="0.82uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323100 "/>
<attribute name="RDC" value="4.79mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744323120">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323120.pdf"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="LR" value="0.94uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323120 "/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_744323150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323150.pdf"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="LR" value="1.28uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323150 "/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744323220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744323220.pdf"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="LR" value="1.9uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744323220 "/>
<attribute name="RDC" value="11.38mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1050" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744325016">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325016.pdf"/>
<attribute name="FRES" value="400MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="58A"/>
<attribute name="LR" value="0.14uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325016 "/>
<attribute name="RDC" value="0.51mOhm"/>
<attribute name="VALUE" value="0.16uH"/>
</technology>
<technology name="_744325040">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325040.pdf"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="24A"/>
<attribute name="ISAT" value="37A"/>
<attribute name="LR" value="0.33uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325040 "/>
<attribute name="RDC" value="0.67mOhm"/>
<attribute name="VALUE" value="0.4uH"/>
</technology>
<technology name="_744325072">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325072.pdf"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="35A"/>
<attribute name="LR" value="0.6uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325072 "/>
<attribute name="RDC" value="1.3mOhm"/>
<attribute name="VALUE" value="0.72uH"/>
</technology>
<technology name="_7443251000">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443251000.pdf"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="LR" value="7.6uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 7443251000 "/>
<attribute name="RDC" value="16.3mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744325120">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325120.pdf"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LR" value="1uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325120 "/>
<attribute name="RDC" value="1.8mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_7443251600">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443251600.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="LR" value="12.7uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 7443251600 "/>
<attribute name="RDC" value="34.5mOhm"/>
<attribute name="VALUE" value="16uH"/>
</technology>
<technology name="_744325180">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325180.pdf"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="LR" value="1.4uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325180 "/>
<attribute name="RDC" value="3.5mOhm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_744325240">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325240.pdf"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="17A"/>
<attribute name="LR" value="1.8uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325240 "/>
<attribute name="RDC" value="4.75mOhm"/>
<attribute name="VALUE" value="2.4uH"/>
</technology>
<technology name="_744325330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325330.pdf"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="LR" value="2.4uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325330 "/>
<attribute name="RDC" value="5.9mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744325420">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325420.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="LR" value="3.3uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325420 "/>
<attribute name="RDC" value="7.1mOhm"/>
<attribute name="VALUE" value="4.2uH"/>
</technology>
<technology name="_744325550">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325550.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="LR" value="4.3uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325550 "/>
<attribute name="RDC" value="10.3mOhm"/>
<attribute name="VALUE" value="5.5uH"/>
</technology>
<technology name="_744325650">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325650.pdf"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="8.4A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="LR" value="5uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325650 "/>
<attribute name="RDC" value="12.5mOhm"/>
<attribute name="VALUE" value="6.5uH"/>
</technology>
<technology name="_744325780">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744325780.pdf"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="LR" value="6uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744325780 "/>
<attribute name="RDC" value="13.6mOhm"/>
<attribute name="VALUE" value="7.8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_5040" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_5040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744316022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316022.pdf"/>
<attribute name="FRES" value="507MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="LR" value="0.18uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316022 "/>
<attribute name="RDC" value="1.25mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744316033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316033.pdf"/>
<attribute name="FRES" value="402MHz"/>
<attribute name="IR" value="18.5A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.24uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316033 "/>
<attribute name="RDC" value="1.75mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744316047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316047.pdf"/>
<attribute name="FRES" value="280MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="LR" value="0.34uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316047 "/>
<attribute name="RDC" value="2.75mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744316068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316068.pdf"/>
<attribute name="FRES" value="253MHz"/>
<attribute name="IR" value="12.75A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="LR" value="0.49uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316068 "/>
<attribute name="RDC" value="4mOhm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_744316100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316100.pdf"/>
<attribute name="FRES" value="158MHz"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="LR" value="0.65uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316100 "/>
<attribute name="RDC" value="4.75mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744316150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316150.pdf"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="LR" value="1.1uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316150 "/>
<attribute name="RDC" value="8.15mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744316220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316220.pdf"/>
<attribute name="FRES" value="108MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="LR" value="1.5uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316220 "/>
<attribute name="RDC" value="11.3mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744316330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316330.pdf"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="IR" value="5.75A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="LR" value="2.25uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316330 "/>
<attribute name="RDC" value="18.5mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744316470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316470.pdf"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="LR" value="3.3uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316470 "/>
<attribute name="RDC" value="24.5mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744316560">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744316560.pdf"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="LR" value="4uH"/>
<attribute name="MATERIAL" value="WE-PERM 2"/>
<attribute name="PART-NUMBER" value=" 744316560 "/>
<attribute name="RDC" value="28.5mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_1040" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_1040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443552100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443552100.pdf"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.78uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443552100 "/>
<attribute name="RDC" value="3.3mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744355215">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355215.pdf"/>
<attribute name="FRES" value="275MHz"/>
<attribute name="IR" value="25A"/>
<attribute name="ISAT" value="60A"/>
<attribute name="LR" value="0.13uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355215 "/>
<attribute name="RDC" value="0.58mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_7443552150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443552150.pdf"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="17A"/>
<attribute name="LR" value="1.1uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443552150 "/>
<attribute name="RDC" value="5.3mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7443552200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443552200.pdf"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LR" value="1.48uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443552200 "/>
<attribute name="RDC" value="7.3mOhm"/>
<attribute name="VALUE" value="2uH"/>
</technology>
<technology name="_7443552280">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443552280.pdf"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="LR" value="2.1uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443552280 "/>
<attribute name="RDC" value="10.6mOhm"/>
<attribute name="VALUE" value="2.8uH"/>
</technology>
<technology name="_744355230">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355230.pdf"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="IR" value="22A"/>
<attribute name="ISAT" value="35A"/>
<attribute name="LR" value="0.25uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355230 "/>
<attribute name="RDC" value="1.1mOhm"/>
<attribute name="VALUE" value="0.3uH"/>
</technology>
<technology name="_7443552430">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443552430.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="LR" value="3uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443552430 "/>
<attribute name="RDC" value="14.1mOhm"/>
<attribute name="VALUE" value="4.3uH"/>
</technology>
<technology name="_744355256">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744355256.pdf"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="30A"/>
<attribute name="LR" value="0.47uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 744355256 "/>
<attribute name="RDC" value="1.61mOhm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_7443552560">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7443552560.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="LR" value="4.15uH"/>
<attribute name="MATERIAL" value="WE-PERM"/>
<attribute name="PART-NUMBER" value=" 7443552560 "/>
<attribute name="RDC" value="20.6mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCI_7050" prefix="L">
<description>&lt;b&gt;WE-HCI SMD Flat Wire High Current Inductor
Shielded
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 qualified

&lt;br&gt;Magnetically shielded

&lt;br&gt;Flat wire coil for low losses at high frequency

&lt;br&gt;Low stray field

&lt;br&gt;Operating temperature: –40 °C to +125°C / +150 °C / +155°C

&lt;br&gt;Recommended solder profile: Reflow

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/B&gt;
&lt;br&gt;
&lt;br&gt; Graphic cards
&lt;br&gt;Laptops
&lt;br&gt;Industrial computers
&lt;br&gt;Motherboards
&lt;br&gt;High current switching regulators
&lt;br&gt;DC/DC converter
&lt;br&gt;Polyphase-switching regulators
&lt;br&gt;Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14796v209%20Family_WE-HCI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13"&gt;https://katalog.we-online.de/en/pbs/WE-HCI#vs_ct:13&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun, Shan 2019-08-06&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-HCI_7050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744314024">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314024.pdf"/>
<attribute name="FRES" value="320MHz"/>
<attribute name="IR" value="20A"/>
<attribute name="ISAT" value="28A"/>
<attribute name="LR" value="0.19uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314024 "/>
<attribute name="RDC" value="1mOhm"/>
<attribute name="VALUE" value="0.24uH"/>
</technology>
<technology name="_744314047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314047.pdf"/>
<attribute name="FRES" value="235MHz"/>
<attribute name="IR" value="18A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="LR" value="0.38uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314047 "/>
<attribute name="RDC" value="1.35mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744314076">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314076.pdf"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="15.5A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="LR" value="0.6uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314076 "/>
<attribute name="RDC" value="2.25mOhm"/>
<attribute name="VALUE" value="0.76uH"/>
</technology>
<technology name="_744314101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314101.pdf"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="LR" value="7.5uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314101 "/>
<attribute name="RDC" value="33mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744314110">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314110.pdf"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="LR" value="0.78uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314110 "/>
<attribute name="RDC" value="3.15mOhm"/>
<attribute name="VALUE" value="1.1uH"/>
</technology>
<technology name="_744314150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314150.pdf"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="13A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="LR" value="1.1uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314150 "/>
<attribute name="RDC" value="4.3mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744314200">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314200.pdf"/>
<attribute name="FRES" value="68MHz"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="LR" value="1.35uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314200 "/>
<attribute name="RDC" value="5.85mOhm"/>
<attribute name="VALUE" value="2uH"/>
</technology>
<technology name="_744314330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314330.pdf"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="LR" value="2.2uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314330 "/>
<attribute name="RDC" value="9mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744314490">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314490.pdf"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="LR" value="3.4uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314490 "/>
<attribute name="RDC" value="14.5mOhm"/>
<attribute name="VALUE" value="4.9uH"/>
</technology>
<technology name="_744314650">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314650.pdf"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="LR" value="4.5uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314650 "/>
<attribute name="RDC" value="21.5mOhm"/>
<attribute name="VALUE" value="6.5uH"/>
</technology>
<technology name="_744314760">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314760.pdf"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="LR" value="6uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314760 "/>
<attribute name="RDC" value="28.2mOhm"/>
<attribute name="VALUE" value="7.6uH"/>
</technology>
<technology name="_744314850">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744314850.pdf"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="LR" value="6.8uH"/>
<attribute name="MATERIAL" value="Superflux"/>
<attribute name="PART-NUMBER" value=" 744314850 "/>
<attribute name="RDC" value="30.5mOhm"/>
<attribute name="VALUE" value="8.5uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
