<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-HCMD&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-10-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HCMD_0910">
</package>
<package name="WE-HCMD_1111">
</package>
</packages>
<symbols>
<symbol name="WE-HCMD">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HCMD_0910" prefix="L">
<description>&lt;b&gt;WE-HCMD High Current Inductor for TLVR Applications&lt;br&gt;
Shielded
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Saturation current up to 190 A
&lt;br&gt;Able to perform up to 125 °C
&lt;br&gt;AEC-Q200
&lt;br&gt;Low Rdc up to 125uΩ
&lt;br&gt;MnZn material, low core losses
&lt;br&gt;Coupling factor up to 0.96

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;TLVR topology
&lt;br&gt;Multiphase voltage regulators
&lt;br&gt;CPU motherboards
&lt;br&gt;Servers
&lt;br&gt;FPGA
&lt;br&gt;Internet switches
&lt;br&gt;High power ASIC applications

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o820933v209%20MODEL-WE-HCMD-7443000x1x070.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o820933v209%20MODEL-WE-HCMD-7443000x1x070.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-HCMD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-10-25 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCMD"/>
</gates>
<devices>
<device name="" package="WE-HCMD_0910">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7443000910070">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443000910070?ae"/>
<attribute name="HEIGHT" value="10.2mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="166A"/>
<attribute name="LENGTH" value="9.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443000910070 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value="0910"/>
<attribute name="VALUE" value="0.07uH"/>
<attribute name="WIDTH" value="6.1mm"/>
</technology>
<technology name="_7443000910100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443000910100?ae"/>
<attribute name="HEIGHT" value="10.2mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="117A"/>
<attribute name="LENGTH" value="9.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443000910100 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value="0910"/>
<attribute name="VALUE" value="0.1uH"/>
<attribute name="WIDTH" value="6.1mm"/>
</technology>
<technology name="_7443000910120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443000910120?ae"/>
<attribute name="HEIGHT" value="10.2mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="98A"/>
<attribute name="LENGTH" value="9.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443000910120 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value="0910"/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="6.1mm"/>
</technology>
<technology name="_7443000910150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443000910150?ae"/>
<attribute name="HEIGHT" value="10.2mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="79A"/>
<attribute name="LENGTH" value="9.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443000910150 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value="0910"/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="6.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HCMD_1111" prefix="L">
<description>&lt;b&gt;WE-HCMD High Current Inductor for TLVR Applications&lt;br&gt;
Shielded
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Saturation current up to 190 A
&lt;br&gt;Able to perform up to 125 °C
&lt;br&gt;AEC-Q200
&lt;br&gt;Low Rdc up to 125uΩ
&lt;br&gt;MnZn material, low core losses
&lt;br&gt;Coupling factor up to 0.96

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;TLVR topology
&lt;br&gt;Multiphase voltage regulators
&lt;br&gt;CPU motherboards
&lt;br&gt;Servers
&lt;br&gt;FPGA
&lt;br&gt;Internet switches
&lt;br&gt;High power ASIC applications

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o820933v209%20MODEL-WE-HCMD-7443000x1x070.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o820933v209%20MODEL-WE-HCMD-7443000x1x070.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HCMD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-HCMD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-10-25 &lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HCMD"/>
</gates>
<devices>
<device name="" package="WE-HCMD_1111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7443001111070">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443001111070?ae"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="190A"/>
<attribute name="LENGTH" value="11.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443001111070 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value=" 1111 "/>
<attribute name="VALUE" value="0.07uH"/>
<attribute name="WIDTH" value="5.7mm"/>
</technology>
<technology name="_7443001111105">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443001111105?ae"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="142A"/>
<attribute name="LENGTH" value="11.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443001111105 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value=" 1111 "/>
<attribute name="VALUE" value="0.105uH"/>
<attribute name="WIDTH" value="5.7mm"/>
</technology>
<technology name="_7443001111120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443001111120?ae"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="122A"/>
<attribute name="LENGTH" value="11.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443001111120 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value=" 1111 "/>
<attribute name="VALUE" value="0.12uH"/>
<attribute name="WIDTH" value="5.7mm"/>
</technology>
<technology name="_7443001111150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443001111150?ae"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="99A"/>
<attribute name="LENGTH" value="11.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443001111150 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value=" 1111 "/>
<attribute name="VALUE" value="0.15uH"/>
<attribute name="WIDTH" value="5.7mm"/>
</technology>
<technology name="_7443001111180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443001111180?ae"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="82A"/>
<attribute name="LENGTH" value="11.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443001111180 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value=" 1111 "/>
<attribute name="VALUE" value="0.18uH"/>
<attribute name="WIDTH" value="5.7mm"/>
</technology>
<technology name="_7443001111200">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443001111200?ae"/>
<attribute name="HEIGHT" value="11mm"/>
<attribute name="IRP" value="78A"/>
<attribute name="ISAT" value="76A"/>
<attribute name="LENGTH" value="11.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443001111200 "/>
<attribute name="RDC" value="0.125mohm"/>
<attribute name="RDC-MAX" value="0.1375mohm"/>
<attribute name="SIZE" value=" 1111 "/>
<attribute name="VALUE" value="0.2uH"/>
<attribute name="WIDTH" value="5.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
