<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-HEPC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-06-19&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HEPC_6030">
<description>&lt;B&gt;WE-HEPC SMT Power Inductor
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Size 6030, SMT, 2pins
&lt;br&gt;LxWxH=5.9x5.9x2.85mm</description>
</package>
<package name="WE-HEPC_5030">
<description>&lt;B&gt;WE-HEPC SMT Power Inductor
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Size 5030, SMT, 2pins
&lt;br&gt;LxWxH=4.9x4.9x2.85mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HEPC_6030" prefix="L">
<description>&lt;b&gt;WE-HEPC SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Magnetically shielded
&lt;br&gt;AECQ-200 grade 1 qualified
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Land pattern matching with WE-LQFS, WE-SPC, WE-TPC
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Compact designs
&lt;br&gt;Embedded laptops and PCs
&lt;br&gt;Filter applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o707820v209%20Family%20WE-HEPC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o707820v209%20Family%20WE-HEPC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HEPC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HEPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2024-06-19&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-HEPC_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74408063004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063004?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063004 "/>
<attribute name="RDC" value="70mohm"/>
<attribute name="RDC-MAX" value="90mohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74408063006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063006?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063006 "/>
<attribute name="RDC" value="80mohm"/>
<attribute name="RDC-MAX" value="100mohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74408063100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063100?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063100 "/>
<attribute name="RDC" value="125mohm"/>
<attribute name="RDC-MAX" value="140mohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74408063101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063101?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063101 "/>
<attribute name="RDC" value="800mohm"/>
<attribute name="RDC-MAX" value="850mohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74408063150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063150?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063150 "/>
<attribute name="RDC" value="160mohm"/>
<attribute name="RDC-MAX" value="180mohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74408063220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063220?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063220 "/>
<attribute name="RDC" value="200mohm"/>
<attribute name="RDC-MAX" value="220mohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74408063330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063330?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063330 "/>
<attribute name="RDC" value="265mohm"/>
<attribute name="RDC-MAX" value="285mohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74408063470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063470?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063470 "/>
<attribute name="RDC" value="365mohm"/>
<attribute name="RDC-MAX" value="385mohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74408063680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408063680?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408063680 "/>
<attribute name="RDC" value="515mohm"/>
<attribute name="RDC-MAX" value="535mohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HEPC_5030" prefix="L">
<description>&lt;b&gt;WE-HEPC SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;Magnetically shielded
&lt;br&gt;AECQ-200 grade 1 qualified
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Land pattern matching with WE-LQFS, WE-SPC, WE-TPC
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC converter
&lt;br&gt;Compact designs
&lt;br&gt;Embedded laptops and PCs
&lt;br&gt;Filter applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o707820v209%20Family%20WE-HEPC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o707820v209%20Family%20WE-HEPC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-HEPC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-HEPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2024-06-19&lt;br&gt;
&lt;/b&gt;2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-HEPC_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74408053003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408053003?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408053003 "/>
<attribute name="RDC" value="60mohm"/>
<attribute name="RDC-MAX" value="75mohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74408053004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408053004?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408053004 "/>
<attribute name="RDC" value="80mohm"/>
<attribute name="RDC-MAX" value="100mohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74408053006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408053006?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408053006 "/>
<attribute name="RDC" value="105mohm"/>
<attribute name="RDC-MAX" value="125mohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74408053100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408053100?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408053100 "/>
<attribute name="RDC" value="120mohm"/>
<attribute name="RDC-MAX" value="140mohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74408053150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408053150?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408053150 "/>
<attribute name="RDC" value="180mohm"/>
<attribute name="RDC-MAX" value="200mohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74408053220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408053220?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408053220 "/>
<attribute name="RDC" value="250mohm"/>
<attribute name="RDC-MAX" value="270mohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74408053330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408053330?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408053330 "/>
<attribute name="RDC" value="345mohm"/>
<attribute name="RDC-MAX" value="365mohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
