<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-HIDA&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-08-24-&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-HIDA_1480">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 1480</description>
</package>
<package name="WE-HIDA_1415_7444XX1415XXX_15_22">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 1415
&lt;br&gt;Pad diameter = φ0.7mm
&lt;br&gt;Hole diameter = φ1.1mm</description>
</package>
<package name="WE-HIDA_3119_7444XX3119XXX">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 3119
&lt;br&gt;Pad diameter = φ1.6mm
&lt;br&gt;Hole diameter = φ2.0mm</description>
</package>
<package name="WE-HIDA_1521_74441521150">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 1521
&lt;br&gt;Pad diameter = φ0.9mm
&lt;br&gt;Hole diameter = φ1.2mm</description>
</package>
<package name="WE-HIDA_1521_74441521XXX">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 1521
&lt;br&gt;Pad diameter = φ1.0mm
&lt;br&gt;Hole diameter = φ1.3mm</description>
</package>
<package name="WE-HIDA_3119_7444XX3119082">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 3119
&lt;br&gt;Pad diameter = φ1.8mm
&lt;br&gt;Hole diameter = φ2.2mm</description>
</package>
<package name="WE-HIDA_1521_74441521220">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 1521
&lt;br&gt;Pad diameter = φ0.8mm
&lt;br&gt;Hole diameter = φ1.1mm</description>
</package>
<package name="WE-HIDA_1415_7444XX1415XXX_8_10">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 1415
&lt;br&gt;Pad diameter = φ0.8mm
&lt;br&gt;Hole diameter = φ1.2mm</description>
</package>
<package name="WE-HIDA_1715">
<description>&lt;B&gt;WE-HIDA THT High Current Inductor 
&lt;BR&gt;&lt;/B&gt;Size : 1715</description>
</package>
</packages>
<symbols>
<symbol name="WE-HIDA_1415">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-HIDA_1480">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-HIDA_1521">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-HIDA_1715">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-HIDA_3119">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-HIDA_1480" prefix="L">
<description>&lt;b&gt;WE-HIDA THT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;2-in-1 designs with low magnetic coupling 
&lt;br&gt;Low core losses 
&lt;br&gt;Very low RDC 
&lt;br&gt;High saturation currents 
&lt;br&gt;Operating temperature: -40°C to +125°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Class D audio amplifiers 
&lt;br&gt;Digital amplifiers 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HIDA/"&gt;https://www.we-online.com/catalog/en/WE-HIDA/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu  2021-08-24&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HIDA_1480"/>
</gates>
<devices>
<device name="" package="WE-HIDA_1480">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_7444011480082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011480082.pdf"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011480082"/>
<attribute name="RDC-TYPE" value="9mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7444011480100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011480100.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011480100"/>
<attribute name="RDC-TYPE" value="9mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7444011480150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011480150.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011480150"/>
<attribute name="RDC-TYPE" value="10mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7444011480220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011480220.pdf"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011480220"/>
<attribute name="RDC-TYPE" value="10mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HIDA_3119" prefix="L">
<description>&lt;b&gt;WE-HIDA THT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;2-in-1 designs with low magnetic coupling 
&lt;br&gt;Low core losses 
&lt;br&gt;Very low RDC 
&lt;br&gt;High saturation currents 
&lt;br&gt;Operating temperature: -40°C to +125°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Class D audio amplifiers 
&lt;br&gt;Digital amplifiers 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HIDA/"&gt;https://www.we-online.com/catalog/en/WE-HIDA/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-12-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HIDA_3119"/>
</gates>
<devices>
<device name="_7444XX3119XXX" package="WE-HIDA_3119_7444XX3119XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7444013119100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444013119100.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="58A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444013119100"/>
<attribute name="RDC-TYPE" value="4.8mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7444013119150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444013119150.pdf"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="41A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444013119150"/>
<attribute name="RDC-TYPE" value="4.8mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7444013119220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444013119220.pdf"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="33A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444013119220"/>
<attribute name="RDC-TYPE" value="5.3mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
<device name="_7444013119082" package="WE-HIDA_3119_7444XX3119082">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444013119082.pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="52A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444013119082"/>
<attribute name="RDC-TYPE" value="2.5mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HIDA_1521" prefix="L">
<description>&lt;b&gt;WE-HIDA THT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;2-in-1 designs with low magnetic coupling 
&lt;br&gt;Low core losses 
&lt;br&gt;Very low RDC 
&lt;br&gt;High saturation currents 
&lt;br&gt;Operating temperature: -40°C to +125°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Class D audio amplifiers 
&lt;br&gt;Digital amplifiers 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HIDA/"&gt;https://www.we-online.com/catalog/en/WE-HIDA/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-12-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HIDA_1521"/>
</gates>
<devices>
<device name="_74441521XXX" package="WE-HIDA_1521_74441521XXX">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_74441521082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74441521082.pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="17.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74441521082 "/>
<attribute name="RDC-TYPE" value="6.2mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74441521100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74441521100.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74441521100 "/>
<attribute name="RDC-TYPE" value="6.3mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_74441521150" package="WE-HIDA_1521_74441521150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74441521150.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74441521150 "/>
<attribute name="RDC-TYPE" value="8.5mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
</technologies>
</device>
<device name="_74441521220" package="WE-HIDA_1521_74441521220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/74441521220.pdf"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74441521220 "/>
<attribute name="RDC-TYPE" value="13.6mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HIDA_1415" prefix="L">
<description>&lt;b&gt;WE-HIDA THT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;2-in-1 designs with low magnetic coupling 
&lt;br&gt;Low core losses 
&lt;br&gt;Very low RDC 
&lt;br&gt;High saturation currents 
&lt;br&gt;Operating temperature: -40°C to +125°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Class D audio amplifiers 
&lt;br&gt;Digital amplifiers 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HIDA/"&gt;https://www.we-online.com/catalog/en/WE-HIDA/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-12-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HIDA_1415"/>
</gates>
<devices>
<device name="_8_10" package="WE-HIDA_1415_7444XX1415XXX_8_10">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7444211415082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444211415082.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444211415082"/>
<attribute name="RDC-TYPE" value="9.2mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7444211415100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444211415100.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="12.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444211415100"/>
<attribute name="RDC-TYPE" value="9.2mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_15_22" package="WE-HIDA_1415_7444XX1415XXX_15_22">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7444211415150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444211415150.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444211415150"/>
<attribute name="RDC-TYPE" value="14.6mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7444211415220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444211415220.pdf"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="5.7A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444211415220"/>
<attribute name="RDC-TYPE" value="14.8mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-HIDA_1715" prefix="L">
<description>&lt;b&gt;WE-HIDA THT High Current Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;2-in-1 designs with low magnetic coupling 
&lt;br&gt;Low core losses 
&lt;br&gt;Very low RDC 
&lt;br&gt;High saturation currents 
&lt;br&gt;Operating temperature: -40°C to +125°C 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Class D audio amplifiers 
&lt;br&gt;Digital amplifiers 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o160187v209%20Family_WE-HIDA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-HIDA/"&gt;https://www.we-online.com/catalog/en/WE-HIDA/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Ella Wu  2019-12-05&lt;br&gt;
&lt;/b&gt;2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-HIDA_1715"/>
</gates>
<devices>
<device name="" package="WE-HIDA_1715">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
</connects>
<technologies>
<technology name="_7444011715082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011715082.pdf"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="34A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011715082"/>
<attribute name="RDC-TYPE" value="7mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7444011715100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011715100.pdf"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="28A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011715100"/>
<attribute name="RDC-TYPE" value="7mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7444011715150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011715150.pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011715150"/>
<attribute name="RDC-TYPE" value="7mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7444011715220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/7444011715220.pdf"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value="7444011715220"/>
<attribute name="RDC-TYPE" value="7mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
