<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For DC/DC Converter - WE-IBTI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-06-07&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-IBTI_EP7_L9.78W9.5H10.54">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP7,SMT,8pins
&lt;br&gt;LXWXH=9.78X9.5X10.54mm</description>
</package>
<package name="WE-IBTI_ER9.5S_L10W14H5">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ER9.5S,SMT,8pins
&lt;br&gt;LXWXH=10X14X5mm</description>
</package>
<package name="WE-IBTI_EFD20_L23.11W29.08H11.43">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EFD20,SMT,12pins
&lt;br&gt;LXWXH=23.11X29.08X11.43mm</description>
</package>
<package name="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ER11.5,SMT,12pins
&lt;br&gt;LXWXH=12.95X12.7X5.98mm</description>
</package>
<package name="WE-IBTI_EE16/8/5_L17.96W20.3H14.3">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/8/5,THT,8pins
&lt;br&gt;LXWXH=17.96X20.3X14.3mm</description>
</package>
<package name="WE-IBTI_EP10_L13.34W15.2411.43">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP10,SMT,8pins
&lt;br&gt;LXWXH=13.34X15.24X11.43mm</description>
</package>
<package name="WE-IBTI_EE16/8/5_L17.78W26.9H13.8">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/8/5,SMT,12pins
&lt;br&gt;LWWH=17.78X26.9X13.8mm</description>
</package>
<package name="WE-IBTI_EE20/10/6_L22.2W25H16_12PINS">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EE20/10/6,THT,12pins
&lt;br&gt;LXWXH=22.2X25X16mm</description>
</package>
<package name="WE-IBTI_EP13_L13.46W17.75H12.7">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP13,SMT,10pins
&lt;br&gt;LXWXH=13.46X17.75X12.7mm</description>
</package>
<package name="WE-IBTI_EP13_L13.97W15.37H12.7">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP13,THT,12pins
&lt;br&gt;LXWXH=13.97X15.37X12.7mm</description>
</package>
<package name="WE-IBTI_EP7_L10.16W13.36H8.64">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP7,SMT,6pins
&lt;br&gt;LXWXH=10.16X13.36X8.64mm</description>
</package>
<package name="WE-IBTI_EP10_L12.4W13.813.6">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP10,SMT,8pins
&lt;br&gt;LXWXH=12.4X13.8X13.6mm</description>
</package>
<package name="WE-IBTI_PQ2020_L23.36W23.88H24.14">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: PQ2020,THT,10pins
&lt;br&gt;LXWXH=23.36X23.88X24.14mm</description>
</package>
<package name="WE-IBTI_EE20/10/6_L22.2W25H16_14PINS">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EE20/10/6,THT,14pins
&lt;br&gt;LXWXH=22.2X25X16mm</description>
</package>
<package name="WE-IBTI_EP5_L8.35W9.5H6.35">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers 
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP5,SMT,8pins
&lt;br&gt;LXWXH=8.35X9.5X6.35mm</description>
</package>
<package name="WE-IBTI_EE16/8/5_L20.32W24.38H16">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/8/5,THT,9pins
&lt;br&gt;LXWXH=20.32X24.38X16mm</description>
</package>
<package name="WE-IBTI_EP5_L6.6W8.26H5.59">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EP5,SMT,6pins
&lt;br&gt;LXWXH=6.6X8.26X5.59mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-IBTI_EP7_1W:1W_750312547">
<pin name="1+2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3+4" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_ER9.5S_1W:2W">
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EE16/8/5_2W:1W_PARALLEL">
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP7_1W:1W_750315703">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EE20/10/6_2W:4W_PARALLEL_CENTERTAP">
<pin name="13" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EFD20_2W:3W_PARALLEL">
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EE16/8/5_2W:4W_CENTERTAP">
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_ER11.5_1W:3W">
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP10_1W:2W">
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP7_1W:2W">
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_ER11.5_1W:4W_CENTERTAP">
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_ER9.5S_1W:1W">
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP7_1W:1W_750314597">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP13_1W:4W">
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="9" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_PQ2020_1W:4W">
<pin name="6" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="13" direction="pas"/>
<pin name="14" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_ER11.5_1W:3W_750315853">
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP13_2W:4W_PARALLEL">
<pin name="14" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="16" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP7_1W:3W_CENTERTAP">
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP10_1W:1W">
<pin name="3" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP7_1W:1W">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP5_1W:2W">
<pin name="3" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EE20/10/6_2W:3W_PARALLEL">
<pin name="2" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="14" direction="pas"/>
<pin name="13" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP5_1W:1W">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_ER11.5_2W:3W_CENTERTAP">
<pin name="5" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EP10_2W:1W_PARALLEL">
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-IBTI_EE16/8/5_2W:2W_CENTERTAP">
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750315703" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:1W_750315703"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L9.78W9.5H10.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315703?ae"/>
<attribute name="FSWITCH" value="200kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="0.5A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="25uH"/>
<attribute name="LENGTH" value="9.78mm"/>
<attribute name="LS" value="380nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750315703 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315703 "/>
<attribute name="VBUCK" value="4.5V"/>
<attribute name="VIN" value="5 - 15 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="2500V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315547" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:1W_750312547"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L9.78W9.5H10.54">
<connects>
<connect gate="G$1" pin="1+2" pad="1 2"/>
<connect gate="G$1" pin="3+4" pad="3 4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315547?ae"/>
<attribute name="FSWITCH" value="300kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="0.1A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L" value="42uH"/>
<attribute name="LENGTH" value="9.78mm"/>
<attribute name="LS" value="800nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.2"/>
<attribute name="PART-NUMBER" value=" 750315547 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750315547 "/>
<attribute name="VBUCK" value="3.3V"/>
<attribute name="VIN" value="12 - 48 V (DC)"/>
<attribute name="VOUT1" value="3.6V"/>
<attribute name="VT" value="2500V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314952" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L9.78W9.5H10.54">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314952?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="0.15A"/>
<attribute name="L" value="2500uH"/>
<attribute name="LENGTH" value="9.78mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.25"/>
<attribute name="PART-NUMBER" value=" 750314952 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750314952 "/>
<attribute name="VBUCK" value="3.3V"/>
<attribute name="VIN" value="10 - 40 V (DC)"/>
<attribute name="VOUT1" value="3.3V"/>
<attribute name="VT" value="2000V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311780" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L9.78W9.5H10.54">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311780?ae"/>
<attribute name="FSWITCH" value="500kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="0.2A"/>
<attribute name="IOUT2" value="0.2A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="L" value="2uH"/>
<attribute name="LENGTH" value="9.78mm"/>
<attribute name="LS" value="200nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:8:8"/>
<attribute name="PART-NUMBER" value=" 750311780 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311780 "/>
<attribute name="VIN" value="2.5 - 3.5 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="15V"/>
<attribute name="VT" value="2000V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316170" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:3W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L9.78W9.5H10.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316170?ae"/>
<attribute name="FSWITCH" value="400kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="0.01A"/>
<attribute name="IOUT2" value="0.01A"/>
<attribute name="IOUT3" value="0.1A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="L" value="2.7uH"/>
<attribute name="LENGTH" value="9.78mm"/>
<attribute name="LS" value="500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:8:8:3"/>
<attribute name="PART-NUMBER" value=" 750316170 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750316170 "/>
<attribute name="VBUCK" value="2.17V"/>
<attribute name="VIN" value="3.5 - 5.5 V (DC)"/>
<attribute name="VOUT1" value="13.5V"/>
<attribute name="VOUT2" value="-13.5V"/>
<attribute name="VOUT3" value="5V"/>
<attribute name="VT" value="1875V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312547" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L9.78W9.5H10.54">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312547?ae"/>
<attribute name="FSWITCH" value="500kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="0.2A"/>
<attribute name="L" value="1uH"/>
<attribute name="L1" value="1uH"/>
<attribute name="LENGTH" value="9.78mm"/>
<attribute name="LS" value="70nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.4"/>
<attribute name="PART-NUMBER" value=" 750312547 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750312547 "/>
<attribute name="VIN" value="3 - 6 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315249" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER9.5S_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER9.5S_L10W14H5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315249?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IOUT1" value="50mA"/>
<attribute name="IOUT2" value="50mA"/>
<attribute name="ISAT" value="0.92A"/>
<attribute name="L" value="30uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="900nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.5:1.5"/>
<attribute name="PART-NUMBER" value=" 750315249 "/>
<attribute name="SIZE" value="ER9.5S"/>
<attribute name="VALUE" value=" 750315249 "/>
<attribute name="VBUCK" value="10.4V"/>
<attribute name="VIN" value="20 - 30 V (DC)"/>
<attribute name="VOUT1" value="-15V"/>
<attribute name="VOUT2" value="15V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315144" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER9.5S_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER9.5S_L10W14H5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315144?ae"/>
<attribute name="FSWITCH" value="300kHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IOUT1" value="30mA"/>
<attribute name="IOUT2" value="45mA"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="80uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="2100nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2:2"/>
<attribute name="PART-NUMBER" value=" 750315144 "/>
<attribute name="SIZE" value="ER9.5S"/>
<attribute name="VALUE" value=" 750315144 "/>
<attribute name="VBUCK" value="9V"/>
<attribute name="VIN" value="12 - 36 V (DC)"/>
<attribute name="VOUT1" value="-17.5V"/>
<attribute name="VOUT2" value="17.5V"/>
<attribute name="VT" value="490V(AC)"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315246" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER9.5S_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER9.5S_L10W14H5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315246?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IOUT1" value="200mA"/>
<attribute name="ISAT" value="0.96A"/>
<attribute name="L" value="26uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="650nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.09"/>
<attribute name="PART-NUMBER" value=" 750315246 "/>
<attribute name="SIZE" value="ER9.5S"/>
<attribute name="VALUE" value=" 750315246 "/>
<attribute name="VBUCK" value="5V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315250" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER9.5S_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER9.5S_L10W14H5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315250?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="30uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="825nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1:1"/>
<attribute name="PART-NUMBER" value=" 750315250 "/>
<attribute name="SIZE" value="ER9.5S"/>
<attribute name="VALUE" value=" 750315250 "/>
<attribute name="VBUCK" value="11V"/>
<attribute name="VIN" value="20 - 30 V (DC)"/>
<attribute name="VOUT1" value="-5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314463" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_1W:3W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314463?ae"/>
<attribute name="FSWITCH" value="200 - 350kHz"/>
<attribute name="HEIGHT" value="5.98mm"/>
<attribute name="IOUT1" value="20mA"/>
<attribute name="IOUT2" value="40mA"/>
<attribute name="IOUT3" value="40mA"/>
<attribute name="ISAT" value="0.96A"/>
<attribute name="L" value="45uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="LS" value="450nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.36:1.16:1.16"/>
<attribute name="PART-NUMBER" value=" 750314463 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750314463 "/>
<attribute name="VBUCK" value="13V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VOUT3" value="-12V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315039" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EFD20_2W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EFD20_L23.11W29.08H11.43">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315039?ae"/>
<attribute name="FSWITCH" value="250kHz"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="IOUT1" value="1000mA"/>
<attribute name="IOUT2" value="200mA"/>
<attribute name="IOUT3" value="200mA"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L" value="40uH"/>
<attribute name="LENGTH" value="23.11mm"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.43:1:2.86:2.86"/>
<attribute name="PART-NUMBER" value=" 750315039 "/>
<attribute name="SIZE" value="EFD20"/>
<attribute name="VALUE" value=" 750315039 "/>
<attribute name="VBUCK" value="7.65V"/>
<attribute name="VIN" value="19 - 30 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="15V"/>
<attribute name="VOUT3" value="15V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="29.08mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314442" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_1W:4W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314442?ae"/>
<attribute name="FSWITCH" value="200 - 350kHz"/>
<attribute name="HEIGHT" value="5.98mm"/>
<attribute name="IOUT1" value="25mA"/>
<attribute name="IOUT2" value="80mA"/>
<attribute name="IOUT3" value="80mA"/>
<attribute name="IOUT4" value="25mA"/>
<attribute name="ISAT" value="0.78A"/>
<attribute name="L" value="45uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="LS" value="930nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2.08:2:1:2:1"/>
<attribute name="PART-NUMBER" value=" 750314442 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750314442 "/>
<attribute name="VBUCK" value="13V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="10V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="-5V"/>
<attribute name="VOUT4" value="-10V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314460" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_1W:4W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314460?ae"/>
<attribute name="FSWITCH" value="200 - 350kHz"/>
<attribute name="HEIGHT" value="5.98mm"/>
<attribute name="IOUT1" value="30mA"/>
<attribute name="IOUT2" value="30mA"/>
<attribute name="IOUT3" value="80mA"/>
<attribute name="IOUT4" value="80mA"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="45uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="LS" value="910nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.79:2.29:2.29:1:1"/>
<attribute name="PART-NUMBER" value=" 750314460 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750314460 "/>
<attribute name="VBUCK" value="13V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VOUT3" value="-5V"/>
<attribute name="VOUT4" value="-5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314459" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_1W:4W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314459?ae"/>
<attribute name="FSWITCH" value="200 - 350kHz"/>
<attribute name="HEIGHT" value="5.98mm"/>
<attribute name="IOUT1" value="30mA"/>
<attribute name="IOUT2" value="80mA"/>
<attribute name="IOUT3" value="80mA"/>
<attribute name="IOUT4" value="30mA"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="45uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="LS" value="1000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.79:1.29:1:1.29:1"/>
<attribute name="PART-NUMBER" value=" 750314459 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750314459 "/>
<attribute name="VBUCK" value="13V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="7V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="-5V"/>
<attribute name="VOUT4" value="-7V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315856" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_1W:3W_750315853"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315856?ae"/>
<attribute name="FSWITCH" value="250kHz"/>
<attribute name="HEIGHT" value="6.35mm"/>
<attribute name="IOUT1" value="40mA"/>
<attribute name="IOUT2" value="50mA"/>
<attribute name="IOUT3" value="20mA"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="L" value="120uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="LS" value="5000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1 : 3 : 0.56 : 0.56"/>
<attribute name="PART-NUMBER" value=" 750315856 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750315856 "/>
<attribute name="VBUCK" value="9V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="27V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="-5V"/>
<attribute name="VT" value="625V(AC)"/>
<attribute name="WIDTH" value="12.85mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315245" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER9.5S_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER9.5S_L10W14H5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315245?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IOUT1" value="200mA"/>
<attribute name="ISAT" value="0.96A"/>
<attribute name="L" value="30uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="750nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750315245 "/>
<attribute name="SIZE" value="ER9.5S"/>
<attribute name="VALUE" value=" 750315245 "/>
<attribute name="VBUCK" value="5.5V"/>
<attribute name="VIN" value="20 - 30 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315248" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER9.5S_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER9.5S_L10W14H5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315248?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="ISAT" value="0.96A"/>
<attribute name="L" value="30uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="750nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1:1"/>
<attribute name="PART-NUMBER" value=" 750315248 "/>
<attribute name="SIZE" value="ER9.5S"/>
<attribute name="VALUE" value=" 750315248 "/>
<attribute name="VBUCK" value="5.5V"/>
<attribute name="VIN" value="20 - 30 V (DC)"/>
<attribute name="VOUT1" value="-5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750311880" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L9.78W9.5H10.54">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750311880?ae"/>
<attribute name="FSWITCH" value="200 - 600kHz"/>
<attribute name="HEIGHT" value="10.54mm"/>
<attribute name="IOUT1" value="0.2A"/>
<attribute name="ISAT" value="12A"/>
<attribute name="L" value="2.5uH"/>
<attribute name="L1" value="2.5uH"/>
<attribute name="LENGTH" value="9.78mm"/>
<attribute name="LS" value="125nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2.5"/>
<attribute name="PART-NUMBER" value=" 750311880 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750311880 "/>
<attribute name="VIN" value="3 - 6 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="2500V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315247" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER9.5S_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER9.5S_L10W14H5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315247?ae"/>
<attribute name="FSWITCH" value="350kHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="ISAT" value="0.88A"/>
<attribute name="L" value="30uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="LS" value="825nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value=" 750315247 "/>
<attribute name="SIZE" value="ER9.5S"/>
<attribute name="VALUE" value=" 750315247 "/>
<attribute name="VBUCK" value="7.8V"/>
<attribute name="VIN" value="20 - 30 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="14mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314462" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_1W:3W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314462?ae"/>
<attribute name="FSWITCH" value="200 - 350kHz"/>
<attribute name="HEIGHT" value="5.98mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="40mA"/>
<attribute name="IOUT3" value="40mA"/>
<attribute name="ISAT" value="0.98A"/>
<attribute name="L" value="45uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="LS" value="450nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.92:1:2.38:2.38"/>
<attribute name="PART-NUMBER" value=" 750314462 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750314462 "/>
<attribute name="VBUCK" value="13V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VOUT3" value="-12V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315393" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EE16/8/5_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EE16/8/5_L17.96W20.3H14.3">
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315393?ae"/>
<attribute name="FSWITCH" value="600kHz"/>
<attribute name="HEIGHT" value="14.3mm"/>
<attribute name="IOUT1" value="600mA"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L" value="37.5uH"/>
<attribute name="LENGTH" value="17.96mm"/>
<attribute name="LS" value="400nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="1:3"/>
<attribute name="PART-NUMBER" value=" 750315393 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 750315393 "/>
<attribute name="VBUCK" value="4.2V"/>
<attribute name="VIN" value="11.8 - 13.2 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="20.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342156" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP10_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP10_L13.34W15.2411.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="3"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342156?ae"/>
<attribute name="FSWITCH" value="600kHz"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="IOUT1" value="600mA"/>
<attribute name="IOUT2" value="600mA"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="L" value="66uH"/>
<attribute name="LENGTH" value="13.34mm"/>
<attribute name="LS" value="1500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750342156 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750342156 "/>
<attribute name="VIN" value="15 - 40 V (DC)"/>
<attribute name="VOUT1" value="12.7V"/>
<attribute name="VOUT2" value="12.7V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="15.24mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342206" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_2W:3W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342206?ae"/>
<attribute name="FSWITCH" value="200 - 400kHz"/>
<attribute name="HEIGHT" value="6.35mm"/>
<attribute name="IOUT1" value="150mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="IOUT3" value="150mA"/>
<attribute name="L" value="50uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2 : 3 : 1 : 3.2 : 1"/>
<attribute name="PART-NUMBER" value=" 750342206 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750342206 "/>
<attribute name="VAUX" value="5V"/>
<attribute name="VIN" value="18 - 24 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="15V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.85mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314225" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP10_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP10_L13.34W15.2411.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314225?ae"/>
<attribute name="FSWITCH" value="250 - 600kHz"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="IOUT1" value="250mA"/>
<attribute name="IOUT2" value="250mA"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="L" value="50uH"/>
<attribute name="LENGTH" value="13.34mm"/>
<attribute name="LS" value="800nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.5:1"/>
<attribute name="PART-NUMBER" value=" 750314225 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750314225 "/>
<attribute name="VBUCK" value="7.8V"/>
<attribute name="VIN" value="15 - 40 V (DC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="15.24mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314226" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP10_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP10_L13.34W15.2411.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314226?ae"/>
<attribute name="FSWITCH" value="250 - 600kHz"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="IOUT1" value="150mA"/>
<attribute name="IOUT2" value="150mA"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="33.8uH"/>
<attribute name="LENGTH" value="13.34mm"/>
<attribute name="LS" value="150nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:1"/>
<attribute name="PART-NUMBER" value=" 750314226 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750314226 "/>
<attribute name="VBUCK" value="7.8V"/>
<attribute name="VIN" value="15 - 40 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="15V"/>
<attribute name="VT" value="1875V(AC)"/>
<attribute name="WIDTH" value="15.24mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315811" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP10_2W:1W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP10_L13.34W15.2411.43">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315811?ae"/>
<attribute name="FSWITCH" value="300kHz"/>
<attribute name="HEIGHT" value="11.43mm"/>
<attribute name="IOUT1" value="830mA"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="13.34mm"/>
<attribute name="LS" value="1700nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750315811 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750315811 "/>
<attribute name="VBUCK" value="12V"/>
<attribute name="VIN" value="36 - 72 V (DC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="15.24mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314461" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_ER11.5_1W:3W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_ER11.5_L12.95W12.7H5.98">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314461?ae"/>
<attribute name="FSWITCH" value="200 - 350kHz"/>
<attribute name="HEIGHT" value="5.98mm"/>
<attribute name="IOUT1" value="33mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="IOUT3" value="100mA"/>
<attribute name="ISAT" value="0.96A"/>
<attribute name="L" value="45uH"/>
<attribute name="LENGTH" value="12.95mm"/>
<attribute name="LS" value="400nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.92:3:1:1"/>
<attribute name="PART-NUMBER" value=" 750314461 "/>
<attribute name="SIZE" value="ER11.5"/>
<attribute name="VALUE" value=" 750314461 "/>
<attribute name="VBUCK" value="13V"/>
<attribute name="VIN" value="16 - 36 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="-5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="12.7mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314624" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EE20/10/6_2W:4W_PARALLEL_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EE20/10/6_L22.2W25H16_12PINS">
<connects>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314624?ae"/>
<attribute name="FSWITCH" value="250 - 600kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="IOUT3" value="100mA"/>
<attribute name="IOUT4" value="100mA"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="LS" value="800nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="1.08:1:1.75:1:1.75"/>
<attribute name="PART-NUMBER" value=" 750314624 "/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value=" 750314624 "/>
<attribute name="VBUCK" value="10.3V"/>
<attribute name="VIN" value="17 - 35 V (DC)"/>
<attribute name="VOUT1" value="9V"/>
<attribute name="VOUT2" value="16V"/>
<attribute name="VOUT3" value="9V"/>
<attribute name="VOUT4" value="16V"/>
<attribute name="VT" value="5000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314851" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EE16/8/5_2W:4W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EE16/8/5_L17.78W26.9H13.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314851?ae"/>
<attribute name="FSWITCH" value="300kHz"/>
<attribute name="HEIGHT" value="13.8mm"/>
<attribute name="IOUT1" value="100mA"/>
<attribute name="IOUT2" value="50mA"/>
<attribute name="IOUT3" value="50mA"/>
<attribute name="IOUT4" value="50mA"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L" value="68uH"/>
<attribute name="LENGTH" value="17.78mm"/>
<attribute name="LS" value="1200nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.83:1.67:1:1.67:1"/>
<attribute name="PART-NUMBER" value=" 750314851 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 750314851 "/>
<attribute name="VBUCK" value="10.2V"/>
<attribute name="VIN" value="14 - 40 V (DC)"/>
<attribute name="VOUT1" value="14V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="14V"/>
<attribute name="VOUT4" value="5V"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="26.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750313995" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP13_1W:4W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP13_L13.46W17.75H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750313995?ae"/>
<attribute name="FSWITCH" value="300 - 600kHz"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IOUT1" value="50mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="IOUT3" value="100mA"/>
<attribute name="IOUT4" value="50mA"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="50uH"/>
<attribute name="LENGTH" value="13.46mm"/>
<attribute name="LS" value="260nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1.5:1:1:2:2"/>
<attribute name="PART-NUMBER" value=" 750313995 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750313995 "/>
<attribute name="VBUCK" value="7.8V"/>
<attribute name="VIN" value="15 - 40 V (DC)"/>
<attribute name="VOUT1" value="15V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="5V"/>
<attribute name="VOUT4" value="15V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="17.75mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750317963" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP13_2W:4W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP13_L13.97W15.37H12.7">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="16" pad="16"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750317963?ae"/>
<attribute name="FSWITCH" value="220 - 350kHz"/>
<attribute name="HEIGHT" value="12.7mm"/>
<attribute name="IOUT1" value="60mA"/>
<attribute name="IOUT2" value="60mA"/>
<attribute name="IOUT3" value="60mA"/>
<attribute name="IOUT4" value="60mA"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="13.97mm"/>
<attribute name="LS" value="200nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="0.5:1:1:1:1"/>
<attribute name="PART-NUMBER" value=" 750317963 "/>
<attribute name="SIZE" value="EP13"/>
<attribute name="VALUE" value=" 750317963 "/>
<attribute name="VIN" value="18 - 60 V (DC)"/>
<attribute name="VOUT1" value="25V"/>
<attribute name="VOUT2" value="25V"/>
<attribute name="VOUT3" value="25V"/>
<attribute name="VOUT4" value="25V"/>
<attribute name="VT" value="1000V(AC)"/>
<attribute name="WIDTH" value="15.37mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750314597" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP7_1W:1W_750314597"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP7_L10.16W13.36H8.64">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750314597?ae"/>
<attribute name="FSWITCH" value="150kHz"/>
<attribute name="HEIGHT" value="8.64mm"/>
<attribute name="IOUT1" value="0.25A"/>
<attribute name="ISAT" value="0.84A"/>
<attribute name="L" value="60uH"/>
<attribute name="LENGTH" value="10.16mm"/>
<attribute name="LS" value="1200nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1.5"/>
<attribute name="PART-NUMBER" value=" 750314597 "/>
<attribute name="SIZE" value="EP7"/>
<attribute name="VALUE" value=" 750314597 "/>
<attribute name="VBUCK" value="8V"/>
<attribute name="VIN" value="10 - 40 V (DC)"/>
<attribute name="VOUT1" value="15.5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="13.36mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750344207" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP10_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP10_L12.4W13.813.6">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750344207?ae"/>
<attribute name="FSWITCH" value="600kHz"/>
<attribute name="HEIGHT" value="13.6mm"/>
<attribute name="IOUT1" value="50mA"/>
<attribute name="L" value="150uH"/>
<attribute name="LENGTH" value="12.4mm"/>
<attribute name="LS" value="3400nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750344207 "/>
<attribute name="SIZE" value="EP10"/>
<attribute name="VALUE" value=" 750344207 "/>
<attribute name="VBUCK" value="9V"/>
<attribute name="VIN" value="36 - 75 V (DC)"/>
<attribute name="VOUT1" value="9V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="13.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750316586" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EE20/10/6_2W:3W_PARALLEL"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EE20/10/6_L22.2W25H16_14PINS">
<connects>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750316586?ae"/>
<attribute name="FSWITCH" value="200kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="300mA"/>
<attribute name="IOUT2" value="50mA"/>
<attribute name="IOUT3" value="75mA"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="L" value="150uH"/>
<attribute name="LENGTH" value="22.2mm"/>
<attribute name="LS" value="1700nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="1.69:1:1.69:4.07"/>
<attribute name="PART-NUMBER" value=" 750316586 "/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value=" 750316586 "/>
<attribute name="VBUCK" value="-12V"/>
<attribute name="VIN" value="10 - 14 V (DC)"/>
<attribute name="VOUT1" value="7V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VOUT3" value="30V"/>
<attribute name="VT" value="4000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750315038" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_PQ2020_1W:4W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_PQ2020_L23.36W23.88H24.14">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="13" pad="13"/>
<connect gate="G$1" pin="14" pad="14"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750315038?ae"/>
<attribute name="FSWITCH" value="250 - 600kHz"/>
<attribute name="HEIGHT" value="24.14mm"/>
<attribute name="IOUT1" value="300mA"/>
<attribute name="IOUT2" value="100mA"/>
<attribute name="IOUT3" value="100mA"/>
<attribute name="IOUT4" value="100mA"/>
<attribute name="L" value="36.5uH"/>
<attribute name="LENGTH" value="23.36mm"/>
<attribute name="LS" value="300nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="1:2.33:2.33:2.33:2.33"/>
<attribute name="PART-NUMBER" value=" 750315038 "/>
<attribute name="SIZE" value="PQ2020"/>
<attribute name="VALUE" value=" 750315038 "/>
<attribute name="VBUCK" value="10.5V"/>
<attribute name="VIN" value="7 - 26 V (DC)"/>
<attribute name="VOUT1" value="23V"/>
<attribute name="VOUT2" value="23V"/>
<attribute name="VOUT3" value="23V"/>
<attribute name="VOUT4" value="23V"/>
<attribute name="VT" value="3600V(AC)"/>
<attribute name="WIDTH" value="23.88mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312924" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP5_1W:2W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP5_L8.35W9.5H6.35">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312924?ae"/>
<attribute name="FSWITCH" value="750kHz"/>
<attribute name="HEIGHT" value="6.35mm"/>
<attribute name="IOUT1" value="0.12A"/>
<attribute name="IOUT2" value="0.08A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="L" value="26uH"/>
<attribute name="LENGTH" value="8.35mm"/>
<attribute name="LS" value="1000nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="2:2:1"/>
<attribute name="PART-NUMBER" value=" 750312924 "/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 750312924 "/>
<attribute name="VBUCK" value="10V"/>
<attribute name="VIN" value="36 - 75 V (DC)"/>
<attribute name="VOUT1" value="10V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="9.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750342627" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EE16/8/5_2W:2W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750342627?ae"/>
<attribute name="FSWITCH" value="200 - 350kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="250mA"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="20uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="LS" value="270nH"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="2.4:1"/>
<attribute name="PART-NUMBER" value=" 750342627 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 750342627 "/>
<attribute name="VIN" value="9 - 15 V (DC)"/>
<attribute name="VOUT1" value="9V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750312750" prefix="T">
<description>&lt;b&gt;WE-IBTI Isolated Buck Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Flybuck™ topology  
&lt;br&gt; Operating Temp: -40°C to +125°C
&lt;br&gt; Excellent leakage inductance and interwinding capacitance performance

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Industrial Programmable Logic Controllers (PLCs)
&lt;br&gt;Building automation and process control
&lt;br&gt;Isolated interface power: RS-422, RS-485, CAN, I2C, LAN
&lt;br&gt;Motor drive control, inverters and industrial automation
&lt;br&gt;Isolated low power drivers &amp; regulators, smart e-meters
&lt;br&gt;Bias power supplies for gate drives and op-amps


&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o790826v209%20family-MID-IBTI.1673.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-IBTI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-IBTI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-06-07&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-IBTI_EP5_1W:1W"/>
</gates>
<devices>
<device name="" package="WE-IBTI_EP5_L6.6W8.26H5.59">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750312750?ae"/>
<attribute name="FSWITCH" value="750kHz"/>
<attribute name="HEIGHT" value="5.59mm"/>
<attribute name="IOUT1" value="0.3A"/>
<attribute name="ISAT" value="0.76A"/>
<attribute name="L" value="23uH"/>
<attribute name="LENGTH" value="6.6mm"/>
<attribute name="LS" value="400nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 750312750 "/>
<attribute name="SIZE" value="EP5"/>
<attribute name="VALUE" value=" 750312750 "/>
<attribute name="VBUCK" value="10V"/>
<attribute name="VIN" value="20 - 100 V (DC)"/>
<attribute name="VOUT1" value="10V"/>
<attribute name="VT" value="1500V(AC)"/>
<attribute name="WIDTH" value="8.26mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
