<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Signal &amp; Communications - Filtered Connectors- WE-LANMX &lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-03-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="749600010">
<description>&lt;b&gt;WE-LANMX Connector
&lt;/b&gt;&lt;br&gt;10/100 Base-T, THR, 10pins</description>
</package>
</packages>
<symbols>
<symbol name="749600010">
<pin name="CTD"/>
<pin name="RD-"/>
<pin name="TD-"/>
<pin name="TD+"/>
<pin name="NC@3" direction="pas"/>
<pin name="NC@4" direction="pas"/>
<pin name="NC@1" direction="pas"/>
<pin name="NC@2" direction="pas"/>
<pin name="CRD"/>
<pin name="RD+"/>
<pin name="SHIELD1" direction="pwr"/>
<pin name="SHIELD2" direction="pwr"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="749600010" prefix="T">
<description>&lt;b&gt;WE-LANMX Connector&lt;br&gt;
&lt;/b&gt;Connector without assembly&lt;br&gt;

&lt;br&gt;&lt;b&gt;Characteristics 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;M12 connector with integrated magnetics
&lt;br&gt; Slim design
&lt;br&gt; High mechanical stability
&lt;br&gt; Robust against dust and water
&lt;br&gt; Through hole reflow (THR) soldering
&lt;br&gt; Compliant with standard IEEE 802.3u
&lt;br&gt; Operating temperature: -40 °C up to +85 °C

&lt;br&gt;&lt;br&gt;
&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;&lt;br&gt;Industrial applications e.g. factory automation, robotics, transportation technology, wind power plants
&lt;br&gt; Standards wie EtherNet/IP, Profinet, EtherCAT, Ethernet Powerlink

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o324305v209%20Family_WE-LANMX_Connector_749600010.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o324305v209%20Family_WE-LANMX_Connector_749600010.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/katalog/en/WE-LANMX_CONNECTOR"&gt;https://www.we-online.com/katalog/en/WE-LANMX_CONNECTOR&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2021-03-18&lt;br&gt;
2021 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="749600010"/>
</gates>
<devices>
<device name="" package="749600010">
<connects>
<connect gate="G$1" pin="CRD" pad="10"/>
<connect gate="G$1" pin="CTD" pad="5"/>
<connect gate="G$1" pin="NC@1" pad="6"/>
<connect gate="G$1" pin="NC@2" pad="1"/>
<connect gate="G$1" pin="NC@3" pad="2"/>
<connect gate="G$1" pin="NC@4" pad="7"/>
<connect gate="G$1" pin="RD+" pad="9"/>
<connect gate="G$1" pin="RD-" pad="8"/>
<connect gate="G$1" pin="SHIELD1" pad="GND"/>
<connect gate="G$1" pin="SHIELD2" pad="GND1"/>
<connect gate="G$1" pin="TD+" pad="4"/>
<connect gate="G$1" pin="TD-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATA-RATE" value="10/100 Base-T"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/749600010.pdf"/>
<attribute name="L" value="350uH"/>
<attribute name="MOUNT" value="THR"/>
<attribute name="ORIENTATION-TYPE" value="Vertical"/>
<attribute name="PART-NUMBER" value=" 749600010 "/>
<attribute name="POE" value="non-PoE"/>
<attribute name="RISO" value="100MOhm"/>
<attribute name="USE-WITH" value="749699910"/>
<attribute name="VALUE" value=" 749600010 "/>
<attribute name="VT" value="2250V (DC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
