<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - EMC Components - Common Mode Chokes for Mains Power Lines - WE-LF&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-06-02&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LF_LH">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: LH, THT, 4pins
&lt;br&gt;DXH = 28.5mmX17mm</description>
</package>
<package name="WE-LF_MH">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: MH, THT, 4pins
&lt;br&gt;DXH = 23mmX14.5mm</description>
</package>
<package name="WE-LF_XV">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: XV, THT, 4pins
&lt;br&gt;LXWXH = 32.5mmX21.5mmX35.5mm</description>
</package>
<package name="WE-LF_XH">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: XH, THT, 4pins
&lt;br&gt;DXH = 33.5mmX20mm</description>
</package>
<package name="WE-LF_SV">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: SV, THT, 4pins
&lt;br&gt;LXWXH = 18.5mmX13.5mmX20.5mm</description>
</package>
<package name="WE-LF_LV">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: LV, THT, 4pins
&lt;br&gt;LXWXH = 26.5mmX18.46mmX30.5mm</description>
</package>
<package name="WE-LF_SH">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: SH, THT, 4pins
&lt;br&gt;DXH = 18mmX13mm</description>
</package>
<package name="WE-LF_MV">
<description>&lt;B&gt;WE-LF Common Mode Power Line Choke
&lt;BR&gt;&lt;/B&gt;Size: MV, THT, 4pins
&lt;br&gt;LXWXH = 24.5mmX17mmX29mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-LF">
<pin name="1" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LF_LH" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_LH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446821027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446821027?ae"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="28.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446821027 "/>
<attribute name="RDC" value="0.64Ohm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="28.5mm"/>
</technology>
<technology name="_7446822006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446822006?ae"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="28.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446822006 "/>
<attribute name="RDC" value="0.16Ohm"/>
<attribute name="VALUE" value="5.6mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="28.5mm"/>
</technology>
<technology name="_7446823003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446823003?ae"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="28.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446823003 "/>
<attribute name="RDC" value="0.06Ohm"/>
<attribute name="VALUE" value="2.7mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="28.5mm"/>
</technology>
<technology name="_7446823006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446823006?ae"/>
<attribute name="HEIGHT" value="17mm"/>
<attribute name="IR" value="2.4A"/>
<attribute name="LENGTH" value="28.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446823006 "/>
<attribute name="RDC" value="0.1Ohm"/>
<attribute name="VALUE" value="5.6mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="28.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_XV" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_XV">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446422007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446422007?ae"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="IR" value="2.5A"/>
<attribute name="LENGTH" value="32.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446422007 "/>
<attribute name="RDC" value="0.12Ohm"/>
<attribute name="VALUE" value="6.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="21.5mm"/>
</technology>
<technology name="_7446424002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446424002?ae"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="IR" value="4.3A"/>
<attribute name="LENGTH" value="32.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446424002 "/>
<attribute name="RDC" value="0.038Ohm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="21.5mm"/>
</technology>
<technology name="_7446424003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446424003?ae"/>
<attribute name="HEIGHT" value="35.5mm"/>
<attribute name="IR" value="4A"/>
<attribute name="LENGTH" value="32.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446424003 "/>
<attribute name="RDC" value="0.065Ohm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="21.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_SV" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_SV">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446120027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446120027?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446120027 "/>
<attribute name="RDC" value="1.2Ohm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7446120039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446120039?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446120039 "/>
<attribute name="RDC" value="1.7Ohm"/>
<attribute name="VALUE" value="39mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7446120047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446120047?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="0.3A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446120047 "/>
<attribute name="RDC" value="2.6Ohm"/>
<attribute name="VALUE" value="47mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7446121007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446121007?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446121007 "/>
<attribute name="RDC" value="0.3Ohm"/>
<attribute name="VALUE" value="6.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7446121010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446121010?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="0.7A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446121010 "/>
<attribute name="RDC" value="0.55Ohm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7446121018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446121018?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="0.5A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446121018 "/>
<attribute name="RDC" value="0.75Ohm"/>
<attribute name="VALUE" value="18mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7446122001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446122001?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446122001 "/>
<attribute name="RDC" value="0.06Ohm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_7446122003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446122003?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="1.5A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446122003 "/>
<attribute name="RDC" value="0.15Ohm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
<technology name="_74461240004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74461240004?ae"/>
<attribute name="HEIGHT" value="20.5mm"/>
<attribute name="IR" value="3.6A"/>
<attribute name="LENGTH" value="18.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74461240004 "/>
<attribute name="RDC" value="0.02Ohm"/>
<attribute name="VALUE" value="0.4mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="13.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_XH" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_XH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446921027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446921027?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="1.2A"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="LENGTH" value="33.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446921027 "/>
<attribute name="PRAT-NUMBER" value="7446921027"/>
<attribute name="RDC" value="0.4Ohm"/>
<attribute name="RDC1" value="0.4Ω"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="33.5mm"/>
</technology>
<technology name="_7446923010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446923010?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="3A"/>
<attribute name="IR1" value="3A"/>
<attribute name="LENGTH" value="33.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446923010 "/>
<attribute name="PRAT-NUMBER" value="7446923010"/>
<attribute name="RDC" value="0.155Ohm"/>
<attribute name="RDC1" value="0.155Ω"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="33.5mm"/>
</technology>
<technology name="_7446924003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446924003?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="4A"/>
<attribute name="IR1" value="4A"/>
<attribute name="LENGTH" value="33.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446924003 "/>
<attribute name="PRAT-NUMBER" value="7446924003"/>
<attribute name="RDC" value="0.065Ohm"/>
<attribute name="RDC1" value="0.065Ω"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="33.5mm"/>
</technology>
<technology name="_7446926002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446926002?ae"/>
<attribute name="HEIGHT" value="20mm"/>
<attribute name="IR" value="6A"/>
<attribute name="IR1" value="6A"/>
<attribute name="LENGTH" value="33.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446926002 "/>
<attribute name="PRAT-NUMBER" value="7446926002"/>
<attribute name="RDC" value="0.03Ohm"/>
<attribute name="RDC1" value="0.03Ω"/>
<attribute name="VALUE" value="1.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="33.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_MH" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_MH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446720047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446720047?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446720047 "/>
<attribute name="RDC" value="2Ohm"/>
<attribute name="VALUE" value="47mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
<technology name="_7446721010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446721010?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR" value="1.3A"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446721010 "/>
<attribute name="RDC" value="0.25Ohm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
<technology name="_7446721027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446721027?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR" value="0.6A"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446721027 "/>
<attribute name="RDC" value="0.7Ohm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
<technology name="_7446722002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446722002?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446722002 "/>
<attribute name="RDC" value="0.06Ohm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
<technology name="_7446722004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446722004?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR" value="1.9A"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446722004 "/>
<attribute name="RDC" value="0.12Ohm"/>
<attribute name="VALUE" value="4.2mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
<technology name="_7446722007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446722007?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR" value="1.5A"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446722007 "/>
<attribute name="RDC" value="0.2Ohm"/>
<attribute name="VALUE" value="6.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
<technology name="_7446723001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446723001?ae"/>
<attribute name="HEIGHT" value="14.5mm"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="23mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446723001 "/>
<attribute name="RDC" value="0.04Ohm"/>
<attribute name="VALUE" value="1.2mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="23mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_SH" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_SH">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446620015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446620015?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="0.5A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446620015 "/>
<attribute name="RDC" value="0.83Ohm"/>
<attribute name="VALUE" value="15mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_7446620027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446620027?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446620027 "/>
<attribute name="RDC" value="1.2Ohm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_7446620039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446620039?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446620039 "/>
<attribute name="RDC" value="1.7Ohm"/>
<attribute name="VALUE" value="39mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_7446621007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446621007?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446621007 "/>
<attribute name="RDC" value="0.3Ohm"/>
<attribute name="VALUE" value="6.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_7446621010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446621010?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="0.7A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446621010 "/>
<attribute name="RDC" value="0.55Ohm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_7446622001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446622001?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446622001 "/>
<attribute name="RDC" value="0.06Ohm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_7446622002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446622002?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446622002 "/>
<attribute name="RDC" value="0.1Ohm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_7446622003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446622003?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="1.5A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446622003 "/>
<attribute name="RDC" value="0.15Ohm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
<technology name="_74466240007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74466240007?ae"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IR" value="4A"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74466240007 "/>
<attribute name="RDC" value="0.027Ohm"/>
<attribute name="VALUE" value="0.7mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_LV" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik
&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/pbs/WE-LF"&gt;https://katalog.we-online.de/en/pbs/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2019-05-30&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_LV">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446321027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446321027?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="1A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446321027 "/>
<attribute name="RDC" value="0.64Ohm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
<technology name="_7446321033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446321033?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="0.8A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446321033 "/>
<attribute name="RDC" value="0.85Ohm"/>
<attribute name="VALUE" value="33mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
<technology name="_7446321050">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446321050?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="0.6A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446321050 "/>
<attribute name="RDC" value="1.2Ohm"/>
<attribute name="VALUE" value="50mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
<technology name="_7446322007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446322007?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="1.9A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446322007 "/>
<attribute name="RDC" value="0.16Ohm"/>
<attribute name="VALUE" value="6.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
<technology name="_7446322010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446322010?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="1.9A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446322010 "/>
<attribute name="RDC" value="0.18Ohm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
<technology name="_7446323003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446323003?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446323003 "/>
<attribute name="RDC" value="0.06Ohm"/>
<attribute name="VALUE" value="2.7mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
<technology name="_7446323004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446323004?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446323004 "/>
<attribute name="RDC" value="0.07Ohm"/>
<attribute name="VALUE" value="4mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
<technology name="_7446326002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446326002?ae"/>
<attribute name="HEIGHT" value="30.5mm"/>
<attribute name="IR" value="6A"/>
<attribute name="LENGTH" value="26.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446326002 "/>
<attribute name="RDC" value="0.023Ohm"/>
<attribute name="VALUE" value="1.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="18.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LF_MV" prefix="L">
<description>&lt;b&gt;WE-LF Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Easy assembling due to 4 pin housing
&lt;br&gt;Compact and small size
&lt;br&gt;4 soldering pins for perfect mechanical decoupling
&lt;br&gt;Toroidal core choke with sector winding
&lt;br&gt;High interference suppression for common mode interferences in low and middle frequency ranges
&lt;br&gt;Low stray field
&lt;br&gt;Operating temperature: -40 °C bis 125 °C
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category: 40/125/21
&lt;br&gt;Certified according IEC 60938-2
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Power line filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14802v209%20WE-LF_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LF/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LF&lt;/a&gt;&lt;p&gt;

Updated by  Ella Wu 2023-06-02&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_MV">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7446220047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446220047?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446220047 "/>
<attribute name="RDC" value="1.6Ohm"/>
<attribute name="VALUE" value="47mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446221010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446221010?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="1.3A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446221010 "/>
<attribute name="RDC" value="0.25Ohm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446221012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446221012?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="1.2A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446221012 "/>
<attribute name="RDC" value="0.28Ohm"/>
<attribute name="VALUE" value="12mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446221027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446221027?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="0.6A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446221027 "/>
<attribute name="RDC" value="0.7Ohm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446222002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446222002?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446222002 "/>
<attribute name="RDC" value="0.06Ohm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446222003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446222003?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446222003 "/>
<attribute name="RDC" value="0.075Ohm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446222004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446222004?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="2A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446222004 "/>
<attribute name="RDC" value="0.12Ohm"/>
<attribute name="VALUE" value="4.2mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446222007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446222007?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="1.5A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446222007 "/>
<attribute name="RDC" value="0.2Ohm"/>
<attribute name="VALUE" value="6.8mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_7446223001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7446223001?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="3A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 7446223001 "/>
<attribute name="RDC" value="0.04Ohm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
<technology name="_74462250007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74462250007?ae"/>
<attribute name="HEIGHT" value="25.5mm"/>
<attribute name="IR" value="4.7A"/>
<attribute name="LENGTH" value="23.5mm"/>
<attribute name="MATERIAL" value="MnZn"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="PART-NUMBER" value=" 74462250007 "/>
<attribute name="RDC" value="0.02Ohm"/>
<attribute name="VALUE" value="0.7mH"/>
<attribute name="VR" value="250V (AC)"/>
<attribute name="VT" value="1500V (AC)"/>
<attribute name="WIDTH" value="16mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
