<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Mains Power Lines - WE-LF SMD&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LF_SMD_SH">
<description>&lt;b&gt;WE-LF SMD Common Mode Power Line Choke
&lt;br&gt;&lt;/b&gt;Size: SH</description>
</package>
</packages>
<symbols>
<symbol name="WE-LF">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LF_SMD_SH" prefix="L">
<description>&lt;B&gt;WE-LF SMD Common Mode Power Line Choke
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMD power line choke
&lt;br&gt;Compact size
&lt;br&gt;Toroidal core with sector winding
&lt;br&gt;High attenuation of common mode interferences in low and middle frequency range
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Mains filter
&lt;br&gt;Power electronics
&lt;br&gt;SMPS
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14801v209%20Family_WE-LFSMD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14801v209%20Family_WE-LFSMD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-LF-SMD"&gt;https://katalog.we-online.com/en/pbs/WE-LF-SMD&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu  2019-05-30&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-LF"/>
</gates>
<devices>
<device name="" package="WE-LF_SMD_SH">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_7446630027">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446630027.pdf"/>
<attribute name="IR" value="0.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446630027 "/>
<attribute name="RDC" value="1.2Ohm"/>
<attribute name="VALUE" value="27mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7446630039">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446630039.pdf"/>
<attribute name="IR" value="0.55A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446630039 "/>
<attribute name="RDC" value="1.7Ohm"/>
<attribute name="VALUE" value="39mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7446630047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446630047.pdf"/>
<attribute name="IR" value="0.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446630047 "/>
<attribute name="RDC" value="2.6Ohm"/>
<attribute name="VALUE" value="47mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7446631007">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446631007.pdf"/>
<attribute name="IR" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446631007 "/>
<attribute name="RDC" value="0.3Ohm"/>
<attribute name="VALUE" value="6.8mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7446631010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446631010.pdf"/>
<attribute name="IR" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446631010 "/>
<attribute name="RDC" value="0.55Ohm"/>
<attribute name="VALUE" value="10mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7446632001">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446632001.pdf"/>
<attribute name="IR" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446632001 "/>
<attribute name="RDC" value="0.06Ohm"/>
<attribute name="VALUE" value="1mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7446632002">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446632002.pdf"/>
<attribute name="IR" value="2.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446632002 "/>
<attribute name="RDC" value="0.1Ohm"/>
<attribute name="VALUE" value="2.2mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_7446632003">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7446632003.pdf"/>
<attribute name="IR" value="2.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7446632003 "/>
<attribute name="RDC" value="0.15Ohm"/>
<attribute name="VALUE" value="3.3mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
<technology name="_74466340007">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74466340007.pdf"/>
<attribute name="IR" value="5.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74466340007 "/>
<attribute name="RDC" value="0.03Ohm"/>
<attribute name="VALUE" value="0.7mH"/>
<attribute name="VR" value="250  V (AC) "/>
<attribute name="VT" value="1500  V (AC) "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
