<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Unshielded Power Inductors - WE-LQ&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LQ_1210">
<description>&lt;b&gt;WE-LQ SMT Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Size: 1210, SMT, 2pins
&lt;br&gt;LXWXH = 3.2X2.5X2mm</description>
</package>
<package name="WE-LQ_1812">
<description>&lt;b&gt;WE-LQ SMT Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;
Size: 1812, SMT, 2pins
&lt;br&gt;LXWXH = 4.5X3.2X2.6mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LQ_1210" prefix="L">
<description>&lt;b&gt;WE-LQ SMT Inductor
&lt;br&gt;Unshielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Miniature chip inductor wound on a special ferrite core
&lt;br&gt;Small inductances for compact circuits
&lt;br&gt;High Q at high frequencies
&lt;br&gt;Low DC-resistance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low power DC/DC-converters from Linear Technology, National Semiconductor, Texas Instruments, Fairchild Semiconductor, 
&lt;br&gt;ON Semiconductor, STMicroelectronics, Maxim, MPS, Semtech, Exar, Analogic Tech, Diodes and Cologne Chip
&lt;br&gt;EMI-Filtering
&lt;br&gt;RF-circuits

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14806v209%20Family_we-lq_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14806v209%20Family_we-lq_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQ/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQ&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu 2022-10-28&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LQ_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744032001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032001?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032001"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_7440320015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440320015?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.66A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440320015"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.13Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_7440320018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440320018?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.64A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440320018"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.14Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032002?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.62A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032002"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.15Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_7440320027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440320027?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L" value="2.7uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440320027"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.18Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="2.7uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032003?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.58A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032003"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.2Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_7440320039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440320039?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.54A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="L" value="3.9uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440320039"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="3.9uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032004?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.49A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032004"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.28Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_7440320056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440320056?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.44A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440320056"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.36Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032006?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032006"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032008?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.39A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032008"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="0.45Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032100?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.32A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032100"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="0.65Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032101?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.1A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032101"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="6.5Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032120?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.29A"/>
<attribute name="ISAT" value="0.78A"/>
<attribute name="L" value="12uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032120"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="12uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032121">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032121?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.095A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="L" value="120uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032121"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="7Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="120uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032150?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.27A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032150"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032180?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.24A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="L" value="18uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032180"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="1.1Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="18uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032220?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032220"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="1.3Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032221?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.075A"/>
<attribute name="ISAT" value="0.24A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032221"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="11.8Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032331?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.065A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="L" value="330uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032331"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="16.5Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="330uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032470?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.146A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032470"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="3Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032471?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.055A"/>
<attribute name="ISAT" value="0.12A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032471"/>
<attribute name="Q" value="46%"/>
<attribute name="RDC-MAX" value="25Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_744032680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744032680?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="0.13A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="L" value="68uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744032680"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="3.8Ohm"/>
<attribute name="SIZE" value="1210"/>
<attribute name="VALUE" value="68uH"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQ_1812" prefix="L">
<description>&lt;b&gt;WE-LQ SMT Inductor
&lt;br&gt;Unshielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Miniature chip inductor wound on a special ferrite core
&lt;br&gt;Small inductances for compact circuits
&lt;br&gt;High Q at high frequencies
&lt;br&gt;Low DC-resistance
&lt;br&gt;Operating temperature: –40 ºC to +125 ºC
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications

&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low power DC/DC-converters from Linear Technology, National Semiconductor, Texas Instruments, Fairchild Semiconductor, 
&lt;br&gt;ON Semiconductor, STMicroelectronics, Maxim, MPS, Semtech, Exar, Analogic Tech, Diodes and Cologne Chip
&lt;br&gt;EMI-Filtering
&lt;br&gt;RF-circuits

&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14806v209%20Family_we-lq_smd_induktivitaet.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14806v209%20Family_we-lq_smd_induktivitaet.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQ/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQ&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu 2025-04-23&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-LQ_1812">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744045001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045001?ae"/>
<attribute name="FRES" value="165MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="4.4A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045001"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="0.08Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_7440450015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440450015?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440450015"/>
<attribute name="Q" value="42%"/>
<attribute name="RDC-MAX" value="0.09Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_7440450018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440450018?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440450018"/>
<attribute name="Q" value="45%"/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045002?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045002"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="0.11Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_7440450027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440450027?ae"/>
<attribute name="FRES" value="63MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="L" value="2.7uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440450027"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="0.12Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2.7uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045003?ae"/>
<attribute name="FRES" value="58MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045003"/>
<attribute name="Q" value="45%"/>
<attribute name="RDC-MAX" value="0.13Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_7440450039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440450039?ae"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.32A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="L" value="3.9uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440450039"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="0.14Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="3.9uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045004?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.24A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045004"/>
<attribute name="Q" value="36%"/>
<attribute name="RDC-MAX" value="0.15Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_7440450056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440450056?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.18A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7440450056"/>
<attribute name="Q" value="36%"/>
<attribute name="RDC-MAX" value="0.18Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045006?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045006"/>
<attribute name="Q" value="36%"/>
<attribute name="RDC-MAX" value="0.2Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045008?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045008"/>
<attribute name="Q" value="36%"/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045100?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045100"/>
<attribute name="Q" value="48%"/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045102?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.07A"/>
<attribute name="ISAT" value="0.16A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045102"/>
<attribute name="Q" value="28%"/>
<attribute name="RDC-MAX" value="30Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045120?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L" value="12uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045120"/>
<attribute name="Q" value="48%"/>
<attribute name="RDC-MAX" value="0.42Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="12uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045150?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.73A"/>
<attribute name="ISAT" value="1.24A"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045150"/>
<attribute name="Q" value="45%"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045152?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.055A"/>
<attribute name="ISAT" value="0.095A"/>
<attribute name="L" value="1500uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045152"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="38.5Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="1500uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045180?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.68A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L" value="18uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045180"/>
<attribute name="Q" value="42%"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="18uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045210?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.27A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045210"/>
<attribute name="Q" value="60%"/>
<attribute name="RDC-MAX" value="2.5Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045215?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.42A"/>
<attribute name="L" value="150uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045215"/>
<attribute name="Q" value="55%"/>
<attribute name="RDC-MAX" value="3.7Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="150uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045220?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.63A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045220"/>
<attribute name="Q" value="50%"/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045222?ae"/>
<attribute name="FRES" value="1MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.04A"/>
<attribute name="ISAT" value="0.078A"/>
<attribute name="L" value="2200uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045222"/>
<attribute name="Q" value="30%"/>
<attribute name="RDC-MAX" value="47Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="2200uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045330?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045330"/>
<attribute name="Q" value="55%"/>
<attribute name="RDC-MAX" value="1.1Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045391">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045391?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.11A"/>
<attribute name="ISAT" value="0.27A"/>
<attribute name="L" value="390uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045391"/>
<attribute name="Q" value="50%"/>
<attribute name="RDC-MAX" value="13Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="390uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045470?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.39A"/>
<attribute name="ISAT" value="0.73A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045470"/>
<attribute name="Q" value="55%"/>
<attribute name="RDC-MAX" value="1.5Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045471?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.105A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045471"/>
<attribute name="Q" value="50%"/>
<attribute name="RDC-MAX" value="14.2Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045680?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.33A"/>
<attribute name="ISAT" value="0.61A"/>
<attribute name="L" value="68uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045680"/>
<attribute name="Q" value="55%"/>
<attribute name="RDC-MAX" value="2.1Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="68uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045681?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.09A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="L" value="680uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045681"/>
<attribute name="Q" value="45%"/>
<attribute name="RDC-MAX" value="16.8Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="680uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045820?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.57A"/>
<attribute name="L" value="82uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045820"/>
<attribute name="Q" value="55%"/>
<attribute name="RDC-MAX" value="2.3Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="82uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744045821">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744045821?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="HEIGHT" value="2.6mm"/>
<attribute name="IR" value="0.085A"/>
<attribute name="ISAT" value="0.15A"/>
<attribute name="L" value="820uH"/>
<attribute name="LENGTH" value="4.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744045821"/>
<attribute name="Q" value="50%"/>
<attribute name="RDC-MAX" value="20Ohm"/>
<attribute name="SIZE" value="1812"/>
<attribute name="VALUE" value="820uH"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
