<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-LQFS&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-03-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LQFS_4828">
<description>&lt;b&gt;WE-LQFS SMT Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 4818, SMT, 2pins
&lt;br&gt;LXWXH=4.8X4.8X2.8mm</description>
</package>
<package name="WE-LQFS_3818">
<description>&lt;b&gt;WE-LQFS SMT Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 3818, SMT, 2pins
&lt;br&gt;LXWXH=3.8X3.8X1.8mm</description>
</package>
<package name="WE-LQFS_4818">
<description>&lt;b&gt;WE-LQFS SMT Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 4818, SMT, 2pins
&lt;br&gt;LXWXH=4.8X4.8X1.8mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LQFS_4828" prefix="L">
<description>&lt;b&gt;WE-LQFS SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT Tiny Shielded Power Inductor
&lt;br&gt;Shielded version of WE-LQ series
&lt;br&gt;Land pattern matching with unshielded version
&lt;br&gt;Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Integrated DC/DC Converters
&lt;br&gt;High efficiency switching controllers
&lt;br&gt;Portable devices (Smartphone, Digital cameras, Tablet, etc.)
&lt;br&gt;Embedded Laptops and PCs
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85071v209%20Family_WE-LQFS_3818-4828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85071v209%20Family_WE-LQFS_3818-4828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQFS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQFS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-18&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LQFS_4828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74406043012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043012?ae"/>
<attribute name="FRES" value="237MHz"/>
<attribute name="IR" value="3.61A"/>
<attribute name="ISAT" value="3.06A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043012 "/>
<attribute name="RDC-MAX" value="21mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74406043027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043027?ae"/>
<attribute name="FRES" value="119MHz"/>
<attribute name="IR" value="2.93A"/>
<attribute name="ISAT" value="2.07A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043027 "/>
<attribute name="RDC-MAX" value="32mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_74406043047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043047?ae"/>
<attribute name="FRES" value="81MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="1.62A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043047 "/>
<attribute name="RDC-MAX" value="51mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74406043068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043068?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="IR" value="2.05A"/>
<attribute name="ISAT" value="1.52A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043068 "/>
<attribute name="RDC-MAX" value="64mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74406043100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043100?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="1.77A"/>
<attribute name="ISAT" value="1.22A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043100 "/>
<attribute name="RDC-MAX" value="86mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74406043101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043101?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="0.62A"/>
<attribute name="ISAT" value="0.37A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043101 "/>
<attribute name="RDC-MAX" value="600mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74406043220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043220?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.23A"/>
<attribute name="ISAT" value="0.77A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043220 "/>
<attribute name="RDC-MAX" value="172mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74406043221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043221?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.26A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043221 "/>
<attribute name="RDC-MAX" value="1326mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74406043330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043330?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.99A"/>
<attribute name="ISAT" value="0.64A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043330 "/>
<attribute name="RDC-MAX" value="251mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74406043331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043331?ae"/>
<attribute name="FRES" value="5.8MHz"/>
<attribute name="IR" value="0.34A"/>
<attribute name="ISAT" value="0.22A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043331 "/>
<attribute name="RDC-MAX" value="1864mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74406043470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043470?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="0.97A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043470 "/>
<attribute name="RDC-MAX" value="260mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74406043471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406043471?ae"/>
<attribute name="FRES" value="4.7MHz"/>
<attribute name="IR" value="0.26A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406043471 "/>
<attribute name="RDC-MAX" value="2803mOhm"/>
<attribute name="SIZE" value=" 4828 "/>
<attribute name="VALUE" value="470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQFS_3818" prefix="L">
<description>&lt;b&gt;WE-LQFS SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT Tiny Shielded Power Inductor
&lt;br&gt;Shielded version of WE-LQ series
&lt;br&gt;Land pattern matching with unshielded version
&lt;br&gt;Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Integrated DC/DC Converters
&lt;br&gt;High efficiency switching controllers
&lt;br&gt;Portable devices (Smartphone, Digital cameras, Tablet, etc.)
&lt;br&gt;Embedded Laptops and PCs
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85071v209%20Family_WE-LQFS_3818-4828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85071v209%20Family_WE-LQFS_3818-4828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQFS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQFS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-18&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LQFS_3818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74406032010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032010?ae"/>
<attribute name="FRES" value="264MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032010 "/>
<attribute name="RDC-MAX" value="31mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74406032015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032015?ae"/>
<attribute name="FRES" value="215MHz"/>
<attribute name="IR" value="2.25A"/>
<attribute name="ISAT" value="1.92A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032015 "/>
<attribute name="RDC-MAX" value="39mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74406032033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032033?ae"/>
<attribute name="FRES" value="132MHz"/>
<attribute name="IR" value="1.59A"/>
<attribute name="ISAT" value="1.31A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032033 "/>
<attribute name="RDC-MAX" value="77mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74406032047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032047?ae"/>
<attribute name="FRES" value="99MHz"/>
<attribute name="IR" value="1.36A"/>
<attribute name="ISAT" value="1.07A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032047 "/>
<attribute name="RDC-MAX" value="110mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74406032068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032068?ae"/>
<attribute name="FRES" value="81MHz"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="0.88A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032068 "/>
<attribute name="RDC-MAX" value="153mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74406032100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032100?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="IR" value="0.94A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032100 "/>
<attribute name="RDC-MAX" value="228mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74406032101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032101?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="0.27A"/>
<attribute name="ISAT" value="0.22A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032101 "/>
<attribute name="RDC-MAX" value="2476mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74406032220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032220?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="0.66A"/>
<attribute name="ISAT" value="0.46A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032220 "/>
<attribute name="RDC-MAX" value="481mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74406032330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032330?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="0.54A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032330 "/>
<attribute name="RDC-MAX" value="715mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74406032470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406032470?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.34A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406032470 "/>
<attribute name="RDC-MAX" value="1000mOhm"/>
<attribute name="SIZE" value=" 3818 "/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQFS_4818" prefix="L">
<description>&lt;b&gt;WE-LQFS SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;SMT Tiny Shielded Power Inductor
&lt;br&gt;Shielded version of WE-LQ series
&lt;br&gt;Land pattern matching with unshielded version
&lt;br&gt;Operating Temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Integrated DC/DC Converters
&lt;br&gt;High efficiency switching controllers
&lt;br&gt;Portable devices (Smartphone, Digital cameras, Tablet, etc.)
&lt;br&gt;Embedded Laptops and PCs
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o85071v209%20Family_WE-LQFS_3818-4828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o85071v209%20Family_WE-LQFS_3818-4828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQFS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-LQFS&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-03-18&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-LQFS_4818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74406042010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042010?ae"/>
<attribute name="FRES" value="237MHz"/>
<attribute name="IR" value="4.47A"/>
<attribute name="ISAT" value="4.06A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042010 "/>
<attribute name="RDC-MAX" value="23mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74406042015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042015?ae"/>
<attribute name="FRES" value="176MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT" value="3.08A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042015 "/>
<attribute name="RDC-MAX" value="30mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74406042022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042022?ae"/>
<attribute name="FRES" value="132MHz"/>
<attribute name="IR" value="3.36A"/>
<attribute name="ISAT" value="2.73A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042022 "/>
<attribute name="RDC-MAX" value="40mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74406042033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042033?ae"/>
<attribute name="FRES" value="99MHz"/>
<attribute name="IR" value="2.72A"/>
<attribute name="ISAT" value="2.12A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042033 "/>
<attribute name="RDC-MAX" value="61mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74406042047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042047?ae"/>
<attribute name="FRES" value="89MHz"/>
<attribute name="IR" value="2.39A"/>
<attribute name="ISAT" value="1.53A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042047 "/>
<attribute name="RDC-MAX" value="70mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74406042068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042068?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="2.04A"/>
<attribute name="ISAT" value="1.26A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042068 "/>
<attribute name="RDC-MAX" value="97mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74406042100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042100?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="1.61A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042100 "/>
<attribute name="RDC-MAX" value="133mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74406042101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042101?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="0.32A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042101 "/>
<attribute name="RDC-MAX" value="1386mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74406042220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042220?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042220 "/>
<attribute name="RDC-MAX" value="339mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74406042330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042330?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="0.83A"/>
<attribute name="ISAT" value="0.58A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042330 "/>
<attribute name="RDC-MAX" value="488mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74406042470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406042470?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.63A"/>
<attribute name="ISAT" value="0.47A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74406042470 "/>
<attribute name="RDC-MAX" value="627mOhm"/>
<attribute name="SIZE" value=" 4818 "/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
