<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-LQSA&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-05-31&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-LQSA_5040">
<description>&lt;B&gt;WE-LQSA SMD Power Inductor
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Size: 5040, SMT, 2pins
&lt;BR&gt;L X W X H = 5mm X 5mm X 4mm</description>
</package>
<package name="WE-LQSA_6045">
<description>&lt;B&gt;WE-LQSA SMD Power Inductor
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Size: 6045, SMT, 2pins
&lt;BR&gt;L X W X H = 5mm X 6mm X 4.6mm</description>
</package>
<package name="WE-LQSA_8040">
<description>&lt;B&gt;WE-LQSA SMD Power Inductor
&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;Size: 8040, SMT, 2pins
&lt;BR&gt;L X W X H = 8mm X 8mm X 4.2mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-LQSA">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-LQSA_5040" prefix="L">
<description>&lt;b&gt;WE-LQSA SMD Semi-Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded construction with magnetic glue
&lt;br&gt;Compact design compared to standard power inductors for high density mounting
&lt;br&gt;Similar sizes and land pattern as WE-LQS
&lt;br&gt;Robust design qualified with AEC-Q200 Grade 0
&lt;br&gt;Operating temperature: -50 °C up to +150 °C
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;LED Headlights (DC/DC-Converter, Control system)
&lt;br&gt;Electric Vehicle (Battery Management System, Inverter, DC/DC)
&lt;br&gt;Car Navigation Systems
&lt;br&gt;Keyless Entry Systems
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o686110v209%20family-we-lqsa-78404084xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o686110v209%20family-we-lqsa-78404084xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-LQSA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-05-31&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-LQSA"/>
</gates>
<devices>
<device name="" package="WE-LQSA_5040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78404054010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054010?ae"/>
<attribute name="FRES" value="187MHz"/>
<attribute name="IR" value="5.7A"/>
<attribute name="ISAT" value="7.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054010 "/>
<attribute name="RDC" value="12mohm"/>
<attribute name="RDC-MAX" value="14mohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78404054015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054015?ae"/>
<attribute name="FRES" value="137MHz"/>
<attribute name="IR" value="5.22A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054015 "/>
<attribute name="RDC" value="15mohm"/>
<attribute name="RDC-MAX" value="18mohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78404054022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054022?ae"/>
<attribute name="FRES" value="77MHz"/>
<attribute name="IR" value="4.54A"/>
<attribute name="ISAT" value="5.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054022 "/>
<attribute name="RDC" value="19mohm"/>
<attribute name="RDC-MAX" value="23mohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78404054033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054033?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="4.06A"/>
<attribute name="ISAT" value="4.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054033 "/>
<attribute name="RDC" value="24mohm"/>
<attribute name="RDC-MAX" value="29mohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78404054047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054047?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="3.64A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054047 "/>
<attribute name="RDC" value="30mohm"/>
<attribute name="RDC-MAX" value="36mohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78404054068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054068?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="3.01A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054068 "/>
<attribute name="RDC" value="43mohm"/>
<attribute name="RDC-MAX" value="52mohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78404054100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054100?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="2.45A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054100 "/>
<attribute name="RDC" value="68mohm"/>
<attribute name="RDC-MAX" value="82mohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_78404054101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054101?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="0.82A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054101 "/>
<attribute name="RDC" value="600mohm"/>
<attribute name="RDC-MAX" value="720mohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_78404054150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054150?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="2.01A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054150 "/>
<attribute name="RDC" value="90mohm"/>
<attribute name="RDC-MAX" value="108mohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_78404054470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054470?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.19A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054470 "/>
<attribute name="RDC" value="290mohm"/>
<attribute name="RDC-MAX" value="348mohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_78404054680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404054680?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="0.97A"/>
<attribute name="ISAT" value="0.99A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404054680 "/>
<attribute name="RDC" value="430mohm"/>
<attribute name="RDC-MAX" value="516mohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSA_6045" prefix="L">
<description>&lt;b&gt;WE-LQSA SMD Semi-Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded construction with magnetic glue
&lt;br&gt;Compact design compared to standard power inductors for high density mounting
&lt;br&gt;Similar sizes and land pattern as WE-LQS
&lt;br&gt;Robust design qualified with AEC-Q200 Grade 0
&lt;br&gt;Operating temperature: -50 °C up to +150 °C
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;LED Headlights (DC/DC-Converter, Control system)
&lt;br&gt;Electric Vehicle (Battery Management System, Inverter, DC/DC)
&lt;br&gt;Car Navigation Systems
&lt;br&gt;Keyless Entry Systems
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o686110v209%20family-we-lqsa-78404084xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o686110v209%20family-we-lqsa-78404084xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-LQSA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-05-31&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-LQSA"/>
</gates>
<devices>
<device name="" package="WE-LQSA_6045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78404064010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064010?ae"/>
<attribute name="FRES" value="159MHz"/>
<attribute name="IR" value="6.7A"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064010 "/>
<attribute name="RDC" value="9mohm"/>
<attribute name="RDC-MAX" value="11mohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78404064015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064015?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="9.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064015 "/>
<attribute name="RDC" value="11mohm"/>
<attribute name="RDC-MAX" value="13mohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78404064022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064022?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="8.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064022 "/>
<attribute name="RDC" value="14mohm"/>
<attribute name="RDC-MAX" value="17mohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78404064033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064033?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064033 "/>
<attribute name="RDC" value="23mohm"/>
<attribute name="RDC-MAX" value="28mohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78404064047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064047?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="3.7A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064047 "/>
<attribute name="RDC" value="28mohm"/>
<attribute name="RDC-MAX" value="34mohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78404064068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064068?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="4.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064068 "/>
<attribute name="RDC" value="35mohm"/>
<attribute name="RDC-MAX" value="42mohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78404064100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064100?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064100 "/>
<attribute name="RDC" value="48mohm"/>
<attribute name="RDC-MAX" value="58mohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_78404064101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064101?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064101 "/>
<attribute name="RDC" value="443mohm"/>
<attribute name="RDC-MAX" value="532mohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_78404064150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064150?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064150 "/>
<attribute name="RDC" value="73mohm"/>
<attribute name="RDC-MAX" value="88mohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_78404064220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064220?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064220 "/>
<attribute name="RDC" value="100mohm"/>
<attribute name="RDC-MAX" value="120mohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_78404064330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064330?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064330 "/>
<attribute name="RDC" value="140mohm"/>
<attribute name="RDC-MAX" value="168mohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_78404064470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064470?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064470 "/>
<attribute name="RDC" value="210mohm"/>
<attribute name="RDC-MAX" value="252mohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_78404064680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404064680?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404064680 "/>
<attribute name="RDC" value="306mohm"/>
<attribute name="RDC-MAX" value="367mohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-LQSA_8040" prefix="L">
<description>&lt;b&gt;WE-LQSA SMD Semi-Shielded Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;BR&gt; 
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Shielded construction with magnetic glue
&lt;br&gt;Compact design compared to standard power inductors for high density mounting
&lt;br&gt;Similar sizes and land pattern as WE-LQS
&lt;br&gt;Robust design qualified with AEC-Q200 Grade 0
&lt;br&gt;Operating temperature: -50 °C up to +150 °C
&lt;BR&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;BR&gt;
&lt;br&gt;&lt;/b&gt;LED Headlights (DC/DC-Converter, Control system)
&lt;br&gt;Electric Vehicle (Battery Management System, Inverter, DC/DC)
&lt;br&gt;Car Navigation Systems
&lt;br&gt;Keyless Entry Systems
&lt;BR&gt;
&lt;BR&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o686110v209%20family-we-lqsa-78404084xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o686110v209%20family-we-lqsa-78404084xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-LQSA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WE-LQSA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu  2022-05-31&lt;br&gt;
2022 (C) Wurth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="WE-LQSA"/>
</gates>
<devices>
<device name="" package="WE-LQSA_8040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78404084150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404084150?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="3.75A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404084150 "/>
<attribute name="RDC" value="50mohm"/>
<attribute name="RDC-MAX" value="60mohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_78404084220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404084220?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404084220 "/>
<attribute name="RDC" value="71mohm"/>
<attribute name="RDC-MAX" value="85mohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_78404084470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404084470?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="2.23A"/>
<attribute name="ISAT" value="2.18A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404084470 "/>
<attribute name="RDC" value="140mohm"/>
<attribute name="RDC-MAX" value="168mohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_78404084680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78404084680?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="1.82A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78404084680 "/>
<attribute name="RDC" value="204mohm"/>
<attribute name="RDC-MAX" value="245mohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
