<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Automotive - Single Coil Power Inductors - WE-MAIA&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024b, 2024-09-13&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MAIA_4020">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:4020, SMT, 2pins
&lt;br&gt;L X W X H = 4.1mm X 4.1mm X 2.1mm</description>
</package>
<package name="WE-MAIA_3020">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:3020, SMT, 2pins
&lt;br&gt;L X W X H = 3mm X 3mm X 2mm</description>
</package>
<package name="WE-MAIA_2506">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:2506, SMT, 2pins
&lt;br&gt;L X W X H = 2.5mm X 2mm X 0.6mm</description>
</package>
<package name="WE-MAIA_1610">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;br&gt;&lt;/b&gt;Size:1610, SMT, 2pins
&lt;br&gt;L X W X H = 1.6mm X 1.6mm X 1mm</description>
</package>
<package name="WE-MAIA_2508">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:2508, SMT, 2pins
&lt;br&gt;L X W X H = 2.5mm X 2mm X 0.8mm</description>
</package>
<package name="WE-MAIA_2512HT">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:2512HT, SMT, 2pins
&lt;br&gt;L X W X H = 2.5mm X 2mm X 1.2mm</description>
</package>
<package name="WE-MAIA_3015">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:3015, SMT, 2pins
&lt;br&gt;L X W X H = 3mm X 3mm X 1.5mm</description>
</package>
<package name="WE-MAIA_3020HT">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:3020HT, SMT, 2pins
&lt;br&gt;L X W X H = 3mm X 3mm X 2mm</description>
</package>
<package name="WE-MAIA_3010">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:3010, SMT, 2pins
&lt;br&gt;L X W X H = 3mm X 3mm X 1mm</description>
</package>
<package name="WE-MAIA_2010">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:2010,SMT,2pins
&lt;br&gt;LXWXH=2X1.6X1mm</description>
</package>
<package name="WE-MAIA_6030HT">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:6030HT, SMT, 2pins
&lt;br&gt;L X W X H = 6.6mm X 6.6mm X 3.1mm</description>
</package>
<package name="WE-MAIA_4020HT">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:4020HT, SMT, 2pins
&lt;br&gt;L X W X H = 4.1mm X 4.1mm X 2.1mm</description>
</package>
<package name="WE-MAIA_5020">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:5020, SMT, 2pins
&lt;br&gt;L X W X H = 5.4mm X 5.4mm X 2.1mm</description>
</package>
<package name="WE-MAIA_5030">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:5030, SMT, 2pins
&lt;br&gt;L X W X H = 5.4mm X 5.4mm X 2.1mm</description>
</package>
<package name="WE-MAIA_4030">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:4030, SMT, 2pins
&lt;br&gt;L X W X H = 4mm X 4mm X 3mm</description>
</package>
<package name="WE-MAIA_2510">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:2510, SMT, 2pins
&lt;br&gt;L X W X H = 2.5mm X 2mm X 1mm</description>
</package>
<package name="WE-MAIA_3015HT">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:3015HT, SMT, 2pins
&lt;br&gt;L X W X H = 3mm X 3mm X 1.5mm</description>
</package>
<package name="WE-MAIA_2512">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:2512, SMT, 2pins
&lt;br&gt;L X W X H = 2.5mm X 2mm X 1.2mm</description>
</package>
<package name="WE-MAIA_4012">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4012,SMT,2pins
&lt;br&gt;LXWXH=4.1X4.1X1.3mm</description>
</package>
<package name="WE-MAIA_3012">
<description>&lt;b&gt;WE-MAIA SMT Power Inductor &lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size:3012, SMT, 2pins
&lt;br&gt;L X W X H = 3mm X 3mm X 1.2mm</description>
</package>
</packages>
<symbols>
<symbol name="L-GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L-GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MAIA_4020" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAIA_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383560033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383560033?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="14.95A"/>
<attribute name="ISAT" value="12.4A"/>
<attribute name="ISAT1" value="7.95A@10%"/>
<attribute name="ISAT2" value="16.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383560033 "/>
<attribute name="RDC-MAX" value="7.2mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383560056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383560056?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="13.65A"/>
<attribute name="ISAT" value="10.8A"/>
<attribute name="ISAT1" value="6.9A@10%"/>
<attribute name="ISAT2" value="14.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383560056 "/>
<attribute name="RDC-MAX" value="8.4mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_784383560068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383560068?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="13.15A"/>
<attribute name="ISAT" value="9.4A"/>
<attribute name="ISAT1" value="5.8A@10%"/>
<attribute name="ISAT2" value="12.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383560068 "/>
<attribute name="RDC-MAX" value="9mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438356010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356010?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="10.1A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="ISAT1" value="5.3A@10%"/>
<attribute name="ISAT2" value="11.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356010 "/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438356012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356012?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="8.9A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="ISAT1" value="5.55A@10%"/>
<attribute name="ISAT2" value="11.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356012 "/>
<attribute name="RDC-MAX" value="18mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438356015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356015?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="8.6A"/>
<attribute name="ISAT" value="7.8A"/>
<attribute name="ISAT1" value="4.8A@10%"/>
<attribute name="ISAT2" value="10.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356015 "/>
<attribute name="RDC-MAX" value="19mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438356018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356018?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="ISAT1" value="4.35A@10%"/>
<attribute name="ISAT2" value="8.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356018 "/>
<attribute name="RDC-MAX" value="30mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_78438356022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356022?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="ISAT1" value="4.05A@10%"/>
<attribute name="ISAT2" value="7.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356022 "/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438356033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356033?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="5.15A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="ISAT1" value="3.55A@10%"/>
<attribute name="ISAT2" value="7.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356033 "/>
<attribute name="RDC-MAX" value="48mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438356047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="ISAT1" value="3.05A@10%"/>
<attribute name="ISAT2" value="5.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356047 "/>
<attribute name="RDC-MAX" value="76mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438356056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356056?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="3.85A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="ISAT1" value="2.65A@10%"/>
<attribute name="ISAT2" value="5.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438356056 "/>
<attribute name="RDC-MAX" value="81mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3020" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
Created By Ella 2024-09-13
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383360033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383360033?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="8.3A"/>
<attribute name="ISAT1" value="5.45A@10%"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383360033 "/>
<attribute name="RDC-MAX" value="17mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383360047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383360047?ae"/>
<attribute name="FRES" value="99MHz"/>
<attribute name="IR" value="7.55A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="ISAT1" value="5.4A@10%"/>
<attribute name="ISAT2" value="9.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383360047 "/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383360068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383360068?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="6.75A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="ISAT1" value="4.1A@10%"/>
<attribute name="ISAT2" value="8.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383360068 "/>
<attribute name="RDC-MAX" value="27mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438336010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336010?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="6.15A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="ISAT1" value="3.25A@10%"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336010 "/>
<attribute name="RDC-MAX" value="32mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438336012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336012?ae"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="IR" value="5.65A"/>
<attribute name="ISAT" value="4.75A"/>
<attribute name="ISAT1" value="3.05A@10%"/>
<attribute name="ISAT2" value="6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336012 "/>
<attribute name="RDC-MAX" value="36mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438336015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336015?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="5.35A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="ISAT1" value="2.95A@10%"/>
<attribute name="ISAT2" value="5.85A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336015 "/>
<attribute name="RDC-MAX" value="39mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438336022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336022?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="3.6A"/>
<attribute name="ISAT" value="4.3A"/>
<attribute name="ISAT1" value="2.75A@10%"/>
<attribute name="ISAT2" value="5.55A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336022 "/>
<attribute name="RDC-MAX" value="80mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438336033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336033?ae"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="4.25A"/>
<attribute name="ISAT1" value="2.85A@10%"/>
<attribute name="ISAT2" value="5.35A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336033 "/>
<attribute name="RDC-MAX" value="114mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438336047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="ISAT1" value="2.4A@10%"/>
<attribute name="ISAT2" value="5.15A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336047 "/>
<attribute name="RDC-MAX" value="158mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438336068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="2.15A"/>
<attribute name="ISAT" value="2.85A"/>
<attribute name="ISAT1" value="1.85A@10%"/>
<attribute name="ISAT2" value="3.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336068 "/>
<attribute name="RDC-MAX" value="193mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78438336100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336100?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="2.35A"/>
<attribute name="ISAT1" value="1.55A@10%"/>
<attribute name="ISAT2" value="3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438336100 "/>
<attribute name="RDC-MAX" value="322mOhm"/>
<attribute name="SIZE" value=" 3020 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2506" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2506">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383210047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383210047?ae"/>
<attribute name="FRES" value="165MHz"/>
<attribute name="IR" value="3.25A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="ISAT1" value="2.55A@10%"/>
<attribute name="ISAT2" value="4.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383210047 "/>
<attribute name="RDC-MAX" value="95mOhm"/>
<attribute name="SIZE" value=" 2506 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_78438321010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438321010?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="ISAT1" value="1.7A@10%"/>
<attribute name="ISAT2" value="3.25A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438321010 "/>
<attribute name="RDC-MAX" value="196mOhm"/>
<attribute name="SIZE" value=" 2506 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_1610" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_1610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383130033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383130033?ae"/>
<attribute name="FRES" value="215MHz"/>
<attribute name="IR" value="3.25A"/>
<attribute name="ISAT" value="4.9A"/>
<attribute name="ISAT1" value="3.35A@10%"/>
<attribute name="ISAT2" value="6.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383130033 "/>
<attribute name="RDC-MAX" value="84mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383130047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383130047?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="2.95A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="ISAT1" value="3.05A@10%"/>
<attribute name="ISAT2" value="5.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383130047 "/>
<attribute name="RDC-MAX" value="101mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383130056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383130056?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="ISAT1" value="2.75A@10%"/>
<attribute name="ISAT2" value="5.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383130056 "/>
<attribute name="RDC-MAX" value="113mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_784383130068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383130068?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="IR" value="2.55A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="ISAT1" value="2.55A@10%"/>
<attribute name="ISAT2" value="4.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383130068 "/>
<attribute name="RDC-MAX" value="126mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_784383130082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383130082?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="2.35A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="4.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383130082 "/>
<attribute name="RDC-MAX" value="144mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_78438313010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438313010?ae"/>
<attribute name="FRES" value="111MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3.4A"/>
<attribute name="ISAT1" value="2.25A@10%"/>
<attribute name="ISAT2" value="4.25A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438313010 "/>
<attribute name="RDC-MAX" value="159mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438313012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438313012?ae"/>
<attribute name="FRES" value="109MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="ISAT1" value="2.2A@10%"/>
<attribute name="ISAT2" value="4.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438313012 "/>
<attribute name="RDC-MAX" value="174mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438313015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438313015?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="ISAT1" value="1.8A@10%"/>
<attribute name="ISAT2" value="3.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438313015 "/>
<attribute name="RDC-MAX" value="237mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438313022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438313022?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="ISAT1" value="1.5A@10%"/>
<attribute name="ISAT2" value="3.25A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438313022 "/>
<attribute name="RDC-MAX" value="388mOhm"/>
<attribute name="SIZE" value=" 1610 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2508" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383220047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383220047?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="3.35A"/>
<attribute name="ISAT" value="4.4A"/>
<attribute name="ISAT1" value="2.85A@10%"/>
<attribute name="ISAT2" value="5.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383220047 "/>
<attribute name="RDC-MAX" value="87mOhm"/>
<attribute name="SIZE" value=" 2508 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_78438322010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438322010?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="2.65A"/>
<attribute name="ISAT" value="3.35A"/>
<attribute name="ISAT1" value="2.15A@10%"/>
<attribute name="ISAT2" value="4.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438322010 "/>
<attribute name="RDC-MAX" value="133mOhm"/>
<attribute name="SIZE" value=" 2508 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438322022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438322022?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="ISAT1" value="1.4A@10%"/>
<attribute name="ISAT2" value="2.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438322022 "/>
<attribute name="RDC-MAX" value="302mOhm"/>
<attribute name="SIZE" value=" 2508 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2512HT" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
Created By Ella 2024-09-13
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2512HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383240033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383240033HT?ae"/>
<attribute name="FRES" value="174MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT1" value="4.1A@10%"/>
<attribute name="ISAT2" value="8.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383240033HT"/>
<attribute name="RDC-MAX" value="26.7mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383240047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383240047HT?ae"/>
<attribute name="FRES" value="131MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383240047HT"/>
<attribute name="RDC-MAX" value="34.7mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383240056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383240056HT?ae"/>
<attribute name="FRES" value="102MHz"/>
<attribute name="IR" value="4.7A"/>
<attribute name="ISAT1" value="3.2A@10%"/>
<attribute name="ISAT2" value="6.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383240056HT"/>
<attribute name="RDC-MAX" value="44.1mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_78438324010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324010HT?ae"/>
<attribute name="FRES" value="71MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT1" value="2.2A@10%"/>
<attribute name="ISAT2" value="4.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438324010HT"/>
<attribute name="RDC-MAX" value="61.5mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438324012HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324012HT?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT1" value="2.3A@10%"/>
<attribute name="ISAT2" value="4.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438324012HT"/>
<attribute name="RDC-MAX" value="74.7mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438324015HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324015HT?ae"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT1" value="1.9A@10%"/>
<attribute name="ISAT2" value="4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438324015HT"/>
<attribute name="RDC-MAX" value="102.1mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438324022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324022HT?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT1" value="1.6A@10%"/>
<attribute name="ISAT2" value="3.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438324022HT"/>
<attribute name="RDC-MAX" value="162.5mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438324033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324033HT?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT1" value="1.4A@10%"/>
<attribute name="ISAT2" value="3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438324033HT"/>
<attribute name="RDC-MAX" value="274.7mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438324047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324047HT?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT1" value="1.1A@10%"/>
<attribute name="ISAT2" value="2.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438324047HT"/>
<attribute name="RDC-MAX" value="367.6mOhm"/>
<attribute name="SIZE" value="2512HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3015" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383350047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383350047?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="ISAT1" value="4.35A@10%"/>
<attribute name="ISAT2" value="7.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383350047 "/>
<attribute name="RDC-MAX" value="23mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383350068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383350068?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="6.3A"/>
<attribute name="ISAT" value="8.1A"/>
<attribute name="ISAT1" value="5.8A@10%"/>
<attribute name="ISAT2" value="9.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383350068 "/>
<attribute name="RDC-MAX" value="30mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_784383350082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383350082?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="5.7A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="ISAT1" value="4.95A@10%"/>
<attribute name="ISAT2" value="9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383350082 "/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_78438335010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335010?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="4.95A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="ISAT1" value="3A@10%"/>
<attribute name="ISAT2" value="5.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335010 "/>
<attribute name="RDC-MAX" value="47mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438335022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335022?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="4.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335022 "/>
<attribute name="RDC-MAX" value="108mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438335033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335033?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="ISAT1" value="2.25A@10%"/>
<attribute name="ISAT2" value="3.85A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335033 "/>
<attribute name="RDC-MAX" value="131mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438335047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="ISAT1" value="1.85A@10%"/>
<attribute name="ISAT2" value="3.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335047 "/>
<attribute name="RDC-MAX" value="162mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438335068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335068?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="ISAT1" value="1.6A@10%"/>
<attribute name="ISAT2" value="3.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335068 "/>
<attribute name="RDC-MAX" value="287mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78438335100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335100?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="ISAT1" value="1.35A@10%"/>
<attribute name="ISAT2" value="3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335100 "/>
<attribute name="RDC-MAX" value="513mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_78438335150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335150?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.71A"/>
<attribute name="ISAT1" value="1.17A@10%"/>
<attribute name="ISAT2" value="2.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335150 "/>
<attribute name="RDC-MAX" value="830mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_78438335220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335220?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="ISAT1" value="1.1A@10%"/>
<attribute name="ISAT2" value="2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335220 "/>
<attribute name="RDC-MAX" value="1040mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_78438335330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335330?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="ISAT1" value="0.9A@10%"/>
<attribute name="ISAT2" value="1.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335330 "/>
<attribute name="RDC-MAX" value="1330mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_78438335470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335470?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="1.18A"/>
<attribute name="ISAT1" value="0.75A@10%"/>
<attribute name="ISAT2" value="1.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438335470 "/>
<attribute name="RDC-MAX" value="2300mOhm"/>
<attribute name="SIZE" value=" 3015 "/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3020HT" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
Created By Ella 2024-09-13
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3020HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383360068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383360068HT?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="6.4A"/>
<attribute name="ISAT1" value="2.8A@10%"/>
<attribute name="ISAT2" value="6.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383360068HT"/>
<attribute name="RDC-MAX" value="28.1mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438336010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336010HT?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT1" value="2.7A@10%"/>
<attribute name="ISAT2" value="6.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438336010HT"/>
<attribute name="RDC-MAX" value="32.8mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438336012HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336012HT?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="5.4A"/>
<attribute name="ISAT1" value="2.7A@10%"/>
<attribute name="ISAT2" value="6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438336012HT"/>
<attribute name="RDC-MAX" value="37.5mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438336015HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336015HT?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT1" value="2.4A@10%"/>
<attribute name="ISAT2" value="5.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438336015HT"/>
<attribute name="RDC-MAX" value="40.5mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438336022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336022HT?ae"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT1" value="2.3A@10%"/>
<attribute name="ISAT2" value="5.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438336022HT"/>
<attribute name="RDC-MAX" value="65.5mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438336033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336033HT?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT1" value="1.9A@10%"/>
<attribute name="ISAT2" value="4.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438336033HT"/>
<attribute name="RDC-MAX" value="98.8mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438336047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336047HT?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT1" value="2A@10%"/>
<attribute name="ISAT2" value="4.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438336047HT"/>
<attribute name="RDC-MAX" value="150.2mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438336068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438336068HT?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT1" value="1.8A@10%"/>
<attribute name="ISAT2" value="3.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438336068HT"/>
<attribute name="RDC-MAX" value="227.1mOhm"/>
<attribute name="SIZE" value="3020HT"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3010" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438333022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438333022?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="2.35A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="ISAT1" value="2.75A@10%"/>
<attribute name="ISAT2" value="4.85A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438333022 "/>
<attribute name="RDC-MAX" value="172mOhm"/>
<attribute name="SIZE" value=" 3010 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438333033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438333033?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="1.85A"/>
<attribute name="ISAT" value="2.95A"/>
<attribute name="ISAT1" value="2.05A@10%"/>
<attribute name="ISAT2" value="3.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438333033 "/>
<attribute name="RDC-MAX" value="266mOhm"/>
<attribute name="SIZE" value=" 3010 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438333047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438333047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="ISAT1" value="1.65A@10%"/>
<attribute name="ISAT2" value="3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438333047 "/>
<attribute name="RDC-MAX" value="409mOhm"/>
<attribute name="SIZE" value=" 3010 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_6030HT" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
Created By Ella 2024-09-13
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAIA_6030HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383770033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383770033HT?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="IR" value="21.6A"/>
<attribute name="ISAT1" value="14.1A@10%"/>
<attribute name="ISAT2" value="27.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383770033HT"/>
<attribute name="RDC-MAX" value="3mOhm"/>
<attribute name="SIZE" value="6030HT"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383770068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383770068HT?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="16.7A"/>
<attribute name="ISAT1" value="10.6A@10%"/>
<attribute name="ISAT2" value="21.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383770068HT"/>
<attribute name="RDC-MAX" value="5.6mOhm"/>
<attribute name="SIZE" value="6030HT"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438377010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438377010HT?ae"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="IR" value="15.2A"/>
<attribute name="ISAT1" value="8.7A@10%"/>
<attribute name="ISAT2" value="18A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438377010HT"/>
<attribute name="RDC-MAX" value="6.9mOhm"/>
<attribute name="SIZE" value="6030HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438377022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438377022HT?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="11.4A"/>
<attribute name="ISAT1" value="6.3A@10%"/>
<attribute name="ISAT2" value="12.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438377022HT"/>
<attribute name="RDC-MAX" value="13.7mOhm"/>
<attribute name="SIZE" value="6030HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438377033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438377033HT?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="9.6A"/>
<attribute name="ISAT1" value="5.2A@10%"/>
<attribute name="ISAT2" value="11.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438377033HT"/>
<attribute name="RDC-MAX" value="20.4mOhm"/>
<attribute name="SIZE" value="6030HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2010" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
Created By Ella 2024-09-13
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383430033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383430033?ae"/>
<attribute name="FRES" value="205MHz"/>
<attribute name="IR" value="4.35A"/>
<attribute name="ISAT1" value="3.9A@10%"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383430033 "/>
<attribute name="RDC-MAX" value="53mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383430047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383430047?ae"/>
<attribute name="FRES" value="175MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT1" value="3.55A@10%"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383430047 "/>
<attribute name="RDC-MAX" value="63mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383430056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383430056?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="IR" value="3.6A"/>
<attribute name="ISAT1" value="3.3A@10%"/>
<attribute name="ISAT2" value="6.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383430056 "/>
<attribute name="RDC-MAX" value="73mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_784383430068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383430068?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT1" value="3.15A@10%"/>
<attribute name="ISAT2" value="5.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383430068 "/>
<attribute name="RDC-MAX" value="84mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_784383430082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383430082?ae"/>
<attribute name="FRES" value="125MHz"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT1" value="2.8A@10%"/>
<attribute name="ISAT2" value="5.35A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383430082 "/>
<attribute name="RDC-MAX" value="92mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_78438343010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438343010?ae"/>
<attribute name="FRES" value="99MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="4.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438343010 "/>
<attribute name="RDC-MAX" value="104mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438343012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438343012?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT1" value="2.55A@10%"/>
<attribute name="ISAT2" value="4.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438343012 "/>
<attribute name="RDC-MAX" value="136mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438343015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438343015?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="2.05A"/>
<attribute name="ISAT1" value="2A@10%"/>
<attribute name="ISAT2" value="3.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438343015 "/>
<attribute name="RDC-MAX" value="180mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438343022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438343022?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT1" value="1.65A@10%"/>
<attribute name="ISAT2" value="3.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438343022 "/>
<attribute name="RDC-MAX" value="270mOhm"/>
<attribute name="SIZE" value=" 2010 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_4020HT" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAIA_4020HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383560033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383560033HT?ae"/>
<attribute name="FRES" value="98MHz"/>
<attribute name="IR" value="13.3A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="ISAT1" value="7.25A@10%"/>
<attribute name="ISAT2" value="14.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383560033HT"/>
<attribute name="RDC-MAX" value="7.5mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383560047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383560047HT?ae"/>
<attribute name="FRES" value="83MHz"/>
<attribute name="IR" value="12.7A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="ISAT1" value="6.45A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383560047HT"/>
<attribute name="RDC-MAX" value="8.1mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383560056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383560056HT?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="IR" value="12.15A"/>
<attribute name="ISAT" value="9.55A"/>
<attribute name="ISAT1" value="6.05A@10%"/>
<attribute name="ISAT2" value="13A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383560056HT"/>
<attribute name="RDC-MAX" value="8.6mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_784383560068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383560068HT?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="11.7A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="ISAT1" value="5.45A@10%"/>
<attribute name="ISAT2" value="11.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383560068HT"/>
<attribute name="RDC-MAX" value="9.2mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438356010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356010HT?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="8.75A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="ISAT1" value="4.25A@10%"/>
<attribute name="ISAT2" value="9.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356010HT"/>
<attribute name="RDC-MAX" value="15.5mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438356012HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356012HT?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="6.9A"/>
<attribute name="ISAT1" value="4.3A@10%"/>
<attribute name="ISAT2" value="9.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356012HT"/>
<attribute name="RDC-MAX" value="18.4mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438356015HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356015HT?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="7.45A"/>
<attribute name="ISAT" value="6.6A"/>
<attribute name="ISAT1" value="4.2A@10%"/>
<attribute name="ISAT2" value="9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356015HT"/>
<attribute name="RDC-MAX" value="20.7mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438356018HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356018HT?ae"/>
<attribute name="FRES" value="37.5MHz"/>
<attribute name="IR" value="6.05A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="ISAT1" value="3.95A@10%"/>
<attribute name="ISAT2" value="8.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356018HT"/>
<attribute name="RDC-MAX" value="29.9mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_78438356022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356022HT?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="5.9A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="ISAT1" value="3.7A@10%"/>
<attribute name="ISAT2" value="7.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356022HT"/>
<attribute name="RDC-MAX" value="32.2mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438356033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356033HT?ae"/>
<attribute name="FRES" value="25.5MHz"/>
<attribute name="IR" value="4.45A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="ISAT1" value="3.1A@10%"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356033HT"/>
<attribute name="RDC-MAX" value="51.8mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438356047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356047HT?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="3.7A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="ISAT1" value="2.35A@10%"/>
<attribute name="ISAT2" value="5.05A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356047HT"/>
<attribute name="RDC-MAX" value="74.8mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438356056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438356056HT?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="ISAT1" value="2.25A@10%"/>
<attribute name="ISAT2" value="4.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438356056HT"/>
<attribute name="RDC-MAX" value="80.5mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_5020" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAIA_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383660082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383660082?ae"/>
<attribute name="FRES" value="53.5MHz"/>
<attribute name="IR" value="13.25A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="ISAT1" value="7.1A@10%"/>
<attribute name="ISAT2" value="15.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383660082 "/>
<attribute name="RDC-MAX" value="9.6mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_78438366010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438366010?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="11.1A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="ISAT1" value="6.25A@10%"/>
<attribute name="ISAT2" value="14A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438366010 "/>
<attribute name="RDC-MAX" value="13.1mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438366015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438366015?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="8.45A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="ISAT1" value="5.85A@10%"/>
<attribute name="ISAT2" value="13.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438366015 "/>
<attribute name="RDC-MAX" value="21.3mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438366022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438366022?ae"/>
<attribute name="FRES" value="31.5MHz"/>
<attribute name="IR" value="7.4A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="ISAT1" value="5.35A@10%"/>
<attribute name="ISAT2" value="12A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438366022 "/>
<attribute name="RDC-MAX" value="27.3mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438366033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438366033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="ISAT1" value="4.4A@10%"/>
<attribute name="ISAT2" value="9.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438366033 "/>
<attribute name="RDC-MAX" value="38.4mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438366047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438366047?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="4.65A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="ISAT1" value="3.5A@10%"/>
<attribute name="ISAT2" value="7.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438366047 "/>
<attribute name="RDC-MAX" value="63mOhm"/>
<attribute name="SIZE" value=" 5020 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_5030" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAIA_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438367010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438367010?ae"/>
<attribute name="FRES" value="44.5MHz"/>
<attribute name="IR" value="11.85A"/>
<attribute name="ISAT" value="9.6A"/>
<attribute name="ISAT1" value="5.95A@10%"/>
<attribute name="ISAT2" value="13.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438367010 "/>
<attribute name="RDC-MAX" value="11.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438367022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438367022?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="9.8A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="ISAT1" value="4.55A@10%"/>
<attribute name="ISAT2" value="10.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438367022 "/>
<attribute name="RDC-MAX" value="16.1mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438367033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438367033?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="7.3A"/>
<attribute name="ISAT1" value="4.35A@10%"/>
<attribute name="ISAT2" value="10A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438367033 "/>
<attribute name="RDC-MAX" value="23mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438367047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438367047?ae"/>
<attribute name="FRES" value="18.5MHz"/>
<attribute name="IR" value="6.45A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="ISAT1" value="3.35A@10%"/>
<attribute name="ISAT2" value="6.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438367047 "/>
<attribute name="RDC-MAX" value="34.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438367068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438367068?ae"/>
<attribute name="FRES" value="15.5MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="5.7A"/>
<attribute name="ISAT1" value="3.7A@10%"/>
<attribute name="ISAT2" value="7.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438367068 "/>
<attribute name="RDC-MAX" value="48.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78438367082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438367082?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="4.85A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="ISAT1" value="3.25A@10%"/>
<attribute name="ISAT2" value="6.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438367082 "/>
<attribute name="RDC-MAX" value="57.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_78438367100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438367100?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="ISAT1" value="3.25A@10%"/>
<attribute name="ISAT2" value="6.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438367100 "/>
<attribute name="RDC-MAX" value="70.2mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_4030" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAIA_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438357010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IR" value="10.25A"/>
<attribute name="ISAT" value="9.6A"/>
<attribute name="ISAT1" value="6.2A@10%"/>
<attribute name="ISAT2" value="12.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357010 "/>
<attribute name="RDC-MAX" value="13.5mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438357012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357012?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="9.4A"/>
<attribute name="ISAT" value="8.8A"/>
<attribute name="ISAT1" value="5.55A@10%"/>
<attribute name="ISAT2" value="11.6A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357012 "/>
<attribute name="RDC-MAX" value="15.5mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438357015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357015?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="8.2A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="ISAT1" value="5.55A@10%"/>
<attribute name="ISAT2" value="11A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357015 "/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438357018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="ISAT1" value="5.05A@10%"/>
<attribute name="ISAT2" value="10.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357018 "/>
<attribute name="RDC-MAX" value="21mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_78438357022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357022?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="ISAT1" value="4.6A@10%"/>
<attribute name="ISAT2" value="9.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357022 "/>
<attribute name="RDC-MAX" value="26mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438357033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357033?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="ISAT1" value="3.3A@10%"/>
<attribute name="ISAT2" value="7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357033 "/>
<attribute name="RDC-MAX" value="33.5mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438357047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357047?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="5.1A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="ISAT1" value="4.15A@10%"/>
<attribute name="ISAT2" value="8.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357047 "/>
<attribute name="RDC-MAX" value="44mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438357056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357056?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="4.7A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="ISAT1" value="3.9A@10%"/>
<attribute name="ISAT2" value="8.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357056 "/>
<attribute name="RDC-MAX" value="51mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_78438357068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357068?ae"/>
<attribute name="FRES" value="19.5MHz"/>
<attribute name="IR" value="3.75A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="ISAT1" value="3.5A@10%"/>
<attribute name="ISAT2" value="7.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357068 "/>
<attribute name="RDC-MAX" value="74mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78438357082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357082?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="3.45A"/>
<attribute name="ISAT" value="5.2A"/>
<attribute name="ISAT1" value="3.35A@10%"/>
<attribute name="ISAT2" value="6.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357082 "/>
<attribute name="RDC-MAX" value="86mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_78438357100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438357100?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="3.05A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="ISAT1" value="3A@10%"/>
<attribute name="ISAT2" value="5.95A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438357100 "/>
<attribute name="RDC-MAX" value="110mOhm"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2510" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383230033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383230033?ae"/>
<attribute name="FRES" value="180MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="ISAT1" value="4.25A@10%"/>
<attribute name="ISAT2" value="8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383230033 "/>
<attribute name="RDC-MAX" value="38mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383230047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383230047?ae"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="6.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383230047 "/>
<attribute name="RDC-MAX" value="48mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383230068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383230068?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="IR" value="4.25A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="ISAT1" value="3.1A@10%"/>
<attribute name="ISAT2" value="6.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383230068 "/>
<attribute name="RDC-MAX" value="60mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_784383230082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383230082?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT" value="4.25A"/>
<attribute name="ISAT1" value="2.7A@10%"/>
<attribute name="ISAT2" value="5.45A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383230082 "/>
<attribute name="RDC-MAX" value="69mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_78438323010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323010?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="3.55A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="ISAT1" value="2.6A@10%"/>
<attribute name="ISAT2" value="5.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323010 "/>
<attribute name="RDC-MAX" value="75mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438323012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323012?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="3.05A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="ISAT1" value="2.45A@10%"/>
<attribute name="ISAT2" value="4.85A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323012 "/>
<attribute name="RDC-MAX" value="106mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438323015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323015?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="2.85A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="ISAT1" value="2.25A@10%"/>
<attribute name="ISAT2" value="4.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323015 "/>
<attribute name="RDC-MAX" value="110mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438323022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323022?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="ISAT1" value="2A@10%"/>
<attribute name="ISAT2" value="3.55A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323022 "/>
<attribute name="RDC-MAX" value="176mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438323033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323033?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="ISAT1" value="1.35A@10%"/>
<attribute name="ISAT2" value="2.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323033 "/>
<attribute name="RDC-MAX" value="264mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438323047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.75A"/>
<attribute name="ISAT1" value="1.1A@10%"/>
<attribute name="ISAT2" value="2.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323047 "/>
<attribute name="RDC-MAX" value="388mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438323068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323068?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1.05A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="ISAT1" value="1.05A@10%"/>
<attribute name="ISAT2" value="2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323068 "/>
<attribute name="RDC-MAX" value="648mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78438323082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323082?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.45A"/>
<attribute name="ISAT1" value="0.9A@10%"/>
<attribute name="ISAT2" value="1.85A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323082 "/>
<attribute name="RDC-MAX" value="743mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_78438323100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438323100?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="ISAT1" value="0.85A@10%"/>
<attribute name="ISAT2" value="1.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438323100 "/>
<attribute name="RDC-MAX" value="843mOhm"/>
<attribute name="SIZE" value=" 2510 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3015HT" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
Created By Ella 2024-09-13
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3015HT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383350056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383350056HT?ae"/>
<attribute name="FRES" value="93MHz"/>
<attribute name="IR" value="7.3A"/>
<attribute name="ISAT1" value="4A@10%"/>
<attribute name="ISAT2" value="7.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383350056HT"/>
<attribute name="RDC-MAX" value="22.2mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_784383350068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383350068HT?ae"/>
<attribute name="FRES" value="78MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="7.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="784383350068HT"/>
<attribute name="RDC-MAX" value="25.5mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438335010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335010HT?ae"/>
<attribute name="FRES" value="73MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT1" value="3A@10%"/>
<attribute name="ISAT2" value="5.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438335010HT"/>
<attribute name="RDC-MAX" value="53.2mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438335022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335022HT?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT1" value="2.4A@10%"/>
<attribute name="ISAT2" value="5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438335022HT"/>
<attribute name="RDC-MAX" value="96mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438335033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335033HT?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT1" value="2A@10%"/>
<attribute name="ISAT2" value="4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438335033HT"/>
<attribute name="RDC-MAX" value="133mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438335047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335047HT?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT1" value="1.4A@10%"/>
<attribute name="ISAT2" value="3.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438335047HT"/>
<attribute name="RDC-MAX" value="187.4mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438335068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335068HT?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT1" value="1.4A@10%"/>
<attribute name="ISAT2" value="3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438335068HT"/>
<attribute name="RDC-MAX" value="310.7mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78438335100HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438335100HT?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT1" value="1.1A@10%"/>
<attribute name="ISAT2" value="2.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438335100HT"/>
<attribute name="RDC-MAX" value="549.5mOhm"/>
<attribute name="SIZE" value="3015HT"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_4012" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
Created By Ella 2024-09-13
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAIA_4012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7843835400033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843835400033?ae"/>
<attribute name="FRES" value="682MHz"/>
<attribute name="IR" value="33.5A"/>
<attribute name="ISAT1" value="19A@10%"/>
<attribute name="ISAT2" value="40A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843835400033 "/>
<attribute name="RDC-MAX" value="1.1mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="0.033uH"/>
</technology>
<technology name="_7843835400068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843835400068?ae"/>
<attribute name="FRES" value="374MHz"/>
<attribute name="IR" value="27A"/>
<attribute name="ISAT1" value="18A@10%"/>
<attribute name="ISAT2" value="38A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7843835400068 "/>
<attribute name="RDC-MAX" value="1.9mOhm"/>
<attribute name="SIZE" value=" 4012 "/>
<attribute name="VALUE" value="0.068uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_2512" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383240047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383240047?ae"/>
<attribute name="FRES" value="145MHz"/>
<attribute name="IR" value="5.35A"/>
<attribute name="ISAT" value="6.25A"/>
<attribute name="ISAT1" value="4.15A@10%"/>
<attribute name="ISAT2" value="8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383240047 "/>
<attribute name="RDC-MAX" value="40mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383240056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383240056?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="4.75A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="ISAT1" value="4.25A@10%"/>
<attribute name="ISAT2" value="7.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383240056 "/>
<attribute name="RDC-MAX" value="49mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_784383240068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383240068?ae"/>
<attribute name="FRES" value="102MHz"/>
<attribute name="IR" value="4.25A"/>
<attribute name="ISAT" value="5.85A"/>
<attribute name="ISAT1" value="3.8A@10%"/>
<attribute name="ISAT2" value="7.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383240068 "/>
<attribute name="RDC-MAX" value="59mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438324010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324010?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="4.05A"/>
<attribute name="ISAT" value="4.9A"/>
<attribute name="ISAT1" value="3.2A@10%"/>
<attribute name="ISAT2" value="6.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324010 "/>
<attribute name="RDC-MAX" value="60mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438324012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324012?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="ISAT1" value="3.05A@10%"/>
<attribute name="ISAT2" value="5.8A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324012 "/>
<attribute name="RDC-MAX" value="80mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438324015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="3.05A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="4.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324015 "/>
<attribute name="RDC-MAX" value="99mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438324022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324022?ae"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="IR" value="2.45A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="ISAT1" value="1.85A@10%"/>
<attribute name="ISAT2" value="3.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324022 "/>
<attribute name="RDC-MAX" value="141mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438324033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324033?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="ISAT1" value="1.75A@10%"/>
<attribute name="ISAT2" value="3.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324033 "/>
<attribute name="RDC-MAX" value="260mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438324047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="ISAT1" value="1.4A@10%"/>
<attribute name="ISAT2" value="2.65A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324047 "/>
<attribute name="RDC-MAX" value="345mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438324056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324056?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.75A"/>
<attribute name="ISAT1" value="1.15A@10%"/>
<attribute name="ISAT2" value="2.2A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324056 "/>
<attribute name="RDC-MAX" value="465mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_78438324068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324068?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="1.05A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="ISAT1" value="1A@10%"/>
<attribute name="ISAT2" value="2.05A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324068 "/>
<attribute name="RDC-MAX" value="640mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_78438324082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324082?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="ISAT1" value="1A@10%"/>
<attribute name="ISAT2" value="1.9A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324082 "/>
<attribute name="RDC-MAX" value="720mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_78438324100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438324100?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="ISAT1" value="0.95A@10%"/>
<attribute name="ISAT2" value="1.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438324100 "/>
<attribute name="RDC-MAX" value="780mOhm"/>
<attribute name="SIZE" value=" 2512 "/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAIA_3012" prefix="L">
<description>&lt;b&gt; WE-MAIA SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics&lt;/B&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;No acoustic noise and no leakage flux noise
&lt;br&gt;Operating temperature range: -40°C up to +125°C
&lt;br&gt;AEC-Q 200

&lt;br&gt;

&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Powertrain coverters
&lt;br&gt;Body electronics &amp; lighting
&lt;br&gt;Infotainment systems
&lt;br&gt;DC/DC-converter 48 V/12 V
&lt;br&gt;POL-converter
&lt;br&gt;DC/DC converter for field programmable gate array
&lt;br&gt;BMS (battery management system)
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o56285v209%20Family_WE-MAIA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAIA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAIA
&lt;/a&gt;&lt;p&gt;
&lt;br&gt;Updated By Ella Wu  2024-02-02
&lt;br&gt;2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-GAP"/>
</gates>
<devices>
<device name="" package="WE-MAIA_3012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784383340033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383340033?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="IR" value="7.4A"/>
<attribute name="ISAT" value="11.1A"/>
<attribute name="ISAT1" value="8.1A@10%"/>
<attribute name="ISAT2" value="13.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383340033 "/>
<attribute name="RDC-MAX" value="22.8mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_784383340047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383340047?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT" value="9.4A"/>
<attribute name="ISAT1" value="5.95A@10%"/>
<attribute name="ISAT2" value="12.3A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383340047 "/>
<attribute name="RDC-MAX" value="26.4mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_784383340056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383340056?ae"/>
<attribute name="FRES" value="108MHz"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="ISAT1" value="5.65A@10%"/>
<attribute name="ISAT2" value="11.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383340056 "/>
<attribute name="RDC-MAX" value="34.8mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_784383340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784383340068?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="5.15A"/>
<attribute name="ISAT" value="7.7A"/>
<attribute name="ISAT1" value="4.95A@10%"/>
<attribute name="ISAT2" value="10A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784383340068 "/>
<attribute name="RDC-MAX" value="43.2mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_78438334010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334010?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="4.75A"/>
<attribute name="ISAT" value="6.6A"/>
<attribute name="ISAT1" value="4.3A@10%"/>
<attribute name="ISAT2" value="8.4A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334010 "/>
<attribute name="RDC-MAX" value="50.5mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_78438334012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334012?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="IR" value="4.05A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="ISAT1" value="4.15A@10%"/>
<attribute name="ISAT2" value="7.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334012 "/>
<attribute name="RDC-MAX" value="66mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_78438334015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="5.7A"/>
<attribute name="ISAT1" value="3.9A@10%"/>
<attribute name="ISAT2" value="7.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334015 "/>
<attribute name="RDC-MAX" value="96mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_78438334022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334022?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="6.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334022 "/>
<attribute name="RDC-MAX" value="115mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_78438334033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334033?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="2.25A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="ISAT1" value="2.75A@10%"/>
<attribute name="ISAT2" value="5.1A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334033 "/>
<attribute name="RDC-MAX" value="179.7mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_78438334047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="ISAT1" value="2.6A@10%"/>
<attribute name="ISAT2" value="4.75A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334047 "/>
<attribute name="RDC-MAX" value="307.8mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_78438334056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334056?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="ISAT1" value="2.1A@10%"/>
<attribute name="ISAT2" value="3.7A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334056 "/>
<attribute name="RDC-MAX" value="389mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_78438334068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438334068?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="ISAT1" value="1.75A@10%"/>
<attribute name="ISAT2" value="3.5A@30%"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 78438334068 "/>
<attribute name="RDC-MAX" value="423.4mOhm"/>
<attribute name="SIZE" value=" 3012 "/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
