<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-MAPI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 20225-03-21&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MAPI_3015">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:3015,SMT,2pins
&lt;br&gt;LXWXH=3X3X1.5mm</description>
</package>
<package name="WE-MAPI_3012">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:3012,SMT,2pins
&lt;br&gt;LXWXH=3X3X1.2mm</description>
</package>
<package name="WE-MAPI_6030">
</package>
<package name="WE-MAPI_2508">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
 &lt;br&gt;Size:2508,SMT,2pins
&lt;br&gt;LXWXH=2.5X2X0.8mm</description>
</package>
<package name="WE-MAPI_5030">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:5030,SMT,2pins
&lt;br&gt;LXWXH=5.4X5.4X3.1mm</description>
</package>
<package name="WE-MAPI_3020">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:3020,SMT,2pins
&lt;br&gt;LXWXH=3X3X2mm</description>
</package>
<package name="WE-MAPI_2510">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
 &lt;br&gt;Size:2510,SMT,2pins
&lt;br&gt;LXWXH=2.5X2X1mm</description>
</package>
<package name="WE-MAPI_5020">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size5020,SMT,2pins
&lt;br&gt;LXWXH=5.4X5.4X2.1mm</description>
</package>
<package name="WE-MAPI_2506">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:2506,SMT,2pins
&lt;br&gt;LXWXH=2.5X2X0.6mm</description>
</package>
<package name="WE-MAPI_4012">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4012,SMT,2pins
&lt;br&gt;LXWXH=4X4X1.3mm</description>
</package>
<package name="WE-MAPI_4030">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4030,SMT,2pins
&lt;br&gt;LXW=4X4mm</description>
</package>
<package name="WE-MAPI_2010">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:2010,SMT,2pins
&lt;br&gt;LXWXH=2X1.6X1mm</description>
</package>
<package name="WE-MAPI_3010">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:3010,SMT,2pins
&lt;br&gt;LXWXH=3X3X1mm</description>
</package>
<package name="WE-MAPI_1610">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
 &lt;br&gt;Size:1610,SMT,2pins
&lt;br&gt;LXWXH=1.6X1.6X1mm</description>
</package>
<package name="WE-MAPI_4020">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4020,SMT,2pins
&lt;br&gt;LXWXH=4X4X2mm</description>
</package>
<package name="WE-MAPI_2512">
<description>&lt;b&gt;WE-MAPI  SMD Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:2512,SMT,2pins
&lt;br&gt;LXWXH=2.5X2X1.2mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MAPI_3015HT" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383350056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383350056HT?ae"/>
<attribute name="FRES" value="93MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="7.3A @40K"/>
<attribute name="ISAT" value="7.8A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383350056HT"/>
<attribute name="RDC-TYP" value="19.3mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_744383350068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383350068HT?ae"/>
<attribute name="FRES" value="78MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="6.8A @40K"/>
<attribute name="ISAT" value="7.4A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383350068HT"/>
<attribute name="RDC-TYP" value="22.1mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438335010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335010HT?ae"/>
<attribute name="FRES" value="73MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="4.5A @40K"/>
<attribute name="ISAT" value="5.9A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335010HT"/>
<attribute name="RDC-TYP" value="46.2mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438335022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335022HT?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="3.2A @40K"/>
<attribute name="ISAT" value="5A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335022HT"/>
<attribute name="RDC-TYP" value="83.4mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438335033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335033HT?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="2.7A @40K"/>
<attribute name="ISAT" value="4A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335033HT"/>
<attribute name="RDC-TYP" value="115.6mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438335047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335047HT?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="2.2A @40K"/>
<attribute name="ISAT" value="3.2A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335047HT"/>
<attribute name="RDC-TYP" value="162.9mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438335068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335068HT?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="1.7A @40K"/>
<attribute name="ISAT" value="3A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335068HT"/>
<attribute name="RDC-TYP" value="270.1mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438335100HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335100HT?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="1.2A @40K"/>
<attribute name="ISAT" value="2.4A @30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335100HT"/>
<attribute name="RDC-TYP" value="477.8mOhm"/>
<attribute name="SIZE" value="3015 HT"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3012" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383340033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383340033?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="7.4A @40K"/>
<attribute name="ISAT" value="13.3A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383340033"/>
<attribute name="RDC-TYP" value="19mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_744383340047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383340047?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="6.8A @40K"/>
<attribute name="ISAT" value="12.3A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383340047"/>
<attribute name="RDC-TYP" value="22mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_744383340056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383340056?ae"/>
<attribute name="FRES" value="108MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="5.8A @40K"/>
<attribute name="ISAT" value="11.1A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383340056"/>
<attribute name="RDC-TYP" value="29mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_744383340068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383340068?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="5.15A @40K"/>
<attribute name="ISAT" value="10A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383340068"/>
<attribute name="RDC-TYP" value="36mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334010?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="4.75A @40K"/>
<attribute name="ISAT" value="8.4A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334010"/>
<attribute name="RDC-TYP" value="42.1mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334012?ae"/>
<attribute name="FRES" value="66MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="4.05A @40K"/>
<attribute name="ISAT" value="7.5A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334012"/>
<attribute name="RDC-TYP" value="55mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="3.3A @40K"/>
<attribute name="ISAT" value="7.1A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334015"/>
<attribute name="RDC-TYP" value="80mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334022?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="2.9A @40K"/>
<attribute name="ISAT" value="6.1A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334022"/>
<attribute name="RDC-TYP" value="100mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334033?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="2.25A @40K"/>
<attribute name="ISAT" value="5.1A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334033"/>
<attribute name="RDC-TYP" value="156.3mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.7A @40K"/>
<attribute name="ISAT" value="4.75A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334047"/>
<attribute name="RDC-TYP" value="267.7mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334056?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.45A @40K"/>
<attribute name="ISAT" value="3.7A @30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334056"/>
<attribute name="RDC-TYP" value="338.3mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438334068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438334068?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.4A @40K"/>
<attribute name="ISAT" value="3.5A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438334068"/>
<attribute name="RDC-TYP" value="368.2mOhm"/>
<attribute name="SIZE" value="3012"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3015" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3015">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383350047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383350047?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="7.1A @40K"/>
<attribute name="ISAT" value="7.4A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383350047"/>
<attribute name="RDC-TYP" value="20mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_744383350068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383350068?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="6.3A @40K"/>
<attribute name="ISAT" value="9.7A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383350068"/>
<attribute name="RDC-TYP" value="25mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_744383350082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383350082?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="5.7A @40K"/>
<attribute name="ISAT" value="8.6A @30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383350082"/>
<attribute name="RDC-TYP" value="30mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335010?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="4.95A @40K"/>
<attribute name="ISAT" value="5.95A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335010"/>
<attribute name="RDC-TYP" value="39mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335022?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="3A @40K"/>
<attribute name="ISAT" value="4.2A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335022"/>
<attribute name="RDC-TYP" value="94mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335033?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="2.7A @40K"/>
<attribute name="ISAT" value="3.85A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335033"/>
<attribute name="RDC-TYP" value="114mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="2.4A @40K"/>
<attribute name="ISAT" value="3.7A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335047"/>
<attribute name="RDC-TYP" value="141mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335068?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="1.75A @40K"/>
<attribute name="ISAT" value="3.1A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335068"/>
<attribute name="RDC-TYP" value="250mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335100?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="1.25A @40K"/>
<attribute name="ISAT" value="2.75A @30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335100"/>
<attribute name="RDC-TYP" value="446mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335150?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="0.95A @40K"/>
<attribute name="ISAT" value="2.2A @30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335150"/>
<attribute name="RDC-TYP" value="720mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335220?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="0.85A @40K"/>
<attribute name="ISAT" value="1.95A @30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335220"/>
<attribute name="RDC-TYP" value="940mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335330?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="0.7A @40K"/>
<attribute name="ISAT" value="1.7A @30%"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335330"/>
<attribute name="RDC-TYP" value="1210mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438335470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438335470?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="1.5mm"/>
<attribute name="IRP" value="0.55A @40K"/>
<attribute name="ISAT" value="1.5A @30%"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438335470"/>
<attribute name="RDC-TYP" value="2090mOhm"/>
<attribute name="SIZE" value="3015"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_6030" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383770033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383770033?ae"/>
<attribute name="FRES" value="93MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="22.8A @40K"/>
<attribute name="ISAT" value="29A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383770033"/>
<attribute name="RDC-TYP" value="2.5mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_744383770068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383770068?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="18.5A @40K"/>
<attribute name="ISAT" value="23.5A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383770068"/>
<attribute name="RDC-TYP" value="3.7mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_74438377010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438377010?ae"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="16.6A @40K"/>
<attribute name="ISAT" value="19.5A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438377010"/>
<attribute name="RDC-TYP" value="4.8mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_74438377015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438377015?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="13.1A @40K"/>
<attribute name="ISAT" value="15.7A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438377015"/>
<attribute name="RDC-TYP" value="8.6mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_74438377022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438377022?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="12.4A @40K"/>
<attribute name="ISAT" value="14A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438377022"/>
<attribute name="RDC-TYP" value="10.3mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_74438377033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438377033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="9.9A @40K"/>
<attribute name="ISAT" value="10.8A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438377033"/>
<attribute name="RDC-TYP" value="15.9mOhm"/>
<attribute name="SIZE" value="6030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_6030HT" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2025-03-21&lt;br&gt;
2025(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_6030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383770030HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383770030HT?ae"/>
<attribute name="FRES" value="119MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="15.8A @40K"/>
<attribute name="ISAT" value="35A @30%"/>
<attribute name="L" value="0.3uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383770030HT"/>
<attribute name="RDC-TYP" value="2.4mOhm"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="VOP" value=""/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_744383770033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383770033HT?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="21.6A @40K"/>
<attribute name="ISAT" value="27.5A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383770033HT"/>
<attribute name="RDC-TYP" value="2.6mOhm"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_744383770068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383770068HT?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="16.7A @40K"/>
<attribute name="ISAT" value="21.5A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383770068HT"/>
<attribute name="RDC-TYP" value="4.8mOhm"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_74438377010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438377010HT?ae"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="15.2A @40K"/>
<attribute name="ISAT" value="18A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438377010HT"/>
<attribute name="RDC-TYP" value="6mOhm"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_74438377022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438377022HT?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="11.4A @40K"/>
<attribute name="ISAT" value="12.8A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438377022HT"/>
<attribute name="RDC-TYP" value="11.9mOhm"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
<technology name="_74438377033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438377033HT?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="9.6A @40K"/>
<attribute name="ISAT" value="11.2A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="6.8mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438377033HT"/>
<attribute name="RDC-TYP" value="17.7mOhm"/>
<attribute name="SIZE" value="6030 HT"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="6.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2508" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2508">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383220047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383220047?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IRP" value="3.35A @40K"/>
<attribute name="ISAT" value="5.65A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383220047"/>
<attribute name="RDC-TYP" value="70mOhm"/>
<attribute name="SIZE" value="2508"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438322010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438322010?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IRP" value="2.65A @40K"/>
<attribute name="ISAT" value="4.4A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438322010"/>
<attribute name="RDC-TYP" value="107mOhm"/>
<attribute name="SIZE" value="2508"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438322022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438322022?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IRP" value="1.65A @40K"/>
<attribute name="ISAT" value="2.8A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438322022"/>
<attribute name="RDC-TYP" value="252mOhm"/>
<attribute name="SIZE" value="2508"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_5030" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383670013">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383670013?ae"/>
<attribute name="FRES" value="189MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="27.4A @40K"/>
<attribute name="ISAT" value="30A @30%"/>
<attribute name="L" value="0.13uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383670013"/>
<attribute name="RDC-TYP" value="1.4mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.13uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_744383670033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383670033?ae"/>
<attribute name="FRES" value="108MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="21.6A @40K"/>
<attribute name="ISAT" value="26.5A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383670033"/>
<attribute name="RDC-TYP" value="2.8mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_744383670047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383670047?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="20.8A @40K"/>
<attribute name="ISAT" value="20A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383670047"/>
<attribute name="RDC-TYP" value="3.5mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438367010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438367010?ae"/>
<attribute name="FRES" value="44.5MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="11.85A @40K"/>
<attribute name="ISAT" value="13.1A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438367010"/>
<attribute name="RDC-TYP" value="10mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438367022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438367022?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="9.8A @40K"/>
<attribute name="ISAT" value="10.2A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438367022"/>
<attribute name="RDC-TYP" value="14mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438367033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438367033?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="8A @40K"/>
<attribute name="ISAT" value="10A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438367033"/>
<attribute name="RDC-TYP" value="20mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438367047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438367047?ae"/>
<attribute name="FRES" value="18.5MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="6.45A @40K"/>
<attribute name="ISAT" value="6.5A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438367047"/>
<attribute name="RDC-TYP" value="30mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438367068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438367068?ae"/>
<attribute name="FRES" value="15.5MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="5.3A @40K"/>
<attribute name="ISAT" value="7.7A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438367068"/>
<attribute name="RDC-TYP" value="42mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438367082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438367082?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="4.85A @40K"/>
<attribute name="ISAT" value="6.6A @30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438367082"/>
<attribute name="RDC-TYP" value="50mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438367100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438367100?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="4.3A @40K"/>
<attribute name="ISAT" value="6.6A @30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438367100"/>
<attribute name="RDC-TYP" value="61mOhm"/>
<attribute name="SIZE" value="5030"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3020HT" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383360068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383360068HT?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="6.4A @40K"/>
<attribute name="ISAT" value="6.7A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383360068HT"/>
<attribute name="RDC-TYP" value="24.4mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438336010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336010HT?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="5.8A @40K"/>
<attribute name="ISAT" value="6.3A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336010HT"/>
<attribute name="RDC-TYP" value="28.5mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438336012HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336012HT?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="5.4A @40K"/>
<attribute name="ISAT" value="6A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336012HT"/>
<attribute name="RDC-TYP" value="32.6mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438336015HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336015HT?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="5.2A @40K"/>
<attribute name="ISAT" value="5.5A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336015HT"/>
<attribute name="RDC-TYP" value="35.2mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438336022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336022HT?ae"/>
<attribute name="FRES" value="47MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="4A @40K"/>
<attribute name="ISAT" value="5.2A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336022HT"/>
<attribute name="RDC-TYP" value="56.9mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438336033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336033HT?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="3.1A @40K"/>
<attribute name="ISAT" value="4.3A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336033HT"/>
<attribute name="RDC-TYP" value="85.9mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438336047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336047HT?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="2.5A @40K"/>
<attribute name="ISAT" value="4.1A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336047HT"/>
<attribute name="RDC-TYP" value="130.6mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_74438336068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336068HT?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="2A @40K"/>
<attribute name="ISAT" value="3.7A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336068HT"/>
<attribute name="RDC-TYP" value="197.4mOhm"/>
<attribute name="SIZE" value="3020 HT"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3020" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383360033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383360033?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="8.7A @40K"/>
<attribute name="ISAT" value="10.5A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383360033"/>
<attribute name="RDC-TYP" value="14mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_744383360047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383360047?ae"/>
<attribute name="FRES" value="99MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="7.55A @40K"/>
<attribute name="ISAT" value="9.8A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383360047"/>
<attribute name="RDC-TYP" value="18mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_744383360068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383360068?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="6.75A @40K"/>
<attribute name="ISAT" value="8.1A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383360068"/>
<attribute name="RDC-TYP" value="22mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336010?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="6.15A @40K"/>
<attribute name="ISAT" value="6.5A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336010"/>
<attribute name="RDC-TYP" value="26mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336012?ae"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="5.65A @40K"/>
<attribute name="ISAT" value="6A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336012"/>
<attribute name="RDC-TYP" value="30mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336015?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="5.35A @40K"/>
<attribute name="ISAT" value="5.85A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336015"/>
<attribute name="RDC-TYP" value="33mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336022?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="3.6A @40K"/>
<attribute name="ISAT" value="5.55A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336022"/>
<attribute name="RDC-TYP" value="67mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336033?ae"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="2.9A @40K"/>
<attribute name="ISAT" value="5.35A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336033"/>
<attribute name="RDC-TYP" value="99mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="2.4A @40K"/>
<attribute name="ISAT" value="5.15A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336047"/>
<attribute name="RDC-TYP" value="137mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336068?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="2.15A @40K"/>
<attribute name="ISAT" value="3.65A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336068"/>
<attribute name="RDC-TYP" value="168mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438336100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438336100?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="1.65A @40K"/>
<attribute name="ISAT" value="3A @30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438336100"/>
<attribute name="RDC-TYP" value="280mOhm"/>
<attribute name="SIZE" value="3020"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2510" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383230033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383230033?ae"/>
<attribute name="FRES" value="180MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="5.5A @40K"/>
<attribute name="ISAT" value="8A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383230033"/>
<attribute name="RDC-TYP" value="29mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_744383230047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383230047?ae"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="4.8A @40K"/>
<attribute name="ISAT" value="6.9A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383230047"/>
<attribute name="RDC-TYP" value="37mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_744383230068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383230068?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="4.25A @40K"/>
<attribute name="ISAT" value="6.1A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383230068"/>
<attribute name="RDC-TYP" value="46mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_744383230082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383230082?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.9A @40K"/>
<attribute name="ISAT" value="5.45A @30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383230082"/>
<attribute name="RDC-TYP" value="53mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323010?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.55A @40K"/>
<attribute name="ISAT" value="5.3A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323010"/>
<attribute name="RDC-TYP" value="63mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323012?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.05A @40K"/>
<attribute name="ISAT" value="4.85A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323012"/>
<attribute name="RDC-TYP" value="82mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323015?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.85A @40K"/>
<attribute name="ISAT" value="4.75A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323015"/>
<attribute name="RDC-TYP" value="92mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323022?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.2A @40K"/>
<attribute name="ISAT" value="3.55A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323022"/>
<attribute name="RDC-TYP" value="147mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323033?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.75A @40K"/>
<attribute name="ISAT" value="2.7A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323033"/>
<attribute name="RDC-TYP" value="220mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.4A @40K"/>
<attribute name="ISAT" value="2.3A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323047"/>
<attribute name="RDC-TYP" value="338mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323068?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.05A @40K"/>
<attribute name="ISAT" value="2A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323068"/>
<attribute name="RDC-TYP" value="563mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323082?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="0.95A @40K"/>
<attribute name="ISAT" value="1.85A @30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323082"/>
<attribute name="RDC-TYP" value="646mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438323100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438323100?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="0.9A @40K"/>
<attribute name="ISAT" value="1.7A @30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438323100"/>
<attribute name="RDC-TYP" value="733mOhm"/>
<attribute name="SIZE" value="2510"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_5020" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_5020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383660033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383660033?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="19.8A @40K"/>
<attribute name="ISAT" value="22.9A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383660033"/>
<attribute name="RDC-TYP" value="3.1mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_744383660047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383660047?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="16A @40K"/>
<attribute name="ISAT" value="18.9A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383660047"/>
<attribute name="RDC-TYP" value="5.1mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_744383660068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383660068?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="14.4A @40K"/>
<attribute name="ISAT" value="16.2A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383660068"/>
<attribute name="RDC-TYP" value="6.3mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_744383660082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383660082?ae"/>
<attribute name="FRES" value="53.5MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="13.25A @40K"/>
<attribute name="ISAT" value="15.3A @30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383660082"/>
<attribute name="RDC-TYP" value="8.3mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438366010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438366010?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="11.1A @40K"/>
<attribute name="ISAT" value="14A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438366010"/>
<attribute name="RDC-TYP" value="11.4mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438366015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438366015?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="8.45A @40K"/>
<attribute name="ISAT" value="13.2A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438366015"/>
<attribute name="RDC-TYP" value="18.5mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438366022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438366022?ae"/>
<attribute name="FRES" value="31.5MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="7.4A @40K"/>
<attribute name="ISAT" value="12A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438366022"/>
<attribute name="RDC-TYP" value="23.7mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438366033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438366033?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="6.1A @40K"/>
<attribute name="ISAT" value="9.7A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438366033"/>
<attribute name="RDC-TYP" value="33.4mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
<technology name="_74438366047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438366047?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="4.65A @40K"/>
<attribute name="ISAT" value="7.7A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="5.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438366047"/>
<attribute name="RDC-TYP" value="54.8mOhm"/>
<attribute name="SIZE" value="5020"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="5.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2506" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2506">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383210047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383210047?ae"/>
<attribute name="FRES" value="165MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="IRP" value="3.25A @40K"/>
<attribute name="ISAT" value="4.65A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383210047"/>
<attribute name="RDC-TYP" value="76mOhm"/>
<attribute name="SIZE" value="2506"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438321010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438321010?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="0.6mm"/>
<attribute name="IRP" value="2.1A @40K"/>
<attribute name="ISAT" value="3.25A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438321010"/>
<attribute name="RDC-TYP" value="163mOhm"/>
<attribute name="SIZE" value="2506"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4012" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7443835400033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443835400033?ae"/>
<attribute name="FRES" value="682MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="33.5A @40K"/>
<attribute name="ISAT" value="40A @30%"/>
<attribute name="L" value="0.033uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443835400033"/>
<attribute name="RDC-TYP" value="0.9mOhm"/>
<attribute name="SIZE" value="4012"/>
<attribute name="VALUE" value="0.033uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_7443835400068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443835400068?ae"/>
<attribute name="FRES" value="374MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="27A @40K"/>
<attribute name="ISAT" value="38A @30%"/>
<attribute name="L" value="0.068uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7443835400068"/>
<attribute name="RDC-TYP" value="1.7mOhm"/>
<attribute name="SIZE" value="4012"/>
<attribute name="VALUE" value="0.068uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4030" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383570033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383570033?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="15.8A @40K"/>
<attribute name="ISAT" value="14.5A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383570033"/>
<attribute name="RDC-TYP" value="4.3mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_744383570056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383570056?ae"/>
<attribute name="FRES" value="79MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="13.4A @40K"/>
<attribute name="ISAT" value="13.2A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383570056"/>
<attribute name="RDC-TYP" value="5.9mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="10.25A @40K"/>
<attribute name="ISAT" value="12.5A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357010"/>
<attribute name="RDC-TYP" value="11.6mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357012?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="9.4A @40K"/>
<attribute name="ISAT" value="11.6A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357012"/>
<attribute name="RDC-TYP" value="13.4mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357015?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="8.2A @40K"/>
<attribute name="ISAT" value="11A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357015"/>
<attribute name="RDC-TYP" value="17.1mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="7.9A @40K"/>
<attribute name="ISAT" value="10.3A @30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357018"/>
<attribute name="RDC-TYP" value="18mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357022?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="7.1A @40K"/>
<attribute name="ISAT" value="9.2A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357022"/>
<attribute name="RDC-TYP" value="22mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357033?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="6.1A @40K"/>
<attribute name="ISAT" value="6.8A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357033"/>
<attribute name="RDC-TYP" value="29mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357047?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="5.1A @40K"/>
<attribute name="ISAT" value="8.2A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357047"/>
<attribute name="RDC-TYP" value="39.9mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357056?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="4.7A @40K"/>
<attribute name="ISAT" value="8.1A @30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357056"/>
<attribute name="RDC-TYP" value="46.5mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357068?ae"/>
<attribute name="FRES" value="19.5MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="3.75A @40K"/>
<attribute name="ISAT" value="7.2A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357068"/>
<attribute name="RDC-TYP" value="69.4mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357082?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="3.45A @40K"/>
<attribute name="ISAT" value="6.8A @30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357082"/>
<attribute name="RDC-TYP" value="81mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
<technology name="_74438357100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438357100?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="3.05A @40K"/>
<attribute name="ISAT" value="5.95A @30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="4.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438357100"/>
<attribute name="RDC-TYP" value="100.8mOhm"/>
<attribute name="SIZE" value="4030"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2010" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383430033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383430033?ae"/>
<attribute name="FRES" value="205MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="4.35A @40K"/>
<attribute name="ISAT" value="7.5A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383430033"/>
<attribute name="RDC-TYP" value="40mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383430047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383430047?ae"/>
<attribute name="FRES" value="175MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.9A @40K"/>
<attribute name="ISAT" value="6.5A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383430047"/>
<attribute name="RDC-TYP" value="49mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383430056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383430056?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.6A @40K"/>
<attribute name="ISAT" value="6.2A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383430056"/>
<attribute name="RDC-TYP" value="56mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383430068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383430068?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.3A @40K"/>
<attribute name="ISAT" value="5.9A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383430068"/>
<attribute name="RDC-TYP" value="65mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383430082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383430082?ae"/>
<attribute name="FRES" value="125MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.15A @40K"/>
<attribute name="ISAT" value="5.35A @30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383430082"/>
<attribute name="RDC-TYP" value="71mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438343010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438343010?ae"/>
<attribute name="FRES" value="99MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.8A @40K"/>
<attribute name="ISAT" value="4.7A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438343010"/>
<attribute name="RDC-TYP" value="86mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438343012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438343012?ae"/>
<attribute name="FRES" value="96MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.4A @40K"/>
<attribute name="ISAT" value="4.9A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438343012"/>
<attribute name="RDC-TYP" value="114mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438343015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438343015?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.05A @40K"/>
<attribute name="ISAT" value="3.95A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438343015"/>
<attribute name="RDC-TYP" value="150mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438343022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438343022?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.65A @40K"/>
<attribute name="ISAT" value="3.3A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438343022"/>
<attribute name="RDC-TYP" value="225mOhm"/>
<attribute name="SIZE" value="2010"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_3010" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_3010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438333022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438333022?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.35A @40K"/>
<attribute name="ISAT" value="4.85A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438333022"/>
<attribute name="RDC-TYP" value="150mOhm"/>
<attribute name="SIZE" value="3010"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438333033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438333033?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.85A @40K"/>
<attribute name="ISAT" value="3.7A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438333033"/>
<attribute name="RDC-TYP" value="232mOhm"/>
<attribute name="SIZE" value="3010"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
<technology name="_74438333047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438333047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.45A @40K"/>
<attribute name="ISAT" value="3A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438333047"/>
<attribute name="RDC-TYP" value="356mOhm"/>
<attribute name="SIZE" value="3010"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_1610" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_1610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383130033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130033?ae"/>
<attribute name="FRES" value="215MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="3.25A @40K"/>
<attribute name="ISAT" value="6.2A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383130033"/>
<attribute name="RDC-TYP" value="65mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383130047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130047?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.95A @40K"/>
<attribute name="ISAT" value="5.6A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383130047"/>
<attribute name="RDC-TYP" value="77mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383130056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130056?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.7A @40K"/>
<attribute name="ISAT" value="5.2A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383130056"/>
<attribute name="RDC-TYP" value="90mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383130068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130068?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.55A @40K"/>
<attribute name="ISAT" value="4.8A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383130068"/>
<attribute name="RDC-TYP" value="101mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_744383130082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383130082?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.35A @40K"/>
<attribute name="ISAT" value="4.6A @30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383130082"/>
<attribute name="RDC-TYP" value="115mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438313010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438313010?ae"/>
<attribute name="FRES" value="111MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.2A @40K"/>
<attribute name="ISAT" value="4.25A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438313010"/>
<attribute name="RDC-TYP" value="127mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438313012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438313012?ae"/>
<attribute name="FRES" value="109MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="2.1A @40K"/>
<attribute name="ISAT" value="4.1A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438313012"/>
<attribute name="RDC-TYP" value="140mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438313015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438313015?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.8A @40K"/>
<attribute name="ISAT" value="3.45A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438313015"/>
<attribute name="RDC-TYP" value="189mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74438313022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438313022?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IRP" value="1.25A @40K"/>
<attribute name="ISAT" value="3.25A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438313022"/>
<attribute name="RDC-TYP" value="337mOhm"/>
<attribute name="SIZE" value="1610"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4020" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383560033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383560033?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="14.95A @40K"/>
<attribute name="ISAT" value="16.7A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383560033"/>
<attribute name="RDC-TYP" value="6mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_744383560056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383560056?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="13.65A @40K"/>
<attribute name="ISAT" value="14.7A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383560056"/>
<attribute name="RDC-TYP" value="7mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_744383560068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383560068?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="13.15A @40K"/>
<attribute name="ISAT" value="12.7A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383560068"/>
<attribute name="RDC-TYP" value="7.5mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356010?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="10.1A @40K"/>
<attribute name="ISAT" value="11.5A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356010"/>
<attribute name="RDC-TYP" value="12mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356012?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="8.9A @40K"/>
<attribute name="ISAT" value="11.2A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356012"/>
<attribute name="RDC-TYP" value="15mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356015?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="8.6A @40K"/>
<attribute name="ISAT" value="10.2A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356015"/>
<attribute name="RDC-TYP" value="16mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356018?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="6.8A @40K"/>
<attribute name="ISAT" value="8.7A @30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356018"/>
<attribute name="RDC-TYP" value="24.5mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356022?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="6.2A @40K"/>
<attribute name="ISAT" value="7.9A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356022"/>
<attribute name="RDC-TYP" value="29mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356033?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="5.15A @40K"/>
<attribute name="ISAT" value="7.1A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356033"/>
<attribute name="RDC-TYP" value="39.9mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356047?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="4A @40K"/>
<attribute name="ISAT" value="5.75A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356047"/>
<attribute name="RDC-TYP" value="63mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356056?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="3.85A @40K"/>
<attribute name="ISAT" value="5.5A @30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356056"/>
<attribute name="RDC-TYP" value="68mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356150?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="2.1A @40K"/>
<attribute name="ISAT" value="2.85A @30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356150"/>
<attribute name="RDC-TYP" value="200mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356220?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="1.85A @40K"/>
<attribute name="ISAT" value="2.45A @30%"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356220"/>
<attribute name="RDC-TYP" value="250mOhm"/>
<attribute name="SIZE" value="4020"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_4020HT" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MAPI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383560033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383560033HT?ae"/>
<attribute name="FRES" value="98MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="13.3A @40K"/>
<attribute name="ISAT" value="14.8A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383560033HT"/>
<attribute name="RDC-TYP" value="6.5mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_744383560047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383560047HT?ae"/>
<attribute name="FRES" value="83MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="12.7A @40K"/>
<attribute name="ISAT" value="13A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383560047HT"/>
<attribute name="RDC-TYP" value="7mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_744383560056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383560056HT?ae"/>
<attribute name="FRES" value="72MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="12.15A @40K"/>
<attribute name="ISAT" value="13A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383560056HT"/>
<attribute name="RDC-TYP" value="7.5mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_744383560068HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383560068HT?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="11.7A @40K"/>
<attribute name="ISAT" value="11.7A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383560068HT"/>
<attribute name="RDC-TYP" value="8mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356010HT?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="8.75A @40K"/>
<attribute name="ISAT" value="9.3A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356010HT"/>
<attribute name="RDC-TYP" value="13.5mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356012HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356012HT?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="8A @40K"/>
<attribute name="ISAT" value="9.3A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356012HT"/>
<attribute name="RDC-TYP" value="16mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356015HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356015HT?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="7.45A @40K"/>
<attribute name="ISAT" value="9A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356015HT"/>
<attribute name="RDC-TYP" value="18mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356018HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356018HT?ae"/>
<attribute name="FRES" value="37.5MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="6.05A @40K"/>
<attribute name="ISAT" value="8.3A @30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356018HT"/>
<attribute name="RDC-TYP" value="26mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356022HT?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="5.9A @40K"/>
<attribute name="ISAT" value="7.6A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356022HT"/>
<attribute name="RDC-TYP" value="28mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356033HT?ae"/>
<attribute name="FRES" value="25.5MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="4.45A @40K"/>
<attribute name="ISAT" value="6.5A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356033HT"/>
<attribute name="RDC-TYP" value="45mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356047HT?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="3.7A @40K"/>
<attribute name="ISAT" value="5.05A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356047HT"/>
<attribute name="RDC-TYP" value="65mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
<technology name="_74438356056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438356056HT?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IRP" value="3.5A @40K"/>
<attribute name="ISAT" value="4.9A @30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438356056HT"/>
<attribute name="RDC-TYP" value="70mOhm"/>
<attribute name="SIZE" value="4020HT"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2512" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383240047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383240047?ae"/>
<attribute name="FRES" value="145MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="5.35A @40K"/>
<attribute name="ISAT" value="8A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383240047"/>
<attribute name="RDC-TYP" value="30mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_744383240056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383240056?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="4.75A @40K"/>
<attribute name="ISAT" value="7.9A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383240056"/>
<attribute name="RDC-TYP" value="37mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_744383240068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383240068?ae"/>
<attribute name="FRES" value="102MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="4.25A @40K"/>
<attribute name="ISAT" value="7.4A @30%"/>
<attribute name="L" value="0.68uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383240068"/>
<attribute name="RDC-TYP" value="45mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324010?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="4.05A @40K"/>
<attribute name="ISAT" value="6.3A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324010"/>
<attribute name="RDC-TYP" value="49mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324012?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="3.4A @40K"/>
<attribute name="ISAT" value="5.8A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324012"/>
<attribute name="RDC-TYP" value="67mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324015?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="3.05A @40K"/>
<attribute name="ISAT" value="4.7A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324015"/>
<attribute name="RDC-TYP" value="82mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324022?ae"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="2.45A @40K"/>
<attribute name="ISAT" value="3.65A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324022"/>
<attribute name="RDC-TYP" value="123mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324033?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.7A @40K"/>
<attribute name="ISAT" value="3.3A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324033"/>
<attribute name="RDC-TYP" value="226mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.45A @40K"/>
<attribute name="ISAT" value="2.65A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324047"/>
<attribute name="RDC-TYP" value="300mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324056?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.25A @40K"/>
<attribute name="ISAT" value="2.2A @30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324056"/>
<attribute name="RDC-TYP" value="405mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324068?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.05A @40K"/>
<attribute name="ISAT" value="2.05A @30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324068"/>
<attribute name="RDC-TYP" value="560mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324082?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="0.95A @40K"/>
<attribute name="ISAT" value="1.9A @30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324082"/>
<attribute name="RDC-TYP" value="630mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74438324100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324100?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="0.9A @40K"/>
<attribute name="ISAT" value="1.75A @30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324100"/>
<attribute name="RDC-TYP" value="680mOhm"/>
<attribute name="SIZE" value="2512"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MAPI_2512HT" prefix="L">
<description>&lt;b&gt; WE-MAPI SMD Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Magnetic iron alloy allows high rated currents
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded
&lt;br&gt;High current capability and handles high transient current spikes
&lt;br&gt;Low acoustic noise and low leakage flux noise
&lt;br&gt;AEC-Q 200 qualified
&lt;br&gt;Operating temperature: –40 °C to 125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;WE-MAPI High Temperature Series
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;High Temperature Series with operating temperature from -55 °C to +150 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14811v209%20Family_WE-MAPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MAPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MAPI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-11-14&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-MAPI_2512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744383240033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383240033HT?ae"/>
<attribute name="FRES" value="174MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="6.2A @40K"/>
<attribute name="ISAT" value="8.6A @30%"/>
<attribute name="L" value="0.33uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383240033HT"/>
<attribute name="RDC-TYP" value="23.2mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_744383240047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383240047HT?ae"/>
<attribute name="FRES" value="131MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="5.3A @40K"/>
<attribute name="ISAT" value="7.5A @30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383240047HT"/>
<attribute name="RDC-TYP" value="30.1mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_744383240056HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744383240056HT?ae"/>
<attribute name="FRES" value="102MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="4.7A @40K"/>
<attribute name="ISAT" value="6.7A @30%"/>
<attribute name="L" value="0.56uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744383240056HT"/>
<attribute name="RDC-TYP" value="38.3mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="0.56uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_74438324010HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324010HT?ae"/>
<attribute name="FRES" value="71MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="3.9A @40K"/>
<attribute name="ISAT" value="4.8A @30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324010HT"/>
<attribute name="RDC-TYP" value="53.4mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_74438324012HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324012HT?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="3.5A @40K"/>
<attribute name="ISAT" value="4.7A @30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324012HT"/>
<attribute name="RDC-TYP" value="64.9mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_74438324015HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324015HT?ae"/>
<attribute name="FRES" value="56MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="2.9A @40K"/>
<attribute name="ISAT" value="4A @30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324015HT"/>
<attribute name="RDC-TYP" value="88.7mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_74438324022HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324022HT?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="2.2A @40K"/>
<attribute name="ISAT" value="3.5A @30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324022HT"/>
<attribute name="RDC-TYP" value="141.3mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_74438324033HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324033HT?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.7A @40K"/>
<attribute name="ISAT" value="3A @30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324033HT"/>
<attribute name="RDC-TYP" value="238.8mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
<technology name="_74438324047HT">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438324047HT?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IRP" value="1.4A @40K"/>
<attribute name="ISAT" value="2.4A @30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="2.7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74438324047HT"/>
<attribute name="RDC-TYP" value="319.6mOhm"/>
<attribute name="SIZE" value="2512 HT"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VOP" value="80V"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
