<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - - Signal &amp; Communications - Antennas - WE-MCA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-16&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MCA_74889302451">
<description>&lt;b&gt;WE-MCA Antennas</description>
</package>
<package name="WE-MCA_74889100921">
<description>&lt;b&gt;WE-MCA Antennas</description>
</package>
<package name="WE-MCA_7488910915">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_74889402450">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_7488912455">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Dual band</description>
</package>
<package name="WE-MCA_7488922455">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Dual band</description>
</package>
<package name="WE-MCA_74889102450">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_7488960245">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_74889302450">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_7488918022">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Dual band</description>
</package>
<package name="WE-MCA_7488920157">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_74889502450">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_7488915724">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Dual band</description>
</package>
<package name="WE-MCA_7488910092">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_7488920245">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_7488930245">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
<package name="WE-MCA_7488910043">
<description>&lt;B&gt;WE-MCA Antennas
&lt;Br&gt;&lt;/b&gt;Single band</description>
</package>
</packages>
<symbols>
<symbol name="WE-MCA">
<pin name="FP" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488910915">
<pin name="FEED" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488912455">
<pin name="FD_LB" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="FD_HB" direction="pas"/>
<pin name="NC1" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488960245">
<pin name="FEED" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488922455">
<pin name="FEED" direction="pas"/>
<pin name="GND2" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488918022">
<pin name="FEED" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488920157">
<pin name="FEED" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="GND1" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488915724">
<pin name="FEED2" direction="pas"/>
<pin name="FEED1" direction="pas"/>
<pin name="GND" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488910092">
<pin name="NC5" direction="pas"/>
<pin name="NC4" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="FP" direction="pas"/>
<pin name="NC1" direction="pas"/>
<pin name="NC6" direction="pas"/>
<pin name="NC7" direction="pas"/>
<pin name="NC8" direction="pas"/>
</symbol>
<symbol name="WE-MCA_7488920245">
<pin name="GND2" direction="pas"/>
<pin name="NC2" direction="pas"/>
<pin name="NC3" direction="pas"/>
<pin name="GND1" direction="pas"/>
<pin name="FP" direction="pas"/>
<pin name="NC1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MCA_74889302451" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Created  by Ella Wu 2025-07-16&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_74889302451">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74889302451?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz"/>
<attribute name="GPEAK" value="0.5dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74889302451"/>
<attribute name="SIZE" value="3.2 x 1.6 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value="1.6"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_74889100921" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2025-07-16&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_74889100921">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74889100921?ae"/>
<attribute name="FREQUENCY-RANGE" value="860-960 MHz"/>
<attribute name="GPEAK" value="-0.7dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74889100921"/>
<attribute name="SIZE" value="11 x 5.1 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="860-960 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488910915" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488910915"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488910915">
<connects>
<connect gate="G$1" pin="FEED" pad="3"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488910915?ae"/>
<attribute name="FREQUENCY-RANGE" value="902-928 MHz"/>
<attribute name="GPEAK" value="0.5dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488910915"/>
<attribute name="SIZE" value="5.2 x 3.7 mm"/>
<attribute name="TYPE" value="Magnetic Antenna"/>
<attribute name="VALUE" value="902-928 MHz"/>
<attribute name="VSWR" value="3"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_74889402450" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Created  by Ella Wu 2021-11-17&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_74889402450">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74889402450?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz"/>
<attribute name="GPEAK" value="2.7dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74889402450"/>
<attribute name="SIZE" value="7.0 x 2.0 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488912455" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488912455"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488912455">
<connects>
<connect gate="G$1" pin="FD_HB" pad="4 6"/>
<connect gate="G$1" pin="FD_LB" pad="3 5"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488912455?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz, 4900-5875 MHz"/>
<attribute name="GPEAK" value="1dBi, -1.5dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488912455"/>
<attribute name="SIZE" value="8.5 x 1.6 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz, 4900-5875 MHz"/>
<attribute name="VSWR" value="2.2, 2.2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488922455" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488922455"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488922455">
<connects>
<connect gate="G$1" pin="FEED" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488922455?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz, 5000-6000 MHz"/>
<attribute name="GPEAK" value="3dBi, 3.3dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488922455"/>
<attribute name="SIZE" value="5.2 x 3.7 mm"/>
<attribute name="TYPE" value="Magnetic Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz, 5000-6000 MHz"/>
<attribute name="VSWR" value="2, 2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_74889102450" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_74889102450">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74889102450?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz"/>
<attribute name="GPEAK" value="3dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74889102450"/>
<attribute name="SIZE" value="9.0 x 2.0 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488960245" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Created  by Ella Wu 2021-11-17&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488960245"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488960245">
<connects>
<connect gate="G$1" pin="FEED" pad="3"/>
<connect gate="G$1" pin="GND1" pad="1"/>
<connect gate="G$1" pin="GND2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488960245?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz"/>
<attribute name="GPEAK" value="3dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488960245"/>
<attribute name="SIZE" value="5.2 x 3.7 mm"/>
<attribute name="TYPE" value="Magnetic Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value="2.5"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_74889302450" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Created  by Ella Wu 2021-11-17&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_74889302450">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74889302450?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz"/>
<attribute name="GPEAK" value="0.5dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74889302450"/>
<attribute name="SIZE" value="3.2 x 1.6 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488918022" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488918022"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488918022">
<connects>
<connect gate="G$1" pin="FEED" pad="4 5"/>
<connect gate="G$1" pin="GND1" pad="3"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488918022?ae"/>
<attribute name="FREQUENCY-RANGE" value="700-960 MHz, 1710-2690 MHz"/>
<attribute name="GPEAK" value="2.1dBi, 5.5dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488918022"/>
<attribute name="SIZE" value="40 x 6 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="700-960 MHz, 1710-2690 MHz"/>
<attribute name="VSWR" value="4, 4"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488920157" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488920157"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488920157">
<connects>
<connect gate="G$1" pin="FEED" pad="3"/>
<connect gate="G$1" pin="GND" pad="1"/>
<connect gate="G$1" pin="GND1" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488920157?ae"/>
<attribute name="FREQUENCY-RANGE" value="1550-1600 MHz"/>
<attribute name="GPEAK" value="3.4dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488920157"/>
<attribute name="SIZE" value="5.2 x 3.7 mm"/>
<attribute name="TYPE" value="Magnetic Antenna"/>
<attribute name="VALUE" value="1550-1600 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_74889502450" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Created  by Ella Wu 2021-11-17&lt;br&gt;
2021 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_74889502450">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74889502450?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz"/>
<attribute name="GPEAK" value="2.5dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74889502450"/>
<attribute name="SIZE" value="5.2 x 2.1 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488915724" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488915724"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488915724">
<connects>
<connect gate="G$1" pin="FEED1" pad="1"/>
<connect gate="G$1" pin="FEED2" pad="2"/>
<connect gate="G$1" pin="GND" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488915724?ae"/>
<attribute name="FREQUENCY-RANGE" value="1570-1580 MHz, 2400-2500 MHz"/>
<attribute name="GPEAK" value="0.69dBi, 0.97dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488915724"/>
<attribute name="SIZE" value="3.2 x 1.7 mm"/>
<attribute name="TYPE" value="Magnetic Antenna"/>
<attribute name="VALUE" value="1570-1580 MHz, 2400-2500 MHz"/>
<attribute name="VSWR" value="2.5"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488910092" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488910092"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488910092">
<connects>
<connect gate="G$1" pin="FP" pad="2"/>
<connect gate="G$1" pin="NC1" pad="1"/>
<connect gate="G$1" pin="NC3" pad="3"/>
<connect gate="G$1" pin="NC4" pad="4"/>
<connect gate="G$1" pin="NC5" pad="5"/>
<connect gate="G$1" pin="NC6" pad="6"/>
<connect gate="G$1" pin="NC7" pad="7"/>
<connect gate="G$1" pin="NC8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488910092?ae"/>
<attribute name="FREQUENCY-RANGE" value="868-960 MHz"/>
<attribute name="GPEAK" value="-0.7dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488910092"/>
<attribute name="SIZE" value="11 x 5.1 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="868-960 MHz"/>
<attribute name="VSWR" value="2.5"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488920245" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA_7488920245"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488920245">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="GND1" pad="2"/>
<connect gate="G$1" pin="GND2" pad="3"/>
<connect gate="G$1" pin="NC1" pad="6"/>
<connect gate="G$1" pin="NC2" pad="5"/>
<connect gate="G$1" pin="NC3" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488920245?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400-2500 MHz"/>
<attribute name="GPEAK" value="1.3dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488920245"/>
<attribute name="SIZE" value="7.6 x 3.5 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="2400-2500 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488930245" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488930245">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488930245?ae"/>
<attribute name="FREQUENCY-RANGE" value="2400 - 2500 MHz"/>
<attribute name="GPEAK" value="0.5dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488930245"/>
<attribute name="SIZE" value="3.2 x 1.6 mm"/>
<attribute name="VALUE" value="2400 - 2500 MHz"/>
<attribute name="VSWR" value=" 2 "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCA_7488910043" prefix="AE">
<description>&lt;b&gt;WE-MCA Antennas
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;SMT multilayer chip antenna
&lt;br&gt; Extremely low profile
&lt;br&gt; Omni-directional radiation pattern
&lt;br&gt; Excellent size to performance ratio
&lt;br&gt; Smallest form factor in the industry
&lt;br&gt; Less ground clearance
&lt;br&gt; Operating temperature: -40 °C to +85°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;me RF/Smart home
&lt;br&gt; GSM 900
&lt;br&gt; WLAN/WiFi
&lt;br&gt; Bluetooth
&lt;br&gt; GPS/GNSS
&lt;br&gt; ZigBee
&lt;br&gt; Cellular Communication, 4G/LTE

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14819v209%20family-WE-MCA-74889xxxxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MCA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-MCA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-08-16&lt;br&gt;
2019 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCA"/>
</gates>
<devices>
<device name="" package="WE-MCA_7488910043">
<connects>
<connect gate="G$1" pin="FP" pad="1"/>
<connect gate="G$1" pin="NC" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7488910043?ae"/>
<attribute name="FREQUENCY-RANGE" value="423-443 MHz"/>
<attribute name="GPEAK" value="-4dBi"/>
<attribute name="IMPEDANCE" value="50ohm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7488910043"/>
<attribute name="SIZE" value="25 x 5 mm"/>
<attribute name="TYPE" value="Electrical Antenna"/>
<attribute name="VALUE" value="423-443 MHz"/>
<attribute name="VSWR" value="2"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
