<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Dual Coil Power Inductors - WE-MCRI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MCRI_1090">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-MCRI SMD Molded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1090</description>
</package>
<package name="WE-MCRI_1040">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-MCRI SMD Molded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1040</description>
</package>
</packages>
<symbols>
<symbol name="WE-MCRI">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MCRI_1090" prefix="L">
<description>&lt;b&gt;WE-MCRI SMD Molded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Composite core material allows high saturation current and compact design
&lt;br&gt;Better Leakage Inductance (Lk) and Rated Current (Ir) than comparable components
&lt;br&gt;Magnetically shielded
&lt;br&gt;1:1 Transformer
&lt;br&gt;Operation temperature: -40°C to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Isolated converter application (e.g. Flyback converter) &lt;br&gt;
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Switching regulator with second, unregulated output voltage
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o106461v209%20Family_WE-MCRI1090-7448990xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o106461v209%20Family_WE-MCRI1090-7448990xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-MCRI"&gt;https://katalog.we-online.com/en/pbs/WE-MCRI&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun, Shan 2019-08-15
&lt;br&gt;
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCRI"/>
</gates>
<devices>
<device name="" package="WE-MCRI_1090">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7448990010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990010.pdf"/>
<attribute name="FRE" value="35MHz"/>
<attribute name="IR1" value="17A"/>
<attribute name="IR2" value="17A"/>
<attribute name="ISAT1" value="43.5A"/>
<attribute name="ISAT2" value="43.5A"/>
<attribute name="L2" value="1uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990010 "/>
<attribute name="RDC1-MAX" value="5.6mOhm"/>
<attribute name="RDC1-TYP" value="4.5mOhm"/>
<attribute name="RDC2-MAX" value="5.6mOhm"/>
<attribute name="RDC2-TYP" value="4.5mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7448990015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990015.pdf"/>
<attribute name="FRE" value="29MHz"/>
<attribute name="IR1" value="12.5A"/>
<attribute name="IR2" value="12.5A"/>
<attribute name="ISAT1" value="34A"/>
<attribute name="ISAT2" value="34A"/>
<attribute name="L2" value="1.5uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990015 "/>
<attribute name="RDC1-MAX" value="9.4mOhm"/>
<attribute name="RDC1-TYP" value="8.8mOhm"/>
<attribute name="RDC2-MAX" value="9.4mOhm"/>
<attribute name="RDC2-TYP" value="8.8mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7448990022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990022.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="11.5A"/>
<attribute name="IR2" value="11.5A"/>
<attribute name="ISAT1" value="29.5A"/>
<attribute name="ISAT2" value="29.5A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990022 "/>
<attribute name="RDC1-MAX" value="12.5mOhm"/>
<attribute name="RDC1-TYP" value="10.5mOhm"/>
<attribute name="RDC2-MAX" value="12.5mOhm"/>
<attribute name="RDC2-TYP" value="10.5mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7448990033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990033.pdf"/>
<attribute name="FRE" value="19MHz"/>
<attribute name="IR1" value="7.5A"/>
<attribute name="IR2" value="7.5A"/>
<attribute name="ISAT1" value="28.2A"/>
<attribute name="ISAT2" value="28.2A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990033 "/>
<attribute name="RDC1-MAX" value="26mOhm"/>
<attribute name="RDC1-TYP" value="23.5mOhm"/>
<attribute name="RDC2-MAX" value="26mOhm"/>
<attribute name="RDC2-TYP" value="23.5mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7448990047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990047.pdf"/>
<attribute name="FRE" value="17.5MHz"/>
<attribute name="IR1" value="5.9A"/>
<attribute name="IR2" value="5.9A"/>
<attribute name="ISAT1" value="24.2A"/>
<attribute name="ISAT2" value="24.2A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990047 "/>
<attribute name="RDC1-MAX" value="40mOhm"/>
<attribute name="RDC1-TYP" value="36mOhm"/>
<attribute name="RDC2-MAX" value="40mOhm"/>
<attribute name="RDC2-TYP" value="36mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7448990068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990068.pdf"/>
<attribute name="FRE" value="13MHz"/>
<attribute name="IR1" value="5A"/>
<attribute name="IR2" value="5A"/>
<attribute name="ISAT1" value="21.2A"/>
<attribute name="ISAT2" value="21.2A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990068 "/>
<attribute name="RDC1-MAX" value="51.5mOhm"/>
<attribute name="RDC1-TYP" value="46mOhm"/>
<attribute name="RDC2-MAX" value="51.5mOhm"/>
<attribute name="RDC2-TYP" value="46mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7448990082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990082.pdf"/>
<attribute name="FRE" value="9.5MHz"/>
<attribute name="IR1" value="4.8A"/>
<attribute name="IR2" value="4.8A"/>
<attribute name="ISAT1" value="18.5A"/>
<attribute name="ISAT2" value="18.5A"/>
<attribute name="L2" value="8.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990082 "/>
<attribute name="RDC1-MAX" value="63mOhm"/>
<attribute name="RDC1-TYP" value="56mOhm"/>
<attribute name="RDC2-MAX" value="63mOhm"/>
<attribute name="RDC2-TYP" value="56mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7448990100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990100.pdf"/>
<attribute name="FRE" value="9MHz"/>
<attribute name="IR1" value="4.5A"/>
<attribute name="IR2" value="4.5A"/>
<attribute name="ISAT1" value="17A"/>
<attribute name="ISAT2" value="17A"/>
<attribute name="L2" value="10uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990100 "/>
<attribute name="RDC1-MAX" value="69mOhm"/>
<attribute name="RDC1-TYP" value="62mOhm"/>
<attribute name="RDC2-MAX" value="69mOhm"/>
<attribute name="RDC2-TYP" value="62mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7448990150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990150.pdf"/>
<attribute name="FRE" value="8.5MHz"/>
<attribute name="IR1" value="3.9A"/>
<attribute name="IR2" value="3.9A"/>
<attribute name="ISAT1" value="9.5A"/>
<attribute name="ISAT2" value="9.5A"/>
<attribute name="L2" value="15uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990150 "/>
<attribute name="RDC1-MAX" value="87mOhm"/>
<attribute name="RDC1-TYP" value="78mOhm"/>
<attribute name="RDC2-MAX" value="87mOhm"/>
<attribute name="RDC2-TYP" value="78mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7448990220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990220.pdf"/>
<attribute name="FRE" value="6.5MHz"/>
<attribute name="IR1" value="3.4A"/>
<attribute name="IR2" value="3.4A"/>
<attribute name="ISAT1" value="8.1A"/>
<attribute name="ISAT2" value="8.1A"/>
<attribute name="L2" value="22uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990220 "/>
<attribute name="RDC1-MAX" value="106mOhm"/>
<attribute name="RDC1-TYP" value="95mOhm"/>
<attribute name="RDC2-MAX" value="106mOhm"/>
<attribute name="RDC2-TYP" value="95mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7448990330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990330.pdf"/>
<attribute name="FRE" value="5.5MHz"/>
<attribute name="IR1" value="2.9A"/>
<attribute name="IR2" value="2.9A"/>
<attribute name="ISAT1" value="6.8A"/>
<attribute name="ISAT2" value="6.8A"/>
<attribute name="L2" value="33uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990330 "/>
<attribute name="RDC1-MAX" value="145mOhm"/>
<attribute name="RDC1-TYP" value="130mOhm"/>
<attribute name="RDC2-MAX" value="145mOhm"/>
<attribute name="RDC2-TYP" value="130mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7448990470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448990470.pdf"/>
<attribute name="FRE" value="4.5MHz"/>
<attribute name="IR1" value="2.3A"/>
<attribute name="IR2" value="2.3A"/>
<attribute name="ISAT1" value="6A"/>
<attribute name="ISAT2" value="6A"/>
<attribute name="L2" value="47uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448990470 "/>
<attribute name="RDC1-MAX" value="240mOhm"/>
<attribute name="RDC1-TYP" value="216mOhm"/>
<attribute name="RDC2-MAX" value="240mOhm"/>
<attribute name="RDC2-TYP" value="216mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MCRI_1040" prefix="L">
<description>&lt;b&gt;WE-MCRI SMD Molded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Composite core material allows high saturation current and compact design
&lt;br&gt;Better Leakage Inductance (Lk) and Rated Current (Ir) than comparable components
&lt;br&gt;Magnetically shielded
&lt;br&gt;1:1 Transformer
&lt;br&gt;Operation temperature: -40°C to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Isolated converter application (e.g. Flyback converter) &lt;br&gt;
&lt;br&gt;Buck, Boost, Sepic, Zeta, CUK Converter
&lt;br&gt;Switching regulator with second, unregulated output voltage
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o106461v209%20Family_WE-MCRI1090-7448990xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o106461v209%20Family_WE-MCRI1090-7448990xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-MCRI"&gt;https://katalog.we-online.com/en/pbs/WE-MCRI&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun, Shan 2019-08-15
&lt;br&gt;
&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MCRI"/>
</gates>
<devices>
<device name="" package="WE-MCRI_1040">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_7448991010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991010.pdf"/>
<attribute name="FRE" value="32MHz"/>
<attribute name="IR1" value="12A"/>
<attribute name="IR2" value="12A"/>
<attribute name="ISAT1" value="30.2A"/>
<attribute name="ISAT2" value="30.2A"/>
<attribute name="L2" value="1uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991010 "/>
<attribute name="RDC1-MAX" value="7.5mOhm"/>
<attribute name="RDC1-TYP" value="6.3mOhm"/>
<attribute name="RDC2-MAX" value="7.5mOhm"/>
<attribute name="RDC2-TYP" value="6.3mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7448991015">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991015.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="11.1A"/>
<attribute name="IR2" value="11.1A"/>
<attribute name="ISAT1" value="28.1A"/>
<attribute name="ISAT2" value="28.1A"/>
<attribute name="L2" value="1.5uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991015 "/>
<attribute name="RDC1-MAX" value="10mOhm"/>
<attribute name="RDC1-TYP" value="8.6mOhm"/>
<attribute name="RDC2-MAX" value="10mOhm"/>
<attribute name="RDC2-TYP" value="8.6mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7448991022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991022.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="8.2A"/>
<attribute name="IR2" value="8.2A"/>
<attribute name="ISAT1" value="20.6A"/>
<attribute name="ISAT2" value="20.6A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991022 "/>
<attribute name="RDC1-MAX" value="16.5mOhm"/>
<attribute name="RDC1-TYP" value="14mOhm"/>
<attribute name="RDC2-MAX" value="16.5mOhm"/>
<attribute name="RDC2-TYP" value="14mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7448991027">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991027.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="7.4A"/>
<attribute name="IR2" value="7.4A"/>
<attribute name="ISAT1" value="16.5A"/>
<attribute name="ISAT2" value="16.5A"/>
<attribute name="L2" value="2.7uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991027 "/>
<attribute name="RDC1-MAX" value="16.8mOhm"/>
<attribute name="RDC1-TYP" value="16.3mOhm"/>
<attribute name="RDC2-MAX" value="16.8mOhm"/>
<attribute name="RDC2-TYP" value="16.3mOhm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_7448991033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991033.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="6.8A"/>
<attribute name="IR2" value="6.8A"/>
<attribute name="ISAT1" value="14.3A"/>
<attribute name="ISAT2" value="14.3A"/>
<attribute name="L2" value="3.3uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991033 "/>
<attribute name="RDC1-MAX" value="23.5mOhm"/>
<attribute name="RDC1-TYP" value="20.7mOhm"/>
<attribute name="RDC2-MAX" value="23.5mOhm"/>
<attribute name="RDC2-TYP" value="20.7mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7448991047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991047.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="6.2A"/>
<attribute name="IR2" value="6.2A"/>
<attribute name="ISAT1" value="13.8A"/>
<attribute name="ISAT2" value="13.8A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991047 "/>
<attribute name="RDC1-MAX" value="29mOhm"/>
<attribute name="RDC1-TYP" value="24.4mOhm"/>
<attribute name="RDC2-MAX" value="29mOhm"/>
<attribute name="RDC2-TYP" value="24.4mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7448991068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991068.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="5A"/>
<attribute name="IR2" value="5A"/>
<attribute name="ISAT1" value="12A"/>
<attribute name="ISAT2" value="12A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991068 "/>
<attribute name="RDC1-MAX" value="44mOhm"/>
<attribute name="RDC1-TYP" value="38mOhm"/>
<attribute name="RDC2-MAX" value="44mOhm"/>
<attribute name="RDC2-TYP" value="38mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7448991082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991082.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="4.7A"/>
<attribute name="IR2" value="4.7A"/>
<attribute name="ISAT1" value="11.3A"/>
<attribute name="ISAT2" value="11.3A"/>
<attribute name="L2" value="8.2uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991082 "/>
<attribute name="RDC1-MAX" value="46mOhm"/>
<attribute name="RDC1-TYP" value="41.2mOhm"/>
<attribute name="RDC2-MAX" value="46mOhm"/>
<attribute name="RDC2-TYP" value="41.2mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7448991100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991100.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="3.7A"/>
<attribute name="IR2" value="3.7A"/>
<attribute name="ISAT1" value="9.8A"/>
<attribute name="ISAT2" value="9.8A"/>
<attribute name="L2" value="10uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991100 "/>
<attribute name="RDC1-MAX" value="62mOhm"/>
<attribute name="RDC1-TYP" value="55mOhm"/>
<attribute name="RDC2-MAX" value="62mOhm"/>
<attribute name="RDC2-TYP" value="55mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7448991150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991150.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="3.25A"/>
<attribute name="IR2" value="3.25A"/>
<attribute name="ISAT1" value="7.8A"/>
<attribute name="ISAT2" value="7.8A"/>
<attribute name="L2" value="15uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991150 "/>
<attribute name="RDC1-MAX" value="95mOhm"/>
<attribute name="RDC1-TYP" value="83mOhm"/>
<attribute name="RDC2-MAX" value="95mOhm"/>
<attribute name="RDC2-TYP" value="83mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7448991220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991220.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="2.2A"/>
<attribute name="IR2" value="2.2A"/>
<attribute name="ISAT1" value="6.1A"/>
<attribute name="ISAT2" value="6.1A"/>
<attribute name="L2" value="22uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991220 "/>
<attribute name="RDC1-MAX" value="160mOhm"/>
<attribute name="RDC1-TYP" value="144mOhm"/>
<attribute name="RDC2-MAX" value="160mOhm"/>
<attribute name="RDC2-TYP" value="144mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7448991330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991330.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="2.05A"/>
<attribute name="IR2" value="2.05A"/>
<attribute name="ISAT1" value="5A"/>
<attribute name="ISAT2" value="5A"/>
<attribute name="L2" value="33uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991330 "/>
<attribute name="RDC1-MAX" value="230mOhm"/>
<attribute name="RDC1-TYP" value="207mOhm"/>
<attribute name="RDC2-MAX" value="230mOhm"/>
<attribute name="RDC2-TYP" value="207mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_7448991470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/77448991470.pdf"/>
<attribute name="FRE" value=""/>
<attribute name="IR1" value="1.5A"/>
<attribute name="IR2" value="1.5A"/>
<attribute name="ISAT1" value="4.4A"/>
<attribute name="ISAT2" value="4.4A"/>
<attribute name="L2" value="47uH"/>
<attribute name="N" value="1:1"/>
<attribute name="PART-NUMBER" value=" 7448991470 "/>
<attribute name="RDC1-MAX" value="340mOhm"/>
<attribute name="RDC1-TYP" value="312mOhm"/>
<attribute name="RDC2-MAX" value="340mOhm"/>
<attribute name="RDC2-TYP" value="312mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
