<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Filter Chokes - WE-MI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-05-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MI_0805_H1.25">
<description>&lt;b&gt;WE-MI SMT Multilayer Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 2pins
&lt;br&gt;LXWXH = 2mmX1.2mmX1.2mm</description>
</package>
<package name="WE-MI_0805_H0.9">
<description>&lt;b&gt;WE-MI SMT Multilayer Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size: 0805, SMT, 2pins
&lt;br&gt;LXWXH = 2mmX1.2mmX0.9mm</description>
</package>
<package name="WE-MI_0603">
<description>&lt;b&gt;WE-MI SMT Multilayer Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;size: 0603, SMT, 2pins
&lt;br&gt;LXWXH = 1.6mmX0.8mmX0.8mm</description>
</package>
<package name="WE-MI_1206">
<description>&lt;b&gt;WE-MI SMT Multilayer Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;size: 1206, SMT, 2pins
&lt;br&gt;LXWXH = 3.2mmX1.6mmX1.1mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MI_1206" prefix="L">
<description>&lt;b&gt;WE-MI SMT Multilayer Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Smallest inductor possible for less space needed on the printed circuit board and therefore perfect suitable for high density mounting
&lt;br&gt; No cross coupling because of closed magnetic circuits
&lt;br&gt; No crosstalk
&lt;br&gt; Operating temperature: –55 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter circuits
&lt;br&gt; Oscillators
&lt;br&gt; Adjustment networks
&lt;br&gt; Discretely built T- or π-Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14820v209%20Family_WE-MI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14820v209%20Family_WE-MI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MI"&gt;www.we-online.com/catalog/WE-MI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-06&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MI_1206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479114">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479114?ae"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479114 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="RDC-MAX" value="0.15Ohm"/>
<attribute name="VALUE" value="0.047uH"/>
</technology>
<technology name="_74479118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479118?ae"/>
<attribute name="IR" value="5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479118 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7447912">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447912?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447912 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_74479122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479122?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479122 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_744791220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744791220?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744791220 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744791282">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744791282?ae"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744791282 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="RDC-MAX" value="0.9Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7447913">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447913?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447913 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_74479132">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479132?ae"/>
<attribute name="IR" value="200mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479132 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74479132J">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479132J?ae"/>
<attribute name="IR" value="200mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479132J"/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74479136">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479136?ae"/>
<attribute name="IR" value="150mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479136 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74479142">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479142?ae"/>
<attribute name="IR" value="100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479142 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74479145">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479145?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479145 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74479148">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479148?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479148 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_7447915">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447915?ae"/>
<attribute name="IR" value="100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447915 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74479152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479152?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479152 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74479152J">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479152J?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479152J"/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74479153">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479153?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479153 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="350mOhm"/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74479157">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479157?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479157 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="350mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_74479159">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479159?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479159 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_7447915J">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447915J?ae"/>
<attribute name="IR" value="100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7447915J"/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7447916">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447916?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447916 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="0.9Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74479168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479168?ae"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479168 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="0.9Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7447918">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447918?ae"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447918 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74479182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479182?ae"/>
<attribute name="IR" value="5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479182 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74479183">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479183?ae"/>
<attribute name="IR" value="5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479183 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="0.9Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74479184">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479184?ae"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479184 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="650mOhm"/>
<attribute name="RDC-MAX" value="0.9Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MI_0603" prefix="L">
<description>&lt;b&gt;WE-MI SMT Multilayer Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Smallest inductor possible for less space needed on the printed circuit board and therefore perfect suitable for high density mounting
&lt;br&gt; No cross coupling because of closed magnetic circuits
&lt;br&gt; No crosstalk
&lt;br&gt; Operating temperature: –55 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter circuits
&lt;br&gt; Oscillators
&lt;br&gt; Adjustment networks
&lt;br&gt; Discretely built T- or π-Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14820v209%20Family_WE-MI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14820v209%20Family_WE-MI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MI"&gt;www.we-online.com/catalog/WE-MI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-06&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-MI_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479614">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479614?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479614 "/>
<attribute name="Q" value=" 10 "/>
<attribute name="RDC" value="0.07mOhm"/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="VALUE" value="0.047uH"/>
</technology>
<technology name="_74479616">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479616?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479616 "/>
<attribute name="Q" value=" 10 "/>
<attribute name="RDC" value="0.055mOhm"/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="VALUE" value="0.068uH"/>
</technology>
<technology name="_7447962">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447962?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447962 "/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.2mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_744796215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744796215?ae"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744796215 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="0.55mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74479623">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479623?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479623 "/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.3mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744796233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744796233?ae"/>
<attribute name="IR" value="35mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744796233 "/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.3mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_74479628">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479628?ae"/>
<attribute name="IR" value="35mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479628 "/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.55mOhm"/>
<attribute name="RDC-MAX" value="2.1Ohm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74479632">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479632?ae"/>
<attribute name="IR" value="35mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479632 "/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.3mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_7447964">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447964?ae"/>
<attribute name="IR" value="35mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447964 "/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.35mOhm"/>
<attribute name="RDC-MAX" value="1.7Ohm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74479645">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479645?ae"/>
<attribute name="IR" value="35mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479645 "/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.5mOhm"/>
<attribute name="RDC-MAX" value="1.55Ohm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_74479645J">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479645J?ae"/>
<attribute name="IR" value="35mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479645J"/>
<attribute name="Q" value=" 15 "/>
<attribute name="RDC" value="0.5mOhm"/>
<attribute name="RDC-MAX" value="1.55Ohm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_7447965">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447965?ae"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447965 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="0.4mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74479651">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479651?ae"/>
<attribute name="IR" value="25mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479651 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="0.65mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_74479652">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479652?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479652 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="0.75mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744796527">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744796527?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744796527 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="1.05mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_74479653">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479653?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479653 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="1.05mOhm"/>
<attribute name="RDC-MAX" value="1.4Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7447966">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447966?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447966 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="1.3mOhm"/>
<attribute name="RDC-MAX" value="1.8Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74479668">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479668?ae"/>
<attribute name="IR" value="5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479668 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="0.8mOhm"/>
<attribute name="RDC-MAX" value="1.7Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7447967">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447967?ae"/>
<attribute name="IR" value="5mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447967 "/>
<attribute name="Q" value=" 35 "/>
<attribute name="RDC" value="1.05mOhm"/>
<attribute name="RDC-MAX" value="2.1Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7447968">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447968?ae"/>
<attribute name="IR" value="3mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447968 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC" value="1.05mOhm"/>
<attribute name="RDC-MAX" value="1.85Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74479681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479681?ae"/>
<attribute name="IR" value="3mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479681 "/>
<attribute name="Q" value=" 30 "/>
<attribute name="RDC" value="1.3mOhm"/>
<attribute name="RDC-MAX" value="2.1Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MI_0805" prefix="L">
<description>&lt;b&gt;WE-MI SMT Multilayer Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Smallest inductor possible for less space needed on the printed circuit board and therefore perfect suitable for high density mounting
&lt;br&gt; No cross coupling because of closed magnetic circuits
&lt;br&gt; No crosstalk
&lt;br&gt; Operating temperature: –55 °C to +125 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Filter circuits
&lt;br&gt; Oscillators
&lt;br&gt; Adjustment networks
&lt;br&gt; Discretely built T- or π-Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14820v209%20Family_WE-MI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14820v209%20Family_WE-MI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MI"&gt;www.we-online.com/catalog/WE-MI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-05-06&lt;br&gt;
2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H0.9" package="WE-MI_0805_H0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479014">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479014?ae"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479014 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="RDC-MAX" value="0.2Ohm"/>
<attribute name="VALUE" value="0.047uH"/>
</technology>
<technology name="_7447902">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447902?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447902 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_74479021">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479021?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479021 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="RDC-MAX" value="0.2Ohm"/>
<attribute name="VALUE" value="0.1uH"/>
</technology>
<technology name="_74479022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479022?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479022 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_74479023">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479023?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479023 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="160mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_74479027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479027?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479027 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="0.27uH"/>
</technology>
<technology name="_744790282">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744790282?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744790282 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="700mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7447903">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447903?ae"/>
<attribute name="IR" value="250mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447903 "/>
<attribute name="Q" value=" 20 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_7447905">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447905?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447905 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="320mOhm"/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74479051">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479051?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479051 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_744790515">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744790515?ae"/>
<attribute name="IR" value="50mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744790515 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="360mOhm"/>
<attribute name="RDC-MAX" value="0.5Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74479052">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479052?ae"/>
<attribute name="IR" value="30mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479052 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="420mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
</technologies>
</device>
<device name="_H1.25" package="WE-MI_0805_H0.9">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479032?ae"/>
<attribute name="IR" value="200mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479032 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="RDC-MAX" value="0.6Ohm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74479035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479035?ae"/>
<attribute name="IR" value="150mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479035 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC" value="450mOhm"/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_7447904">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447904?ae"/>
<attribute name="IR" value="150mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447904 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74479045">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479045?ae"/>
<attribute name="IR" value="150mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479045 "/>
<attribute name="Q" value=" 25 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74479053">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479053?ae"/>
<attribute name="IR" value="30mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479053 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74479056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479056?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479056 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="0.9Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_7447906">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447906?ae"/>
<attribute name="IR" value="30mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447906 "/>
<attribute name="Q" value=" 45 "/>
<attribute name="RDC" value="600mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74479068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479068?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479068 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7447908">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447908?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447908 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="RDC-MAX" value="1Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74479081">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479081?ae"/>
<attribute name="IR" value="15mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74479081 "/>
<attribute name="Q" value=" 50 "/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="RDC-MAX" value="1.1Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
