<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Dual Coil Power Inductors - WE-MTCI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MTCI_5030">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-MTCI SMD Multi-Turn Ratio coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;5030</description>
</package>
</packages>
<symbols>
<symbol name="WE-MTCI_5030">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MTCI_5030" prefix="L">
<description>&lt;b&gt;WE-MTCI SMD Multi-Turn Ratio coupled Inductor&lt;/b&gt;&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Smallest Coupled Inductor with different Turn Ratio and 0.8kV isolation
&lt;br&gt;Magnetically Shielded
&lt;br&gt;1:N Transformer
&lt;br&gt;Operation temperature: -40°C to +125°C
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Ideal solution for buck/boost converter with regulated and un-regulated output voltage
&lt;br&gt;High density Isolated converter application (e.g. Flyback converter)
&lt;br&gt;Step-up or Step-Down Converter with Auxilary winding
&lt;br&gt;Can be use in Auto-transformer application
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o97635v209%20Family_WE-DPC_HV_5030.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o97635v209%20Family_WE-DPC_HV_5030.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-MTCI"&gt;https://katalog.we-online.com/en/pbs/WE-MTCI&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun,Shan 2019-08-15
&lt;br&gt;

2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-MTCI_5030"/>
</gates>
<devices>
<device name="" package="WE-MTCI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="_744889015100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889015100.pdf"/>
<attribute name="FRE" value="13MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="22.5uH"/>
<attribute name="N" value="1:1.5"/>
<attribute name="PART-NUMBER" value="744889015100"/>
<attribute name="RDC1-MAX" value="500mOhm"/>
<attribute name="RDC1-TYP" value="349mOhm"/>
<attribute name="RDC2-MAX" value="600mOhm"/>
<attribute name="RDC2-TYP" value="408mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744889015220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889015220.pdf"/>
<attribute name="FRE" value="9.5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L2" value="49.5uH"/>
<attribute name="N" value="1:1.5"/>
<attribute name="PART-NUMBER" value="744889015220"/>
<attribute name="RDC1-MAX" value="1000mOhm"/>
<attribute name="RDC1-TYP" value="662mOhm"/>
<attribute name="RDC2-MAX" value="1200mOhm"/>
<attribute name="RDC2-TYP" value="874mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744889015330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889015330.pdf"/>
<attribute name="FRE" value="7MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="L2" value="74.25uH"/>
<attribute name="N" value="1:1.5"/>
<attribute name="PART-NUMBER" value="744889015330"/>
<attribute name="RDC1-MAX" value="1900mOhm"/>
<attribute name="RDC1-TYP" value="1338mOhm"/>
<attribute name="RDC2-MAX" value="2400mOhm"/>
<attribute name="RDC2-TYP" value="1782mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744889020100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889020100.pdf"/>
<attribute name="FRE" value="11.5MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="40uH"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value="744889020100"/>
<attribute name="RDC1-MAX" value="500mOhm"/>
<attribute name="RDC1-TYP" value="358mOhm"/>
<attribute name="RDC2-MAX" value="750mOhm"/>
<attribute name="RDC2-TYP" value="552mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744889020220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889020220.pdf"/>
<attribute name="FRE" value="7MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L2" value="88uH"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value="744889020220"/>
<attribute name="RDC1-MAX" value="1000mOhm"/>
<attribute name="RDC1-TYP" value="712mOhm"/>
<attribute name="RDC2-MAX" value="1600mOhm"/>
<attribute name="RDC2-TYP" value="1208mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744889020330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889020330.pdf"/>
<attribute name="FRE" value="5.8MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="L2" value="132uH"/>
<attribute name="N" value="1:2"/>
<attribute name="PART-NUMBER" value="744889020330"/>
<attribute name="RDC1-MAX" value="1900mOhm"/>
<attribute name="RDC1-TYP" value="1383mOhm"/>
<attribute name="RDC2-MAX" value="3200mOhm"/>
<attribute name="RDC2-TYP" value="2418mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744889030100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889030100.pdf"/>
<attribute name="FRE" value="8MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L2" value="90uH"/>
<attribute name="N" value="1:3"/>
<attribute name="PART-NUMBER" value="744889030100"/>
<attribute name="RDC1-MAX" value="500mOhm"/>
<attribute name="RDC1-TYP" value="363mOhm"/>
<attribute name="RDC2-MAX" value="1100mOhm"/>
<attribute name="RDC2-TYP" value="846mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744889030220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889030220.pdf"/>
<attribute name="FRE" value="5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L2" value="198uH"/>
<attribute name="N" value="1:3"/>
<attribute name="PART-NUMBER" value="744889030220"/>
<attribute name="RDC1-MAX" value="1000mOhm"/>
<attribute name="RDC1-TYP" value="732mOhm"/>
<attribute name="RDC2-MAX" value="2500mOhm"/>
<attribute name="RDC2-TYP" value="1872mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744889030330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744889030330.pdf"/>
<attribute name="FRE" value="4MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="L2" value="297uH"/>
<attribute name="N" value="1:3"/>
<attribute name="PART-NUMBER" value="744889030330"/>
<attribute name="RDC1-MAX" value="1900mOhm"/>
<attribute name="RDC1-TYP" value="1466mOhm"/>
<attribute name="RDC2-MAX" value="5200mOhm"/>
<attribute name="RDC2-TYP" value="3758mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
