<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-MXGA&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-09-03&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MXGA_4020">
<description>&lt;b&gt;WE-MXGA SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4020,SMT,2pins
&lt;br&gt;LXWXH=4.1X4.1X2.1mm</description>
</package>
<package name="WE-MXGA_5030">
<description>&lt;b&gt;WE-MXGA SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:5030,SMT,2pins
&lt;br&gt;LXWXH=5.4X5.4X3.1mm</description>
</package>
<package name="WE-MXGA_4020_IPC-7351">
<description>&lt;b&gt;WE-MXGA SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4020,SMT,2pins
&lt;br&gt;LXWXH=4.1X4.1X2.1mm
&lt;br&gt;This Land pattern is based on the IPC-7351 Standard</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MXGA_5030" prefix="L">
<description>&lt;b&gt;WE-MXGA SMT Power Inductor&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Innovative iron alloy material
&lt;br&gt;Ultra-low RDC and AC losses
&lt;br&gt;High efficiency and current capability
&lt;br&gt;Optimized for high switching frequencies beyond 1 MHz
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Operating temperature: -40 °C to 125°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;High frequency applications (GaN and SiC)

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o864782v209%20FAMILY-WE-MXGA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o864782v209%20FAMILY-WE-MXGA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MXGA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-MXGA&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-09-03 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MXGA_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438450300022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438450300022?ae"/>
<attribute name="FRES" value="155MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="28.1A@40K"/>
<attribute name="ISAT1" value="11.8A@10%"/>
<attribute name="ISAT2" value="25.4A@30%"/>
<attribute name="L" value="0.22uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438450300022"/>
<attribute name="RDC-MAX" value="1.7mohm"/>
<attribute name="RDC-TYP" value="1.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_78438450300047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438450300047?ae"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="23A@40K"/>
<attribute name="ISAT1" value="9.4A@10%"/>
<attribute name="ISAT2" value="20A@30%"/>
<attribute name="L" value="0.47uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438450300047"/>
<attribute name="RDC-MAX" value="2.8mohm"/>
<attribute name="RDC-TYP" value="2.4mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_78438450300060">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438450300060?ae"/>
<attribute name="FRES" value="73MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="21.5A@40K"/>
<attribute name="ISAT1" value="9.5A@10%"/>
<attribute name="ISAT2" value="21.2A@30%"/>
<attribute name="L" value="0.6uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438450300060"/>
<attribute name="RDC-MAX" value="3.2mohm"/>
<attribute name="RDC-TYP" value="2.8mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.6uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_78438450300082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438450300082?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="19A@40K"/>
<attribute name="ISAT1" value="8.1A@10%"/>
<attribute name="ISAT2" value="16.7A@30%"/>
<attribute name="L" value="0.82uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438450300082"/>
<attribute name="RDC-MAX" value="4mohm"/>
<attribute name="RDC-TYP" value="3.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030010?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="15.8A@40K"/>
<attribute name="ISAT1" value="7A@10%"/>
<attribute name="ISAT2" value="14.3A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030010"/>
<attribute name="RDC-MAX" value="5.8mohm"/>
<attribute name="RDC-TYP" value="5.2mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030012?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="17.2A@40K"/>
<attribute name="ISAT1" value="6.8A@10%"/>
<attribute name="ISAT2" value="14.3A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030012"/>
<attribute name="RDC-MAX" value="5.2mohm"/>
<attribute name="RDC-TYP" value="4.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030015?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="14.9A@40K"/>
<attribute name="ISAT1" value="6A@10%"/>
<attribute name="ISAT2" value="12.3A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030015"/>
<attribute name="RDC-MAX" value="6.3mohm"/>
<attribute name="RDC-TYP" value="5.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030022?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="12.4A@40K"/>
<attribute name="ISAT1" value="5.2A@10%"/>
<attribute name="ISAT2" value="10.5A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030022"/>
<attribute name="RDC-MAX" value="9.3mohm"/>
<attribute name="RDC-TYP" value="8.1mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="10A@40K"/>
<attribute name="ISAT1" value="4A@10%"/>
<attribute name="ISAT2" value="8.2A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030033"/>
<attribute name="RDC-MAX" value="14.8mohm"/>
<attribute name="RDC-TYP" value="12.9mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030047?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="8.2A@40K"/>
<attribute name="ISAT1" value="3.7A@10%"/>
<attribute name="ISAT2" value="7.7A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030047"/>
<attribute name="RDC-MAX" value="24.5mohm"/>
<attribute name="RDC-TYP" value="22.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030056?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="7.1A@40K"/>
<attribute name="ISAT1" value="3.3A@10%"/>
<attribute name="ISAT2" value="6.8A@30%"/>
<attribute name="L" value="5.6uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030056"/>
<attribute name="RDC-MAX" value="27mohm"/>
<attribute name="RDC-TYP" value="24.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030068?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="6.5A@40K"/>
<attribute name="ISAT1" value="3.2A@10%"/>
<attribute name="ISAT2" value="6.8A@30%"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030068"/>
<attribute name="RDC-MAX" value="31.7mohm"/>
<attribute name="RDC-TYP" value="28.3mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030082?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="6.1A@40K"/>
<attribute name="ISAT1" value="2.6A@10%"/>
<attribute name="ISAT2" value="5.9A@30%"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030082"/>
<attribute name="RDC-MAX" value="39mohm"/>
<attribute name="RDC-TYP" value="34mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030100?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="5.5A@40K"/>
<attribute name="ISAT1" value="2.5A@10%"/>
<attribute name="ISAT2" value="5.4A@30%"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030100"/>
<attribute name="RDC-MAX" value="47.7mohm"/>
<attribute name="RDC-TYP" value="41.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030120?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="5A@40K"/>
<attribute name="ISAT1" value="2.1A@10%"/>
<attribute name="ISAT2" value="4.9A@30%"/>
<attribute name="L" value="12uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030120"/>
<attribute name="RDC-MAX" value="57mohm"/>
<attribute name="RDC-TYP" value="52.3mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
<technology name="_7843845030150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843845030150?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="IRP" value="4.5A@40K"/>
<attribute name="ISAT1" value="1.9A@10%"/>
<attribute name="ISAT2" value="4.3A@30%"/>
<attribute name="L" value="15uH"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843845030150"/>
<attribute name="RDC-MAX" value="74.4mohm"/>
<attribute name="RDC-TYP" value="64.5mohm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="WIDTH" value="5.4mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MXGA_4020" prefix="L">
<description>&lt;b&gt;WE-MXGA SMT Power Inductor&lt;br&gt;

&lt;br&gt;Characteristics 
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Innovative iron alloy material
&lt;br&gt;Ultra-low RDC and AC losses
&lt;br&gt;High efficiency and current capability
&lt;br&gt;Optimized for high switching frequencies beyond 1 MHz
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Operating temperature: -40 °C to 125°C

&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications 
&lt;/b&gt;&lt;br&gt;&lt;br&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;High frequency applications (GaN and SiC)

&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o864782v209%20FAMILY-WE-MXGA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o864782v209%20FAMILY-WE-MXGA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-MXGA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-MXGA&lt;/a&gt;&lt;p&gt;

Created by Ella 2025-09-03 &lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MXGA_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438440200016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200016?ae"/>
<attribute name="FRES" value="197MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="24.2A@40K"/>
<attribute name="ISAT1" value="12A@10%"/>
<attribute name="ISAT2" value="27.9A@30%"/>
<attribute name="L" value="0.16uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200016"/>
<attribute name="RDC-MAX" value="1.7mohm"/>
<attribute name="RDC-TYP" value="1.5mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_78438440200030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200030?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="23.2A@40K"/>
<attribute name="ISAT1" value="8.4A@10%"/>
<attribute name="ISAT2" value="17.6A@30%"/>
<attribute name="L" value="0.3uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200030"/>
<attribute name="RDC-MAX" value="2.3mohm"/>
<attribute name="RDC-TYP" value="2mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_78438440200040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200040?ae"/>
<attribute name="FRES" value="122MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="16.9A@40K"/>
<attribute name="ISAT1" value="7.3A@10%"/>
<attribute name="ISAT2" value="14.8A@30%"/>
<attribute name="L" value="0.4uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200040"/>
<attribute name="RDC-MAX" value="4.4mohm"/>
<attribute name="RDC-TYP" value="3.8mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_78438440200065">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200065?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="15.2A@40K"/>
<attribute name="ISAT1" value="6.2A@10%"/>
<attribute name="ISAT2" value="12.6A@30%"/>
<attribute name="L" value="0.65uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200065"/>
<attribute name="RDC-MAX" value="5.5mohm"/>
<attribute name="RDC-TYP" value="4.8mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.65uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="12.1A@40K"/>
<attribute name="ISAT1" value="4.9A@10%"/>
<attribute name="ISAT2" value="9.8A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020010"/>
<attribute name="RDC-MAX" value="7.9mohm"/>
<attribute name="RDC-TYP" value="6.9mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020012?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="11A@40K"/>
<attribute name="ISAT1" value="4.3A@10%"/>
<attribute name="ISAT2" value="8.8A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020012"/>
<attribute name="RDC-MAX" value="9.8mohm"/>
<attribute name="RDC-TYP" value="8.4mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020015?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="10.3A@40K"/>
<attribute name="ISAT1" value="4.1A@10%"/>
<attribute name="ISAT2" value="8.4A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020015"/>
<attribute name="RDC-MAX" value="11.5mohm"/>
<attribute name="RDC-TYP" value="10mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="9.5A@40K"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="7.1A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020018"/>
<attribute name="RDC-MAX" value="13.6mohm"/>
<attribute name="RDC-TYP" value="11.9mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="7.8A@40K"/>
<attribute name="ISAT1" value="2.9A@10%"/>
<attribute name="ISAT2" value="5.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020022"/>
<attribute name="RDC-MAX" value="17.9mohm"/>
<attribute name="RDC-TYP" value="15.6mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020033?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="6.1A@40K"/>
<attribute name="ISAT1" value="2.6A@10%"/>
<attribute name="ISAT2" value="5.3A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020033"/>
<attribute name="RDC-MAX" value="30.6mohm"/>
<attribute name="RDC-TYP" value="26.6mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="5.2A@40K"/>
<attribute name="ISAT1" value="2.8A@10%"/>
<attribute name="ISAT2" value="5.7A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020047"/>
<attribute name="RDC-MAX" value="46.4mohm"/>
<attribute name="RDC-TYP" value="40.3mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MXGA_4020_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438440200016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200016?ae"/>
<attribute name="FRES" value="197MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="24.2A@40K"/>
<attribute name="ISAT1" value="12A@10%"/>
<attribute name="ISAT2" value="27.9A@30%"/>
<attribute name="L" value="0.16uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200016"/>
<attribute name="RDC-MAX" value="1.7mohm"/>
<attribute name="RDC-TYP" value="1.5mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_78438440200030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200030?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="23.2A@40K"/>
<attribute name="ISAT1" value="8.4A@10%"/>
<attribute name="ISAT2" value="17.6A@30%"/>
<attribute name="L" value="0.3uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200030"/>
<attribute name="RDC-MAX" value="2.3mohm"/>
<attribute name="RDC-TYP" value="2mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_78438440200040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200040?ae"/>
<attribute name="FRES" value="122MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="16.9A@40K"/>
<attribute name="ISAT1" value="7.3A@10%"/>
<attribute name="ISAT2" value="14.8A@30%"/>
<attribute name="L" value="0.4uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200040"/>
<attribute name="RDC-MAX" value="4.4mohm"/>
<attribute name="RDC-TYP" value="3.8mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_78438440200065">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200065?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="15.2A@40K"/>
<attribute name="ISAT1" value="6.2A@10%"/>
<attribute name="ISAT2" value="12.6A@30%"/>
<attribute name="L" value="0.65uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="78438440200065"/>
<attribute name="RDC-MAX" value="5.5mohm"/>
<attribute name="RDC-TYP" value="4.8mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.65uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="12.1A@40K"/>
<attribute name="ISAT1" value="4.9A@10%"/>
<attribute name="ISAT2" value="9.8A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020010"/>
<attribute name="RDC-MAX" value="7.9mohm"/>
<attribute name="RDC-TYP" value="6.9mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020012?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="11A@40K"/>
<attribute name="ISAT1" value="4.3A@10%"/>
<attribute name="ISAT2" value="8.8A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020012"/>
<attribute name="RDC-MAX" value="9.8mohm"/>
<attribute name="RDC-TYP" value="8.4mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020015?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="10.3A@40K"/>
<attribute name="ISAT1" value="4.1A@10%"/>
<attribute name="ISAT2" value="8.4A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020015"/>
<attribute name="RDC-MAX" value="11.5mohm"/>
<attribute name="RDC-TYP" value="10mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="9.5A@40K"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="7.1A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020018"/>
<attribute name="RDC-MAX" value="13.6mohm"/>
<attribute name="RDC-TYP" value="11.9mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="7.8A@40K"/>
<attribute name="ISAT1" value="2.9A@10%"/>
<attribute name="ISAT2" value="5.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020022"/>
<attribute name="RDC-MAX" value="17.9mohm"/>
<attribute name="RDC-TYP" value="15.6mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020033?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="6.1A@40K"/>
<attribute name="ISAT1" value="2.6A@10%"/>
<attribute name="ISAT2" value="5.3A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020033"/>
<attribute name="RDC-MAX" value="30.6mohm"/>
<attribute name="RDC-TYP" value="26.6mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
<technology name="_7843844020047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="IRP" value="5.2A@40K"/>
<attribute name="ISAT1" value="2.8A@10%"/>
<attribute name="ISAT2" value="5.7A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7843844020047"/>
<attribute name="RDC-MAX" value="46.4mohm"/>
<attribute name="RDC-TYP" value="40.3mohm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="4.1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
