<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Automotive - Single Coil Power Inductors - WE-MXGA

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-09-22
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MXGA_4030">
<description>WE-MXGA SMT Power Inductor

Size:4030,SMT,2pins 
LXWXH=4.1X4.1X3.1mm</description>
</package>
<package name="WE-MXGA_4030_IPC-7351">
<description>WE-MXGA SMT Power Inductor

Size:4030,SMT,2pins 
LXWXH=4.1X4.1X3.1mm
This Land pattern is based on the IPC-7351 Standard</description>
</package>
<package name="WE-MXGA_5030">
<description>WE-MXGA SMT Power Inductor

Size:5030,SMT,2pins

LXWXH=5.4X5.4X3.1mm</description>
</package>
<package name="WE-MXGA_4020_IPC-7351">
<description>WE-MXGA SMT Power Inductor

Size:4020,SMT,2pins

LXWXH=4.1X4.1X2.1mm

This Land pattern is based on the IPC-7351 Standard</description>
</package>
<package name="WE-MXGA_4020">
<description>WE-MXGA SMT Power Inductor

Size:4020,SMT,2pins

LXWXH=4.1X4.1X2.1mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MXGA_4030">
<description>WE-MXGA SMT Power Inductor

Characteristics
Innovative iron alloy material
Ultra low RDC and AC losses
High efficiency and current capability
Optimized for high switching frequencies beyond 1 MHz
Magnetically shielded construction
Compact design
Operating temperature: -40 ºC up to 125 ºC

Applications
Body electronics &amp; lighting
Infotainment systems
DC/DC-converter 48 V / 12 V
POL-converter
DC/DC converter for field programmable gate array
BMS (battery management system)

Details see: www.we-online.com/components/products/WE-MXGA

Created by Ella 2026-09-22
2026 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MXGA_4030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="VALUE" value=""/>
<attribute name="DATASHEET" value=""/>
<attribute name="MANUFACTURER" value=""/>
<attribute name="MPN" value=""/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MXGA_4030_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438440300004">
<attribute name="VALUE" value="0.04 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440300004?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440300004"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.04 uH"/>
<attribute name="SATURATION_CURRENT_1" value="20.8 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="44.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="0.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="0.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="630 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="37.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440300010">
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440300010?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440300010"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.1 uH"/>
<attribute name="SATURATION_CURRENT_1" value="14.7 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="29.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1.1 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="1.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="293 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="30.3 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440300016">
<attribute name="VALUE" value="0.16 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440300016?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440300016"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.16 uH"/>
<attribute name="SATURATION_CURRENT_1" value="12.7 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="27 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1.2 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="1.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="214 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="28.7 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440300033">
<attribute name="VALUE" value="0.33 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440300033?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440300033"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.33 uH"/>
<attribute name="SATURATION_CURRENT_1" value="9.2 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="18.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="2.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="117 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="24.5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440300040">
<attribute name="VALUE" value="0.4 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440300040?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440300040"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.4 uH"/>
<attribute name="SATURATION_CURRENT_1" value="9.1 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="18.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="2.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="113 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="23 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440300062">
<attribute name="VALUE" value="0.62 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440300062?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440300062"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.62 uH"/>
<attribute name="SATURATION_CURRENT_1" value="7.1 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="14.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="4.3 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="4.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="79 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="15.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030010">
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030010?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030010"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="SATURATION_CURRENT_1" value="5.6 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="11.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6.3 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="7.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="60 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="13 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030012">
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030012?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030012"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="5.1 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="10.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8.4 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="9.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="57 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030015">
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030015?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030015"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="SATURATION_CURRENT_1" value="4.7 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="9.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8.8 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="10.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="47 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10.8 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030018">
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030018?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030018"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="SATURATION_CURRENT_1" value="4.4 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="8.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="9.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="11.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="40 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10.4 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030022">
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030022?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030022"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="4 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="7.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="12.3 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="14.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="37 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="9 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030033">
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030033?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030033"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="SATURATION_CURRENT_1" value="3.3 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="6.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="16.4 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="19.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="30 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.6 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030039">
<attribute name="VALUE" value="3.9 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030039?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030039"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="3.9 uH"/>
<attribute name="SATURATION_CURRENT_1" value="3.2 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="6.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="21.7 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="26 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.6 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030047">
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030047?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030047"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="SATURATION_CURRENT_1" value="3 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="24.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="29.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="23 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030056">
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030056?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030056"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.7 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="5.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="27.3 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="32.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="20 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.1 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030068">
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030068?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030068"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.5 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="5.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="32.6 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="39.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="17 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.3 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030082">
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030082?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030082"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.3 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="4.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="43.2 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="51.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="16 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.6 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844030100">
<attribute name="VALUE" value="10 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844030100?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844030100"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4030 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="SATURATION_CURRENT_1" value="1.9 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="4.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="57.8 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="69.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="16 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.1 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MXGA_5030" prefix="L">
<description>WE-MXGA SMT Power Inductor

Characteristics
Innovative iron alloy material
Ultra low RDC and AC losses
High efficiency and current capability
Optimized for high switching frequencies beyond 1 MHz
Magnetically shielded construction
Compact design
Operating temperature: -40 ºC up to 125 ºC

Applications
Body electronics &amp; lighting
Infotainment systems
DC/DC-converter 48 V / 12 V
POL-converter
DC/DC converter for field programmable gate array
BMS (battery management system)

Details see: www.we-online.com/components/products/WE-MXGA

Created by Ella 2025-09-03
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MXGA_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438450300022">
<attribute name="VALUE" value="0.22 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438450300022?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438450300022"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.22 uH"/>
<attribute name="SATURATION_CURRENT_1" value="11.8 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="25.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="1.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="155 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="28.1 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438450300047">
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438450300047?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438450300047"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.47 uH"/>
<attribute name="SATURATION_CURRENT_1" value="9.4 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="20 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2.4 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="2.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="84 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="23 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438450300060">
<attribute name="VALUE" value="0.6 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438450300060?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438450300060"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.6 uH"/>
<attribute name="SATURATION_CURRENT_1" value="9.5 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="21.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2.8 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="3.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="73 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="21.5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438450300082">
<attribute name="VALUE" value="0.82 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438450300082?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438450300082"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.82 uH"/>
<attribute name="SATURATION_CURRENT_1" value="8.1 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="16.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="3.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="55 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="19 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030010">
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030010?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030010"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="SATURATION_CURRENT_1" value="7 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="14.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="5.2 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="5.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="52 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="15.8 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030012">
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030012?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030012"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="6.8 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="14.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="4.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="5.2 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="43 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="17.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030015">
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030015?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030015"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="SATURATION_CURRENT_1" value="6 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="12.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="5.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="6.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="36 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="14.9 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030022">
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030022?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030022"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="5.2 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="10.5 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8.1 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="9.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="35 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.4 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030033">
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030033?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030033"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="SATURATION_CURRENT_1" value="4 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="8.2 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="12.9 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="14.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030047">
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030047?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030047"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="SATURATION_CURRENT_1" value="3.7 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="7.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="22.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="24.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="21 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="8.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030056">
<attribute name="VALUE" value="5.6 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030056?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030056"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="5.6 uH"/>
<attribute name="SATURATION_CURRENT_1" value="3.3 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="6.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="24.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="27 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="19 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.1 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030068">
<attribute name="VALUE" value="6.8 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030068?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030068"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="6.8 uH"/>
<attribute name="SATURATION_CURRENT_1" value="3.2 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="6.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="28.3 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="31.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="18 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030082">
<attribute name="VALUE" value="8.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030082?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030082"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="8.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.6 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="5.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="34 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="39 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="15 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.1 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030100">
<attribute name="VALUE" value="10 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030100?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030100"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="10 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.5 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="5.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="41.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="47.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="12 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030120">
<attribute name="VALUE" value="12 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030120?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030120"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="12 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.1 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="4.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="52.3 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="57 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="11 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843845030150">
<attribute name="VALUE" value="15 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843845030150?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843845030150"/>
<attribute name="HEIGHT" value="3.1mm"/>
<attribute name="LENGTH" value="5.4mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="5030"/>
<attribute name="WIDTH" value="5.4mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="15 uH"/>
<attribute name="SATURATION_CURRENT_1" value="1.9 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="4.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="64.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="74.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="10 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="4.5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MXGA_4020" prefix="L">
<description>WE-MXGA SMT Power Inductor

Characteristics
Innovative iron alloy material
Ultra low RDC and AC losses
High efficiency and current capability
Optimized for high switching frequencies beyond 1 MHz
Magnetically shielded construction
Compact design
Operating temperature: -40 ºC up to 125 ºC

Applications
Body electronics &amp; lighting
Infotainment systems
DC/DC-converter 48 V / 12 V
POL-converter
DC/DC converter for field programmable gate array
BMS (battery management system)

Details see: www.we-online.com/components/products/WE-MXGA

Created by Ella 2025-09-03
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MXGA_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438440200016">
<attribute name="VALUE" value="0.16uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200016?ae"/>
<attribute name="FRES" value="197MHz"/>
<attribute name="IRP" value="24.2A@40K"/>
<attribute name="ISAT1" value="12A@10%"/>
<attribute name="ISAT2" value="27.9A@30%"/>
<attribute name="L" value="0.16uH"/>
<attribute name="PART-NUMBER" value="78438440200016"/>
<attribute name="RDC-MAX" value="1.7mohm"/>
<attribute name="RDC-TYP" value="1.5mohm"/>
</technology>
<technology name="_78438440200030">
<attribute name="VALUE" value="0.3uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200030?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="IRP" value="23.2A@40K"/>
<attribute name="ISAT1" value="8.4A@10%"/>
<attribute name="ISAT2" value="17.6A@30%"/>
<attribute name="L" value="0.3uH"/>
<attribute name="PART-NUMBER" value="78438440200030"/>
<attribute name="RDC-MAX" value="2.3mohm"/>
<attribute name="RDC-TYP" value="2mohm"/>
</technology>
<technology name="_78438440200040">
<attribute name="VALUE" value="0.4uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200040?ae"/>
<attribute name="FRES" value="122MHz"/>
<attribute name="IRP" value="16.9A@40K"/>
<attribute name="ISAT1" value="7.3A@10%"/>
<attribute name="ISAT2" value="14.8A@30%"/>
<attribute name="L" value="0.4uH"/>
<attribute name="PART-NUMBER" value="78438440200040"/>
<attribute name="RDC-MAX" value="4.4mohm"/>
<attribute name="RDC-TYP" value="3.8mohm"/>
</technology>
<technology name="_78438440200065">
<attribute name="VALUE" value="0.65uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/78438440200065?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IRP" value="15.2A@40K"/>
<attribute name="ISAT1" value="6.2A@10%"/>
<attribute name="ISAT2" value="12.6A@30%"/>
<attribute name="L" value="0.65uH"/>
<attribute name="PART-NUMBER" value="78438440200065"/>
<attribute name="RDC-MAX" value="5.5mohm"/>
<attribute name="RDC-TYP" value="4.8mohm"/>
</technology>
<technology name="_7843844020010">
<attribute name="VALUE" value="1uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IRP" value="12.1A@40K"/>
<attribute name="ISAT1" value="4.9A@10%"/>
<attribute name="ISAT2" value="9.8A@30%"/>
<attribute name="L" value="1uH"/>
<attribute name="PART-NUMBER" value="7843844020010"/>
<attribute name="RDC-MAX" value="7.9mohm"/>
<attribute name="RDC-TYP" value="6.9mohm"/>
</technology>
<technology name="_7843844020012">
<attribute name="VALUE" value="1.2uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020012?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IRP" value="11A@40K"/>
<attribute name="ISAT1" value="4.3A@10%"/>
<attribute name="ISAT2" value="8.8A@30%"/>
<attribute name="L" value="1.2uH"/>
<attribute name="PART-NUMBER" value="7843844020012"/>
<attribute name="RDC-MAX" value="9.8mohm"/>
<attribute name="RDC-TYP" value="8.4mohm"/>
</technology>
<technology name="_7843844020015">
<attribute name="VALUE" value="1.5uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020015?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IRP" value="10.3A@40K"/>
<attribute name="ISAT1" value="4.1A@10%"/>
<attribute name="ISAT2" value="8.4A@30%"/>
<attribute name="L" value="1.5uH"/>
<attribute name="PART-NUMBER" value="7843844020015"/>
<attribute name="RDC-MAX" value="11.5mohm"/>
<attribute name="RDC-TYP" value="10mohm"/>
</technology>
<technology name="_7843844020018">
<attribute name="VALUE" value="1.8uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IRP" value="9.5A@40K"/>
<attribute name="ISAT1" value="3.6A@10%"/>
<attribute name="ISAT2" value="7.1A@30%"/>
<attribute name="L" value="1.8uH"/>
<attribute name="PART-NUMBER" value="7843844020018"/>
<attribute name="RDC-MAX" value="13.6mohm"/>
<attribute name="RDC-TYP" value="11.9mohm"/>
</technology>
<technology name="_7843844020022">
<attribute name="VALUE" value="2.2uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IRP" value="7.8A@40K"/>
<attribute name="ISAT1" value="2.9A@10%"/>
<attribute name="ISAT2" value="5.8A@30%"/>
<attribute name="L" value="2.2uH"/>
<attribute name="PART-NUMBER" value="7843844020022"/>
<attribute name="RDC-MAX" value="17.9mohm"/>
<attribute name="RDC-TYP" value="15.6mohm"/>
</technology>
<technology name="_7843844020033">
<attribute name="VALUE" value="3.3uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020033?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IRP" value="6.1A@40K"/>
<attribute name="ISAT1" value="2.6A@10%"/>
<attribute name="ISAT2" value="5.3A@30%"/>
<attribute name="L" value="3.3uH"/>
<attribute name="PART-NUMBER" value="7843844020033"/>
<attribute name="RDC-MAX" value="30.6mohm"/>
<attribute name="RDC-TYP" value="26.6mohm"/>
</technology>
<technology name="_7843844020047">
<attribute name="VALUE" value="4.7uH"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7843844020047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IRP" value="5.2A@40K"/>
<attribute name="ISAT1" value="2.8A@10%"/>
<attribute name="ISAT2" value="5.7A@30%"/>
<attribute name="L" value="4.7uH"/>
<attribute name="PART-NUMBER" value="7843844020047"/>
<attribute name="RDC-MAX" value="46.4mohm"/>
<attribute name="RDC-TYP" value="40.3mohm"/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MXGA_4020_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_78438440200016">
<attribute name="VALUE" value="0.16 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440200016?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440200016"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.16 uH"/>
<attribute name="SATURATION_CURRENT_1" value="12 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="27.9 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="1.5 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="1.7 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="197 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="24.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440200030">
<attribute name="VALUE" value="0.3 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440200030?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440200030"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.3 uH"/>
<attribute name="SATURATION_CURRENT_1" value="8.4 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="17.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="2 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="2.3 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="135 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="23.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440200040">
<attribute name="VALUE" value="0.4 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440200040?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440200040"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.4 uH"/>
<attribute name="SATURATION_CURRENT_1" value="7.3 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="14.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="3.8 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="4.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="122 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="16.9 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_78438440200065">
<attribute name="VALUE" value="0.65 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/78438440200065?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="78438440200065"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="0.65 uH"/>
<attribute name="SATURATION_CURRENT_1" value="6.2 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="12.6 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="4.8 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="5.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="80 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="15.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844020010">
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844020010?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844020010"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1 uH"/>
<attribute name="SATURATION_CURRENT_1" value="4.9 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="9.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="6.9 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="7.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="59 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="12.1 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844020012">
<attribute name="VALUE" value="1.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844020012?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844020012"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="4.3 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="8.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="8.4 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="9.8 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="53 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="11 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844020015">
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844020015?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844020015"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.5 uH"/>
<attribute name="SATURATION_CURRENT_1" value="4.1 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="8.4 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="10 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="11.5 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="50 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="10.3 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844020018">
<attribute name="VALUE" value="1.8 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844020018?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844020018"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="1.8 uH"/>
<attribute name="SATURATION_CURRENT_1" value="3.6 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="7.1 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="11.9 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="13.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="42 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="9.5 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844020022">
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844020022?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844020022"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="2.2 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.9 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="5.8 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="15.6 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="17.9 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="37 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="7.8 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844020033">
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844020033?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844020033"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="3.3 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.6 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="5.3 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="26.6 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="30.6 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="29 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="6.1 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
<technology name="_7843844020047">
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/7843844020047?ae"/>
<attribute name="MANUFACTURER" value="Würth Elektronik"/>
<attribute name="MPN" value="7843844020047"/>
<attribute name="HEIGHT" value="2.1mm"/>
<attribute name="LENGTH" value="4.1mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="SIZE" value="4020"/>
<attribute name="WIDTH" value="4.1mm"/>
<attribute name="CATEGORY" value="Inductors"/>
<attribute name="INDUCTANCE" value="4.7 uH"/>
<attribute name="SATURATION_CURRENT_1" value="2.8 A@10%"/>
<attribute name="SATURATION_CURRENT_2" value="5.7 A@30%"/>
<attribute name="DC_RESISTANCE_TYP" value="40.3 mohm"/>
<attribute name="DC_RESISTANCE_MAX" value="46.4 mohm"/>
<attribute name="SELF_RESONANT_FREQUENCY" value="25 MHz"/>
<attribute name="PERFORMANCE_RATED_CURRENT" value="5.2 A@40K"/>
<attribute name="PREFIX" value="L"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
