<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-MXGI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024b, 2024-12-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-MXGI_5030">
<description>&lt;b&gt;WE-MXGI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:5030,SMT,2pins
&lt;br&gt;LXWXH=5.4X5.4X3.1mm</description>
</package>
<package name="WE-MXGI_4020">
<description>&lt;b&gt;WE-MXGI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4020,SMT,2pins
&lt;br&gt;LXWXH=4.1X4.1X2.1mm</description>
</package>
<package name="WE-MXGI_4020_IPC-7351">
<description>&lt;b&gt;WE-MXGI SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size:4020,SMT,2pins
&lt;br&gt;LXWXH=4.1X4.1X2.1mm
&lt;br&gt;This Land pattern is based on the IPC-7351 Standard</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-MXGI_5030" prefix="L">
<description>&lt;b&gt; WE-MXGI SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Innovative iron alloy material
&lt;br&gt;Ultra low RDC and AC losses
&lt;br&gt;High efficiency and current capability
&lt;br&gt;Optimized for high switching frequencies beyond 1 MHz
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Operating temperature: -40 °C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798531v209%20FAMILY-WE-MXGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798531v209%20FAMILY-WE-MXGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-MXGI"&gt;www.we-online.com/en/components/products/WE-MXGI&lt;/a&gt;&lt;p&gt;

Created by Ella 2024-06-07&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MXGI_5030">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438450300022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438450300022?ae"/>
<attribute name="FRES" value="155MHz"/>
<attribute name="IR" value="28.1A"/>
<attribute name="ISAT" value="25.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438450300022 "/>
<attribute name="RDC-TYP" value="1.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_74438450300047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438450300047?ae"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="IR" value="23A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438450300047 "/>
<attribute name="RDC-TYP" value="2.4mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_74438450300060">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438450300060?ae"/>
<attribute name="FRES" value="73MHz"/>
<attribute name="IR" value="21.5A"/>
<attribute name="ISAT" value="21.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438450300060 "/>
<attribute name="RDC-TYP" value="2.8mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.6uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_74438450300082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438450300082?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="16.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438450300082 "/>
<attribute name="RDC-TYP" value="3.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="0.82uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030010?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="15.8A"/>
<attribute name="ISAT" value="14.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030010 "/>
<attribute name="RDC-TYP" value="5.2mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030012?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="17.2A"/>
<attribute name="ISAT" value="14.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030012 "/>
<attribute name="RDC-TYP" value="4.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030015?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="14.9A"/>
<attribute name="ISAT" value="12.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030015 "/>
<attribute name="RDC-TYP" value="5.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030022?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="12.4A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030022 "/>
<attribute name="RDC-TYP" value="8.1mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030033?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="8.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030033 "/>
<attribute name="RDC-TYP" value="12.9mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030047?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="8.2A"/>
<attribute name="ISAT" value="7.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030047 "/>
<attribute name="RDC-TYP" value="22.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030056?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030056 "/>
<attribute name="RDC-TYP" value="24.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030068?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030068 "/>
<attribute name="RDC-TYP" value="28.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030082?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="5.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030082 "/>
<attribute name="RDC-TYP" value="34mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030100?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030100 "/>
<attribute name="RDC-TYP" value="41.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030120?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="4.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030120 "/>
<attribute name="RDC-TYP" value="52.3mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443845030150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443845030150?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="4.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443845030150 "/>
<attribute name="RDC-TYP" value="64.5mOhm"/>
<attribute name="SIZE" value=" 5030 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VDC" value="80V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-MXGI_4020" prefix="L">
<description>&lt;b&gt; WE-MXGI SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Innovative iron alloy material
&lt;br&gt;Ultra low RDC and AC losses
&lt;br&gt;High efficiency and current capability
&lt;br&gt;Optimized for high switching frequencies beyond 1 MHz
&lt;br&gt;Compact design
&lt;br&gt;Magnetically shielded construction
&lt;br&gt;Operating temperature: -40 °C to 125°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;DC/DC-converter for high current power supplies
&lt;br&gt;DC/DC-converter for Field Programmable Gate Array (FPGA)
&lt;br&gt;POL-converters
&lt;br&gt;Portable power like PDA, digital camera
&lt;br&gt;Mainboards/graphic cards
&lt;br&gt;Battery powered devices
&lt;br&gt;Wireless communication devices
&lt;br&gt;Power supplies for smartphones, tablet PCs and other mobile devices
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o798531v209%20FAMILY-WE-MXGI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o798531v209%20FAMILY-WE-MXGI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-MXGI"&gt;www.we-online.com/en/components/products/WE-MXGI&lt;/a&gt;&lt;p&gt;

Updated by Ella 2024-09-27&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-MXGI_4020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438440200016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438440200016?ae"/>
<attribute name="FRES" value="197MHz"/>
<attribute name="IR" value="24.2A"/>
<attribute name="ISAT" value="27.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438440200016 "/>
<attribute name="RDC-TYP" value="1.5mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IR" value="12.1A"/>
<attribute name="ISAT" value="9.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020010 "/>
<attribute name="RDC-TYP" value="6.9mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="7.8A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020022 "/>
<attribute name="RDC-TYP" value="15.6mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="5.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020047 "/>
<attribute name="RDC-TYP" value="40.3mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VDC" value="80V"/>
</technology>
</technologies>
</device>
<device name="_IPC-7351" package="WE-MXGI_4020_IPC-7351">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74438440200016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438440200016?ae"/>
<attribute name="FRES" value="197MHz"/>
<attribute name="IR" value="24.2A"/>
<attribute name="ISAT" value="27.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438440200016 "/>
<attribute name="RDC-TYP" value="1.5mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.16uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_74438440200030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438440200030?ae"/>
<attribute name="FRES" value="135MHz"/>
<attribute name="IR" value="23.2A"/>
<attribute name="ISAT" value="17.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438440200030 "/>
<attribute name="RDC-TYP" value="2mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.3uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_74438440200040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438440200040?ae"/>
<attribute name="FRES" value="122MHz"/>
<attribute name="IR" value="16.9A"/>
<attribute name="ISAT" value="14.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438440200040 "/>
<attribute name="RDC-TYP" value="3.8mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.4uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_74438440200065">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74438440200065?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="15.2A"/>
<attribute name="ISAT" value="12.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74438440200065 "/>
<attribute name="RDC-TYP" value="4.8mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="0.65uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020010?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IR" value="12.1A"/>
<attribute name="ISAT" value="9.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020010 "/>
<attribute name="RDC-TYP" value="6.9mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020012?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="8.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020012 "/>
<attribute name="RDC-TYP" value="8.4mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020015?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="10.3A"/>
<attribute name="ISAT" value="8.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020015 "/>
<attribute name="RDC-TYP" value="10mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020018?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="ISAT" value="7.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020018 "/>
<attribute name="RDC-TYP" value="11.9mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020022?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="7.8A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020022 "/>
<attribute name="RDC-TYP" value="15.6mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020033?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IR" value="6.1A"/>
<attribute name="ISAT" value="5.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020033 "/>
<attribute name="RDC-TYP" value="26.6mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VDC" value="80V"/>
</technology>
<technology name="_7443844020047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7443844020047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="5.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7443844020047 "/>
<attribute name="RDC-TYP" value="40.3mOhm"/>
<attribute name="SIZE" value=" 4020 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VDC" value="80V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
