<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For AC/DC Converter - WE-OLEFD&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-04-10&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-OLEFD_EFD20_SMT">
<description>&lt;b&gt;WE-OLEE EE-Style Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EFD20,SMT,12pins
&lt;br&gt;LXWXH=21.5X33.8X12mm</description>
</package>
<package name="WE-OLEFD_EFD25_THT">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EFD25,THT,12pins
&lt;br&gt;LXWXH=26.3X33X14.81mm</description>
</package>
<package name="WE-OLEFD_EFD20_THT">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EFD20,THT,10pins
&lt;br&gt;LXWXH=21.5X29X12mm</description>
</package>
</packages>
<symbols>
<symbol name="750811644">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508116313">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811914">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="750811643">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508112330">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811645">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811613">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508112327">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="750811614">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811616">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508112510">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="7508112511">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="750811612">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811913">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="12" direction="pas"/>
</symbol>
<symbol name="7508116312">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508112514">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="7508112512">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508112513">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508112334">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
<symbol name="7508116314">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811512">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811611">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="750811617">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="10" direction="pas"/>
</symbol>
<symbol name="7508112515">
<pin name="1" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="11" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="750811913" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811913"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811913?ae"/>
<attribute name="F-SWTICH" value="68 - 130kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1.25A"/>
<attribute name="IOUT2" value="1.25A"/>
<attribute name="IOUT3" value="1.1A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="16.66 : 0.833 : 0.833 : 1.166 : 2.166 : 1"/>
<attribute name="PART-NUMBER" value=" 750811913 "/>
<attribute name="VALUE" value=" 750811913 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="7V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811643" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811643"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811643?ae"/>
<attribute name="F-SWTICH" value="68 - 120kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="0.5A"/>
<attribute name="IOUT2" value="0.5A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="20:3.6:3.6:2.2:1"/>
<attribute name="PART-NUMBER" value=" 750811643 "/>
<attribute name="VALUE" value=" 750811643 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="24V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811914" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811914"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811914?ae"/>
<attribute name="F-SWTICH" value="68 - 140kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1.3A"/>
<attribute name="IOUT2" value="1.3A"/>
<attribute name="IOUT3" value="0.5A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="20 : 0.8 : 0.8 : 2.8 : 2.2 : 1"/>
<attribute name="PART-NUMBER" value=" 750811914 "/>
<attribute name="VALUE" value=" 750811914 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VOUT3" value="19V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508116312" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508116312"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508116312?ae"/>
<attribute name="F-SWTICH" value="68 - 120kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1A"/>
<attribute name="IOUT2" value="1A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="20:1.8:1.8:2.2:1"/>
<attribute name="PART-NUMBER" value=" 7508116312 "/>
<attribute name="VALUE" value=" 7508116312 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112334" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112334"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112334?ae"/>
<attribute name="F-SWTICH" value="68 - 110kHz"/>
<attribute name="HEIGHT" value="14.81mm"/>
<attribute name="IOUT1" value="1.6A"/>
<attribute name="ISAT1" value="2.2A"/>
<attribute name="L1" value="414µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16:2.33:2:1"/>
<attribute name="PART-NUMBER" value=" 7508112334 "/>
<attribute name="VALUE" value=" 7508112334 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="16V"/>
<attribute name="VT" value="4501 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811645" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811645"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811645?ae"/>
<attribute name="F-SWTICH" value="68 - 100kHz"/>
<attribute name="HEIGHT" value="14.48mm"/>
<attribute name="IOUT1" value="0.71A"/>
<attribute name="IOUT2" value="0.71A"/>
<attribute name="ISAT1" value="2A"/>
<attribute name="L1" value="470µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16.66:4:4:2.33:1"/>
<attribute name="PART-NUMBER" value=" 750811645 "/>
<attribute name="VALUE" value=" 750811645 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="24V"/>
<attribute name="VT" value="4508 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508116314" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508116314"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508116314?ae"/>
<attribute name="F-SWTICH" value="68 - 110kHz"/>
<attribute name="HEIGHT" value="14.81mm"/>
<attribute name="IOUT1" value="1.3A"/>
<attribute name="IOUT2" value="1.3A"/>
<attribute name="ISAT1" value="2.1A"/>
<attribute name="L1" value="450µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16.66:2:2.33:1"/>
<attribute name="PART-NUMBER" value=" 7508116314 "/>
<attribute name="VALUE" value=" 7508116314 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="4507 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811611" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811611"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811611?ae"/>
<attribute name="F-SWTICH" value="68 - 100kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="2A"/>
<attribute name="IOUT2" value="2A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="20 : 0.833 : 0.833 : 2.16 : 1"/>
<attribute name="PART-NUMBER" value=" 750811611 "/>
<attribute name="VALUE" value=" 750811611 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811612" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811612"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811612?ae"/>
<attribute name="F-SWTICH" value="68 - 110kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1.3A"/>
<attribute name="IOUT2" value="1.3A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="5.26:0.26:0.26:1"/>
<attribute name="PART-NUMBER" value=" 750811612 "/>
<attribute name="VALUE" value=" 750811612 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811617" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811617"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811617?ae"/>
<attribute name="F-SWTICH" value="68 - 170kHz"/>
<attribute name="HEIGHT" value="14.81mm"/>
<attribute name="IOUT1" value="1.1A"/>
<attribute name="IOUT2" value="0.6A"/>
<attribute name="ISAT1" value="2A"/>
<attribute name="L1" value="793µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="20:4.5:1:2.75:1.25"/>
<attribute name="PART-NUMBER" value=" 750811617 "/>
<attribute name="VALUE" value=" 750811617 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="24V"/>
<attribute name="VT" value="4506 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112515" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112515"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112515?ae"/>
<attribute name="F-SWTICH" value="68 - 105kHz"/>
<attribute name="HEIGHT" value="14.81mm"/>
<attribute name="IOUT1" value="0.8A"/>
<attribute name="ISAT1" value="1.9A"/>
<attribute name="L1" value="500µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16.66:6.33:2.33:1"/>
<attribute name="PART-NUMBER" value=" 7508112515 "/>
<attribute name="VALUE" value=" 7508112515 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="40V"/>
<attribute name="VT" value="4503 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112327" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112327"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112327?ae"/>
<attribute name="F-SWTICH" value="68 - 130kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1.3A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="20:2.4:2.2:1"/>
<attribute name="PART-NUMBER" value=" 7508112327 "/>
<attribute name="VALUE" value=" 7508112327 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="16V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112510" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125��C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112510"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112510?ae"/>
<attribute name="F-SWTICH" value="68 - 120kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="0.75A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="20:4.8:2.2:1"/>
<attribute name="PART-NUMBER" value=" 7508112510 "/>
<attribute name="VALUE" value=" 7508112510 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="32V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811644" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811644"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811644?ae"/>
<attribute name="F-SWTICH" value="68 - 140kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="0.4A"/>
<attribute name="IOUT2" value="0.4A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="11.11:1.88:1"/>
<attribute name="PART-NUMBER" value=" 750811644 "/>
<attribute name="VALUE" value=" 750811644 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="24V"/>
<attribute name="VOUT2" value="24V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112511" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112511"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_SMT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112511?ae"/>
<attribute name="F-SWTICH" value="68 - 120kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="0.6A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="N" value="20:6:2.2:1"/>
<attribute name="PART-NUMBER" value=" 7508112511 "/>
<attribute name="VALUE" value=" 7508112511 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="40V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="33.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811512" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811512"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811512?ae"/>
<attribute name="F-SWTICH" value="68 - 120kHz"/>
<attribute name="HEIGHT" value="14mm"/>
<attribute name="IOUT1" value="1.575A"/>
<attribute name="IOUT2" value="1.575A"/>
<attribute name="ISAT1" value="2A"/>
<attribute name="L1" value="770µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="20:1:1:2.75:1.25"/>
<attribute name="PART-NUMBER" value=" 750811512 "/>
<attribute name="VALUE" value=" 750811512 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="4504 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811616" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811616"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811616?ae"/>
<attribute name="F-SWTICH" value="68 - 170kHz"/>
<attribute name="HEIGHT" value="14.81mm"/>
<attribute name="IOUT1" value="1.7A"/>
<attribute name="IOUT2" value="2A"/>
<attribute name="ISAT1" value="2.5A"/>
<attribute name="L1" value="468µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="20:1:2.33:2.66:1.33"/>
<attribute name="PART-NUMBER" value=" 750811616 "/>
<attribute name="VALUE" value=" 750811616 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="4505 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508116313" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508116313"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508116313?ae"/>
<attribute name="F-SWTICH" value="68 - 120kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="0.85A"/>
<attribute name="IOUT2" value="0.85A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="9.09:0.27:1.18:1"/>
<attribute name="PART-NUMBER" value=" 7508116313 "/>
<attribute name="VALUE" value=" 7508116313 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811614" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811614"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811614?ae"/>
<attribute name="F-SWTICH" value="68 - 190kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1.2A"/>
<attribute name="IOUT2" value="0.62A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="8.33:1.16:1.16:1"/>
<attribute name="PART-NUMBER" value=" 750811614 "/>
<attribute name="VALUE" value=" 750811614 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="24V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112514" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112514"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD25_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="11" pad="11"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112514?ae"/>
<attribute name="F-SWTICH" value="68 - 115kHz"/>
<attribute name="HEIGHT" value="14.81mm"/>
<attribute name="IOUT1" value="1A"/>
<attribute name="ISAT1" value="1.9A"/>
<attribute name="L1" value="460µH"/>
<attribute name="LENGTH" value="26.3mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16:4.66:2:1"/>
<attribute name="PART-NUMBER" value=" 7508112514 "/>
<attribute name="VALUE" value=" 7508112514 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VAUX1" value="6V"/>
<attribute name="VAUX2" value="14V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="32V"/>
<attribute name="VT" value="4502 V (AC)"/>
<attribute name="WIDTH" value="33mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112330" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112330"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112330?ae"/>
<attribute name="F-SWTICH" value="68 - 120kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1.15A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="8.333:1:1.25"/>
<attribute name="PART-NUMBER" value=" 7508112330 "/>
<attribute name="VALUE" value=" 7508112330 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="16V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811613" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="750811613"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811613?ae"/>
<attribute name="F-SWTICH" value="68 - 160kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="1.8A"/>
<attribute name="IOUT2" value="0.9A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="6.66:0.6:0.6:1"/>
<attribute name="PART-NUMBER" value=" 750811613 "/>
<attribute name="VALUE" value=" 750811613 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VOUT2" value="12V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112512" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112512"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112512?ae"/>
<attribute name="F-SWTICH" value="68 - 170kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="0.75A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="11.11:1.55:1"/>
<attribute name="PART-NUMBER" value=" 7508112512 "/>
<attribute name="VALUE" value=" 7508112512 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="32V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508112513" prefix="T">
<description>&lt;b&gt;WE-OLEFD EFD-Style Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal input voltage
&lt;br&gt; Switching frequency: 68kHz to 170kHz
&lt;br&gt; Low Profile
&lt;br&gt; Isolation voltage: 4500VAC at 1 second
&lt;br&gt; Operating temp: -40°C to +125°C
&lt;br&gt; Designed for IEC61558-2 Reinforced 400VDC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;LED lighting
&lt;br&gt; Offline switching power
&lt;br&gt; Power electronics
&lt;br&gt; Electronics ballasts
&lt;br&gt; White goods
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o32905v209%20Family_MID-OLEFD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-OLEFD"&gt;www.we-online.com/en/components/products/WE-OLEFD&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2023-04-11&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="7508112513"/>
</gates>
<devices>
<device name="" package="WE-OLEFD_EFD20_THT">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508112513?ae"/>
<attribute name="F-SWTICH" value="68 - 170kHz"/>
<attribute name="HEIGHT" value="12mm"/>
<attribute name="IOUT1" value="0.58A"/>
<attribute name="ISAT1" value="1.4A"/>
<attribute name="L1" value="800µH"/>
<attribute name="LENGTH" value="21.5mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="6.66:0.8:1"/>
<attribute name="PART-NUMBER" value=" 7508112513 "/>
<attribute name="VALUE" value=" 7508112513 "/>
<attribute name="VAUX" value="20V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="40V"/>
<attribute name="VT" value="4500 V (AC)"/>
<attribute name="WIDTH" value="29mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
