<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Transformers For AC/DC Converter - WE-OLPI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-07-03&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-OLPI_EE16/8/5_L20.32W24.38H16">
<description>&lt;b&gt;MID-OLPI Offline Flyback Transformers for Power Integrations
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/8/5,THT,9pins
&lt;br&gt;LXWXH=20.32X24.38X16mm</description>
</package>
<package name="WE-OLPI_ER28/14_L31W31H25">
<description>&lt;b&gt;MID-OLPI Offline Flyback Transformers for Power Integrations
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: ER28/14,THT,12pins
&lt;br&gt;LXWXH=31X31X25mm</description>
</package>
<package name="WE-OLPI_EE16/7/5_L16.9W18.8H13.97">
<description>&lt;b&gt;MID-OLTI Offline Flyback Transformers for Texas Instruments
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/7/5,THT,10pins
&lt;br&gt;LXWXH=16.9X18.8X13.97mm</description>
</package>
<package name="WE-OLPI_EE20/10/6_L21W25H16">
<description>&lt;b&gt;MID-OLPI Offline Flyback Transformers for Power Integrations
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size:EE20/10/6,THT,14pins
&lt;br&gt;LXWXH=21X25X16mm</description>
</package>
<package name="WE-OLPI_EE16/7/5_L16.9W18.8H13">
<description>&lt;b&gt;MID-OLPI Offline Flyback Transformers for Power Integrations
&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Size: EE16/7/5,THT,8pins
&lt;br&gt;LXWXH=16.9X18.8X13mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-OLPI_EE16/8/5_7508110100">
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="WE-OLPI_EE16/8/5_4W:1W_CENTERTAP">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-OLPI_ER28/14_3W:2W_CENTERTAP">
<pin name="5" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="11+12" direction="pas"/>
<pin name="9+10" direction="pas"/>
</symbol>
<symbol name="WE-OLPI_EE16/8/5_750811019">
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="WE-OLPI_EE16/8/5_750811023">
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="WE-OLPI_EE16/7/5_750811016">
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-OLPI_EE16/7/5_750871032">
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="10" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
<symbol name="WE-OLPI_EE20/10/6_4W:1W_CENTERTAP">
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="12" direction="pas"/>
<pin name="9" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="7508110101" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE16/8/5_4W:1W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508110101?ae"/>
<attribute name="FSWITCH" value="65kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1000A"/>
<attribute name="ISAT" value="700V"/>
<attribute name="L" value="1.07uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="15:1:0.86:0.86"/>
<attribute name="PART-NUMBER" value=" 7508110101 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 7508110101 "/>
<attribute name="VAUX" value="8.6V"/>
<attribute name="VAUX1" value="4.3A"/>
<attribute name="VAUX2" value="4.3V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508110102" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE16/8/5_4W:1W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508110102?ae"/>
<attribute name="FSWITCH" value="65kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="555A"/>
<attribute name="ISAT" value="330V"/>
<attribute name="L" value="2.58uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="18.3:1:0.86:0.86"/>
<attribute name="PART-NUMBER" value=" 7508110102 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 7508110102 "/>
<attribute name="VAUX" value="8.6V"/>
<attribute name="VAUX1" value="4.3A"/>
<attribute name="VAUX2" value="4.3V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811630" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_ER28/14_3W:2W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-OLPI_ER28/14_L31W31H25">
<connects>
<connect gate="G$1" pin="11+12" pad="11 12"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="9+10" pad="9 10"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811630?ae"/>
<attribute name="FSWITCH" value="66kHz"/>
<attribute name="HEIGHT" value="25mm"/>
<attribute name="IOUT1" value="2000A"/>
<attribute name="IOUT2" value="2.2A"/>
<attribute name="ISAT" value="2200V"/>
<attribute name="L" value="1.04uH"/>
<attribute name="LENGTH" value="31mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="23.33 : 1.33 : 1 : 2.33"/>
<attribute name="PART-NUMBER" value=" 750811630 "/>
<attribute name="SIZE" value="ER28/14"/>
<attribute name="VALUE" value=" 750811630 "/>
<attribute name="VAUX" value="11.65V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VOUT2" value="5V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="31mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="7508110100" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE16/8/5_7508110100"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7508110100?ae"/>
<attribute name="FSWITCH" value="132kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="322A"/>
<attribute name="ISAT" value="350V"/>
<attribute name="L" value="2.64uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="11.07:1"/>
<attribute name="PART-NUMBER" value=" 7508110100 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 7508110100 "/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="6.2V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811023" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE16/8/5_750811023"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811023?ae"/>
<attribute name="FSWITCH" value="66kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="300A"/>
<attribute name="ISAT" value="300V"/>
<attribute name="L" value="2.28uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="10.8:1:0.9"/>
<attribute name="PART-NUMBER" value=" 750811023 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 750811023 "/>
<attribute name="VAUX" value="7.2V"/>
<attribute name="VAUX2" value="`"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="8V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750871032" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE16/7/5_750871032"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE16/7/5_L16.9W18.8H13.97">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="10" pad="10"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750871032?ae"/>
<attribute name="FSWITCH" value="66kHz"/>
<attribute name="HEIGHT" value="13.97mm"/>
<attribute name="IOUT1" value="350A"/>
<attribute name="L" value="1.55uH"/>
<attribute name="LENGTH" value="16.9mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="7.14 : 1 : 1.08"/>
<attribute name="PART-NUMBER" value=" 750871032 "/>
<attribute name="SIZE" value="EE16/7/5"/>
<attribute name="VALUE" value=" 750871032 "/>
<attribute name="VAUX" value="12.96V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="3000V(AC)"/>
<attribute name="WIDTH" value="18.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750310849" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE20/10/6_4W:1W_CENTERTAP"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE20/10/6_L21W25H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="12" pad="12"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750310849?ae"/>
<attribute name="FSWITCH" value="132kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="1000A"/>
<attribute name="ISAT" value="900V"/>
<attribute name="L" value="0.9uH"/>
<attribute name="LENGTH" value="21mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="8 : 1 : 2"/>
<attribute name="PART-NUMBER" value=" 750310849 "/>
<attribute name="SIZE" value="EE20/10/6"/>
<attribute name="VALUE" value=" 750310849 "/>
<attribute name="VAUX" value="22V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="12V"/>
<attribute name="VT" value="5000V(AC)"/>
<attribute name="WIDTH" value="25mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811019" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE16/8/5_750811019"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE16/8/5_L20.32W24.38H16">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="7" pad="7"/>
<connect gate="G$1" pin="8" pad="8"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811019?ae"/>
<attribute name="FSWITCH" value="132kHz"/>
<attribute name="HEIGHT" value="16mm"/>
<attribute name="IOUT1" value="330A"/>
<attribute name="ISAT" value="250V"/>
<attribute name="L" value="2.7uH"/>
<attribute name="LENGTH" value="20.32mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="13.5:1:3.13"/>
<attribute name="PART-NUMBER" value=" 750811019 "/>
<attribute name="SIZE" value="EE16/8/5"/>
<attribute name="VALUE" value=" 750811019 "/>
<attribute name="VAUX" value="18.78V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="6V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="24.38mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="750811016" prefix="T">
<description>&lt;b&gt;WE-OLPI Offline Flyback Transformers
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt;Universal offline input voltage
&lt;br&gt; Output power from 2 to 35 W
&lt;br&gt; Operating temperature: –40 °C to +125 °C
&lt;br&gt; Isolation voltage: up to 5000VAC

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Offline-switch mode power supplies
&lt;br&gt; Especially designed for several ICs from Power Integrations

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o801423v209%20FAMILY-MID-OLPI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-OLPI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-OLPI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-07-03&lt;br&gt;
2024 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-OLPI_EE16/7/5_750811016"/>
</gates>
<devices>
<device name="" package="WE-OLPI_EE16/7/5_L16.9W18.8H13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
<connect gate="G$1" pin="9" pad="9"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/750811016?ae"/>
<attribute name="FSWITCH" value="100kHz"/>
<attribute name="HEIGHT" value="13mm"/>
<attribute name="IOUT1" value="1200A"/>
<attribute name="ISAT" value="450V"/>
<attribute name="L" value="1.67uH"/>
<attribute name="LENGTH" value="16.9mm"/>
<attribute name="MOUNT" value="THT"/>
<attribute name="N" value="16.42 : 1 : 2.71"/>
<attribute name="PART-NUMBER" value=" 750811016 "/>
<attribute name="SIZE" value="EE16/7/5"/>
<attribute name="VALUE" value=" 750811016 "/>
<attribute name="VAUX" value="13.5V"/>
<attribute name="VIN" value="85 - 265 V (AC)"/>
<attribute name="VOUT1" value="5V"/>
<attribute name="VT" value="4500V(AC)"/>
<attribute name="WIDTH" value="18.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
