<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-PD&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-02-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PD_7332R">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7332R, SMT, 2pins
&lt;br&gt;LxWxH=7.3x7.3x3.2mm</description>
</package>
<package name="WE-PD_1245">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1245, SMT, 2pins
&lt;br&gt;LxWxH=12x12x4.5mm</description>
</package>
<package name="WE-PD_1510">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1510, SMT, 2pins
&lt;br&gt;LxWxH=15x15x10mm</description>
</package>
<package name="WE-PD_1280">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1280, SMT, 2pins
&lt;br&gt;LxWxH=12x12x8mm</description>
</package>
<package name="WE-PD_6050R">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 6050R, SMT, 2pins
&lt;br&gt;LxWxH=5.9x6.2x5mm</description>
</package>
<package name="WE-PD_7332">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7332, SMT, 2pins
&lt;br&gt;LxWxH=7.3x7.3x3.2mm</description>
</package>
<package name="WE-PD_7345P">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7345P, SMT, 2pins
&lt;br&gt;LxWxH=7.3x7.3x4.5mm</description>
</package>
<package name="WE-PD_7332P">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7332P, SMT, 2pins
&lt;br&gt;LxWxH=7.3x7.3x3.2mm</description>
</package>
<package name="WE-PD_1260P">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1260P, SMT, 2pins
&lt;br&gt;LxWxH=12x12x6mm</description>
</package>
<package name="WE-PD_7345R">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7345R, SMT, 2pins
&lt;br&gt;LxWxH=7.3x7.3x4.5mm</description>
</package>
<package name="WE-PD_1260">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1260, SMT, 2pins
&lt;br&gt;LxWxH=12x12x6mm</description>
</package>
<package name="WE-PD_1030P">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1030P, SMT, 2pins
&lt;br&gt;LxWxH=10x10x3mm</description>
</package>
<package name="WE-PD_7345">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 7345, SMT, 2pins
&lt;br&gt;LxWxH=7.3x7.3x4.5mm</description>
</package>
<package name="WE-PD_6033R">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 6033R, SMT, 2pins
&lt;br&gt;LxWxH=5.9x6.2x3.3mm</description>
</package>
<package name="WE-PD_1050P">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1050P, SMT, 2pins
&lt;br&gt;LxWxH=10x10x5mm</description>
</package>
<package name="WE-PD_1280P">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1280P, SMT, 2pins
&lt;br&gt;LxWxH=12x12x8mm</description>
</package>
<package name="WE-PD_1210">
<description>&lt;b&gt; WE-PD SMD Power Inductor&lt;br&gt;&lt;/b&gt;

&lt;br&gt;Size: 1210, SMT, 2pins
&lt;br&gt;LxWxH=12x12x10mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PD_7332R" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_7332R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447789001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789001?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="5.37A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789001 "/>
<attribute name="RDC-MAX" value="12mohm"/>
<attribute name="RDC-TYP" value="10mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789002?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="4.02A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789002 "/>
<attribute name="RDC-MAX" value="25mohm"/>
<attribute name="RDC-TYP" value="20mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789003?ae"/>
<attribute name="FRES" value="61MHz"/>
<attribute name="IR" value="3.42A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789003 "/>
<attribute name="RDC-MAX" value="30mohm"/>
<attribute name="RDC-TYP" value="24mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789004?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789004 "/>
<attribute name="RDC-MAX" value="39mohm"/>
<attribute name="RDC-TYP" value="33mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789006?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789006 "/>
<attribute name="RDC-MAX" value="50mohm"/>
<attribute name="RDC-TYP" value="42mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744778910">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778910?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="1.83A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778910 "/>
<attribute name="RDC-MAX" value="72mohm"/>
<attribute name="RDC-TYP" value="64mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789112?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="1.73A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789112 "/>
<attribute name="RDC-MAX" value="98mohm"/>
<attribute name="RDC-TYP" value="76mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789115?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="1.51A"/>
<attribute name="ISAT" value="1.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789115 "/>
<attribute name="RDC-MAX" value="130mohm"/>
<attribute name="RDC-TYP" value="100mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789118?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="1.41A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789118 "/>
<attribute name="RDC-MAX" value="140mohm"/>
<attribute name="RDC-TYP" value="114mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789122?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.38A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789122 "/>
<attribute name="RDC-MAX" value="190mohm"/>
<attribute name="RDC-TYP" value="119mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789127?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="1.27A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789127 "/>
<attribute name="RDC-MAX" value="210mohm"/>
<attribute name="RDC-TYP" value="130mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789133?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="1.22A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789133 "/>
<attribute name="RDC-MAX" value="240mohm"/>
<attribute name="RDC-TYP" value="153mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789139?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="1.03A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789139 "/>
<attribute name="RDC-MAX" value="320mohm"/>
<attribute name="RDC-TYP" value="209mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="39uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789147?ae"/>
<attribute name="FRES" value="13.5MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789147 "/>
<attribute name="RDC-MAX" value="360mohm"/>
<attribute name="RDC-TYP" value="315mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789156?ae"/>
<attribute name="FRES" value="12.5MHz"/>
<attribute name="IR" value="0.84A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789156 "/>
<attribute name="RDC-MAX" value="470mohm"/>
<attribute name="RDC-TYP" value="335mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="56uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789168?ae"/>
<attribute name="FRES" value="11.5MHz"/>
<attribute name="IR" value="0.74A"/>
<attribute name="ISAT" value="0.84A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789168 "/>
<attribute name="RDC-MAX" value="520mohm"/>
<attribute name="RDC-TYP" value="420mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789182?ae"/>
<attribute name="FRES" value="9.8MHz"/>
<attribute name="IR" value="0.69A"/>
<attribute name="ISAT" value="0.78A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789182 "/>
<attribute name="RDC-MAX" value="690mohm"/>
<attribute name="RDC-TYP" value="470mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744778920">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778920?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="0.62A"/>
<attribute name="ISAT" value="0.76A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778920 "/>
<attribute name="RDC-MAX" value="790mohm"/>
<attribute name="RDC-TYP" value="585mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789212?ae"/>
<attribute name="FRES" value="8.5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789212 "/>
<attribute name="RDC-MAX" value="890mohm"/>
<attribute name="RDC-TYP" value="563mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789215?ae"/>
<attribute name="FRES" value="7.2MHz"/>
<attribute name="IR" value="0.56A"/>
<attribute name="ISAT" value="0.53A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789215 "/>
<attribute name="RDC-MAX" value="1270mohm"/>
<attribute name="RDC-TYP" value="720mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789218?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.49A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789218 "/>
<attribute name="RDC-MAX" value="1450mohm"/>
<attribute name="RDC-TYP" value="960mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789222?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.42A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789222 "/>
<attribute name="RDC-MAX" value="1650mohm"/>
<attribute name="RDC-TYP" value="1350mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789233?ae"/>
<attribute name="FRES" value="4.8MHz"/>
<attribute name="IR" value="0.32A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789233 "/>
<attribute name="RDC-MAX" value="2620mohm"/>
<attribute name="RDC-TYP" value="2280mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789239?ae"/>
<attribute name="FRES" value="4.4MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.34A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789239 "/>
<attribute name="RDC-MAX" value="2940mohm"/>
<attribute name="RDC-TYP" value="2490mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="390uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744778924">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778924?ae"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.31A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778924 "/>
<attribute name="RDC-MAX" value="4180mohm"/>
<attribute name="RDC-TYP" value="2600mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744778925">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778925?ae"/>
<attribute name="FRES" value="3.7MHz"/>
<attribute name="IR" value="0.27A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778925 "/>
<attribute name="RDC-MAX" value="4670mohm"/>
<attribute name="RDC-TYP" value="3000mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="560uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744778926">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778926?ae"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.22A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778926 "/>
<attribute name="RDC-MAX" value="5730mohm"/>
<attribute name="RDC-TYP" value="4500mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447789270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447789270?ae"/>
<attribute name="FRES" value="5.2MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.39A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447789270 "/>
<attribute name="RDC-MAX" value="2310mohm"/>
<attribute name="RDC-TYP" value="1470mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="270uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744778928">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778928?ae"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="0.21A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778928 "/>
<attribute name="RDC-MAX" value="6540mohm"/>
<attribute name="RDC-TYP" value="4990mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744778930">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778930?ae"/>
<attribute name="FRES" value="2.6MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778930 "/>
<attribute name="RDC-MAX" value="9440mohm"/>
<attribute name="RDC-TYP" value="5570mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1245" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1245">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447715001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715001?ae"/>
<attribute name="FRES" value="76MHz"/>
<attribute name="IR" value="7.6A"/>
<attribute name="ISAT" value="10.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715001 "/>
<attribute name="RDC-MAX" value="9.5mohm"/>
<attribute name="RDC-TYP" value="7.5mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="1.8uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715002?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715002 "/>
<attribute name="RDC-MAX" value="11mohm"/>
<attribute name="RDC-TYP" value="8.5mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="2.5uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715003?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="5.9A"/>
<attribute name="ISAT" value="7.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715003 "/>
<attribute name="RDC-MAX" value="13mohm"/>
<attribute name="RDC-TYP" value="11.5mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715004?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715004 "/>
<attribute name="RDC-MAX" value="16mohm"/>
<attribute name="RDC-TYP" value="13.5mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715006?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715006 "/>
<attribute name="RDC-MAX" value="25mohm"/>
<attribute name="RDC-TYP" value="20mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715100?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715100 "/>
<attribute name="RDC-MAX" value="30mohm"/>
<attribute name="RDC-TYP" value="25mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715101?ae"/>
<attribute name="FRES" value="6.9MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715101 "/>
<attribute name="RDC-MAX" value="270mohm"/>
<attribute name="RDC-TYP" value="250mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715120?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715120 "/>
<attribute name="RDC-MAX" value="38mohm"/>
<attribute name="RDC-TYP" value="30mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715180?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715180 "/>
<attribute name="RDC-MAX" value="51mohm"/>
<attribute name="RDC-TYP" value="37mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715220?ae"/>
<attribute name="FRES" value="15.5MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715220 "/>
<attribute name="RDC-MAX" value="65mohm"/>
<attribute name="RDC-TYP" value="45mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715221?ae"/>
<attribute name="FRES" value="4.7MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715221 "/>
<attribute name="RDC-MAX" value="480mohm"/>
<attribute name="RDC-TYP" value="460mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715330?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715330 "/>
<attribute name="RDC-MAX" value="85mohm"/>
<attribute name="RDC-TYP" value="75mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715470?ae"/>
<attribute name="FRES" value="9.7MHz"/>
<attribute name="IR" value="1.95A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715470 "/>
<attribute name="RDC-MAX" value="125mohm"/>
<attribute name="RDC-TYP" value="105mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715906">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715906?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715906 "/>
<attribute name="RDC-MAX" value="5.5mohm"/>
<attribute name="RDC-TYP" value="4.5mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="0.6uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447715910">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447715910?ae"/>
<attribute name="FRES" value="98MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="13.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447715910 "/>
<attribute name="RDC-MAX" value="7mohm"/>
<attribute name="RDC-TYP" value="5.5mohm"/>
<attribute name="SIZE" value=" 1245 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1280" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1280">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74477001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477001?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="13.5A"/>
<attribute name="ISAT" value="21A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477001 "/>
<attribute name="RDC-MAX" value="7mohm"/>
<attribute name="RDC-TYP" value="4.6mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="1.2uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770015?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="16.5A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770015 "/>
<attribute name="RDC-MAX" value="5mohm"/>
<attribute name="RDC-TYP" value="3.2mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477002?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477002 "/>
<attribute name="RDC-MAX" value="9mohm"/>
<attribute name="RDC-TYP" value="6.3mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="2.4uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477003?ae"/>
<attribute name="FRES" value="37.5MHz"/>
<attribute name="IR" value="10.2A"/>
<attribute name="ISAT" value="12.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477003 "/>
<attribute name="RDC-MAX" value="11mohm"/>
<attribute name="RDC-TYP" value="8mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="3.5uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477004?ae"/>
<attribute name="FRES" value="31.2MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477004 "/>
<attribute name="RDC-MAX" value="12mohm"/>
<attribute name="RDC-TYP" value="9mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477005?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="8.7A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477005 "/>
<attribute name="RDC-MAX" value="13.5mohm"/>
<attribute name="RDC-TYP" value="10.5mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477006?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477006 "/>
<attribute name="RDC-MAX" value="14mohm"/>
<attribute name="RDC-TYP" value="11mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="6.1uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477007?ae"/>
<attribute name="FRES" value="21.3MHz"/>
<attribute name="IR" value="8.4A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477007 "/>
<attribute name="RDC-MAX" value="15mohm"/>
<attribute name="RDC-TYP" value="11.5mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="7.6uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477008?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="17A"/>
<attribute name="ISAT" value="27A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477008 "/>
<attribute name="RDC-MAX" value="5mohm"/>
<attribute name="RDC-TYP" value="3.2mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="0.75uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477009?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="23.5A"/>
<attribute name="ISAT" value="34A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477009 "/>
<attribute name="RDC-MAX" value="3mohm"/>
<attribute name="RDC-TYP" value="1.7mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477010?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477010 "/>
<attribute name="RDC-MAX" value="20mohm"/>
<attribute name="RDC-TYP" value="15mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770112?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770112 "/>
<attribute name="RDC-MAX" value="21mohm"/>
<attribute name="RDC-TYP" value="16mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770115?ae"/>
<attribute name="FRES" value="14.5MHz"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770115 "/>
<attribute name="RDC-MAX" value="23mohm"/>
<attribute name="RDC-TYP" value="18mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770118?ae"/>
<attribute name="FRES" value="13.2MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770118 "/>
<attribute name="RDC-MAX" value="32mohm"/>
<attribute name="RDC-TYP" value="25mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770122?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770122 "/>
<attribute name="RDC-MAX" value="35mohm"/>
<attribute name="RDC-TYP" value="29mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770127?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="4.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770127 "/>
<attribute name="RDC-MAX" value="38mohm"/>
<attribute name="RDC-TYP" value="31mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770133?ae"/>
<attribute name="FRES" value="8.5MHz"/>
<attribute name="IR" value="3.6A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770133 "/>
<attribute name="RDC-MAX" value="53mohm"/>
<attribute name="RDC-TYP" value="44mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770139?ae"/>
<attribute name="FRES" value="8.2MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770139 "/>
<attribute name="RDC-MAX" value="56mohm"/>
<attribute name="RDC-TYP" value="47mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="39uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770147?ae"/>
<attribute name="FRES" value="7.9MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770147 "/>
<attribute name="RDC-MAX" value="64mohm"/>
<attribute name="RDC-TYP" value="53mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770156?ae"/>
<attribute name="FRES" value="7.1MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770156 "/>
<attribute name="RDC-MAX" value="71mohm"/>
<attribute name="RDC-TYP" value="59mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="56uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770168?ae"/>
<attribute name="FRES" value="6.4MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770168 "/>
<attribute name="RDC-MAX" value="90mohm"/>
<attribute name="RDC-TYP" value="76mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770182?ae"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770182 "/>
<attribute name="RDC-MAX" value="105mohm"/>
<attribute name="RDC-TYP" value="86mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477020">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477020?ae"/>
<attribute name="FRES" value="5.2MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477020 "/>
<attribute name="RDC-MAX" value="140mohm"/>
<attribute name="RDC-TYP" value="117mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770215?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770215 "/>
<attribute name="RDC-MAX" value="175mohm"/>
<attribute name="RDC-TYP" value="145mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770218?ae"/>
<attribute name="FRES" value="4.2MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770218 "/>
<attribute name="RDC-MAX" value="220mohm"/>
<attribute name="RDC-TYP" value="182mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770222?ae"/>
<attribute name="FRES" value="3.8MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770222 "/>
<attribute name="RDC-MAX" value="275mohm"/>
<attribute name="RDC-TYP" value="230mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770233?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770233 "/>
<attribute name="RDC-MAX" value="410mohm"/>
<attribute name="RDC-TYP" value="345mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770247?ae"/>
<attribute name="FRES" value="2.6MHz"/>
<attribute name="IR" value="0.98A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770247 "/>
<attribute name="RDC-MAX" value="540mohm"/>
<attribute name="RDC-TYP" value="450mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770256">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770256?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="0.87A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770256 "/>
<attribute name="RDC-MAX" value="680mohm"/>
<attribute name="RDC-TYP" value="570mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="560uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770268?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770268 "/>
<attribute name="RDC-MAX" value="930mohm"/>
<attribute name="RDC-TYP" value="780mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744770282">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744770282?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744770282 "/>
<attribute name="RDC-MAX" value="1050mohm"/>
<attribute name="RDC-TYP" value="870mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477030?ae"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="IR" value="0.65A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477030 "/>
<attribute name="RDC-MAX" value="1180mohm"/>
<attribute name="RDC-TYP" value="980mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1510" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1510">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447704150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447704150?ae"/>
<attribute name="FRES" value="20.5MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="8.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447704150 "/>
<attribute name="RDC-MAX" value="26mohm"/>
<attribute name="RDC-TYP" value="19.5mohm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447704220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447704220?ae"/>
<attribute name="FRES" value="11.5MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="7.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447704220 "/>
<attribute name="RDC-MAX" value="33mohm"/>
<attribute name="RDC-TYP" value="25mohm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447704471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447704471?ae"/>
<attribute name="FRES" value="1.7MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447704471 "/>
<attribute name="RDC-MAX" value="500mohm"/>
<attribute name="RDC-TYP" value="425mohm"/>
<attribute name="SIZE" value=" 1510 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_6050R" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_6050R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447786001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447786001?ae"/>
<attribute name="FRES" value="180MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447786001 "/>
<attribute name="RDC-MAX" value="34mohm"/>
<attribute name="RDC-TYP" value="28mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447786002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447786002?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447786002 "/>
<attribute name="RDC-MAX" value="49mohm"/>
<attribute name="RDC-TYP" value="40mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447786004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447786004?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447786004 "/>
<attribute name="RDC-MAX" value="65mohm"/>
<attribute name="RDC-TYP" value="57mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447786006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447786006?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447786006 "/>
<attribute name="RDC-MAX" value="75mohm"/>
<attribute name="RDC-TYP" value="62mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447786008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447786008?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447786008 "/>
<attribute name="RDC-MAX" value="80mohm"/>
<attribute name="RDC-TYP" value="66mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_744778610">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778610?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778610 "/>
<attribute name="RDC-MAX" value="88mohm"/>
<attribute name="RDC-TYP" value="74mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447786122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447786122?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447786122 "/>
<attribute name="RDC-MAX" value="115mohm"/>
<attribute name="RDC-TYP" value="98mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447786147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447786147?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447786147 "/>
<attribute name="RDC-MAX" value="295mohm"/>
<attribute name="RDC-TYP" value="260mohm"/>
<attribute name="SIZE" value=" 6050 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7332" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_7332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744778001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778001?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="5.37A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778001 "/>
<attribute name="RDC-MAX" value="12mohm"/>
<attribute name="RDC-TYP" value="9mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778002?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="4.02A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778002 "/>
<attribute name="RDC-MAX" value="20mohm"/>
<attribute name="RDC-TYP" value="14mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778003?ae"/>
<attribute name="FRES" value="61MHz"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="4.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778003 "/>
<attribute name="RDC-MAX" value="32mohm"/>
<attribute name="RDC-TYP" value="24mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778004?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="2.32A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778004 "/>
<attribute name="RDC-MAX" value="60mohm"/>
<attribute name="RDC-TYP" value="42mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778005?ae"/>
<attribute name="FRES" value="155MHz"/>
<attribute name="IR" value="5.6A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778005 "/>
<attribute name="RDC-MAX" value="8.5mohm"/>
<attribute name="RDC-TYP" value="7.2mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="0.54uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_74477810">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477810?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="1.83A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477810 "/>
<attribute name="RDC-MAX" value="72mohm"/>
<attribute name="RDC-TYP" value="68mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778112?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="1.73A"/>
<attribute name="ISAT" value="2.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778112 "/>
<attribute name="RDC-MAX" value="98mohm"/>
<attribute name="RDC-TYP" value="76mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778115?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="1.51A"/>
<attribute name="ISAT" value="1.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778115 "/>
<attribute name="RDC-MAX" value="130mohm"/>
<attribute name="RDC-TYP" value="100mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778118?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="1.41A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778118 "/>
<attribute name="RDC-MAX" value="140mohm"/>
<attribute name="RDC-TYP" value="114mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778122?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.38A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778122 "/>
<attribute name="RDC-MAX" value="190mohm"/>
<attribute name="RDC-TYP" value="119mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778127?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="1.27A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778127 "/>
<attribute name="RDC-MAX" value="240mohm"/>
<attribute name="RDC-TYP" value="140mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778133?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="1.22A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778133 "/>
<attribute name="RDC-MAX" value="240mohm"/>
<attribute name="RDC-TYP" value="153mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778139?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="1.03A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778139 "/>
<attribute name="RDC-MAX" value="320mohm"/>
<attribute name="RDC-TYP" value="214mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="39uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778147?ae"/>
<attribute name="FRES" value="13.5MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778147 "/>
<attribute name="RDC-MAX" value="360mohm"/>
<attribute name="RDC-TYP" value="315mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778156?ae"/>
<attribute name="FRES" value="12.5MHz"/>
<attribute name="IR" value="0.84A"/>
<attribute name="ISAT" value="0.88A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778156 "/>
<attribute name="RDC-MAX" value="470mohm"/>
<attribute name="RDC-TYP" value="322mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="56uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778168?ae"/>
<attribute name="FRES" value="11.5MHz"/>
<attribute name="IR" value="0.74A"/>
<attribute name="ISAT" value="0.84A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778168 "/>
<attribute name="RDC-MAX" value="520mohm"/>
<attribute name="RDC-TYP" value="420mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778182?ae"/>
<attribute name="FRES" value="9.8MHz"/>
<attribute name="IR" value="0.69A"/>
<attribute name="ISAT" value="0.78A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778182 "/>
<attribute name="RDC-MAX" value="690mohm"/>
<attribute name="RDC-TYP" value="480mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_74477820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477820?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="0.62A"/>
<attribute name="ISAT" value="0.76A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477820 "/>
<attribute name="RDC-MAX" value="790mohm"/>
<attribute name="RDC-TYP" value="580mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778212?ae"/>
<attribute name="FRES" value="8.5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778212 "/>
<attribute name="RDC-MAX" value="890mohm"/>
<attribute name="RDC-TYP" value="630mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778215?ae"/>
<attribute name="FRES" value="7.2MHz"/>
<attribute name="IR" value="0.56A"/>
<attribute name="ISAT" value="0.53A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778215 "/>
<attribute name="RDC-MAX" value="1270mohm"/>
<attribute name="RDC-TYP" value="720mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778218?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.49A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778218 "/>
<attribute name="RDC-MAX" value="1450mohm"/>
<attribute name="RDC-TYP" value="960mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778222?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.42A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778222 "/>
<attribute name="RDC-MAX" value="1650mohm"/>
<attribute name="RDC-TYP" value="1220mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778233?ae"/>
<attribute name="FRES" value="4.8MHz"/>
<attribute name="IR" value="0.32A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778233 "/>
<attribute name="RDC-MAX" value="2620mohm"/>
<attribute name="RDC-TYP" value="2280mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778239?ae"/>
<attribute name="FRES" value="4.4MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.34A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778239 "/>
<attribute name="RDC-MAX" value="2940mohm"/>
<attribute name="RDC-TYP" value="2490mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="390uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_74477824">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477824?ae"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.31A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477824 "/>
<attribute name="RDC-MAX" value="4180mohm"/>
<attribute name="RDC-TYP" value="2600mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_74477825">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477825?ae"/>
<attribute name="FRES" value="3.7MHz"/>
<attribute name="IR" value="0.27A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477825 "/>
<attribute name="RDC-MAX" value="4670mohm"/>
<attribute name="RDC-TYP" value="3000mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="560uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_74477826">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477826?ae"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.22A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477826 "/>
<attribute name="RDC-MAX" value="5730mohm"/>
<attribute name="RDC-TYP" value="4500mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_744778270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778270?ae"/>
<attribute name="FRES" value="5.2MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.39A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778270 "/>
<attribute name="RDC-MAX" value="2310mohm"/>
<attribute name="RDC-TYP" value="1440mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="270uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_74477828">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477828?ae"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="0.21A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477828 "/>
<attribute name="RDC-MAX" value="6500mohm"/>
<attribute name="RDC-TYP" value="5070mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
<technology name="_74477830">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477830?ae"/>
<attribute name="FRES" value="2.6MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477830 "/>
<attribute name="RDC-MAX" value="9440mohm"/>
<attribute name="RDC-TYP" value="5570mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Standard "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1260P" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1260P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447706015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706015?ae"/>
<attribute name="FRES" value="50.5MHz"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706015 "/>
<attribute name="RDC-MAX" value="7mohm"/>
<attribute name="RDC-TYP" value="5mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706022?ae"/>
<attribute name="FRES" value="40.2MHz"/>
<attribute name="IR" value="10.2A"/>
<attribute name="ISAT" value="16.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706022 "/>
<attribute name="RDC-MAX" value="8.5mohm"/>
<attribute name="RDC-TYP" value="6.2mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706033?ae"/>
<attribute name="FRES" value="32.2MHz"/>
<attribute name="IR" value="9.2A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706033 "/>
<attribute name="RDC-MAX" value="10mohm"/>
<attribute name="RDC-TYP" value="7.5mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706047?ae"/>
<attribute name="FRES" value="27.4MHz"/>
<attribute name="IR" value="8.1A"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706047 "/>
<attribute name="RDC-MAX" value="12mohm"/>
<attribute name="RDC-TYP" value="9mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706062">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706062?ae"/>
<attribute name="FRES" value="22.5MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706062 "/>
<attribute name="RDC-MAX" value="15mohm"/>
<attribute name="RDC-TYP" value="12mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="6.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706100?ae"/>
<attribute name="FRES" value="17.6MHz"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="7.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706100 "/>
<attribute name="RDC-MAX" value="20mohm"/>
<attribute name="RDC-TYP" value="16.3mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706101?ae"/>
<attribute name="FRES" value="5.2MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706101 "/>
<attribute name="RDC-MAX" value="140mohm"/>
<attribute name="RDC-TYP" value="122mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706102?ae"/>
<attribute name="FRES" value="1.45MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706102 "/>
<attribute name="RDC-MAX" value="1250mohm"/>
<attribute name="RDC-TYP" value="1150mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706150?ae"/>
<attribute name="FRES" value="13.9MHz"/>
<attribute name="IR" value="4.7A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706150 "/>
<attribute name="RDC-MAX" value="28mohm"/>
<attribute name="RDC-TYP" value="22.9mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706151?ae"/>
<attribute name="FRES" value="4.2MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706151 "/>
<attribute name="RDC-MAX" value="200mohm"/>
<attribute name="RDC-TYP" value="175mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706220?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="3.7A"/>
<attribute name="ISAT" value="5.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706220 "/>
<attribute name="RDC-MAX" value="41mohm"/>
<attribute name="RDC-TYP" value="34.3mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706221?ae"/>
<attribute name="FRES" value="3.3MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706221 "/>
<attribute name="RDC-MAX" value="310mohm"/>
<attribute name="RDC-TYP" value="273mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706330?ae"/>
<attribute name="FRES" value="9.2MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706330 "/>
<attribute name="RDC-MAX" value="60mohm"/>
<attribute name="RDC-TYP" value="50.8mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706331?ae"/>
<attribute name="FRES" value="2.6MHz"/>
<attribute name="IR" value="1.05A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706331 "/>
<attribute name="RDC-MAX" value="450mohm"/>
<attribute name="RDC-TYP" value="395mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706470?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706470 "/>
<attribute name="RDC-MAX" value="72mohm"/>
<attribute name="RDC-TYP" value="61.2mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706471?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.86A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706471 "/>
<attribute name="RDC-MAX" value="610mohm"/>
<attribute name="RDC-TYP" value="543mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706680?ae"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706680 "/>
<attribute name="RDC-MAX" value="97mohm"/>
<attribute name="RDC-TYP" value="82mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447706681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447706681?ae"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447706681 "/>
<attribute name="RDC-MAX" value="860mohm"/>
<attribute name="RDC-TYP" value="780mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7345P" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_7345P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447773010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773010?ae"/>
<attribute name="FRES" value="98MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773010 "/>
<attribute name="RDC-MAX" value="12mohm"/>
<attribute name="RDC-TYP" value="8.4mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773022?ae"/>
<attribute name="FRES" value="61MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773022 "/>
<attribute name="RDC-MAX" value="17.5mohm"/>
<attribute name="RDC-TYP" value="12.5mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773033?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="6.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773033 "/>
<attribute name="RDC-MAX" value="21mohm"/>
<attribute name="RDC-TYP" value="15.5mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773047?ae"/>
<attribute name="FRES" value="35.5MHz"/>
<attribute name="IR" value="3.6A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773047 "/>
<attribute name="RDC-MAX" value="26mohm"/>
<attribute name="RDC-TYP" value="20mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773062">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773062?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="4.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773062 "/>
<attribute name="RDC-MAX" value="30mohm"/>
<attribute name="RDC-TYP" value="25mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="6.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773100?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773100 "/>
<attribute name="RDC-MAX" value="45mohm"/>
<attribute name="RDC-TYP" value="37.5mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773101?ae"/>
<attribute name="FRES" value="6.7MHz"/>
<attribute name="IR" value="0.97A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773101 "/>
<attribute name="RDC-MAX" value="335mohm"/>
<attribute name="RDC-TYP" value="270mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773102?ae"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773102 "/>
<attribute name="RDC-MAX" value="3300mohm"/>
<attribute name="RDC-TYP" value="2850mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773150?ae"/>
<attribute name="FRES" value="20.7MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773150 "/>
<attribute name="RDC-MAX" value="69.5mohm"/>
<attribute name="RDC-TYP" value="53mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773151?ae"/>
<attribute name="FRES" value="5.2MHz"/>
<attribute name="IR" value="0.78A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773151 "/>
<attribute name="RDC-MAX" value="515mohm"/>
<attribute name="RDC-TYP" value="410mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773220?ae"/>
<attribute name="FRES" value="16.1MHz"/>
<attribute name="IR" value="1.85A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773220 "/>
<attribute name="RDC-MAX" value="87mohm"/>
<attribute name="RDC-TYP" value="75mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773221?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="0.63A"/>
<attribute name="ISAT" value="0.81A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773221 "/>
<attribute name="RDC-MAX" value="770mohm"/>
<attribute name="RDC-TYP" value="640mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773330?ae"/>
<attribute name="FRES" value="13.5MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773330 "/>
<attribute name="RDC-MAX" value="147mohm"/>
<attribute name="RDC-TYP" value="120mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773331?ae"/>
<attribute name="FRES" value="3.6MHz"/>
<attribute name="IR" value="0.53A"/>
<attribute name="ISAT" value="0.66A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773331 "/>
<attribute name="RDC-MAX" value="1085mohm"/>
<attribute name="RDC-TYP" value="900mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773470?ae"/>
<attribute name="FRES" value="10.3MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773470 "/>
<attribute name="RDC-MAX" value="182mohm"/>
<attribute name="RDC-TYP" value="150mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773471?ae"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773471 "/>
<attribute name="RDC-MAX" value="1700mohm"/>
<attribute name="RDC-TYP" value="1360mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773680?ae"/>
<attribute name="FRES" value="8.4MHz"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="1.45A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773680 "/>
<attribute name="RDC-MAX" value="230mohm"/>
<attribute name="RDC-TYP" value="190mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447773681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447773681?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.36A"/>
<attribute name="ISAT" value="0.46A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447773681 "/>
<attribute name="RDC-MAX" value="2300mohm"/>
<attribute name="RDC-TYP" value="1950mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7332P" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_7332P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447783015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783015?ae"/>
<attribute name="FRES" value="73MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="7.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783015 "/>
<attribute name="RDC-MAX" value="15mohm"/>
<attribute name="RDC-TYP" value="12mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783022?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783022 "/>
<attribute name="RDC-MAX" value="19mohm"/>
<attribute name="RDC-TYP" value="15.5mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783033?ae"/>
<attribute name="FRES" value="51MHz"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="5.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783033 "/>
<attribute name="RDC-MAX" value="24mohm"/>
<attribute name="RDC-TYP" value="18mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783047?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783047 "/>
<attribute name="RDC-MAX" value="35mohm"/>
<attribute name="RDC-TYP" value="27mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783068?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783068 "/>
<attribute name="RDC-MAX" value="41mohm"/>
<attribute name="RDC-TYP" value="33mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783100?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783100 "/>
<attribute name="RDC-MAX" value="68mohm"/>
<attribute name="RDC-TYP" value="56mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783101?ae"/>
<attribute name="FRES" value="7.8MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783101 "/>
<attribute name="RDC-MAX" value="450mohm"/>
<attribute name="RDC-TYP" value="390mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783102?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.32A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783102 "/>
<attribute name="RDC-MAX" value="4600mohm"/>
<attribute name="RDC-TYP" value="4000mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783150?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783150 "/>
<attribute name="RDC-MAX" value="85mohm"/>
<attribute name="RDC-TYP" value="68mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783151?ae"/>
<attribute name="FRES" value="6.25MHz"/>
<attribute name="IR" value="0.63A"/>
<attribute name="ISAT" value="0.84A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783151 "/>
<attribute name="RDC-MAX" value="750mohm"/>
<attribute name="RDC-TYP" value="630mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783220?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="2.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783220 "/>
<attribute name="RDC-MAX" value="115mohm"/>
<attribute name="RDC-TYP" value="90mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783221?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.54A"/>
<attribute name="ISAT" value="0.69A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783221 "/>
<attribute name="RDC-MAX" value="1040mohm"/>
<attribute name="RDC-TYP" value="870mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783330?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="1.32A"/>
<attribute name="ISAT" value="1.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783330 "/>
<attribute name="RDC-MAX" value="165mohm"/>
<attribute name="RDC-TYP" value="138mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783331?ae"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783331 "/>
<attribute name="RDC-MAX" value="1430mohm"/>
<attribute name="RDC-TYP" value="1240mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783470?ae"/>
<attribute name="FRES" value="11.6MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.45A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783470 "/>
<attribute name="RDC-MAX" value="210mohm"/>
<attribute name="RDC-TYP" value="180mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783471?ae"/>
<attribute name="FRES" value="3.3MHz"/>
<attribute name="IR" value="0.37A"/>
<attribute name="ISAT" value="0.47A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783471 "/>
<attribute name="RDC-MAX" value="2040mohm"/>
<attribute name="RDC-TYP" value="1780mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783680?ae"/>
<attribute name="FRES" value="9.3MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783680 "/>
<attribute name="RDC-MAX" value="300mohm"/>
<attribute name="RDC-TYP" value="260mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447783681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447783681?ae"/>
<attribute name="FRES" value="2.75MHz"/>
<attribute name="IR" value="0.31A"/>
<attribute name="ISAT" value="0.39A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447783681 "/>
<attribute name="RDC-MAX" value="2900mohm"/>
<attribute name="RDC-TYP" value="2520mohm"/>
<attribute name="SIZE" value=" 7332 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7345" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744777001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777001?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="6.84A"/>
<attribute name="ISAT" value="10.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777001 "/>
<attribute name="RDC-MAX" value="10mohm"/>
<attribute name="RDC-TYP" value="8.4mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777002?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777002 "/>
<attribute name="RDC-MAX" value="20mohm"/>
<attribute name="RDC-TYP" value="13mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777003?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777003 "/>
<attribute name="RDC-MAX" value="30mohm"/>
<attribute name="RDC-TYP" value="25mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777004?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777004 "/>
<attribute name="RDC-MAX" value="40mohm"/>
<attribute name="RDC-TYP" value="25mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477710">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477710?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477710 "/>
<attribute name="RDC-MAX" value="49mohm"/>
<attribute name="RDC-TYP" value="45mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777112?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.82A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777112 "/>
<attribute name="RDC-MAX" value="58mohm"/>
<attribute name="RDC-TYP" value="54mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777115?ae"/>
<attribute name="FRES" value="19.5MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777115 "/>
<attribute name="RDC-MAX" value="81mohm"/>
<attribute name="RDC-TYP" value="70mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777118?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="2.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777118 "/>
<attribute name="RDC-MAX" value="91mohm"/>
<attribute name="RDC-TYP" value="80mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777122?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="1.41A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777122 "/>
<attribute name="RDC-MAX" value="110mohm"/>
<attribute name="RDC-TYP" value="90mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777127?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="1.24A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777127 "/>
<attribute name="RDC-MAX" value="150mohm"/>
<attribute name="RDC-TYP" value="117mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777133?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="1.13A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777133 "/>
<attribute name="RDC-MAX" value="170mohm"/>
<attribute name="RDC-TYP" value="140mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777139?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.11A"/>
<attribute name="ISAT" value="1.23A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777139 "/>
<attribute name="RDC-MAX" value="230mohm"/>
<attribute name="RDC-TYP" value="145mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="39uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777147?ae"/>
<attribute name="FRES" value="10.5MHz"/>
<attribute name="IR" value="1.03A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777147 "/>
<attribute name="RDC-MAX" value="260mohm"/>
<attribute name="RDC-TYP" value="170mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777156?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.93A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777156 "/>
<attribute name="RDC-MAX" value="350mohm"/>
<attribute name="RDC-TYP" value="210mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="56uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777168?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="0.87A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777168 "/>
<attribute name="RDC-MAX" value="380mohm"/>
<attribute name="RDC-TYP" value="240mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777182?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.84A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777182 "/>
<attribute name="RDC-MAX" value="430mohm"/>
<attribute name="RDC-TYP" value="260mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477720">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477720?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="0.79A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477720 "/>
<attribute name="RDC-MAX" value="610mohm"/>
<attribute name="RDC-TYP" value="290mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777212?ae"/>
<attribute name="FRES" value="6.7MHz"/>
<attribute name="IR" value="0.67A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777212 "/>
<attribute name="RDC-MAX" value="660mohm"/>
<attribute name="RDC-TYP" value="400mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777215?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.52A"/>
<attribute name="ISAT" value="0.63A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777215 "/>
<attribute name="RDC-MAX" value="880mohm"/>
<attribute name="RDC-TYP" value="660mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777218?ae"/>
<attribute name="FRES" value="5.3MHz"/>
<attribute name="IR" value="0.51A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777218 "/>
<attribute name="RDC-MAX" value="980mohm"/>
<attribute name="RDC-TYP" value="680mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777222?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.44A"/>
<attribute name="ISAT" value="0.54A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777222 "/>
<attribute name="RDC-MAX" value="1170mohm"/>
<attribute name="RDC-TYP" value="920mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777233?ae"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.39A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777233 "/>
<attribute name="RDC-MAX" value="1860mohm"/>
<attribute name="RDC-TYP" value="1150mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777239?ae"/>
<attribute name="FRES" value="3.8MHz"/>
<attribute name="IR" value="0.38A"/>
<attribute name="ISAT" value="0.42A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777239 "/>
<attribute name="RDC-MAX" value="2850mohm"/>
<attribute name="RDC-TYP" value="1250mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="390uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477724">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477724?ae"/>
<attribute name="FRES" value="3.2MHz"/>
<attribute name="IR" value="0.29A"/>
<attribute name="ISAT" value="0.34A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477724 "/>
<attribute name="RDC-MAX" value="3010mohm"/>
<attribute name="RDC-TYP" value="1600mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477725">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477725?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.28A"/>
<attribute name="ISAT" value="0.31A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477725 "/>
<attribute name="RDC-MAX" value="3620mohm"/>
<attribute name="RDC-TYP" value="1720mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="560uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477726">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477726?ae"/>
<attribute name="FRES" value="2.7MHz"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.28A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477726 "/>
<attribute name="RDC-MAX" value="4630mohm"/>
<attribute name="RDC-TYP" value="2600mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744777270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777270?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.48A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777270 "/>
<attribute name="RDC-MAX" value="1640mohm"/>
<attribute name="RDC-TYP" value="970mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="270uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477728">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477728?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="0.21A"/>
<attribute name="ISAT" value="0.26A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477728 "/>
<attribute name="RDC-MAX" value="5200mohm"/>
<attribute name="RDC-TYP" value="3000mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477730">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477730?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477730 "/>
<attribute name="RDC-MAX" value="6000mohm"/>
<attribute name="RDC-TYP" value="3270mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_6033R" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_6033R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447785001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785001?ae"/>
<attribute name="FRES" value="192MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785001 "/>
<attribute name="RDC-MAX" value="39mohm"/>
<attribute name="RDC-TYP" value="31mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785002?ae"/>
<attribute name="FRES" value="88MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785002 "/>
<attribute name="RDC-MAX" value="54mohm"/>
<attribute name="RDC-TYP" value="43mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785003?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785003 "/>
<attribute name="RDC-MAX" value="67mohm"/>
<attribute name="RDC-TYP" value="43mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785004?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785004 "/>
<attribute name="RDC-MAX" value="78mohm"/>
<attribute name="RDC-TYP" value="60mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785006?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785006 "/>
<attribute name="RDC-MAX" value="100mohm"/>
<attribute name="RDC-TYP" value="79mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_744778510">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778510?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778510 "/>
<attribute name="RDC-MAX" value="125mohm"/>
<attribute name="RDC-TYP" value="100mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785115?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785115 "/>
<attribute name="RDC-MAX" value="200mohm"/>
<attribute name="RDC-TYP" value="165mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785122?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785122 "/>
<attribute name="RDC-MAX" value="250mohm"/>
<attribute name="RDC-TYP" value="210mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785127?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785127 "/>
<attribute name="RDC-MAX" value="360mohm"/>
<attribute name="RDC-TYP" value="300mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785133?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785133 "/>
<attribute name="RDC-MAX" value="400mohm"/>
<attribute name="RDC-TYP" value="340mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_7447785147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447785147?ae"/>
<attribute name="FRES" value="16.5MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.74A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447785147 "/>
<attribute name="RDC-MAX" value="600mohm"/>
<attribute name="RDC-TYP" value="500mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
<technology name="_744778520">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744778520?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="0.65A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744778520 "/>
<attribute name="RDC-MAX" value="1060mohm"/>
<attribute name="RDC-TYP" value="950mohm"/>
<attribute name="SIZE" value=" 6033 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Robust"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1280P" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1280P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447707015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707015?ae"/>
<attribute name="FRES" value="49.2MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="24A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707015 "/>
<attribute name="RDC-MAX" value="5.5mohm"/>
<attribute name="RDC-TYP" value="4.6mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707022?ae"/>
<attribute name="FRES" value="41.7MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="20.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707022 "/>
<attribute name="RDC-MAX" value="6.8mohm"/>
<attribute name="RDC-TYP" value="5.7mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707033?ae"/>
<attribute name="FRES" value="32.3MHz"/>
<attribute name="IR" value="9.4A"/>
<attribute name="ISAT" value="17.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707033 "/>
<attribute name="RDC-MAX" value="9mohm"/>
<attribute name="RDC-TYP" value="7.5mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707047?ae"/>
<attribute name="FRES" value="28.8MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="15.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707047 "/>
<attribute name="RDC-MAX" value="10mohm"/>
<attribute name="RDC-TYP" value="8.5mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707068?ae"/>
<attribute name="FRES" value="19.1MHz"/>
<attribute name="IR" value="6.8A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707068 "/>
<attribute name="RDC-MAX" value="14mohm"/>
<attribute name="RDC-TYP" value="11.8mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707100?ae"/>
<attribute name="FRES" value="15.1MHz"/>
<attribute name="IR" value="5.6A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707100 "/>
<attribute name="RDC-MAX" value="21mohm"/>
<attribute name="RDC-TYP" value="18mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707101?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707101 "/>
<attribute name="RDC-MAX" value="120mohm"/>
<attribute name="RDC-TYP" value="105mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707102?ae"/>
<attribute name="FRES" value="1.2MHz"/>
<attribute name="IR" value="0.66A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707102 "/>
<attribute name="RDC-MAX" value="1090mohm"/>
<attribute name="RDC-TYP" value="985mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707150?ae"/>
<attribute name="FRES" value="13.2MHz"/>
<attribute name="IR" value="4.7A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707150 "/>
<attribute name="RDC-MAX" value="26.5mohm"/>
<attribute name="RDC-TYP" value="23mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707151?ae"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707151 "/>
<attribute name="RDC-MAX" value="190mohm"/>
<attribute name="RDC-TYP" value="165mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707220?ae"/>
<attribute name="FRES" value="10.2MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="7.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707220 "/>
<attribute name="RDC-MAX" value="36mohm"/>
<attribute name="RDC-TYP" value="31.5mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707221?ae"/>
<attribute name="FRES" value="2.9MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="2.35A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707221 "/>
<attribute name="RDC-MAX" value="265mohm"/>
<attribute name="RDC-TYP" value="240mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707330?ae"/>
<attribute name="FRES" value="8.3MHz"/>
<attribute name="IR" value="3.15A"/>
<attribute name="ISAT" value="6.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707330 "/>
<attribute name="RDC-MAX" value="53mohm"/>
<attribute name="RDC-TYP" value="46.5mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707331?ae"/>
<attribute name="FRES" value="2.1MHz"/>
<attribute name="IR" value="1.08A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707331 "/>
<attribute name="RDC-MAX" value="410mohm"/>
<attribute name="RDC-TYP" value="370mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707470?ae"/>
<attribute name="FRES" value="7.2MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="5.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707470 "/>
<attribute name="RDC-MAX" value="63mohm"/>
<attribute name="RDC-TYP" value="55mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707471?ae"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="IR" value="0.93A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707471 "/>
<attribute name="RDC-MAX" value="540mohm"/>
<attribute name="RDC-TYP" value="490mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707680?ae"/>
<attribute name="FRES" value="5.5MHz"/>
<attribute name="IR" value="2.45A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707680 "/>
<attribute name="RDC-MAX" value="90mohm"/>
<attribute name="RDC-TYP" value="78mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447707681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447707681?ae"/>
<attribute name="FRES" value="1.5MHz"/>
<attribute name="IR" value="0.78A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447707681 "/>
<attribute name="RDC-MAX" value="770mohm"/>
<attribute name="RDC-TYP" value="700mohm"/>
<attribute name="SIZE" value=" 1280 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1050P" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1050P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447714015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714015?ae"/>
<attribute name="FRES" value="69MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="12.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714015 "/>
<attribute name="RDC-MAX" value="6.6mohm"/>
<attribute name="RDC-TYP" value="5.55mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714022?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="8.6A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714022 "/>
<attribute name="RDC-MAX" value="8mohm"/>
<attribute name="RDC-TYP" value="6.8mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714033?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714033 "/>
<attribute name="RDC-MAX" value="10.5mohm"/>
<attribute name="RDC-TYP" value="8.9mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714047?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714047 "/>
<attribute name="RDC-MAX" value="12.4mohm"/>
<attribute name="RDC-TYP" value="10.4mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714056?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="ISAT" value="7.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714056 "/>
<attribute name="RDC-MAX" value="14.4mohm"/>
<attribute name="RDC-TYP" value="12mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="5.6uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714068?ae"/>
<attribute name="FRES" value="23.5MHz"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714068 "/>
<attribute name="RDC-MAX" value="22mohm"/>
<attribute name="RDC-TYP" value="18.5mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714100?ae"/>
<attribute name="FRES" value="20.5MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714100 "/>
<attribute name="RDC-MAX" value="27mohm"/>
<attribute name="RDC-TYP" value="23mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714101?ae"/>
<attribute name="FRES" value="5.9MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714101 "/>
<attribute name="RDC-MAX" value="198mohm"/>
<attribute name="RDC-TYP" value="165mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714102?ae"/>
<attribute name="FRES" value="1.7MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714102 "/>
<attribute name="RDC-MAX" value="2050mohm"/>
<attribute name="RDC-TYP" value="1860mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714150?ae"/>
<attribute name="FRES" value="16.8MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="4.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714150 "/>
<attribute name="RDC-MAX" value="43mohm"/>
<attribute name="RDC-TYP" value="36mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714151?ae"/>
<attribute name="FRES" value="4.9MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714151 "/>
<attribute name="RDC-MAX" value="300mohm"/>
<attribute name="RDC-TYP" value="251mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714220?ae"/>
<attribute name="FRES" value="14.5MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714220 "/>
<attribute name="RDC-MAX" value="50mohm"/>
<attribute name="RDC-TYP" value="42mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714221?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714221 "/>
<attribute name="RDC-MAX" value="439mohm"/>
<attribute name="RDC-TYP" value="366mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714270?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="3.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714270 "/>
<attribute name="RDC-MAX" value="74mohm"/>
<attribute name="RDC-TYP" value="63mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714330?ae"/>
<attribute name="FRES" value="11.1MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714330 "/>
<attribute name="RDC-MAX" value="79mohm"/>
<attribute name="RDC-TYP" value="66mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714331?ae"/>
<attribute name="FRES" value="3.15MHz"/>
<attribute name="IR" value="0.71A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714331 "/>
<attribute name="RDC-MAX" value="750mohm"/>
<attribute name="RDC-TYP" value="655mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714470?ae"/>
<attribute name="FRES" value="8.8MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714470 "/>
<attribute name="RDC-MAX" value="99mohm"/>
<attribute name="RDC-TYP" value="83mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714471?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.82A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714471 "/>
<attribute name="RDC-MAX" value="1100mohm"/>
<attribute name="RDC-TYP" value="960mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714560?ae"/>
<attribute name="FRES" value="8.6MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714560 "/>
<attribute name="RDC-MAX" value="121mohm"/>
<attribute name="RDC-TYP" value="101mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="56uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714680?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714680 "/>
<attribute name="RDC-MAX" value="132mohm"/>
<attribute name="RDC-TYP" value="110mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714681?ae"/>
<attribute name="FRES" value="2.05MHz"/>
<attribute name="IR" value="0.51A"/>
<attribute name="ISAT" value="0.71A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714681 "/>
<attribute name="RDC-MAX" value="1220mohm"/>
<attribute name="RDC-TYP" value="1140mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447714820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447714820?ae"/>
<attribute name="FRES" value="6.6MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.85A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447714820 "/>
<attribute name="RDC-MAX" value="176mohm"/>
<attribute name="RDC-TYP" value="147mohm"/>
<attribute name="SIZE" value=" 1050 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1030P" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1030P">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447713015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713015?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713015 "/>
<attribute name="RDC-MAX" value="16mohm"/>
<attribute name="RDC-TYP" value="13.7mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713022?ae"/>
<attribute name="FRES" value="71MHz"/>
<attribute name="IR" value="5.1A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713022 "/>
<attribute name="RDC-MAX" value="20mohm"/>
<attribute name="RDC-TYP" value="16.8mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713033?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="7.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713033 "/>
<attribute name="RDC-MAX" value="24mohm"/>
<attribute name="RDC-TYP" value="20.4mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713047?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713047 "/>
<attribute name="RDC-MAX" value="31mohm"/>
<attribute name="RDC-TYP" value="26mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713082?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713082 "/>
<attribute name="RDC-MAX" value="49mohm"/>
<attribute name="RDC-TYP" value="41mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713100?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="4.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713100 "/>
<attribute name="RDC-MAX" value="62mohm"/>
<attribute name="RDC-TYP" value="52mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713101?ae"/>
<attribute name="FRES" value="7.7MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713101 "/>
<attribute name="RDC-MAX" value="478mohm"/>
<attribute name="RDC-TYP" value="398mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713102?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713102 "/>
<attribute name="RDC-MAX" value="4600mohm"/>
<attribute name="RDC-TYP" value="4000mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713121">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713121?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713121 "/>
<attribute name="RDC-MAX" value="598mohm"/>
<attribute name="RDC-TYP" value="498mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713150?ae"/>
<attribute name="FRES" value="19.5MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713150 "/>
<attribute name="RDC-MAX" value="89mohm"/>
<attribute name="RDC-TYP" value="74mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713151?ae"/>
<attribute name="FRES" value="6.1MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713151 "/>
<attribute name="RDC-MAX" value="684mohm"/>
<attribute name="RDC-TYP" value="570mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713220?ae"/>
<attribute name="FRES" value="17.5MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713220 "/>
<attribute name="RDC-MAX" value="133mohm"/>
<attribute name="RDC-TYP" value="111mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713330?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713330 "/>
<attribute name="RDC-MAX" value="204mohm"/>
<attribute name="RDC-TYP" value="170mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713331?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="0.48A"/>
<attribute name="ISAT" value="0.73A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713331 "/>
<attribute name="RDC-MAX" value="1500mohm"/>
<attribute name="RDC-TYP" value="1230mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713470?ae"/>
<attribute name="FRES" value="11.4MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713470 "/>
<attribute name="RDC-MAX" value="248mohm"/>
<attribute name="RDC-TYP" value="207mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713471?ae"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713471 "/>
<attribute name="RDC-MAX" value="2200mohm"/>
<attribute name="RDC-TYP" value="1850mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713680?ae"/>
<attribute name="FRES" value="9.4MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713680 "/>
<attribute name="RDC-MAX" value="330mohm"/>
<attribute name="RDC-TYP" value="275mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
<technology name="_7447713820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447713820?ae"/>
<attribute name="FRES" value="8.8MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447713820 "/>
<attribute name="RDC-MAX" value="419mohm"/>
<attribute name="RDC-TYP" value="349mohm"/>
<attribute name="SIZE" value=" 1030 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Performance"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_7345R" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_7345R">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447779001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779001?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779001 "/>
<attribute name="RDC-MAX" value="15mohm"/>
<attribute name="RDC-TYP" value="10mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_74477790015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477790015?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="7.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477790015 "/>
<attribute name="RDC-MAX" value="18mohm"/>
<attribute name="RDC-TYP" value="15mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779002?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779002 "/>
<attribute name="RDC-MAX" value="20mohm"/>
<attribute name="RDC-TYP" value="16mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779003?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779003 "/>
<attribute name="RDC-MAX" value="30mohm"/>
<attribute name="RDC-TYP" value="26mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779004?ae"/>
<attribute name="FRES" value="37MHz"/>
<attribute name="IR" value="3.16A"/>
<attribute name="ISAT" value="4.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779004 "/>
<attribute name="RDC-MAX" value="32mohm"/>
<attribute name="RDC-TYP" value="28mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779006?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="2.91A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779006 "/>
<attribute name="RDC-MAX" value="35mohm"/>
<attribute name="RDC-TYP" value="33mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779008?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779008 "/>
<attribute name="RDC-MAX" value="53mohm"/>
<attribute name="RDC-TYP" value="47mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744777910">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777910?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777910 "/>
<attribute name="RDC-MAX" value="49mohm"/>
<attribute name="RDC-TYP" value="45mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779112?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.82A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779112 "/>
<attribute name="RDC-MAX" value="62mohm"/>
<attribute name="RDC-TYP" value="52mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779115?ae"/>
<attribute name="FRES" value="19.5MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779115 "/>
<attribute name="RDC-MAX" value="81mohm"/>
<attribute name="RDC-TYP" value="70mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779118?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="2.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779118 "/>
<attribute name="RDC-MAX" value="91mohm"/>
<attribute name="RDC-TYP" value="80mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779122?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="1.41A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779122 "/>
<attribute name="RDC-MAX" value="110mohm"/>
<attribute name="RDC-TYP" value="90mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779127?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="1.24A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779127 "/>
<attribute name="RDC-MAX" value="150mohm"/>
<attribute name="RDC-TYP" value="120mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779133?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="1.13A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779133 "/>
<attribute name="RDC-MAX" value="170mohm"/>
<attribute name="RDC-TYP" value="140mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779139?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.11A"/>
<attribute name="ISAT" value="1.23A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779139 "/>
<attribute name="RDC-MAX" value="230mohm"/>
<attribute name="RDC-TYP" value="145mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="39uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779147?ae"/>
<attribute name="FRES" value="10.5MHz"/>
<attribute name="IR" value="1.03A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779147 "/>
<attribute name="RDC-MAX" value="260mohm"/>
<attribute name="RDC-TYP" value="190mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779156?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.93A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779156 "/>
<attribute name="RDC-MAX" value="350mohm"/>
<attribute name="RDC-TYP" value="228mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="56uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779168?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="0.87A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779168 "/>
<attribute name="RDC-MAX" value="380mohm"/>
<attribute name="RDC-TYP" value="239mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779182?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.84A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779182 "/>
<attribute name="RDC-MAX" value="430mohm"/>
<attribute name="RDC-TYP" value="250mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744777920">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777920?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="0.79A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777920 "/>
<attribute name="RDC-MAX" value="380mohm"/>
<attribute name="RDC-TYP" value="290mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779212?ae"/>
<attribute name="FRES" value="6.7MHz"/>
<attribute name="IR" value="0.67A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779212 "/>
<attribute name="RDC-MAX" value="660mohm"/>
<attribute name="RDC-TYP" value="396mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779215?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.52A"/>
<attribute name="ISAT" value="0.63A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779215 "/>
<attribute name="RDC-MAX" value="880mohm"/>
<attribute name="RDC-TYP" value="529mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779218?ae"/>
<attribute name="FRES" value="5.3MHz"/>
<attribute name="IR" value="0.51A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779218 "/>
<attribute name="RDC-MAX" value="980mohm"/>
<attribute name="RDC-TYP" value="603mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779222?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.44A"/>
<attribute name="ISAT" value="0.54A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779222 "/>
<attribute name="RDC-MAX" value="1170mohm"/>
<attribute name="RDC-TYP" value="920mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779233?ae"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.39A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779233 "/>
<attribute name="RDC-MAX" value="1860mohm"/>
<attribute name="RDC-TYP" value="1150mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779239?ae"/>
<attribute name="FRES" value="3.8MHz"/>
<attribute name="IR" value="0.38A"/>
<attribute name="ISAT" value="0.42A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779239 "/>
<attribute name="RDC-MAX" value="2850mohm"/>
<attribute name="RDC-TYP" value="1400mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="390uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744777924">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777924?ae"/>
<attribute name="FRES" value="3.2MHz"/>
<attribute name="IR" value="0.29A"/>
<attribute name="ISAT" value="0.34A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777924 "/>
<attribute name="RDC-MAX" value="3010mohm"/>
<attribute name="RDC-TYP" value="1600mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744777925">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777925?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.28A"/>
<attribute name="ISAT" value="0.31A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777925 "/>
<attribute name="RDC-MAX" value="3620mohm"/>
<attribute name="RDC-TYP" value="1720mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="560uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744777926">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777926?ae"/>
<attribute name="FRES" value="2.7MHz"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.28A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777926 "/>
<attribute name="RDC-MAX" value="4630mohm"/>
<attribute name="RDC-TYP" value="2600mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_7447779270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447779270?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.48A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447779270 "/>
<attribute name="RDC-MAX" value="1640mohm"/>
<attribute name="RDC-TYP" value="1090mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="270uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744777928">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777928?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="0.21A"/>
<attribute name="ISAT" value="0.26A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777928 "/>
<attribute name="RDC-MAX" value="5200mohm"/>
<attribute name="RDC-TYP" value="2960mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
<technology name="_744777930">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744777930?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744777930 "/>
<attribute name="RDC-MAX" value="6000mohm"/>
<attribute name="RDC-TYP" value="3270mohm"/>
<attribute name="SIZE" value=" 7345 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Robust "/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1210" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447709001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709001?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="13A"/>
<attribute name="ISAT" value="25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709001 "/>
<attribute name="RDC-MAX" value="6mohm"/>
<attribute name="RDC-TYP" value="4mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709002?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709002 "/>
<attribute name="RDC-MAX" value="6mohm"/>
<attribute name="RDC-TYP" value="5mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709003?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="11A"/>
<attribute name="ISAT" value="16.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709003 "/>
<attribute name="RDC-MAX" value="9mohm"/>
<attribute name="RDC-TYP" value="6mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="3.5uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709004?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="9.3A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709004 "/>
<attribute name="RDC-MAX" value="11mohm"/>
<attribute name="RDC-TYP" value="7mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709006?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="8.4A"/>
<attribute name="ISAT" value="12.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709006 "/>
<attribute name="RDC-MAX" value="14mohm"/>
<attribute name="RDC-TYP" value="9mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709100?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709100 "/>
<attribute name="RDC-MAX" value="21mohm"/>
<attribute name="RDC-TYP" value="13mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709101?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709101 "/>
<attribute name="RDC-MAX" value="110mohm"/>
<attribute name="RDC-TYP" value="100mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709102?ae"/>
<attribute name="FRES" value="1MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709102 "/>
<attribute name="RDC-MAX" value="1200mohm"/>
<attribute name="RDC-TYP" value="930mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709150?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709150 "/>
<attribute name="RDC-MAX" value="26mohm"/>
<attribute name="RDC-TYP" value="21mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709151?ae"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709151 "/>
<attribute name="RDC-MAX" value="200mohm"/>
<attribute name="RDC-TYP" value="151mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709152?ae"/>
<attribute name="FRES" value="0.9MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709152 "/>
<attribute name="RDC-MAX" value="2300mohm"/>
<attribute name="RDC-TYP" value="1800mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="1500uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709220?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709220 "/>
<attribute name="RDC-MAX" value="28mohm"/>
<attribute name="RDC-TYP" value="23mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709221?ae"/>
<attribute name="FRES" value="2.7MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709221 "/>
<attribute name="RDC-MAX" value="300mohm"/>
<attribute name="RDC-TYP" value="193mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709222?ae"/>
<attribute name="FRES" value="0.66MHz"/>
<attribute name="IR" value="0.53A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709222 "/>
<attribute name="RDC-MAX" value="3750mohm"/>
<attribute name="RDC-TYP" value="3250mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="2200uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709270?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709270 "/>
<attribute name="RDC-MAX" value="40mohm"/>
<attribute name="RDC-TYP" value="30mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709271">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709271?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709271 "/>
<attribute name="RDC-MAX" value="330mohm"/>
<attribute name="RDC-TYP" value="248mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="270uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709330?ae"/>
<attribute name="FRES" value="8.5MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709330 "/>
<attribute name="RDC-MAX" value="45mohm"/>
<attribute name="RDC-TYP" value="37mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709331?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709331 "/>
<attribute name="RDC-MAX" value="430mohm"/>
<attribute name="RDC-TYP" value="363mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709390?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709390 "/>
<attribute name="RDC-MAX" value="56mohm"/>
<attribute name="RDC-TYP" value="44mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="39uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709470?ae"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709470 "/>
<attribute name="RDC-MAX" value="60mohm"/>
<attribute name="RDC-TYP" value="46mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709471?ae"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709471 "/>
<attribute name="RDC-MAX" value="560mohm"/>
<attribute name="RDC-TYP" value="437mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709680?ae"/>
<attribute name="FRES" value="5.5MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709680 "/>
<attribute name="RDC-MAX" value="89mohm"/>
<attribute name="RDC-TYP" value="69mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709681?ae"/>
<attribute name="FRES" value="1.5MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709681 "/>
<attribute name="RDC-MAX" value="825mohm"/>
<attribute name="RDC-TYP" value="660mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709820?ae"/>
<attribute name="FRES" value="4.5MHz"/>
<attribute name="IR" value="2.75A"/>
<attribute name="ISAT" value="3.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709820 "/>
<attribute name="RDC-MAX" value="105mohm"/>
<attribute name="RDC-TYP" value="90.5mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_7447709821">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447709821?ae"/>
<attribute name="FRES" value="1.2MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447709821 "/>
<attribute name="RDC-MAX" value="1000mohm"/>
<attribute name="RDC-TYP" value="815mohm"/>
<attribute name="SIZE" value=" 1210 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD_1260" prefix="L">
<description>&lt;b&gt;WE-PD SMT Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; AECQ 200 Qualified
&lt;br&gt;Ultra low RDC and RAC
&lt;br&gt;Highest possible saturation current based on Ferrite
&lt;br&gt;Suitable for switching frequency up to 10MHz
&lt;br&gt;Temperature dependent parameter available on Redexpert
&lt;br&gt;Operating Temperature from -40°C to +125°C / +150°C
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Types
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;WE-PD: Since always with low loss material, tight tolerances and high saturation behavior compared to other manufacturers &lt;br&gt;in the market
&lt;br&gt;WE-PD Robust: Plastic base improves the mechanical stability and efficiency
&lt;br&gt;WE-PD Performance: MnZn core improves Saturation and RDC for highest efficiency
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Switch Mode Power supplies from 0,1W up to 300W
&lt;br&gt;Integrated DC DC Converter
&lt;br&gt;Ideal for Switch Mode Power supplies with extreme high efficiency (&gt;95%)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o194227v209%20Family_WE-PD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-PD"&gt;www.we-online.com/en/components/products/WE-PD&lt;/a&gt;&lt;p&gt;


Updated by Ella Wu 2023-02-17&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PD_1260">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744771001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771001?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771001 "/>
<attribute name="RDC-MAX" value="6mohm"/>
<attribute name="RDC-TYP" value="4mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771002?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="ISAT" value="11A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771002 "/>
<attribute name="RDC-MAX" value="7mohm"/>
<attribute name="RDC-TYP" value="5mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771003?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="9.25A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771003 "/>
<attribute name="RDC-MAX" value="8mohm"/>
<attribute name="RDC-TYP" value="5.5mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="3.5uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771004?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="8.25A"/>
<attribute name="ISAT" value="8.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771004 "/>
<attribute name="RDC-MAX" value="11mohm"/>
<attribute name="RDC-TYP" value="8.5mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771006?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="6.3A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771006 "/>
<attribute name="RDC-MAX" value="18mohm"/>
<attribute name="RDC-TYP" value="14mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771008?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771008 "/>
<attribute name="RDC-MAX" value="20mohm"/>
<attribute name="RDC-TYP" value="15.5mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771010?ae"/>
<attribute name="FRES" value="88MHz"/>
<attribute name="IR" value="14A"/>
<attribute name="ISAT" value="15.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771010 "/>
<attribute name="RDC-MAX" value="5mohm"/>
<attribute name="RDC-TYP" value="3mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="1uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477110?ae"/>
<attribute name="FRES" value="21.5MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477110 "/>
<attribute name="RDC-MAX" value="24mohm"/>
<attribute name="RDC-TYP" value="18.5mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771112?ae"/>
<attribute name="FRES" value="19.7MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="4.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771112 "/>
<attribute name="RDC-MAX" value="26mohm"/>
<attribute name="RDC-TYP" value="20mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="12uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771115?ae"/>
<attribute name="FRES" value="16.6MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771115 "/>
<attribute name="RDC-MAX" value="28mohm"/>
<attribute name="RDC-TYP" value="22mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="15uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771118">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771118?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771118 "/>
<attribute name="RDC-MAX" value="30mohm"/>
<attribute name="RDC-TYP" value="24mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="18uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771122?ae"/>
<attribute name="FRES" value="13.5MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771122 "/>
<attribute name="RDC-MAX" value="36mohm"/>
<attribute name="RDC-TYP" value="30mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="22uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771127">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771127?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771127 "/>
<attribute name="RDC-MAX" value="45mohm"/>
<attribute name="RDC-TYP" value="37mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="27uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771133?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771133 "/>
<attribute name="RDC-MAX" value="57mohm"/>
<attribute name="RDC-TYP" value="49mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="33uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771139?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771139 "/>
<attribute name="RDC-MAX" value="68mohm"/>
<attribute name="RDC-TYP" value="57mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="39uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771147?ae"/>
<attribute name="FRES" value="9.2MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771147 "/>
<attribute name="RDC-MAX" value="77mohm"/>
<attribute name="RDC-TYP" value="64mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="47uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771156?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771156 "/>
<attribute name="RDC-MAX" value="92mohm"/>
<attribute name="RDC-TYP" value="77mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="56uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771168?ae"/>
<attribute name="FRES" value="7.6MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771168 "/>
<attribute name="RDC-MAX" value="105mohm"/>
<attribute name="RDC-TYP" value="86mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="68uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771182?ae"/>
<attribute name="FRES" value="7.2MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771182 "/>
<attribute name="RDC-MAX" value="135mohm"/>
<attribute name="RDC-TYP" value="112mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="82uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477120?ae"/>
<attribute name="FRES" value="6.6MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477120 "/>
<attribute name="RDC-MAX" value="160mohm"/>
<attribute name="RDC-TYP" value="135mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771212?ae"/>
<attribute name="FRES" value="5.2MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771212 "/>
<attribute name="RDC-MAX" value="180mohm"/>
<attribute name="RDC-TYP" value="150mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="120uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771215?ae"/>
<attribute name="FRES" value="4.4MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.45A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771215 "/>
<attribute name="RDC-MAX" value="220mohm"/>
<attribute name="RDC-TYP" value="185mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="150uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771218?ae"/>
<attribute name="FRES" value="4.1MHz"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771218 "/>
<attribute name="RDC-MAX" value="280mohm"/>
<attribute name="RDC-TYP" value="230mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="180uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771220?ae"/>
<attribute name="FRES" value="3.8MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771220 "/>
<attribute name="RDC-MAX" value="340mohm"/>
<attribute name="RDC-TYP" value="280mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="220uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771233?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.97A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771233 "/>
<attribute name="RDC-MAX" value="490mohm"/>
<attribute name="RDC-TYP" value="410mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="330uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771239?ae"/>
<attribute name="FRES" value="2.8MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771239 "/>
<attribute name="RDC-MAX" value="640mohm"/>
<attribute name="RDC-TYP" value="540mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="390uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477124">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477124?ae"/>
<attribute name="FRES" value="2.6MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477124 "/>
<attribute name="RDC-MAX" value="710mohm"/>
<attribute name="RDC-TYP" value="590mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="470uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477125">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477125?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="0.65A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477125 "/>
<attribute name="RDC-MAX" value="890mohm"/>
<attribute name="RDC-TYP" value="740mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="560uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477126">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477126?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477126 "/>
<attribute name="RDC-MAX" value="1020mohm"/>
<attribute name="RDC-TYP" value="850mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="680uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_744771270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744771270?ae"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744771270 "/>
<attribute name="RDC-MAX" value="400mohm"/>
<attribute name="RDC-TYP" value="330mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="270uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477128">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477128?ae"/>
<attribute name="FRES" value="2.1MHz"/>
<attribute name="IR" value="0.55A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477128 "/>
<attribute name="RDC-MAX" value="1200mohm"/>
<attribute name="RDC-TYP" value="980mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="820uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
<technology name="_74477130">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74477130?ae"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74477130 "/>
<attribute name="RDC-MAX" value="1600mohm"/>
<attribute name="RDC-TYP" value="1330mohm"/>
<attribute name="SIZE" value=" 1260 "/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VERSION" value="Standard"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
