<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-PD2SA&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PD2SA_7850">
<description>&lt;B&gt;WE-PD2SA SMD Power Inductor
&lt;BR&gt;&lt;/B&gt;Size : 7850
&lt;BR&gt;L X W X H = 7.8mm X 7mm X 5mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PD2SA_7850" prefix="L">
<description>&lt;b&gt;WE-PD2SA SMD Power Inductor&lt;br&gt;
&lt;br&gt;
Characteristics 
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Magnetic shielded version from the WE-PD2A, which results in a low leakage field
&lt;br&gt;Pad compatible with the WE-PD2A size 7850
&lt;br&gt;High saturation current due to the self- centering shielding ring construction
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications 
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Switching regulators with low operating voltage
&lt;br&gt;Multimedia applications
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.de/media/images/v2/o85064v209%20Family_WE-PD2SA.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.de/media/images/v2/o85064v209%20Family_WE-PD2SA.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.de/en/am/WE-PD2SA"&gt;https://katalog.we-online.de/en/am/WE-PD2SA&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2019-09-10&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PD2SA_7850">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784787012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787012.pdf"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="4.85A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787012 "/>
<attribute name="RDC-MAX" value="13mOhm"/>
<attribute name="RDC-TYP" value="8.5mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_784787027">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787027.pdf"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="4.35A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787027 "/>
<attribute name="RDC-MAX" value="17mOhm"/>
<attribute name="RDC-TYP" value="13.5mOhm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_784787039">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787039.pdf"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787039 "/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="RDC-TYP" value="16.7mOhm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_784787047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787047.pdf"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787047 "/>
<attribute name="RDC-MAX" value="29mOhm"/>
<attribute name="RDC-TYP" value="24.3mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_784787068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787068.pdf"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787068 "/>
<attribute name="RDC-MAX" value="33mOhm"/>
<attribute name="RDC-TYP" value="27mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_784787082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787082.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787082 "/>
<attribute name="RDC-MAX" value="39mOhm"/>
<attribute name="RDC-TYP" value="33mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_784787100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787100.pdf"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787100 "/>
<attribute name="RDC-MAX" value="43mOhm"/>
<attribute name="RDC-TYP" value="36.5mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_784787101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787101.pdf"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="0.87A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787101 "/>
<attribute name="RDC-MAX" value="467mOhm"/>
<attribute name="RDC-TYP" value="396mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_784787120">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787120.pdf"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="2.45A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787120 "/>
<attribute name="RDC-MAX" value="52mOhm"/>
<attribute name="RDC-TYP" value="45mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_784787121">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787121.pdf"/>
<attribute name="FRES" value="4.5MHz"/>
<attribute name="IR" value="0.73A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787121 "/>
<attribute name="RDC-MAX" value="643mOhm"/>
<attribute name="RDC-TYP" value="545mOhm"/>
<attribute name="VALUE" value="120uH"/>
</technology>
<technology name="_784787150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787150.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787150 "/>
<attribute name="RDC-MAX" value="60mOhm"/>
<attribute name="RDC-TYP" value="52mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_784787151">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787151.pdf"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.71A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787151 "/>
<attribute name="RDC-MAX" value="719mOhm"/>
<attribute name="RDC-TYP" value="610mOhm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_784787180">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787180.pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="2.15A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787180 "/>
<attribute name="RDC-MAX" value="78mOhm"/>
<attribute name="RDC-TYP" value="67mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_784787181">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787181.pdf"/>
<attribute name="FRES" value="3.8MHz"/>
<attribute name="IR" value="0.68A"/>
<attribute name="ISAT" value="0.62A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787181 "/>
<attribute name="RDC-MAX" value="794mOhm"/>
<attribute name="RDC-TYP" value="673mOhm"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_784787220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787220.pdf"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="1.83A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787220 "/>
<attribute name="RDC-MAX" value="103mOhm"/>
<attribute name="RDC-TYP" value="88mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_784787221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787221.pdf"/>
<attribute name="FRES" value="3.5MHz"/>
<attribute name="IR" value="0.67A"/>
<attribute name="ISAT" value="0.58A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787221 "/>
<attribute name="RDC-MAX" value="876mOhm"/>
<attribute name="RDC-TYP" value="743mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_784787330">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787330.pdf"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.48A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787330 "/>
<attribute name="RDC-MAX" value="161mOhm"/>
<attribute name="RDC-TYP" value="137mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_784787470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787470.pdf"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787470 "/>
<attribute name="RDC-MAX" value="243mOhm"/>
<attribute name="RDC-TYP" value="206mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_784787680">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787680.pdf"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="1.12A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787680 "/>
<attribute name="RDC-MAX" value="290mOhm"/>
<attribute name="RDC-TYP" value="246mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_784787820">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.de/am/datasheet/784787820.pdf"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="1.04A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784787820 "/>
<attribute name="RDC-MAX" value="328mOhm"/>
<attribute name="RDC-TYP" value="278mOhm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
