<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-PD3&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-08-23&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PD3_M">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: M, SMT, 2pins
&lt;br&gt;LXWXH = 12.7X10.1X2.7mm</description>
</package>
<package name="WE-PD3_X">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: X, SMT, 2pins
&lt;br&gt;LXWXH = 18.54X15.24X7.62
mm</description>
</package>
<package name="WE-PD3_S">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: S, SMT, 2pins
&lt;br&gt;LXWXH = 6.6X4.45X2.92mm</description>
</package>
<package name="WE-PD3_L">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: L, SMT, 2pins
&lt;br&gt;LXWXH = 12.7X10X4.9mm</description>
</package>
</packages>
<symbols>
<symbol name="L_POINT_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PD3_M" prefix="L">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded version which results in a low leakage field
&lt;br&gt;Working frequency up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets expect Type S
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;EMI-filter, DC/DC Converter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD3/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-PD3&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-23&lt;br&gt;
2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-PD3_M">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445301?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="PART-NUMBER" value=" 7445301 "/>
<attribute name="RDC-MAX" value="0.038Ohm"/>
<attribute name="RDC-TYP" value="0.029Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74453010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453010?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="IR" value="1.24A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="PART-NUMBER" value=" 74453010 "/>
<attribute name="RDC-MAX" value="0.145Ohm"/>
<attribute name="RDC-TYP" value="0.117Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7445302">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445302?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="2.76A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 7445302 "/>
<attribute name="RDC-MAX" value="0.045Ohm"/>
<attribute name="RDC-TYP" value="0.037Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7445303">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445303?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="PART-NUMBER" value=" 7445303 "/>
<attribute name="RDC-MAX" value="0.07Ohm"/>
<attribute name="RDC-TYP" value="0.058Ohm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_74453031">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453031?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="PART-NUMBER" value=" 74453031 "/>
<attribute name="RDC-MAX" value="0.062Ohm"/>
<attribute name="RDC-TYP" value="0.052Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7445304">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445304?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="PART-NUMBER" value=" 7445304 "/>
<attribute name="RDC-MAX" value="0.078Ohm"/>
<attribute name="RDC-TYP" value="0.065Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7445306">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445306?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="PART-NUMBER" value=" 7445306 "/>
<attribute name="RDC-MAX" value="0.085Ohm"/>
<attribute name="RDC-TYP" value="0.064Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74453112">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453112?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="PART-NUMBER" value=" 74453112 "/>
<attribute name="RDC-MAX" value="0.185Ohm"/>
<attribute name="RDC-TYP" value="0.16Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_74453115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453115?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="PART-NUMBER" value=" 74453115 "/>
<attribute name="RDC-MAX" value="0.2Ohm"/>
<attribute name="RDC-TYP" value="0.17Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74453122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453122?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 74453122 "/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="RDC-TYP" value="0.248Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74453133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453133?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="PART-NUMBER" value=" 74453133 "/>
<attribute name="RDC-MAX" value="0.45Ohm"/>
<attribute name="RDC-TYP" value="0.371Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74453147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453147?ae"/>
<attribute name="FRES" value="12.5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 74453147 "/>
<attribute name="RDC-MAX" value="0.65Ohm"/>
<attribute name="RDC-TYP" value="0.481Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74453156">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453156?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="0.52A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="PART-NUMBER" value=" 74453156 "/>
<attribute name="RDC-MAX" value="0.68Ohm"/>
<attribute name="RDC-TYP" value="0.552Ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_74453168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453168?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.48A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 74453168 "/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="RDC-TYP" value="0.62Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_74453182">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74453182?ae"/>
<attribute name="FRES" value="9.5MHz"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 74453182 "/>
<attribute name="RDC-MAX" value="1.2Ohm"/>
<attribute name="RDC-TYP" value="1.03Ohm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
<technology name="_7445320">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445320?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 7445320 "/>
<attribute name="RDC-MAX" value="1.4Ohm"/>
<attribute name="RDC-TYP" value="1.164Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD3_X" prefix="L">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded version which results in a low leakage field
&lt;br&gt;Working frequency up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets expect Type S
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;EMI-filter, DC/DC Converter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD3/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-PD3&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-23&lt;br&gt;
2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-PD3_X">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74459010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459010?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="PART-NUMBER" value=" 74459010 "/>
<attribute name="RDC-MAX" value="0.04Ohm"/>
<attribute name="RDC-TYP" value="0.023Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74459115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459115?ae"/>
<attribute name="FRES" value="16.5MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="PART-NUMBER" value=" 74459115 "/>
<attribute name="RDC-MAX" value="0.048Ohm"/>
<attribute name="RDC-TYP" value="0.03Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74459122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459122?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 74459122 "/>
<attribute name="RDC-MAX" value="0.059Ohm"/>
<attribute name="RDC-TYP" value="0.048Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74459133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459133?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="PART-NUMBER" value=" 74459133 "/>
<attribute name="RDC-MAX" value="0.075Ohm"/>
<attribute name="RDC-TYP" value="0.071Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74459147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459147?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 74459147 "/>
<attribute name="RDC-MAX" value="0.097Ohm"/>
<attribute name="RDC-TYP" value="0.085Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74459168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459168?ae"/>
<attribute name="FRES" value="7.2MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 74459168 "/>
<attribute name="RDC-MAX" value="0.138Ohm"/>
<attribute name="RDC-TYP" value="0.105Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7445920">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445920?ae"/>
<attribute name="FRES" value="5.5MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 7445920 "/>
<attribute name="RDC-MAX" value="0.207Ohm"/>
<attribute name="RDC-TYP" value="0.151Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74459215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459215?ae"/>
<attribute name="FRES" value="4.6MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="PART-NUMBER" value=" 74459215 "/>
<attribute name="RDC-MAX" value="0.293Ohm"/>
<attribute name="RDC-TYP" value="0.209Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74459222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459222?ae"/>
<attribute name="FRES" value="3.7MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 74459222 "/>
<attribute name="RDC-MAX" value="0.47Ohm"/>
<attribute name="RDC-TYP" value="0.311Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74459233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459233?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 74459233 "/>
<attribute name="RDC-MAX" value="0.78Ohm"/>
<attribute name="RDC-TYP" value="0.457Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74459247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459247?ae"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 74459247 "/>
<attribute name="RDC-MAX" value="1.08Ohm"/>
<attribute name="RDC-TYP" value="0.661Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_74459268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74459268?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.96A"/>
<attribute name="PART-NUMBER" value=" 74459268 "/>
<attribute name="RDC-MAX" value="1.4Ohm"/>
<attribute name="RDC-TYP" value="1.059Ohm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_7445930">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445930?ae"/>
<attribute name="FRES" value="1.6MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 7445930 "/>
<attribute name="RDC-MAX" value="2.01Ohm"/>
<attribute name="RDC-TYP" value="1.427Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD3_S" prefix="L">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded version which results in a low leakage field
&lt;br&gt;Working frequency up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets expect Type S
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;EMI-filter, DC/DC Converter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD3/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-PD3&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-23&lt;br&gt;
2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-PD3_S">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7445101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445101?ae"/>
<attribute name="FRES" value="83MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="1.62A"/>
<attribute name="PART-NUMBER" value=" 7445101 "/>
<attribute name="RDC-MAX" value="0.04Ohm"/>
<attribute name="RDC-TYP" value="0.014Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74451015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451015?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="1.13A"/>
<attribute name="PART-NUMBER" value=" 74451015 "/>
<attribute name="RDC-MAX" value="0.045Ohm"/>
<attribute name="RDC-TYP" value="0.018Ohm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_74451022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451022?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="1.08A"/>
<attribute name="PART-NUMBER" value=" 74451022 "/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="RDC-TYP" value="0.021Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74451033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451033?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="0.77A"/>
<attribute name="PART-NUMBER" value=" 74451033 "/>
<attribute name="RDC-MAX" value="0.055Ohm"/>
<attribute name="RDC-TYP" value="0.025Ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74451039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451039?ae"/>
<attribute name="FRES" value="53MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="0.77A"/>
<attribute name="PART-NUMBER" value=" 74451039 "/>
<attribute name="RDC-MAX" value="0.057Ohm"/>
<attribute name="RDC-TYP" value="0.04Ohm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_74451047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451047?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="0.72A"/>
<attribute name="PART-NUMBER" value=" 74451047 "/>
<attribute name="RDC-MAX" value="0.06Ohm"/>
<attribute name="RDC-TYP" value="0.045Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74451068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451068?ae"/>
<attribute name="FRES" value="36.5MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 74451068 "/>
<attribute name="RDC-MAX" value="0.065Ohm"/>
<attribute name="RDC-TYP" value="0.055Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7445110">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445110?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="PART-NUMBER" value=" 7445110 "/>
<attribute name="RDC-MAX" value="0.075Ohm"/>
<attribute name="RDC-TYP" value="0.056Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74451115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451115?ae"/>
<attribute name="FRES" value="25.5MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="0.27A"/>
<attribute name="PART-NUMBER" value=" 74451115 "/>
<attribute name="RDC-MAX" value="0.09Ohm"/>
<attribute name="RDC-TYP" value="0.075Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74451122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451122?ae"/>
<attribute name="FRES" value="20.5MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.16A"/>
<attribute name="PART-NUMBER" value=" 74451122 "/>
<attribute name="RDC-MAX" value="0.11Ohm"/>
<attribute name="RDC-TYP" value="0.09Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74451133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451133?ae"/>
<attribute name="FRES" value="14.5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.15A"/>
<attribute name="PART-NUMBER" value=" 74451133 "/>
<attribute name="RDC-MAX" value="0.19Ohm"/>
<attribute name="RDC-TYP" value="0.114Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74451147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451147?ae"/>
<attribute name="FRES" value="11.5MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.14A"/>
<attribute name="PART-NUMBER" value=" 74451147 "/>
<attribute name="RDC-MAX" value="0.23Ohm"/>
<attribute name="RDC-TYP" value="0.16Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74451168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451168?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.12A"/>
<attribute name="PART-NUMBER" value=" 74451168 "/>
<attribute name="RDC-MAX" value="0.29Ohm"/>
<attribute name="RDC-TYP" value="0.221Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7445120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445120?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.09A"/>
<attribute name="PART-NUMBER" value=" 7445120 "/>
<attribute name="RDC-MAX" value="0.48Ohm"/>
<attribute name="RDC-TYP" value="0.393Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74451215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451215?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.26A"/>
<attribute name="ISAT" value="0.05A"/>
<attribute name="PART-NUMBER" value=" 74451215 "/>
<attribute name="RDC-MAX" value="0.59Ohm"/>
<attribute name="RDC-TYP" value="0.41Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74451222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451222?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.08A"/>
<attribute name="PART-NUMBER" value=" 74451222 "/>
<attribute name="RDC-MAX" value="0.77Ohm"/>
<attribute name="RDC-TYP" value="0.58Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74451233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451233?ae"/>
<attribute name="FRES" value="3.2MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.02A"/>
<attribute name="PART-NUMBER" value=" 74451233 "/>
<attribute name="RDC-MAX" value="1.4Ohm"/>
<attribute name="RDC-TYP" value="1Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74451247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74451247?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.19A"/>
<attribute name="ISAT" value="0.02A"/>
<attribute name="PART-NUMBER" value=" 74451247 "/>
<attribute name="RDC-MAX" value="1.8Ohm"/>
<attribute name="RDC-TYP" value="1.7Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PD3_L" prefix="L">
<description>&lt;b&gt;WE-PD3 SMT Power Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Magnetically shielded version which results in a low leakage field
&lt;br&gt;Working frequency up to 10 MHz
&lt;br&gt;Operating temperature: –40°C to +125°C
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Now with impedance graph in datasheets expect Type S
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;EMI-filter, DC/DC Converter
&lt;br&gt;Perfectly suitable for switching regulators e.g. National Semiconductor, Linear Technology, Texas Instruments, Maxim, Semtech, ON Semiconductor, Cologne Chip, STMicroelectronics, Maxim, MPS, Diodes, Analogic Tech and Exar
&lt;br&gt;Perfectly suitable for switching regulators with extremely high efficiency
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14831v209%20Family_WE-PD3.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PD3/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-PD3&lt;/a&gt;&lt;p&gt;

Updated by Ella 2023-08-23&lt;br&gt;
2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_POINT_GAP"/>
</gates>
<devices>
<device name="" package="WE-PD3_L">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74454010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454010?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="PART-NUMBER" value=" 74454010 "/>
<attribute name="RDC-MAX" value="0.065Ohm"/>
<attribute name="RDC-TYP" value="0.048Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7445402">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445402?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="PART-NUMBER" value=" 7445402 "/>
<attribute name="RDC-MAX" value="0.027Ohm"/>
<attribute name="RDC-TYP" value="0.023Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7445403">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445403?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="2.9A"/>
<attribute name="ISAT" value="5.9A"/>
<attribute name="PART-NUMBER" value=" 7445403 "/>
<attribute name="RDC-MAX" value="0.03Ohm"/>
<attribute name="RDC-TYP" value="0.026Ohm"/>
<attribute name="VALUE" value="3uH"/>
</technology>
<technology name="_7445404">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445404?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="PART-NUMBER" value=" 7445404 "/>
<attribute name="RDC-MAX" value="0.04Ohm"/>
<attribute name="RDC-TYP" value="0.034Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74454068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454068?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="4.1A"/>
<attribute name="PART-NUMBER" value=" 74454068 "/>
<attribute name="RDC-MAX" value="0.055Ohm"/>
<attribute name="RDC-TYP" value="0.041Ohm"/>
<attribute name="VALUE" value="7uH"/>
</technology>
<technology name="_74454115">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454115?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 74454115 "/>
<attribute name="RDC-MAX" value="0.085Ohm"/>
<attribute name="RDC-TYP" value="0.064Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74454122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454122?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="PART-NUMBER" value=" 74454122 "/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="RDC-TYP" value="0.076Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74454133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454133?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 74454133 "/>
<attribute name="RDC-MAX" value="0.16Ohm"/>
<attribute name="RDC-TYP" value="0.127Ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74454147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454147?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="PART-NUMBER" value=" 74454147 "/>
<attribute name="RDC-MAX" value="0.19Ohm"/>
<attribute name="RDC-TYP" value="0.158Ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74454168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454168?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="PART-NUMBER" value=" 74454168 "/>
<attribute name="RDC-MAX" value="0.34Ohm"/>
<attribute name="RDC-TYP" value="0.285Ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_7445420">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445420?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="0.68A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7445420 "/>
<attribute name="RDC-MAX" value="0.42Ohm"/>
<attribute name="RDC-TYP" value="0.373Ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74454215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454215?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.55A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 74454215 "/>
<attribute name="RDC-MAX" value="0.52Ohm"/>
<attribute name="RDC-TYP" value="0.456Ohm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_74454220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454220?ae"/>
<attribute name="FRES" value="4.5MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 74454220 "/>
<attribute name="RDC-MAX" value="0.8Ohm"/>
<attribute name="RDC-TYP" value="0.683Ohm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_74454233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454233?ae"/>
<attribute name="FRES" value="3.4MHz"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="PART-NUMBER" value=" 74454233 "/>
<attribute name="RDC-MAX" value="1.2Ohm"/>
<attribute name="RDC-TYP" value="1.044Ohm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_74454239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454239?ae"/>
<attribute name="FRES" value="3.3MHz"/>
<attribute name="IR" value="0.33A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="PART-NUMBER" value=" 74454239 "/>
<attribute name="RDC-MAX" value="1.4Ohm"/>
<attribute name="RDC-TYP" value="1.175Ohm"/>
<attribute name="VALUE" value="390uH"/>
</technology>
<technology name="_74454247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454247?ae"/>
<attribute name="FRES" value="3.2MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 74454247 "/>
<attribute name="RDC-MAX" value="1.6Ohm"/>
<attribute name="RDC-TYP" value="1.35Ohm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_74454268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74454268?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="0.26A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="PART-NUMBER" value=" 74454268 "/>
<attribute name="RDC-MAX" value="2.3Ohm"/>
<attribute name="RDC-TYP" value="1.94Ohm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_7445430">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7445430?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="PART-NUMBER" value=" 7445430 "/>
<attribute name="RDC-MAX" value="3.2Ohm"/>
<attribute name="RDC-TYP" value="2.75Ohm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
