<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Single Coil Power Inductors - WE-PDA&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2026a, 2026-01-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PDA_7345">
<description>&lt;b&gt;WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size:7345, SMT, 2pins
&lt;br&gt;L X W X H = 7.3mm X 7.3mm X 4mm</description>
</package>
<package name="WE-PDA_7332">
<description>&lt;b&gt;WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size:7332, SMT, 2pins
&lt;br&gt;L X W X H = 7.3mm X 7.3mm X 3.2mm</description>
</package>
<package name="WE-PDA_1050">
<description>&lt;b&gt;WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size:1050, SMT, 2pins
&lt;br&gt;L X W X H = 10mm X 10mm X 5mm</description>
</package>
<package name="WE-PDA_1260">
<description>&lt;b&gt;WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Size:1260, SMT, 2pins
&lt;br&gt;L X W X H = 12mm X 12mm X 6mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PDA_7345" prefix="L">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Very low self-losses at high switching frequency's
&lt;br&gt;Wide inductance spectrum available at all sizes
&lt;br&gt;Core Material: NiZn
&lt;br&gt;Wire connection: welding technology
&lt;br&gt;Automotive approved
&lt;br&gt;Size 1050: Operating temperature -50°C up to +150°C
&lt;br&gt;Size 7332, 7345, 1260: Operating temperature -40°C up to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with extremely high efficiency
&lt;br&gt;Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PDA
&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2026-01-20&lt;br&gt;
&lt;/b&gt;2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDA_7345">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784777010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777010?ae"/>
<attribute name="FRES" value="195MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="3.7A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777010 "/>
<attribute name="RDC-MAX" value="38.5mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777022?ae"/>
<attribute name="FRES" value="95.2MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="5.25A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777022 "/>
<attribute name="RDC-MAX" value="61mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777033?ae"/>
<attribute name="FRES" value="87.5MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777033 "/>
<attribute name="RDC-MAX" value="70mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777047?ae"/>
<attribute name="FRES" value="64.7MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="2.35A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777047 "/>
<attribute name="RDC-MAX" value="84mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777068?ae"/>
<attribute name="FRES" value="47.3MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777068 "/>
<attribute name="RDC-MAX" value="98mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777082?ae"/>
<attribute name="FRES" value="36.7MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777082 "/>
<attribute name="RDC-MAX" value="117mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777100?ae"/>
<attribute name="FRES" value="32.5MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777100 "/>
<attribute name="RDC-MAX" value="126mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777101?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777101 "/>
<attribute name="RDC-MAX" value="470mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777102?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="0.25A"/>
<attribute name="ISAT" value="0.28A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777102 "/>
<attribute name="RDC-MAX" value="5750mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777220?ae"/>
<attribute name="FRES" value="18.5MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777220 "/>
<attribute name="RDC-MAX" value="215mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777221?ae"/>
<attribute name="FRES" value="3.9MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777221 "/>
<attribute name="RDC-MAX" value="1135mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777331?ae"/>
<attribute name="FRES" value="4.2MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="L" value="330uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777331 "/>
<attribute name="RDC-MAX" value="1872mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="330uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777470?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777470 "/>
<attribute name="RDC-MAX" value="300mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784777471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784777471?ae"/>
<attribute name="FRES" value="2.9MHz"/>
<attribute name="HEIGHT" value="4mm"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784777471 "/>
<attribute name="RDC-MAX" value="2720mOhm"/>
<attribute name="SIZE" value="7345"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_7332" prefix="L">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Very low self-losses at high switching frequency's
&lt;br&gt;Wide inductance spectrum available at all sizes
&lt;br&gt;Core Material: NiZn
&lt;br&gt;Wire connection: welding technology
&lt;br&gt;Automotive approved
&lt;br&gt;Size 1050: Operating temperature -50°C up to +150°C
&lt;br&gt;Size 7332, 7345, 1260: Operating temperature -40°C up to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with extremely high efficiency
&lt;br&gt;Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PDA
&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2026-01-20&lt;br&gt;
&lt;/b&gt;2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDA_7332">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784778010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778010?ae"/>
<attribute name="FRES" value="183.7MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="7A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778010 "/>
<attribute name="RDC-MAX" value="36mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778022?ae"/>
<attribute name="FRES" value="110.5MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778022 "/>
<attribute name="RDC-MAX" value="50mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778033?ae"/>
<attribute name="FRES" value="71.3MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="2.65A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778033 "/>
<attribute name="RDC-MAX" value="65mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778047?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778047 "/>
<attribute name="RDC-MAX" value="79mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778068?ae"/>
<attribute name="FRES" value="40.7MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778068 "/>
<attribute name="RDC-MAX" value="94mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778082?ae"/>
<attribute name="FRES" value="36.9MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778082 "/>
<attribute name="RDC-MAX" value="103mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778100?ae"/>
<attribute name="FRES" value="34.1MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="1.85A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778100 "/>
<attribute name="RDC-MAX" value="126mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778101?ae"/>
<attribute name="FRES" value="9.7MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778101 "/>
<attribute name="RDC-MAX" value="720mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778102?ae"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778102 "/>
<attribute name="RDC-MAX" value="7200mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778220?ae"/>
<attribute name="FRES" value="17.2MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778220 "/>
<attribute name="RDC-MAX" value="187mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778221?ae"/>
<attribute name="FRES" value="6.1MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.48A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778221 "/>
<attribute name="RDC-MAX" value="1620mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778470?ae"/>
<attribute name="FRES" value="13.5MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778470 "/>
<attribute name="RDC-MAX" value="348mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
<technology name="_784778471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784778471?ae"/>
<attribute name="FRES" value="3.9MHz"/>
<attribute name="HEIGHT" value="3.2mm"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="7.3mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784778471 "/>
<attribute name="RDC-MAX" value="3300mOhm"/>
<attribute name="SIZE" value="7332"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="7.3mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_1050" prefix="L">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Very low self-losses at high switching frequency's
&lt;br&gt;Wide inductance spectrum available at all sizes
&lt;br&gt;Core Material: NiZn
&lt;br&gt;Wire connection: welding technology
&lt;br&gt;Automotive approved
&lt;br&gt;Size 1050: Operating temperature -50°C up to +150°C
&lt;br&gt;Size 7332, 7345, 1260: Operating temperature -40°C up to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with extremely high efficiency
&lt;br&gt;Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PDA
&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2026-01-20&lt;br&gt;
&lt;/b&gt;2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDA_1050">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7847714033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714033?ae"/>
<attribute name="FRES" value="29MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="7.11A"/>
<attribute name="ISAT" value="9.4A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714033 "/>
<attribute name="RDC-MAX" value="15mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714047?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="6.81A"/>
<attribute name="ISAT" value="8.2A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714047 "/>
<attribute name="RDC-MAX" value="17mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714100?ae"/>
<attribute name="FRES" value="16.75MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="5.12A"/>
<attribute name="ISAT" value="5.6A"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714100 "/>
<attribute name="RDC-MAX" value="32mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714101?ae"/>
<attribute name="FRES" value="4.4MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="1.43A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714101 "/>
<attribute name="RDC-MAX" value="294mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714220?ae"/>
<attribute name="FRES" value="9.6MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="3.13A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714220 "/>
<attribute name="RDC-MAX" value="75mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714221?ae"/>
<attribute name="FRES" value="2.9MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="1.05A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714221 "/>
<attribute name="RDC-MAX" value="708mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714330?ae"/>
<attribute name="FRES" value="8.4MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="2.92A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714330 "/>
<attribute name="RDC-MAX" value="95mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714331?ae"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="330uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714331 "/>
<attribute name="RDC-MAX" value="900mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="330uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714470?ae"/>
<attribute name="FRES" value="6.4MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="2.26A"/>
<attribute name="ISAT" value="2.45A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714470 "/>
<attribute name="RDC-MAX" value="148mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
<technology name="_7847714680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847714680?ae"/>
<attribute name="FRES" value="5.53MHz"/>
<attribute name="HEIGHT" value="5mm"/>
<attribute name="IR" value="1.85A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="L" value="68uH"/>
<attribute name="LENGTH" value="10mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7847714680 "/>
<attribute name="RDC-MAX" value="176.4mOhm"/>
<attribute name="SIZE" value="1050"/>
<attribute name="VALUE" value="68uH"/>
<attribute name="WIDTH" value="10mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDA_1260" prefix="L">
<description>&lt;b&gt; WE-PDA SMD Shielded Power Inductor
&lt;br&gt;&lt;/B&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Magnetically shielded version which results in a low leakage field High storage capacity
&lt;br&gt;Very low self-losses at high switching frequency's
&lt;br&gt;Wide inductance spectrum available at all sizes
&lt;br&gt;Core Material: NiZn
&lt;br&gt;Wire connection: welding technology
&lt;br&gt;Automotive approved
&lt;br&gt;Size 1050: Operating temperature -50°C up to +150°C
&lt;br&gt;Size 7332, 7345, 1260: Operating temperature -40°C up to +125°C

&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Multimedia applications
&lt;br&gt;Switching regulators with low operating voltages
&lt;br&gt;Integrated DC/DC-converter
&lt;br&gt;Perfect suitable for switching regulators with extremely high efficiency
&lt;br&gt;Plastic base: Because of the one piece construction these are more suitable for high vibration or shock applications
&lt;br&gt;
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o55118v209%20family_IndPDA_78477_PCN.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PDA/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PDA
&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2026-01-20&lt;br&gt;
&lt;/b&gt;2026(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-PDA_1260">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_784771010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771010?ae"/>
<attribute name="FRES" value="139.4MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="16.5A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771010 "/>
<attribute name="RDC-MAX" value="8.5mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771022?ae"/>
<attribute name="FRES" value="82.7MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="L" value="2.2uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771022 "/>
<attribute name="RDC-MAX" value="12.5mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771033?ae"/>
<attribute name="FRES" value="68.1MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771033 "/>
<attribute name="RDC-MAX" value="14.5mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771047?ae"/>
<attribute name="FRES" value="49.8MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="L" value="4.7uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771047 "/>
<attribute name="RDC-MAX" value="17.5mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771068?ae"/>
<attribute name="FRES" value="25.5MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="L" value="6.8uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771068 "/>
<attribute name="RDC-MAX" value="21.5mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771082?ae"/>
<attribute name="FRES" value="25.2MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="5.05A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="L" value="8.2uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771082 "/>
<attribute name="RDC-MAX" value="24mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="8.2uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771100?ae"/>
<attribute name="FRES" value="22.3MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="5.25A"/>
<attribute name="L" value="10uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771100 "/>
<attribute name="RDC-MAX" value="26.5mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771101?ae"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L" value="100uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771101 "/>
<attribute name="RDC-MAX" value="174mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771102?ae"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.48A"/>
<attribute name="ISAT" value="0.53A"/>
<attribute name="L" value="1000uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771102 "/>
<attribute name="RDC-MAX" value="1705mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771220?ae"/>
<attribute name="FRES" value="14.9MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="L" value="22uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771220 "/>
<attribute name="RDC-MAX" value="40mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="22uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771221?ae"/>
<attribute name="FRES" value="3.9MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.99A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L" value="220uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771221 "/>
<attribute name="RDC-MAX" value="348mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771330?ae"/>
<attribute name="FRES" value="11.5MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="L" value="33uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771330 "/>
<attribute name="RDC-MAX" value="62.5mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="33uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771331?ae"/>
<attribute name="FRES" value="3.3MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="330uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771331 "/>
<attribute name="RDC-MAX" value="594mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="330uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771470?ae"/>
<attribute name="FRES" value="10.1MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="L" value="47uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771470 "/>
<attribute name="RDC-MAX" value="77mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="47uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771471?ae"/>
<attribute name="FRES" value="2.9MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="0.65A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="L" value="470uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771471 "/>
<attribute name="RDC-MAX" value="706mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="470uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
<technology name="_784771680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/784771680?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="HEIGHT" value="6mm"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="68uH"/>
<attribute name="LENGTH" value="12mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 784771680 "/>
<attribute name="RDC-MAX" value="138mOhm"/>
<attribute name="SIZE" value="1260"/>
<attribute name="VALUE" value="68uH"/>
<attribute name="WIDTH" value="12mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
