<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-PDF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PDF_1045">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PDF SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1045</description>
</package>
<package name="WE-PDF_1064">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PDF SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1064</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PDF_1045" prefix="L">
<description>&lt;b&gt;WE-PDF SMD Power Inductor
&lt;br&gt; 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt; Flat wire power inductor
&lt;br&gt; Advanced operating temperature: –40 °C up to +150 °C
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt; Low self-losses
&lt;br&gt; High saturation current
&lt;br&gt; Flat wire coil for lower losses at high frequency ranges
&lt;br&gt; High Self Resonance Frequency
&lt;br&gt; Recommended solder profile: Reflow
&lt;br&gt; 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for high frequency switching regulators
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14833v209%20Family_WE-PDF%20Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14833v209%20Family_WE-PDF%20Gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PDF?"&gt;https://katalog.we-online.com/en/pbs/WE-PDF?&lt;/a&gt;&lt;p&gt;


Updated  by  Yingchun,Shan 2019-07-31&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDF_1045">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447797022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797022.pdf"/>
<attribute name="FRES" value="328MHz"/>
<attribute name="IR" value="16A"/>
<attribute name="ISAT" value="32A"/>
<attribute name="PART-NUMBER" value="7447797022"/>
<attribute name="RDC-MAX" value="3.5mohm"/>
<attribute name="RDC-TYP" value="2.9mohm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_7447797050">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797050.pdf"/>
<attribute name="FRES" value="182MHz"/>
<attribute name="IR" value="13.2A"/>
<attribute name="ISAT" value="23A"/>
<attribute name="PART-NUMBER" value=" 7447797050 "/>
<attribute name="RDC-MAX" value="5mohm"/>
<attribute name="RDC-TYP" value="4.3mohm"/>
<attribute name="VALUE" value="0.5uH"/>
</technology>
<technology name="_7447797110">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797110.pdf"/>
<attribute name="FRES" value="116MHz"/>
<attribute name="IR" value="11.2A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="PART-NUMBER" value=" 7447797110 "/>
<attribute name="RDC-MAX" value="6.65mohm"/>
<attribute name="RDC-TYP" value="5.9mohm"/>
<attribute name="VALUE" value="1.1uH"/>
</technology>
<technology name="_7447797180">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797180.pdf"/>
<attribute name="FRES" value="86MHz"/>
<attribute name="IR" value="9.4A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="PART-NUMBER" value=" 7447797180 "/>
<attribute name="RDC-MAX" value="8.4mohm"/>
<attribute name="RDC-TYP" value="7.4mohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_7447797250">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797250.pdf"/>
<attribute name="FRES" value="61MHz"/>
<attribute name="IR" value="8.4A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="PART-NUMBER" value=" 7447797250 "/>
<attribute name="RDC-MAX" value="10.2mohm"/>
<attribute name="RDC-TYP" value="9mohm"/>
<attribute name="VALUE" value="2.5uH"/>
</technology>
<technology name="_7447797360">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797360.pdf"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="8.2A"/>
<attribute name="ISAT" value="8.5A"/>
<attribute name="PART-NUMBER" value=" 7447797360 "/>
<attribute name="RDC-MAX" value="12.2mohm"/>
<attribute name="RDC-TYP" value="10.8mohm"/>
<attribute name="VALUE" value="3.6uH"/>
</technology>
<technology name="_7447797470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797470.pdf"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="PART-NUMBER" value=" 7447797470 "/>
<attribute name="RDC-MAX" value="19.5mohm"/>
<attribute name="RDC-TYP" value="17.3mohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7447797620">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797620.pdf"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="5.7A"/>
<attribute name="ISAT" value="7.4A"/>
<attribute name="PART-NUMBER" value=" 7447797620 "/>
<attribute name="RDC-MAX" value="22.4mohm"/>
<attribute name="RDC-TYP" value="19.8mohm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_7447797820">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447797820.pdf"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="5.05A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="PART-NUMBER" value=" 7447797820 "/>
<attribute name="RDC-MAX" value="28.6mohm"/>
<attribute name="RDC-TYP" value="25.3mohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PDF_1064" prefix="L">
<description>&lt;b&gt;WE-PDF SMD Power Inductor
&lt;br&gt; 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt; Flat wire power inductor
&lt;br&gt; Advanced operating temperature: –40 °C up to +150 °C
&lt;br&gt; Magnetically shielded which results in a low leakage field
&lt;br&gt; Low self-losses
&lt;br&gt; High saturation current
&lt;br&gt; Flat wire coil for lower losses at high frequency ranges
&lt;br&gt; High Self Resonance Frequency
&lt;br&gt; Recommended solder profile: Reflow
&lt;br&gt; 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Suitable for high frequency switching regulators
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14833v209%20Family_WE-PDF%20Gruppe.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14833v209%20Family_WE-PDF%20Gruppe.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-PDF?"&gt;https://katalog.we-online.com/en/pbs/WE-PDF?&lt;/a&gt;&lt;p&gt;


Updated  by  Yingchun,Shan 2019-07-31&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PDF_1064">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447798022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798022.pdf"/>
<attribute name="FRES" value="337MHz"/>
<attribute name="IR" value="19A"/>
<attribute name="ISAT" value="20A"/>
<attribute name="PART-NUMBER" value=" 7447798022 "/>
<attribute name="RDC-MAX" value="1.95mOhm"/>
<attribute name="RDC-TYP" value="1.6mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_7447798050">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798050.pdf"/>
<attribute name="FRES" value="172MHz"/>
<attribute name="IR" value="18.5A"/>
<attribute name="ISAT" value="18A"/>
<attribute name="PART-NUMBER" value=" 7447798050 "/>
<attribute name="RDC-MAX" value="2.65mOhm"/>
<attribute name="RDC-TYP" value="2.2mOhm"/>
<attribute name="VALUE" value="0.5uH"/>
</technology>
<technology name="_7447798110">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798110.pdf"/>
<attribute name="FRES" value="104MHz"/>
<attribute name="IR" value="16.5A"/>
<attribute name="ISAT" value="16A"/>
<attribute name="PART-NUMBER" value=" 7447798110 "/>
<attribute name="RDC-MAX" value="3.5mOhm"/>
<attribute name="RDC-TYP" value="3mOhm"/>
<attribute name="VALUE" value="1.1uH"/>
</technology>
<technology name="_7447798111">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798111.pdf"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="6.9A"/>
<attribute name="ISAT" value="5.3A"/>
<attribute name="PART-NUMBER" value=" 7447798111 "/>
<attribute name="RDC-MAX" value="15.8mOhm"/>
<attribute name="RDC-TYP" value="14mOhm"/>
<attribute name="VALUE" value="11uH"/>
</technology>
<technology name="_7447798131">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798131.pdf"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="5.85A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="PART-NUMBER" value=" 7447798131 "/>
<attribute name="RDC-MAX" value="22.5mOhm"/>
<attribute name="RDC-TYP" value="19.9mOhm"/>
<attribute name="VALUE" value="13uH"/>
</technology>
<technology name="_7447798151">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798151.pdf"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="5.45A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 7447798151 "/>
<attribute name="RDC-MAX" value="25.8mOhm"/>
<attribute name="RDC-TYP" value="21.8mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7447798180">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798180.pdf"/>
<attribute name="FRES" value="74MHz"/>
<attribute name="IR" value="14.5A"/>
<attribute name="ISAT" value="12.8A"/>
<attribute name="PART-NUMBER" value=" 7447798180 "/>
<attribute name="RDC-MAX" value="4.5mOhm"/>
<attribute name="RDC-TYP" value="3.8mOhm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_7447798181">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798181.pdf"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="PART-NUMBER" value=" 7447798181 "/>
<attribute name="RDC-MAX" value="34.4mOhm"/>
<attribute name="RDC-TYP" value="30.5mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7447798221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798221.pdf"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="4.7A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="PART-NUMBER" value=" 7447798221 "/>
<attribute name="RDC-MAX" value="37.3mOhm"/>
<attribute name="RDC-TYP" value="33mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_7447798241">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798241.pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="3.25A"/>
<attribute name="PART-NUMBER" value=" 7447798241 "/>
<attribute name="RDC-MAX" value="39.5mOhm"/>
<attribute name="RDC-TYP" value="35mOhm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
<technology name="_7447798250">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798250.pdf"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="IR" value="13.7A"/>
<attribute name="ISAT" value="10.1A"/>
<attribute name="PART-NUMBER" value=" 7447798250 "/>
<attribute name="RDC-MAX" value="4.95mOhm"/>
<attribute name="RDC-TYP" value="4.4mOhm"/>
<attribute name="VALUE" value="2.5uH"/>
</technology>
<technology name="_7447798271">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798271.pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="PART-NUMBER" value=" 7447798271 "/>
<attribute name="RDC-MAX" value="42.5mOhm"/>
<attribute name="RDC-TYP" value="37.6mOhm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_7447798360">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798360.pdf"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="ISAT" value="8.6A"/>
<attribute name="PART-NUMBER" value=" 7447798360 "/>
<attribute name="RDC-MAX" value="5.95mOhm"/>
<attribute name="RDC-TYP" value="5.25mOhm"/>
<attribute name="VALUE" value="3.6uH"/>
</technology>
<technology name="_7447798470">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798470.pdf"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="ISAT" value="7.6A"/>
<attribute name="PART-NUMBER" value=" 7447798470 "/>
<attribute name="RDC-MAX" value="8.4mOhm"/>
<attribute name="RDC-TYP" value="7.4mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7447798620">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798620.pdf"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="9.4A"/>
<attribute name="ISAT" value="6.7A"/>
<attribute name="PART-NUMBER" value=" 7447798620 "/>
<attribute name="RDC-MAX" value="9.5mOhm"/>
<attribute name="RDC-TYP" value="8.4mOhm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_7447798720">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798720.pdf"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="7.9A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 7447798720 "/>
<attribute name="RDC-MAX" value="12.8mOhm"/>
<attribute name="RDC-TYP" value="11.3mOhm"/>
<attribute name="VALUE" value="7.2uH"/>
</technology>
<technology name="_7447798910">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7447798910.pdf"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="7.35A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="PART-NUMBER" value=" 7447798910 "/>
<attribute name="RDC-MAX" value="14.35mOhm"/>
<attribute name="RDC-TYP" value="12.7mOhm"/>
<attribute name="VALUE" value="9.1uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
