<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.7.0">
<drawing>
<library>
<description>Würth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-PMFI

Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, 
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. 
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. 
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. 

Please contact us for more information: libraries@we-online.com 

Würth Elektronik eiSos GmbH &amp; Co. KG
EMC &amp; Inductive Solutions
www.we-online.com

Fusion360, Library Revision 2026a, 2026-07-13
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PMFI_201610">
<description>WE-PMFI Power Molded Flatwire Inductor

201610, SMT, 2pins
LXWXH=2X1.6X1mm</description>
</package>
<package name="WE-PMFI_201610_LP2">
<description>WE-PMFI Power Molded Flatwire Inductor

201610, SMT, 2pins
LXWXH=2X1.6X1mm

This Land Pattern is compatible with the WE-PMCI series</description>
</package>
<package name="WE-PMFI_322512_LP2">
<description>WE-PMFI Power Molded Flatwire Inductor

322512, SMT, 2pins
LXWXH=3.2X2.5X1.2mm

This Land Pattern is compatible with the WE-PMCI series</description>
</package>
<package name="WE-PMFI_322512">
<description>WE-PMFI Power Molded Flatwire Inductor

322512, SMT, 2pins
LXWXH=3.2X2.5X1.2mm</description>
</package>
<package name="WE-PMFI_252012">
<description>WE-PMFI Power Molded Flatwire Inductor

252012, SMT, 2pins
LXWXH=2.5X2X1.2mm</description>
</package>
<package name="WE-PMFI_252012_LP2">
<description>WE-PMFI Power Molded Flatwire Inductor

252012, SMT, 2pins
LXWXH=2.5X2X1.2mm

This Land Pattern is compatible with the WE-PMCI series</description>
</package>
<package name="WE-PMFI_353220">
<description>WE-PMFI Power Molded Flatwire Inductor

353220, SMT, 2pins
LXWXH=3.5X3.2X2mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PMFI_201610" prefix="L">
<description>WE-PMFI Power Molded Flatwire Inductor

Characteristics
Very small profile molded power inductor
High range of inductance values due to inner core construction
Flat wire technology decreases RDC, starting at 4.8 mΩ
High rated current values due to low RDC, up to 16 A
Very low total losses lead to a high efficiency
Hohe Betriebstemperatur von -55°C bis +150°C
AEC-Q 200 qualified

Applications
DC/DC-converters for high current power supplies
Wearables like smartphones, tablets and cameras
CPU power supllies (IMX95)
RAM power supplies (DDR5)
Devices with low profiles and case sizes (Sensors)
Battery powered devices
High frequency devices (GaN and SiC)

Details see: www.we-online.com/en/components/products/WE-PMFI

Updated by Ella 2025-07-01
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_201610">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479320165110">
<attribute name="FRES" value="325 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="10.2 A"/>
<attribute name="ISAT" value="13.7 A"/>
<attribute name="L" value="0.1 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165110"/>
<attribute name="RDC-TYP" value="7.2 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165110?ae"/>
</technology>
<technology name="_74479320165147">
<attribute name="FRES" value="100 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="6.2 A"/>
<attribute name="ISAT" value="7.5 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165147"/>
<attribute name="RDC-TYP" value="18.4 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165147?ae"/>
</technology>
<technology name="_74479320165210">
<attribute name="FRES" value="67 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="4.7 A"/>
<attribute name="ISAT" value="5.25 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165210"/>
<attribute name="RDC-TYP" value="31.7 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165210?ae"/>
</technology>
<technology name="_74479320165222">
<attribute name="FRES" value="51 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.75 A"/>
<attribute name="ISAT" value="3.9 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165222"/>
<attribute name="RDC-TYP" value="81.9 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165222?ae"/>
</technology>
<technology name="_74479320165233">
<attribute name="FRES" value="35 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1 A"/>
<attribute name="ISAT" value="2.25 A"/>
<attribute name="L" value="3.3 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165233"/>
<attribute name="RDC-TYP" value="146 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165233?ae"/>
</technology>
<technology name="_74479320165247">
<attribute name="FRES" value="30 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1 A"/>
<attribute name="ISAT" value="2 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165247"/>
<attribute name="RDC-TYP" value="195 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165247?ae"/>
</technology>
</technologies>
</device>
<device name="_LP2" package="WE-PMFI_201610_LP2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479320165110">
<attribute name="FRES" value="325 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="10.2 A"/>
<attribute name="ISAT" value="13.7 A"/>
<attribute name="L" value="0.1 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165110"/>
<attribute name="RDC-TYP" value="7.2 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165110?ae"/>
</technology>
<technology name="_74479320165147">
<attribute name="FRES" value="100 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="6.2 A"/>
<attribute name="ISAT" value="7.5 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165147"/>
<attribute name="RDC-TYP" value="18.4 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165147?ae"/>
</technology>
<technology name="_74479320165210">
<attribute name="FRES" value="67 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="4.7 A"/>
<attribute name="ISAT" value="5.25 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165210"/>
<attribute name="RDC-TYP" value="31.7 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165210?ae"/>
</technology>
<technology name="_74479320165222">
<attribute name="FRES" value="51 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.75 A"/>
<attribute name="ISAT" value="3.9 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165222"/>
<attribute name="RDC-TYP" value="81.9 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165222?ae"/>
</technology>
<technology name="_74479320165233">
<attribute name="FRES" value="35 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1 A"/>
<attribute name="ISAT" value="2.25 A"/>
<attribute name="L" value="3.3 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165233"/>
<attribute name="RDC-TYP" value="146 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="3.3 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165233?ae"/>
</technology>
<technology name="_74479320165247">
<attribute name="FRES" value="30 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="2.1 A"/>
<attribute name="ISAT" value="2 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165247"/>
<attribute name="RDC-TYP" value="195 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165247?ae"/>
</technology>
<technology name="_74479320165168">
<attribute name="FRES" value="90 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR" value="5.5 A"/>
<attribute name="ISAT" value="5.7 A"/>
<attribute name="L" value="0.68 uH"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479320165168"/>
<attribute name="RDC-TYP" value="24.8 mohm"/>
<attribute name="SIZE" value="201610"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="1.6mm"/>
<attribute name="VALUE" value="0.68 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479320165168?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMFI_322512" prefix="L">
<description>WE-PMFI Power Molded Flatwire Inductor

Characteristics
Very small profile molded power inductor
High range of inductance values due to inner core construction
Flat wire technology decreases RDC, starting at 4.8 mΩ
High rated current values due to low RDC, up to 16 A
Very low total losses lead to a high efficiency
Hohe Betriebstemperatur von -55°C bis +150°C
AEC-Q 200 qualified

Applications
DC/DC-converters for high current power supplies
Wearables like smartphones, tablets and cameras
CPU power supllies (IMX95)
RAM power supplies (DDR5)
Devices with low profiles and case sizes (Sensors)
Battery powered devices
High frequency devices (GaN and SiC)

Details see: www.we-online.com/en/components/products/WE-PMFI


Updated by Ella 2025-07-01
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_322512">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479332257110">
<attribute name="FRES" value="405 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="11.4 A"/>
<attribute name="ISAT" value="21.5 A"/>
<attribute name="L" value="0.1 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257110"/>
<attribute name="RDC-TYP" value="7.4 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257110?ae"/>
</technology>
<technology name="_74479332257147">
<attribute name="FRES" value="126 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="7.9 A"/>
<attribute name="ISAT" value="10.6 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257147"/>
<attribute name="RDC-TYP" value="14.2 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257147?ae"/>
</technology>
<technology name="_74479332257210">
<attribute name="FRES" value="67 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="5.8 A"/>
<attribute name="ISAT" value="9.15 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257210"/>
<attribute name="RDC-TYP" value="23.3 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257210?ae"/>
</technology>
<technology name="_74479332257222">
<attribute name="FRES" value="44 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4.1 A"/>
<attribute name="ISAT" value="5.4 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257222"/>
<attribute name="RDC-TYP" value="49.6 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257222?ae"/>
</technology>
<technology name="_74479332257247">
<attribute name="FRES" value="25 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.7 A"/>
<attribute name="ISAT" value="4 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257247"/>
<attribute name="RDC-TYP" value="107 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257247?ae"/>
</technology>
</technologies>
</device>
<device name="_LP2" package="WE-PMFI_322512_LP2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479332257110">
<attribute name="FRES" value="405 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="11.4 A"/>
<attribute name="ISAT" value="21.5 A"/>
<attribute name="L" value="0.1 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257110"/>
<attribute name="RDC-TYP" value="7.4 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257110?ae"/>
</technology>
<technology name="_74479332257147">
<attribute name="FRES" value="126 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="7.9 A"/>
<attribute name="ISAT" value="10.6 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257147"/>
<attribute name="RDC-TYP" value="14.2 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257147?ae"/>
</technology>
<technology name="_74479332257210">
<attribute name="FRES" value="67 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="5.8 A"/>
<attribute name="ISAT" value="9.15 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257210"/>
<attribute name="RDC-TYP" value="23.3 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257210?ae"/>
</technology>
<technology name="_74479332257222">
<attribute name="FRES" value="44 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4.1 A"/>
<attribute name="ISAT" value="5.4 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257222"/>
<attribute name="RDC-TYP" value="49.6 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257222?ae"/>
</technology>
<technology name="_74479332257247">
<attribute name="FRES" value="25 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.7 A"/>
<attribute name="ISAT" value="4 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479332257247"/>
<attribute name="RDC-TYP" value="107 mohm"/>
<attribute name="SIZE" value="322512"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2.5mm"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479332257247?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMFI_252012" prefix="L">
<description>WE-PMFI Power Molded Flatwire Inductor

Characteristics
Very small profile molded power inductor
High range of inductance values due to inner core construction
Flat wire technology decreases RDC, starting at 4.8 mΩ
High rated current values due to low RDC, up to 16 A
Very low total losses lead to a high efficiency
Hohe Betriebstemperatur von -55°C bis +150°C
AEC-Q 200 qualified

Applications
DC/DC-converters for high current power supplies
Wearables like smartphones, tablets and cameras
CPU power supllies (IMX95)
RAM power supplies (DDR5)
Devices with low profiles and case sizes (Sensors)
Battery powered devices
High frequency devices (GaN and SiC)

Details see: www.we-online.com/en/components/products/WE-PMFI

Updated by Ella 2025-10-29
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_252012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479325207110">
<attribute name="FRES" value="438 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="12.3 A"/>
<attribute name="ISAT" value="18.7 A"/>
<attribute name="L" value="0.1 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207110"/>
<attribute name="RDC-TYP" value="5.6 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207110?ae"/>
</technology>
<technology name="_74479325207124">
<attribute name="FRES" value="166MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="9A"/>
<attribute name="ISAT" value="11.5A"/>
<attribute name="L" value="0.24uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMD/SMT Soldering"/>
<attribute name="PART-NUMBER" value="74479325207124"/>
<attribute name="RDC-TYP" value="11.1mOhm"/>
<attribute name="SIZE" value=" 252012 "/>
<attribute name="VOP" value="48V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="0.24uH"/>
<attribute name="DATASHEET" value=""/>
</technology>
<technology name="_74479325207147">
<attribute name="FRES" value="97 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="9.3 A"/>
<attribute name="ISAT" value="7.9 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207147"/>
<attribute name="RDC-TYP" value="11.3 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207147?ae"/>
</technology>
<technology name="_74479325207210">
<attribute name="FRES" value="58 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="6.1 A"/>
<attribute name="ISAT" value="6.1 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207210"/>
<attribute name="RDC-TYP" value="23.8 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207210?ae"/>
</technology>
<technology name="_74479325207222">
<attribute name="FRES" value="39 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4 A"/>
<attribute name="ISAT" value="4.5 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207222"/>
<attribute name="RDC-TYP" value="50.1 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207222?ae"/>
</technology>
<technology name="_74479325207247">
<attribute name="FRES" value="25 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.75 A"/>
<attribute name="ISAT" value="2.7 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207247"/>
<attribute name="RDC-TYP" value="114 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207247?ae"/>
</technology>
</technologies>
</device>
<device name="_LP2" package="WE-PMFI_252012_LP2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479325207110">
<attribute name="FRES" value="438 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="12.3 A"/>
<attribute name="ISAT" value="18.7 A"/>
<attribute name="L" value="0.1 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207110"/>
<attribute name="RDC-TYP" value="5.6 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207110?ae"/>
</technology>
<technology name="_74479325207124">
<attribute name="FRES" value="166 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="9 A"/>
<attribute name="ISAT" value="11.5 A"/>
<attribute name="L" value="0.24 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207124"/>
<attribute name="RDC-TYP" value="11.1 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="0.24 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207124?ae"/>
</technology>
<technology name="_74479325207147">
<attribute name="FRES" value="97 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="9.3 A"/>
<attribute name="ISAT" value="7.9 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207147"/>
<attribute name="RDC-TYP" value="11.3 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207147?ae"/>
</technology>
<technology name="_74479325207210">
<attribute name="FRES" value="58 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="6.1 A"/>
<attribute name="ISAT" value="6.1 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207210"/>
<attribute name="RDC-TYP" value="23.8 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207210?ae"/>
</technology>
<technology name="_74479325207222">
<attribute name="FRES" value="39 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4 A"/>
<attribute name="ISAT" value="4.5 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207222"/>
<attribute name="RDC-TYP" value="50.1 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207222?ae"/>
</technology>
<technology name="_74479325207247">
<attribute name="FRES" value="25 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="2.75 A"/>
<attribute name="ISAT" value="2.7 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207247"/>
<attribute name="RDC-TYP" value="114 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207247?ae"/>
</technology>
<technology name="_74479325207215">
<attribute name="FRES" value="46 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR" value="4.6 A"/>
<attribute name="ISAT" value="5.25 A"/>
<attribute name="L" value="1.5 uH"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479325207215"/>
<attribute name="RDC-TYP" value="37.3 mohm"/>
<attribute name="SIZE" value="252012"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="2mm"/>
<attribute name="VALUE" value="1.5 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479325207215?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMFI_353220" prefix="L">
<description>WE-PMFI Power Molded Flatwire Inductor

Characteristics
Very small profile molded power inductor
High range of inductance values due to inner core construction
Flat wire technology decreases RDC, starting at 4.8 mΩ
High rated current values due to low RDC, up to 16 A
Very low total losses lead to a high efficiency
Hohe Betriebstemperatur von -55°C bis +150°C
AEC-Q 200 qualified

Applications
DC/DC-converters for high current power supplies
Wearables like smartphones, tablets and cameras
CPU power supllies (IMX95)
RAM power supplies (DDR5)
Devices with low profiles and case sizes (Sensors)
Battery powered devices
High frequency devices (GaN and SiC)

Details see: www.we-online.com/en/components/products/WE-PMFI

Updated by Ella 2025-07-01
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-PMFI_353220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479335329110">
<attribute name="FRES" value="310 MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="16 A"/>
<attribute name="ISAT" value="25 A"/>
<attribute name="L" value="0.1 uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479335329110"/>
<attribute name="RDC-TYP" value="4.8 mohm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="VALUE" value="0.1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479335329110?ae"/>
</technology>
<technology name="_74479335329147">
<attribute name="FRES" value="92 MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="9.9 A"/>
<attribute name="ISAT" value="13.2 A"/>
<attribute name="L" value="0.47 uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479335329147"/>
<attribute name="RDC-TYP" value="12.7 mohm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="VALUE" value="0.47 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479335329147?ae"/>
</technology>
<technology name="_74479335329210">
<attribute name="FRES" value="56 MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="7.3 A"/>
<attribute name="ISAT" value="10.8 A"/>
<attribute name="L" value="1 uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479335329210"/>
<attribute name="RDC-TYP" value="18.4 mohm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="VALUE" value="1 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479335329210?ae"/>
</technology>
<technology name="_74479335329222">
<attribute name="FRES" value="31 MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="5.8 A"/>
<attribute name="ISAT" value="7.8 A"/>
<attribute name="L" value="2.2 uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479335329222"/>
<attribute name="RDC-TYP" value="31.6 mohm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="VALUE" value="2.2 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479335329222?ae"/>
</technology>
<technology name="_74479335329247">
<attribute name="FRES" value="21 MHz"/>
<attribute name="HEIGHT" value="2mm"/>
<attribute name="IR" value="3.85 A"/>
<attribute name="ISAT" value="5.6 A"/>
<attribute name="L" value="4.7 uH"/>
<attribute name="LENGTH" value="3.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="74479335329247"/>
<attribute name="RDC-TYP" value="63.2 mohm"/>
<attribute name="SIZE" value="353220"/>
<attribute name="VOP" value="48 V"/>
<attribute name="WIDTH" value="3.2mm"/>
<attribute name="VALUE" value="4.7 uH"/>
<attribute name="DATASHEET" value="https://www.we-online.com/redexpert/spec/74479335329247?ae"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
