<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-PMI&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-11-16&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-PMI_1008_H1.2">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2.5mmX2mmX1.2mm</description>
</package>
<package name="WE-PMI_0805_H0.5">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.25mmX0.5mm</description>
</package>
<package name="WE-PMI_1008_H0.8">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2.5mmX2mmX0.8mm</description>
</package>
<package name="WE-PMI_0603_H0.8">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0603, SMT 2pins
&lt;br&gt;L X W X H=1.6mmX0.8mmX1mm</description>
</package>
<package name="WE-PMI_1008_H1">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2.5mmX2mmX1mm</description>
</package>
<package name="WE-PMI_0603_H0.5">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0603, SMT 2pins
&lt;br&gt;L X W X H=1.6mmX0.8mmX0.5mm</description>
</package>
<package name="WE-PMI_0805_H1">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.2mmX1mm</description>
</package>
<package name="WE-PMI_0806_H1">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0806, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.6mmX1mm</description>
</package>
<package name="WE-PMI_0806_H1.1">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0806, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.6mmX1.1mm</description>
</package>
<package name="WE-PMI_0805_H1.25">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor&lt;/b&gt;
&lt;br&gt;&lt;br&gt;Size:0805, SMT 2pins
&lt;br&gt;L X W X H=2mmX1.25mmX1.2mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-PMI_1008" prefix="L">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;Suitable for applications with high currents up to 2.7 A
&lt;br&gt;Smallest RDC-Values starting at 7 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow
&lt;br&gt;4 sizes and 3 different types available (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1MHz
&lt;br&gt;Electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-16&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H1" package="WE-PMI_1008_H1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479787147B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787147B?ae"/>
<attribute name="FRES" value="105MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="2.7A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787147B"/>
<attribute name="Q" value="18"/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787210A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787210A?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.7A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787210A"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="92.95mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787210B">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787210B?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.95A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787210B"/>
<attribute name="Q" value="23"/>
<attribute name="RDC" value="75mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787215A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787215A?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.9A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787215A"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="87.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787222A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787222A?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.8A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787222A"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="106.25mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787233A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787233A?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.6A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787233A"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="125mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479787247A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479787247A?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.5A"/>
<attribute name="ISAT" value="0.27A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479787247A"/>
<attribute name="Q" value="32"/>
<attribute name="RDC" value="137.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887124C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887124C?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="3.8A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887124C"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="0.24uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887147C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887147C?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="2.8A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887147C"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887210C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887210C?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="2.5A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887210C"/>
<attribute name="Q" value="17"/>
<attribute name="RDC" value="68.75mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887222A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887222A?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.35A"/>
<attribute name="ISAT" value="0.825A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887222A"/>
<attribute name="Q" value="20"/>
<attribute name="RDC" value="140mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887222C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887222C?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.6A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887222C"/>
<attribute name="Q" value="20"/>
<attribute name="RDC" value="137.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887233A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887233A?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.15A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887233A"/>
<attribute name="Q" value="20"/>
<attribute name="RDC" value="180mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887247A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887247A?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887247A"/>
<attribute name="Q" value="23"/>
<attribute name="RDC" value="230mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887268A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887268A?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="0.95A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887268A"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479887310A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479887310A?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="0.85A"/>
<attribute name="ISAT" value="0.125A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479887310A"/>
<attribute name="Q" value="27"/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479888222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479888222?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479888222"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479888233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479888233?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479888233"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="312.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479888247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479888247?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479888247"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="475mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479888268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479888268?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479888268"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="562.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479888310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479888310?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479888310"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="625mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
<device name="_H1.2" package="WE-PMI_1008_H1.2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479889210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889210?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="2A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889210"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="106.25mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889222?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889222"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="312.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889233?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889233"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="312.5mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889247?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889247"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889268?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889268"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="625mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_74479889310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479889310?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="PART-NUMBER" value="74479889310"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="625mOhm"/>
<attribute name="SIZE" value="1008"/>
<attribute name="TYPE" value="High Saturation Current"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_0603" prefix="L">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;Suitable for applications with high currents up to 2.7 A
&lt;br&gt;Smallest RDC-Values starting at 7 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow
&lt;br&gt;4 sizes and 3 different types available (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1MHz
&lt;br&gt;Electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-16&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H0.5" package="WE-PMI_0603_H0.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479762122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479762122?ae"/>
<attribute name="FRES" value="250MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value=" 74479762122 "/>
<attribute name="Q" value="7"/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.22uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479762133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479762133?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479762133"/>
<attribute name="Q" value="7"/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
<device name="_H0.8" package="WE-PMI_0603_H0.8">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479762168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479762168?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="1A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479762168"/>
<attribute name="Q" value="9"/>
<attribute name="RDC" value="275mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763147A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763147A?ae"/>
<attribute name="FRES" value="190MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="1.5A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763147A"/>
<attribute name="Q" value="10"/>
<attribute name="RDC" value="112.5mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763168?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="1A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763168"/>
<attribute name="Q" value="10"/>
<attribute name="RDC" value="225mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763210A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763210A?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763210A"/>
<attribute name="Q" value="12"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763215?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="0.85A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763215"/>
<attribute name="Q" value="12"/>
<attribute name="RDC" value="287.5mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
<technology name="_74479763222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479763222?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="ISAT" value="0.28A"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="PART-NUMBER" value="74479763222"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="375mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="0.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_0805" prefix="L">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;Suitable for applications with high currents up to 2.7 A
&lt;br&gt;Smallest RDC-Values starting at 7 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow
&lt;br&gt;4 sizes and 3 different types available (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1MHz
&lt;br&gt;Electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-16&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H0.5" package="WE-PMI_0805_H0.5">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479773133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479773133?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479773133"/>
<attribute name="Q" value="8"/>
<attribute name="RDC" value="125mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.33uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479773147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479773147?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479773147"/>
<attribute name="Q" value="10"/>
<attribute name="RDC" value="125mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479773154">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479773154?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479773154"/>
<attribute name="Q" value="10"/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.54uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479773210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479773210?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479773210"/>
<attribute name="Q" value="14"/>
<attribute name="RDC" value="225mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479774147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479774147?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479774147"/>
<attribute name="Q" value="8"/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479774210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479774210?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479774210"/>
<attribute name="Q" value="12"/>
<attribute name="RDC" value="237.5mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479774215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479774215?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479774215"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="325mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479774222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479774222?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="0.5mm"/>
<attribute name="IR1" value="0.7A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479774222"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="425mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low Profile"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
</technologies>
</device>
<device name="_H1" package="WE-PMI_0805_H1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479775147A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775147A?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775147A"/>
<attribute name="Q" value="10"/>
<attribute name="RDC" value="125mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775210A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775210A?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775210A"/>
<attribute name="Q" value="18"/>
<attribute name="RDC" value="137.5mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775215?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775215"/>
<attribute name="Q" value="20"/>
<attribute name="RDC" value="200mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775222A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775222A?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775222A"/>
<attribute name="Q" value="23"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775233?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1A"/>
<attribute name="ISAT" value="0.28A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775233"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479775247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479775247?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="0.85A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479775247"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="312.5mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479875210C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479875210C?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.6A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479875210C"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="143.75mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479875222C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479875222C?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479875222C"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="175mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
</technologies>
</device>
<device name="_H1.25" package="WE-PMI_0805_H1.25">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479777268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479777268?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479777268"/>
<attribute name="Q" value="17"/>
<attribute name="RDC" value="375mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479777310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479777310?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="IR1" value="0.65A"/>
<attribute name="ISAT" value="0.125A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479777310"/>
<attribute name="Q" value="35"/>
<attribute name="RDC" value="625mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
<technology name="_74479777310A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479777310A?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="HEIGHT" value="1.25mm"/>
<attribute name="IR1" value="0.9A"/>
<attribute name="ISAT" value="0.12A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479777310A"/>
<attribute name="Q" value="20"/>
<attribute name="RDC" value="375mOhm"/>
<attribute name="SIZE" value="0805"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="1.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-PMI_0806" prefix="L">
<description>&lt;b&gt;WE-PMI Power Multilayer Inductor
&lt;br&gt;Shielded
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Compact multilayer type
&lt;br&gt;Suitable for applications with high currents up to 2.7 A
&lt;br&gt;Smallest RDC-Values starting at 7 mΩ
&lt;br&gt;Magnetically shielded construction: No crosstalk
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Recommended soldering profile: Reflow
&lt;br&gt;4 sizes and 3 different types available (Low Profile, Low RDC &amp; High Saturation Current)
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; DC/DC converters especially at high switching frequencies &gt; 1MHz
&lt;br&gt;Electronic devices with very low profile
&lt;br&gt;Portable devices like Smart Phones, Tablets, Notebooks and Digital Cameras
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14838v209%20Family_WE-PMI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-PMI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-PMI&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-11-16&lt;br&gt;
2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_H1" package="WE-PMI_0806_H1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479776147">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479776147?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.6A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479776147"/>
<attribute name="Q" value="10"/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479776210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479776210?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.4A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479776210"/>
<attribute name="Q" value="18"/>
<attribute name="RDC" value="112.5mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479776215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479776215?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479776215"/>
<attribute name="Q" value="18"/>
<attribute name="RDC" value="137.5mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479776222A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479776222A?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479776222A"/>
<attribute name="Q" value="22"/>
<attribute name="RDC" value="137.5mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479776233A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479776233A?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.25A"/>
<attribute name="ISAT" value="0.33A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479776233A"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="156mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="3.3uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479776247A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479776247A?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479776247A"/>
<attribute name="Q" value="20"/>
<attribute name="RDC" value="221mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="4.7uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479876124C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479876124C?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="3.2A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479876124C"/>
<attribute name="Q" value="12"/>
<attribute name="RDC" value="32.5mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="0.24uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479876147C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479876147C?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="2.6A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479876147C"/>
<attribute name="Q" value="13"/>
<attribute name="RDC" value="55mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="0.47uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479876168C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479876168C?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="2A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479876168C"/>
<attribute name="Q" value="14"/>
<attribute name="RDC" value="85mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="0.68uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479876210C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479876210C?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.8A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479876210C"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="93.75mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="1uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479876215C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479876215C?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.5A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479876215C"/>
<attribute name="Q" value="15"/>
<attribute name="RDC" value="143.75mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="1.5uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479876222C">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479876222C?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479876222C"/>
<attribute name="Q" value="16"/>
<attribute name="RDC" value="262.5mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC &amp; High Saturation Current"/>
<attribute name="VALUE" value="2.2uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
<device name="_H1.1" package="WE-PMI_0806_H1.1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74479778268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479778268?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR1" value="1.2A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479778268"/>
<attribute name="Q" value="20"/>
<attribute name="RDC" value="212.5mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="6.8uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_74479778310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74479778310?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="IR1" value="1A"/>
<attribute name="ISAT" value="0.15A"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="PART-NUMBER" value="74479778310"/>
<attribute name="Q" value="25"/>
<attribute name="RDC" value="312.5mOhm"/>
<attribute name="SIZE" value="0806"/>
<attribute name="TYPE" value="Low RDC"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
