<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Transformers For DC/DC Converter - WE-POEH&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-POEH_EPQ13">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-PoEH Power over Ethernet High Power Transformer&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;EPQ13 SMD 10Pin</description>
</package>
</packages>
<symbols>
<symbol name="WE-POEH">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="6" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-POEH_EPQ13" prefix="T">
<description>&lt;b&gt;WE-PoEH Power over Ethernet High Power Transformer
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; DFlyback or Forward Transformer
&lt;br&gt;Input voltage: 9 V or 33 V to 57 V
&lt;br&gt;Switching frequencies: 200-400 kHz
&lt;br&gt;Operating temperature: -40°C up to +125°C
&lt;br&gt;Insulation test voltage: 1.5 kVAC
&lt;br&gt;Different output voltages available
&lt;br&gt;Optimized core and bobbin design for 30% more power handling
&lt;br&gt;Standard footprint to EP13

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; PoE and PoE+ powered devices
&lt;br&gt;Telecom
&lt;br&gt;Industrial applications
&lt;br&gt;WLAN acess point
&lt;br&gt;Safety cameras

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; The "VALUE"shown for symbol and pakaging is the Output Voltage 1 Output Current 1.&lt;/b&gt; &lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14841v209%20Family_WE-PoEH.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14841v209%20Family_WE-PoEH.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-POEH"&gt;https://katalog.we-online.com/en/pbs/WE-POEH&lt;/a&gt;&lt;p&gt;
&lt;br&gt;
&lt;br&gt;Updated by Yingchun,Shan 2019-08-20
&lt;br&gt;

&lt;br&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-POEH"/>
</gates>
<devices>
<device name="" package="WE-POEH_EPQ13">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="4"/>
<connect gate="G$1" pin="4" pad="5"/>
<connect gate="G$1" pin="5" pad="7"/>
<connect gate="G$1" pin="6" pad="10"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="9"/>
</connects>
<technologies>
<technology name="_7491195112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491195112.pdf"/>
<attribute name="IO2" value="1,5A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="L1" value="41uH"/>
<attribute name="LSMIN" value="0.5uH"/>
<attribute name="N" value="2.67:1:1:1"/>
<attribute name="PART-NUMBER" value=" 7491195112 "/>
<attribute name="VALUE" value="12V 1,5A"/>
<attribute name="VAUX" value="12V"/>
<attribute name="VI" value="33-57V(DC)"/>
<attribute name="VO2" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491195212">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491195212.pdf"/>
<attribute name="IO2" value="1A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="L1" value="21uH"/>
<attribute name="LSMIN" value="0.3uH"/>
<attribute name="N" value="1.33:1:1:0.89"/>
<attribute name="PART-NUMBER" value=" 7491195212 "/>
<attribute name="VALUE" value="12V 1A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="9-57V(DC)"/>
<attribute name="VO2" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491195224">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491195224.pdf"/>
<attribute name="IO2" value="0,5A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="L1" value="21uH"/>
<attribute name="LSMIN" value="0.3uH"/>
<attribute name="N" value="0,67:1:1:0.89"/>
<attribute name="PART-NUMBER" value=" 7491195224 "/>
<attribute name="VALUE" value="24V 0,5A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="9-57V(DC)"/>
<attribute name="VO2" value="24V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749119533">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749119533.pdf"/>
<attribute name="IO2" value="3.5A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L1" value="54uH"/>
<attribute name="LSMIN" value="0.8uH"/>
<attribute name="N" value="8:1:1:3"/>
<attribute name="PART-NUMBER" value=" 749119533 "/>
<attribute name="VALUE" value="3.3V 3.5A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="33-57V(DC)"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491195331">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491195331.pdf"/>
<attribute name="IO2" value="3.2A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="L1" value="21uH"/>
<attribute name="LSMIN" value="0.3uH"/>
<attribute name="N" value="4:1:1:3"/>
<attribute name="PART-NUMBER" value=" 7491195331 "/>
<attribute name="VALUE" value="3.3V 3.2A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="9-57V(DC)"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749119550">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749119550.pdf"/>
<attribute name="IO2" value="3A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="L1" value="48uH"/>
<attribute name="LSMIN" value="0.7uH"/>
<attribute name="N" value="5.33:1:1:2"/>
<attribute name="PART-NUMBER" value=" 749119550 "/>
<attribute name="VALUE" value="5V 3A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="33-57V(DC)"/>
<attribute name="VO2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491195501">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491195501.pdf"/>
<attribute name="IO2" value="2.2A"/>
<attribute name="ISAT" value="6.2A"/>
<attribute name="L1" value="21uH"/>
<attribute name="LSMIN" value="0.3uH"/>
<attribute name="N" value="3:1:1:2"/>
<attribute name="PART-NUMBER" value=" 7491195501 "/>
<attribute name="VALUE" value="5V 2.2A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="9-57V(DC)"/>
<attribute name="VO2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491196112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491196112.pdf"/>
<attribute name="IO2" value="2.5A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L1" value="100uH"/>
<attribute name="LSMIN" value="0.5uH"/>
<attribute name="N" value="1.71:1:1:0.86"/>
<attribute name="PART-NUMBER" value=" 7491196112 "/>
<attribute name="VALUE" value="12V 2.5A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="33-57V(DC)"/>
<attribute name="VO2" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491196212">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491196212.pdf"/>
<attribute name="IO2" value="1.6A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="L1" value="128uH"/>
<attribute name="LSMIN" value="0.3uH"/>
<attribute name="N" value="0.47:1:1:0.82"/>
<attribute name="PART-NUMBER" value=" 7491196212 "/>
<attribute name="VALUE" value="12V 1.6A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="9-57V(DC)"/>
<attribute name="VO2" value="12V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749119633">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749119633.pdf"/>
<attribute name="IO2" value="8A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L1" value="100uH"/>
<attribute name="LSMIN" value="0.5uH"/>
<attribute name="N" value="6:1:1:3"/>
<attribute name="PART-NUMBER" value=" 749119633 "/>
<attribute name="VALUE" value="3.3V 8A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="33-57V(DC)"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491196331">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491196331.pdf"/>
<attribute name="IO2" value="5.5A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L1" value="128uH"/>
<attribute name="LSMIN" value="0.5uH"/>
<attribute name="N" value="3.2:1:1:2.8"/>
<attribute name="PART-NUMBER" value=" 7491196331 "/>
<attribute name="VALUE" value="3.3V 5.5A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="9-57V(DC)"/>
<attribute name="VO2" value="3.3V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_749119650">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/749119650.pdf"/>
<attribute name="IO2" value="7A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L1" value="100uH"/>
<attribute name="LSMIN" value="0.5uH"/>
<attribute name="N" value="4:1:1:2"/>
<attribute name="PART-NUMBER" value=" 749119650 "/>
<attribute name="VALUE" value="5V 7A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="33-57V(DC)"/>
<attribute name="VO2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
<technology name="_7491196501">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7491196501.pdf"/>
<attribute name="IO2" value="3.5A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="L1" value="128uH"/>
<attribute name="LSMIN" value="0.3uH"/>
<attribute name="N" value="1.14:1:1:2"/>
<attribute name="PART-NUMBER" value=" 7491196501 "/>
<attribute name="VALUE" value="5V 3.5A"/>
<attribute name="VAUX" value="10V"/>
<attribute name="VI" value="9-57V(DC)"/>
<attribute name="VO2" value="5V"/>
<attribute name="VT" value="1500V(AC)"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
