<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Automotive - Filter Chokes - WE-RCIS&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025b, 2025-08-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-RCIS_7847227010">
<description>&lt;B&gt;WE-RCIS Rod Core Inductor SMT
&lt;BR&gt; &lt;/B&gt;7847227010 
&lt;BR&gt;L X W X H = 15mm X 7.1mm X 7.8mm</description>
</package>
<package name="WE-RCIS_7847229020">
<description>&lt;B&gt;WE-RCIS Rod Core Inductor SMT
&lt;BR&gt; &lt;/B&gt;7847229020
&lt;BR&gt;L X W X H = 18.1mm X 9.3mm X 10mm</description>
</package>
<package name="WE-RCIS_7847227027">
<description>&lt;B&gt;WE-RCIS Rod Core Inductor SMT
&lt;BR&gt; &lt;/B&gt;7847227027 
&lt;BR&gt;L X W X H = 14.9mm X 6.5mm X 7mm</description>
</package>
<package name="WE-RCIS_7847232045">
<description>&lt;B&gt;WE-RCIS Rod Core Inductor SMT
&lt;BR&gt; &lt;/B&gt;7847229020
&lt;BR&gt;L X W X H = 25mm X 11.5mm X 11.85mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-RCIS">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-RCIS" prefix="L">
<description>&lt;b&gt; WE-RCIS Rod Core Inductor SMT
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Characteristics
&lt;br&gt;
&lt;/b&gt;&lt;/b&gt; 
&lt;br&gt;High Current capability
&lt;br&gt;Very high saturation performance
&lt;br&gt;High insertion loss at FM band
&lt;br&gt;Broadband suppression
&lt;br&gt;Robust mechanical design
&lt;br&gt;Packaging: tape &amp; reel / pick &amp; place
&lt;br&gt;Operating temperature up to +150ºC
&lt;br&gt;Automotive approved

&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Integrated DC/DC converters
&lt;br&gt;EMC suppression in motor drive systems
&lt;br&gt;Infotainment Systems

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o153336v209%20Family-RCIS-78472xxx.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o153336v209%20Family-RCIS-78472xxx.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-RCIS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-RCIS&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-08-06&lt;br&gt;
&lt;/b&gt;2025(C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-RCIS"/>
</gates>
<devices>
<device name="_7847227010" package="WE-RCIS_7847227010">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847227010?ae"/>
<attribute name="DIAMETER" value="7.1mm"/>
<attribute name="FRES" value="213MHz"/>
<attribute name="IR" value="22.5A"/>
<attribute name="L" value="1uH"/>
<attribute name="LENGTH" value="15mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7847227010"/>
<attribute name="PIN-DIAMETER" value="1.5mm"/>
<attribute name="PIN-LENGTH" value="7mm"/>
<attribute name="RDC" value="2mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
</technologies>
</device>
<device name="_7847227027" package="WE-RCIS_7847227027">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847227027?ae"/>
<attribute name="DIAMETER" value="6.5mm"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="10A"/>
<attribute name="L" value="2.72uH"/>
<attribute name="LENGTH" value="14.9mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7847227027"/>
<attribute name="PIN-DIAMETER" value="1mm"/>
<attribute name="PIN-LENGTH" value="6.5mm"/>
<attribute name="RDC" value="6.4mOhm"/>
<attribute name="VALUE" value="2.72uH"/>
</technology>
</technologies>
</device>
<device name="_7847229020" package="WE-RCIS_7847229020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847229020?ae"/>
<attribute name="DIAMETER" value="9.3mm"/>
<attribute name="FRES" value="134MHz"/>
<attribute name="IR" value="15A"/>
<attribute name="L" value="1.96uH"/>
<attribute name="LENGTH" value="18mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7847229020"/>
<attribute name="PIN-DIAMETER" value="1.5mm"/>
<attribute name="PIN-LENGTH" value="5.5mm"/>
<attribute name="RDC" value="2.4mOhm"/>
<attribute name="VALUE" value="1.96uH"/>
</technology>
</technologies>
</device>
<device name="_7847232045" package="WE-RCIS_7847232045">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7847232045?ae"/>
<attribute name="DIAMETER" value="11.5mm"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="L" value="4.45uH"/>
<attribute name="LENGTH" value="25mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="7847232045"/>
<attribute name="PIN-DIAMETER" value="1.5mm"/>
<attribute name="PIN-LENGTH" value="6mm"/>
<attribute name="RDC" value="3.8mOhm"/>
<attribute name="VALUE" value="4.45uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
