<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Signal &amp; Communications - RF Inductors - WE-RFI&lt;br&gt;

&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2024a, 2024-03-06&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-RFI_0603">
<description>&lt;B&gt;WE-RFI Ferrite SMD Inductor&lt;BR&gt;
&lt;/B&gt;&lt;BR&gt;Size: 0603, SMT, 2pins
&lt;BR&gt;LxWxH=1.65x1.1x0.9mm</description>
</package>
<package name="WE-RFI_0402">
<description>&lt;B&gt;WE-RFI Ferrite SMD Inductor&lt;BR&gt;
&lt;/B&gt;&lt;BR&gt;Size: 0402, SMT, 2pins
&lt;BR&gt;LxWxH=1.0x0.55x0.55mm</description>
</package>
<package name="WE-RFI_1008A">
<description>&lt;B&gt;WE-RFI Ferrite SMD Inductor&lt;BR&gt;
&lt;/B&gt;&lt;BR&gt;Size: 1008A, SMT, 2pins
&lt;BR&gt;LxWxH=2.5x2x1.6mm</description>
</package>
<package name="WE-RFI_0805A">
<description>&lt;B&gt;WE-RFI Ferrite SMD Inductor&lt;BR&gt;
&lt;/B&gt;&lt;BR&gt;Size: 0805A, SMT, 2pins
&lt;BR&gt;LxWxH=2x1.25x1.2mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-RFI_0603" prefix="L">
<description>&lt;b&gt;WE-RFI Ferrite SMT Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High inductances
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Custom designs on request
&lt;br&gt;AEC-Q200 Grade 3 (−40°C to +85°C)
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Especially developed for RF-applications
&lt;br&gt;RFID
&lt;br&gt;Low frequency radio applications (keyless)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-RFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-RFI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-06&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-RFI_0603">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447610139">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610139?ae"/>
<attribute name="FRES" value="2320MHz"/>
<attribute name="IR" value="1170mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610139 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="42mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="39nH"/>
</technology>
<technology name="_7447610168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610168?ae"/>
<attribute name="FRES" value="1925MHz"/>
<attribute name="IR" value="1050mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610168 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="68nH"/>
</technology>
<technology name="_7447610211">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610211?ae"/>
<attribute name="FRES" value="1925MHz"/>
<attribute name="IR" value="750mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610211 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="78mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="110nH"/>
</technology>
<technology name="_7447610215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610215?ae"/>
<attribute name="FRES" value="1885MHz"/>
<attribute name="IR" value="720mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610215 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="150nH"/>
</technology>
<technology name="_7447610220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610220?ae"/>
<attribute name="FRES" value="1730MHz"/>
<attribute name="IR" value="700mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610220 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="105mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="200nH"/>
</technology>
<technology name="_7447610224">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610224?ae"/>
<attribute name="FRES" value="1345MHz"/>
<attribute name="IR" value="490mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610224 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="180mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="240nH"/>
</technology>
<technology name="_7447610227">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610227?ae"/>
<attribute name="FRES" value="1540MHz"/>
<attribute name="IR" value="480mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610227 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="165mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="270nH"/>
</technology>
<technology name="_7447610236">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610236?ae"/>
<attribute name="FRES" value="1040MHz"/>
<attribute name="IR" value="470mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610236 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="185mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="360nH"/>
</technology>
<technology name="_7447610239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610239?ae"/>
<attribute name="FRES" value="990MHz"/>
<attribute name="IR" value="365mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610239 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="285mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="390nH"/>
</technology>
<technology name="_7447610242">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610242?ae"/>
<attribute name="FRES" value="1110MHz"/>
<attribute name="IR" value="425mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610242 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="255mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="420nH"/>
</technology>
<technology name="_7447610247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610247?ae"/>
<attribute name="FRES" value="1020MHz"/>
<attribute name="IR" value="370mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610247 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="285mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="470nH"/>
</technology>
<technology name="_7447610256">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610256?ae"/>
<attribute name="FRES" value="915MHz"/>
<attribute name="IR" value="390mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610256 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="270mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="560nH"/>
</technology>
<technology name="_7447610260">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610260?ae"/>
<attribute name="FRES" value="1000MHz"/>
<attribute name="IR" value="330mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610260 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="380mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="600nH"/>
</technology>
<technology name="_7447610268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610268?ae"/>
<attribute name="FRES" value="770MHz"/>
<attribute name="IR" value="330mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610268 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="390mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="680nH"/>
</technology>
<technology name="_7447610282">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610282?ae"/>
<attribute name="FRES" value="830MHz"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610282 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="450mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="820nH"/>
</technology>
<technology name="_7447610310">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610310?ae"/>
<attribute name="FRES" value="680MHz"/>
<attribute name="IR" value="230mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610310 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="700mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1000nH"/>
</technology>
<technology name="_7447610315">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610315?ae"/>
<attribute name="FRES" value="605MHz"/>
<attribute name="IR" value="200mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610315 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="1070mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="1500nH"/>
</technology>
<technology name="_7447610322">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610322?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="350mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610322 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="2200nH"/>
</technology>
<technology name="_7447610333">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610333?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="220mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610333 "/>
<attribute name="Q-FACTOR" value=" 14 "/>
<attribute name="RDC" value="950mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="3300nH"/>
</technology>
<technology name="_7447610347">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610347?ae"/>
<attribute name="FRES" value="67MHz"/>
<attribute name="IR" value="200mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610347 "/>
<attribute name="Q-FACTOR" value=" 14 "/>
<attribute name="RDC" value="1125mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="4700nH"/>
</technology>
<technology name="_7447610356">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610356?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="IR" value="195mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610356 "/>
<attribute name="Q-FACTOR" value=" 14 "/>
<attribute name="RDC" value="1055mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="5600nH"/>
</technology>
<technology name="_7447610368">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610368?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="170mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610368 "/>
<attribute name="Q-FACTOR" value=" 14 "/>
<attribute name="RDC" value="1380mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="6800nH"/>
</technology>
<technology name="_7447610382">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610382?ae"/>
<attribute name="FRES" value="46MHz"/>
<attribute name="IR" value="150mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610382 "/>
<attribute name="Q-FACTOR" value=" 14 "/>
<attribute name="RDC" value="1550mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="8200nH"/>
</technology>
<technology name="_7447610410">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610410?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="160mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610410 "/>
<attribute name="Q-FACTOR" value=" 14 "/>
<attribute name="RDC" value="1700mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="10000nH"/>
</technology>
<technology name="_7447610415">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610415?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="90mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610415 "/>
<attribute name="Q-FACTOR" value=" 13 "/>
<attribute name="RDC" value="3900mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="15000nH"/>
</technology>
<technology name="_7447610422">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447610422?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="85mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447610422 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="4900mOhm"/>
<attribute name="SIZE" value="0603"/>
<attribute name="VALUE" value="22000nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RFI_1008A" prefix="L">
<description>&lt;b&gt;WE-RFI Ferrite SMT Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High inductances
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Custom designs on request
&lt;br&gt;AEC-Q200 Grade 3 (−40°C to +85°C)
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Especially developed for RF-applications
&lt;br&gt;RFID
&lt;br&gt;Low frequency radio applications (keyless)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-RFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-RFI&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu 2022-07-21&lt;br&gt;
2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-RFI_1008A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744762312A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762312A?ae"/>
<attribute name="FRES" value="280MHz"/>
<attribute name="IR" value="230mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762312A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="1300mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="1200nH"/>
</technology>
<technology name="_744762315A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762315A?ae"/>
<attribute name="FRES" value="250MHz"/>
<attribute name="IR" value="220mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762315A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="1650mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="1500nH"/>
</technology>
<technology name="_744762318A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762318A?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="210mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762318A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="2200mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="1800nH"/>
</technology>
<technology name="_744762322A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762322A?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="200mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762322A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="2350mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="2200nH"/>
</technology>
<technology name="_744762327A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762327A?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="195mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762327A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="2600mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="2700nH"/>
</technology>
<technology name="_744762333A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762333A?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="185mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762333A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="2850mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="3300nH"/>
</technology>
<technology name="_744762339A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762339A?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="180mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762339A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="4000mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="3900nH"/>
</technology>
<technology name="_744762347A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762347A?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="175mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762347A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="4300mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="4700nH"/>
</technology>
<technology name="_744762356A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762356A?ae"/>
<attribute name="FRES" value="42MHz"/>
<attribute name="IR" value="170mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762356A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="2600mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="5600nH"/>
</technology>
<technology name="_744762368A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762368A?ae"/>
<attribute name="FRES" value="39MHz"/>
<attribute name="IR" value="165mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762368A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="2800mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="6800nH"/>
</technology>
<technology name="_744762382A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762382A?ae"/>
<attribute name="FRES" value="36MHz"/>
<attribute name="IR" value="160mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762382A"/>
<attribute name="Q-FACTOR" value=" 20 "/>
<attribute name="RDC" value="3050mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="8200nH"/>
</technology>
<technology name="_744762410A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762410A?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="150mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762410A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="3500mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="10000nH"/>
</technology>
<technology name="_744762415A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762415A?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="130mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762415A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="4000mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="15000nH"/>
</technology>
<technology name="_744762418A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762418A?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="120mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762418A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="4500mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="18000nH"/>
</technology>
<technology name="_744762422A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762422A?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="110mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762422A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="5000mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="22000nH"/>
</technology>
<technology name="_744762427A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762427A?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="95mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762427A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="6000mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="27000nH"/>
</technology>
<technology name="_744762433A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762433A?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="85mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762433A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="6500mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="33000nH"/>
</technology>
<technology name="_744762439A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762439A?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="60mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762439A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="8500mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="39000nH"/>
</technology>
<technology name="_744762447A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744762447A?ae"/>
<attribute name="FRES" value="17MHz"/>
<attribute name="IR" value="45mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744762447A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="14000mOhm"/>
<attribute name="SIZE" value="1008A"/>
<attribute name="VALUE" value="47000nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RFI_0805A" prefix="L">
<description>&lt;b&gt;WE-RFI Ferrite SMT Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High inductances
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Custom designs on request
&lt;br&gt;AEC-Q200 Grade 3 (−40°C to +85°C)
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Especially developed for RF-applications
&lt;br&gt;RFID
&lt;br&gt;Low frequency radio applications (keyless)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-RFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-RFI&lt;/a&gt;&lt;p&gt;

Updated  by Ella Wu 2022-07-21&lt;br&gt;
2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-RFI_0805A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744760247A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760247A?ae"/>
<attribute name="FRES" value="375MHz"/>
<attribute name="IR" value="500mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760247A"/>
<attribute name="Q-FACTOR" value=" 45 "/>
<attribute name="RDC" value="500mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="470nH"/>
</technology>
<technology name="_744760256A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760256A?ae"/>
<attribute name="FRES" value="340MHz"/>
<attribute name="IR" value="450mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760256A"/>
<attribute name="Q-FACTOR" value=" 45 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="560nH"/>
</technology>
<technology name="_744760268A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760268A?ae"/>
<attribute name="FRES" value="188MHz"/>
<attribute name="IR" value="400mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760268A"/>
<attribute name="Q-FACTOR" value=" 35 "/>
<attribute name="RDC" value="850mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="680nH"/>
</technology>
<technology name="_744760282A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760282A?ae"/>
<attribute name="FRES" value="215MHz"/>
<attribute name="IR" value="300mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760282A"/>
<attribute name="Q-FACTOR" value=" 35 "/>
<attribute name="RDC" value="1050mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="820nH"/>
</technology>
<technology name="_744760310A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760310A?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="180mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760310A"/>
<attribute name="Q-FACTOR" value=" 35 "/>
<attribute name="RDC" value="1050mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="1000nH"/>
</technology>
<technology name="_744760312A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760312A?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="150mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760312A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="1200mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="1200nH"/>
</technology>
<technology name="_744760315A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760315A?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="130mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760315A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="1450mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="1500nH"/>
</technology>
<technology name="_744760318A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760318A?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="120mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760318A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="2000mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="1800nH"/>
</technology>
<technology name="_744760322A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760322A?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="110mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760322A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="1750mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="2200nH"/>
</technology>
<technology name="_744760327A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760327A?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="100mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760327A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="1750mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="2700nH"/>
</technology>
<technology name="_744760333A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760333A?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="210mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760333A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="2000mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="3300nH"/>
</technology>
<technology name="_744760339A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760339A?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="200mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760339A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="2150mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="3900nH"/>
</technology>
<technology name="_744760347A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760347A?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="180mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760347A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="1900mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="4700nH"/>
</technology>
<technology name="_744760356A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760356A?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="160mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760356A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="2200mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="5600nH"/>
</technology>
<technology name="_744760382A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760382A?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="120mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760382A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="2400mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="8200nH"/>
</technology>
<technology name="_744760410A">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744760410A?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="80mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744760410A"/>
<attribute name="Q-FACTOR" value=" 15 "/>
<attribute name="RDC" value="3600mOhm"/>
<attribute name="SIZE" value="0805A"/>
<attribute name="VALUE" value="10000nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-RFI_0402" prefix="L">
<description>&lt;b&gt;WE-RFI Ferrite SMT Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;High inductances
&lt;br&gt;Recommended soldering: Reflow
&lt;br&gt;Custom designs on request
&lt;br&gt;AEC-Q200 Grade 3 (−40°C to +85°C)
&lt;br&gt;Operating temperature: –40 °C to +85 °C
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Especially developed for RF-applications
&lt;br&gt;RFID
&lt;br&gt;Low frequency radio applications (keyless)
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14843v209%20Family_WE-RFI.jpg"  width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-RFI/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-RFI&lt;/a&gt;&lt;p&gt;

Created by Ella Wu 2024-03-06&lt;br&gt;
2024(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="" package="WE-RFI_0402">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447650120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650120?ae"/>
<attribute name="FRES" value="7720MHz"/>
<attribute name="IR" value="1080mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650120 "/>
<attribute name="Q-FACTOR" value=" 11 "/>
<attribute name="RDC" value="25mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="20nH"/>
</technology>
<technology name="_7447650130">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650130?ae"/>
<attribute name="FRES" value="3800MHz"/>
<attribute name="IR" value="900mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650130 "/>
<attribute name="Q-FACTOR" value=" 11 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="30nH"/>
</technology>
<technology name="_7447650133">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650133?ae"/>
<attribute name="FRES" value="3875MHz"/>
<attribute name="IR" value="900mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650133 "/>
<attribute name="Q-FACTOR" value=" 11 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="33nH"/>
</technology>
<technology name="_7447650136">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650136?ae"/>
<attribute name="FRES" value="3875MHz"/>
<attribute name="IR" value="850mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650136 "/>
<attribute name="Q-FACTOR" value=" 11 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="36nH"/>
</technology>
<technology name="_7447650177">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650177?ae"/>
<attribute name="FRES" value="2980MHz"/>
<attribute name="IR" value="640mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650177 "/>
<attribute name="Q-FACTOR" value=" 11 "/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="77nH"/>
</technology>
<technology name="_7447650190">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650190?ae"/>
<attribute name="FRES" value="3140MHz"/>
<attribute name="IR" value="640mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650190 "/>
<attribute name="Q-FACTOR" value=" 11 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="90nH"/>
</technology>
<technology name="_7447650210">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650210?ae"/>
<attribute name="FRES" value="2955MHz"/>
<attribute name="IR" value="550mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650210 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="130mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="100nH"/>
</technology>
<technology name="_7447650212">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650212?ae"/>
<attribute name="FRES" value="2955MHz"/>
<attribute name="IR" value="575mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650212 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="110mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="120nH"/>
</technology>
<technology name="_7447650215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650215?ae"/>
<attribute name="FRES" value="2590MHz"/>
<attribute name="IR" value="545mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650215 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="130mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="150nH"/>
</technology>
<technology name="_7447650218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650218?ae"/>
<attribute name="FRES" value="2955MHz"/>
<attribute name="IR" value="470mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650218 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="160mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="180nH"/>
</technology>
<technology name="_7447650222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650222?ae"/>
<attribute name="FRES" value="2170MHz"/>
<attribute name="IR" value="390mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650222 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="220mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="220nH"/>
</technology>
<technology name="_7447650227">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650227?ae"/>
<attribute name="FRES" value="2015MHz"/>
<attribute name="IR" value="370mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650227 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="260mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="270nH"/>
</technology>
<technology name="_7447650233">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650233?ae"/>
<attribute name="FRES" value="1565MHz"/>
<attribute name="IR" value="mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650233 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="410mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="330nH"/>
</technology>
<technology name="_7447650236">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650236?ae"/>
<attribute name="FRES" value="1565MHz"/>
<attribute name="IR" value="320mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650236 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="375mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="360nH"/>
</technology>
<technology name="_7447650242">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650242?ae"/>
<attribute name="FRES" value="1810MHz"/>
<attribute name="IR" value="270mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650242 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="460mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="420nH"/>
</technology>
<technology name="_7447650247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650247?ae"/>
<attribute name="FRES" value="1600MHz"/>
<attribute name="IR" value="260mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650247 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="510mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="470nH"/>
</technology>
<technology name="_7447650253">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650253?ae"/>
<attribute name="FRES" value="1600MHz"/>
<attribute name="IR" value="230mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650253 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="615mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="530nH"/>
</technology>
<technology name="_7447650259">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650259?ae"/>
<attribute name="FRES" value="1370MHz"/>
<attribute name="IR" value="220mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650259 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="670mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="590nH"/>
</technology>
<technology name="_7447650270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650270?ae"/>
<attribute name="FRES" value="1565MHz"/>
<attribute name="IR" value="160mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650270 "/>
<attribute name="Q-FACTOR" value=" 11 "/>
<attribute name="RDC" value="1125mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="700nH"/>
</technology>
<technology name="_7447650277">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7447650277?ae"/>
<attribute name="FRES" value="1240MHz"/>
<attribute name="IR" value="155mA"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 7447650277 "/>
<attribute name="Q-FACTOR" value=" 12 "/>
<attribute name="RDC" value="1250mOhm"/>
<attribute name="SIZE" value="0402"/>
<attribute name="VALUE" value="770nH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
