<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-SI&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-SI_744101">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7mm;Diameter of Pin=0.3mm</description>
</package>
<package name="WE-SI_744131">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=8mm;Diameter of Pin=0.8mm</description>
</package>
<package name="WE-SI_744103">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7mm;Diameter of Pin=0.3mm</description>
</package>
<package name="WE-SI_7441110">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=12.5mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744136">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13.0mm;Diameter of Pin=0.7mm</description>
</package>
<package name="WE-SI_744107">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=10.5mm;Diameter of Pin=0.3mm</description>
</package>
<package name="WE-SI_744106">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7mm;Diameter of Pin=0.3mm</description>
</package>
<package name="WE-SI_744156">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13.5mm;Diameter of Pin=1.0mm</description>
</package>
<package name="WE-SI_744102">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7mm;Diameter of Pin=0.3mm</description>
</package>
<package name="WE-SI_744134">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=10mm;Diameter of Pin=0.9mm</description>
</package>
<package name="WE-SI_744139">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=16mm;Diameter of Pin=0.7mm</description>
</package>
<package name="WE-SI_744115">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7.5mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744119">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744117">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=11mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744153">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13mm;Diameter of Pin=1.0mm</description>
</package>
<package name="WE-SI_744133">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=11.5mm;Diameter of Pin=0.8mm</description>
</package>
<package name="WE-SI_744152">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=10mm;Diameter of Pin=1.0mm</description>
</package>
<package name="WE-SI_744105">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7.0mm;Diameter of Pin=0.3mm</description>
</package>
<package name="WE-SI_744155">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13mm;Diameter of Pin=1.1mm</description>
</package>
<package name="WE-SI_744111">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7.5mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744118">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=12.5mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_7441501">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=12mm;Diameter of Pin=1.2mm</description>
</package>
<package name="WE-SI_744104">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7mm;Diameter of Pin=0.3mm</description>
</package>
<package name="WE-SI_744112">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7.5mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744151">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=10mm;Diameter of Pin=1.0mm</description>
</package>
<package name="WE-SI_744132">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=8.5mm;Diameter of Pin=0.8mm</description>
</package>
<package name="WE-SI_744114">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7.5mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744135">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=10mm;Diameter of Pin=0.9mm</description>
</package>
<package name="WE-SI_744150">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=11.5mm;Diameter of Pin=1.2mm</description>
</package>
<package name="WE-SI_744113">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=7.5mm;Diameter of Pin=0.5mm</description>
</package>
<package name="WE-SI_744138">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13mm;Diameter of Pin=0.7mm</description>
</package>
<package name="WE-SI_744154">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13mm;Diameter of Pin=1mm</description>
</package>
<package name="WE-SI_744137">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=13mm;Diameter of Pin=0.7mm</description>
</package>
<package name="WE-SI_744116">
<description>&lt;B&gt;WE-SI&lt;B&gt;Leaded Toroidal Storage Choke
&lt;BR&gt; Pitch=8.0mm;Diameter of Pin=0.5mm</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-SI" prefix="L">
<description>&lt;b&gt;WE-SI Leaded Toroidal Storage Choke
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Low magnetic stray field
&lt;br&gt;Low core loss due to iron powder materials
&lt;br&gt;Available for rated current 1,1 A to 14,5 A
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Perfectly suitable for switching regulators from 
&lt;br&gt;National Semiconductor (LM) 
&lt;br&gt; Maxim
&lt;br&gt;Used for example in switching power supplies and voltage transformers
&lt;br&gt;Switching regulators up to 100 kHz
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14849v209%20Family_WE-SI.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14849v209%20Family_WE-SI.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-SI"&gt;https://katalog.we-online.com/en/pbs/WE-SI&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Yingchun,Shan 2019-09-03&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_744101" package="WE-SI_744101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744101pdf"/>
<attribute name="FRES" value="19.1MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="15mm"/>
<attribute name="LR" value="40uH"/>
<attribute name="PART-NUMBER" value=" 744101 "/>
<attribute name="RDC-MAX" value="0.18Ohm"/>
<attribute name="VALUE" value="50uH"/>
<attribute name="W" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_744102" package="WE-SI_744102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744102pdf"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="L" value="15mm"/>
<attribute name="LR" value="65uH"/>
<attribute name="PART-NUMBER" value=" 744102 "/>
<attribute name="RDC-MAX" value="0.23Ohm"/>
<attribute name="VALUE" value="73uH"/>
<attribute name="W" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_744103" package="WE-SI_744103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744103pdf"/>
<attribute name="FRES" value="9.2MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="15mm"/>
<attribute name="LR" value="99uH"/>
<attribute name="PART-NUMBER" value=" 744103 "/>
<attribute name="RDC-MAX" value="0.3Ohm"/>
<attribute name="VALUE" value="109uH"/>
<attribute name="W" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_744104" package="WE-SI_744104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744104pdf"/>
<attribute name="FRES" value="4.1MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="0.72A"/>
<attribute name="L" value="17.5mm"/>
<attribute name="LR" value="135uH"/>
<attribute name="PART-NUMBER" value=" 744104 "/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="167uH"/>
<attribute name="W" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_744105" package="WE-SI_744105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744105pdf"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="L" value="17.5mm"/>
<attribute name="LR" value="200uH"/>
<attribute name="PART-NUMBER" value=" 744105 "/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="258uH"/>
<attribute name="W" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_744106" package="WE-SI_744106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744106pdf"/>
<attribute name="FRES" value="2.1MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="17.5mm"/>
<attribute name="LR" value="290uH"/>
<attribute name="PART-NUMBER" value=" 744106 "/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="VALUE" value="393uH"/>
<attribute name="W" value="8mm"/>
</technology>
</technologies>
</device>
<device name="_744107" package="WE-SI_744107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744107pdf"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="L" value="22.5mm"/>
<attribute name="LR" value="450uH"/>
<attribute name="PART-NUMBER" value=" 744107 "/>
<attribute name="RDC-MAX" value="0.7Ohm"/>
<attribute name="VALUE" value="557uH"/>
<attribute name="W" value="12mm"/>
</technology>
</technologies>
</device>
<device name="_744111" package="WE-SI_744111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744111pdf"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L" value="15.5mm"/>
<attribute name="LR" value="31uH"/>
<attribute name="PART-NUMBER" value=" 744111 "/>
<attribute name="RDC-MAX" value="0.06Ohm"/>
<attribute name="VALUE" value="37uH"/>
<attribute name="W" value="8.5mm"/>
</technology>
</technologies>
</device>
<device name="_7441110" package="WE-SI_7441110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7441110pdf"/>
<attribute name="FRES" value="0.5MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="L" value="30mm"/>
<attribute name="LR" value="1020uH"/>
<attribute name="PART-NUMBER" value=" 7441110 "/>
<attribute name="RDC-MAX" value="0.48Ohm"/>
<attribute name="VALUE" value="1619uH"/>
<attribute name="W" value="14.5mm"/>
</technology>
</technologies>
</device>
<device name="_744112" package="WE-SI_744112">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744112pdf"/>
<attribute name="FRES" value="16.8MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L" value="17mm"/>
<attribute name="LR" value="38uH"/>
<attribute name="PART-NUMBER" value=" 744112 "/>
<attribute name="RDC-MAX" value="0.08Ohm"/>
<attribute name="VALUE" value="53uH"/>
<attribute name="W" value="9.5mm"/>
</technology>
</technologies>
</device>
<device name="_744113" package="WE-SI_744113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744113pdf"/>
<attribute name="FRES" value="6.5MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="17mm"/>
<attribute name="LR" value="56uH"/>
<attribute name="PART-NUMBER" value=" 744113 "/>
<attribute name="RDC-MAX" value="0.1Ohm"/>
<attribute name="VALUE" value="80uH"/>
<attribute name="W" value="9.5mm"/>
</technology>
</technologies>
</device>
<device name="_744114" package="WE-SI_744114">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744114pdf"/>
<attribute name="FRES" value="4.8MHz"/>
<attribute name="H" value="20mm"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="18mm"/>
<attribute name="LR" value="80uH"/>
<attribute name="PART-NUMBER" value=" 744114 "/>
<attribute name="RDC-MAX" value="0.12Ohm"/>
<attribute name="VALUE" value="127uH"/>
<attribute name="W" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_744115" package="WE-SI_744115">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744115pdf"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="H" value="20mm"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="18mm"/>
<attribute name="LR" value="110uH"/>
<attribute name="PART-NUMBER" value=" 744115 "/>
<attribute name="RDC-MAX" value="0.18Ohm"/>
<attribute name="VALUE" value="200uH"/>
<attribute name="W" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_744116" package="WE-SI_744116">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744116pdf"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="L" value="18mm"/>
<attribute name="LR" value="170uH"/>
<attribute name="PART-NUMBER" value=" 744116 "/>
<attribute name="RDC-MAX" value="0.2Ohm"/>
<attribute name="VALUE" value="345uH"/>
<attribute name="W" value="9mm"/>
</technology>
</technologies>
</device>
<device name="_744117" package="WE-SI_744117">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744117pdf"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="23mm"/>
<attribute name="LR" value="365uH"/>
<attribute name="PART-NUMBER" value=" 744117 "/>
<attribute name="RDC-MAX" value="0.25Ohm"/>
<attribute name="VALUE" value="390uH"/>
<attribute name="W" value="12.5mm"/>
</technology>
</technologies>
</device>
<device name="_744118" package="WE-SI_744118">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744118pdf"/>
<attribute name="FRES" value="1.3MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L" value="30mm"/>
<attribute name="LR" value="440uH"/>
<attribute name="PART-NUMBER" value=" 744118 "/>
<attribute name="RDC-MAX" value="0.33Ohm"/>
<attribute name="VALUE" value="600uH"/>
<attribute name="W" value="14mm"/>
</technology>
</technologies>
</device>
<device name="_744119" package="WE-SI_744119">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744119pdf"/>
<attribute name="FRES" value="0.85MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="L" value="30mm"/>
<attribute name="LR" value="620uH"/>
<attribute name="PART-NUMBER" value=" 744119 "/>
<attribute name="RDC-MAX" value="0.4Ohm"/>
<attribute name="VALUE" value="890uH"/>
<attribute name="W" value="14mm"/>
</technology>
</technologies>
</device>
<device name="_744131" package="WE-SI_744131">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744131pdf"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="5.2A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L" value="17mm"/>
<attribute name="LR" value="19uH"/>
<attribute name="PART-NUMBER" value=" 744131 "/>
<attribute name="RDC-MAX" value="0.038Ohm"/>
<attribute name="VALUE" value="34uH"/>
<attribute name="W" value="11mm"/>
</technology>
</technologies>
</device>
<device name="_744132" package="WE-SI_744132">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744132pdf"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="L" value="21mm"/>
<attribute name="LR" value="30uH"/>
<attribute name="PART-NUMBER" value=" 744132 "/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="VALUE" value="49uH"/>
<attribute name="W" value="9.5mm"/>
</technology>
</technologies>
</device>
<device name="_744133" package="WE-SI_744133">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744133pdf"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="5.8A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="24mm"/>
<attribute name="LR" value="40uH"/>
<attribute name="PART-NUMBER" value=" 744133 "/>
<attribute name="RDC-MAX" value="0.04Ohm"/>
<attribute name="VALUE" value="75uH"/>
<attribute name="W" value="13mm"/>
</technology>
</technologies>
</device>
<device name="_744134" package="WE-SI_744134">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744134pdf"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="5.4A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="L" value="31mm"/>
<attribute name="LR" value="59uH"/>
<attribute name="PART-NUMBER" value=" 744134 "/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="VALUE" value="92uH"/>
<attribute name="W" value="13.5mm"/>
</technology>
</technologies>
</device>
<device name="_744135" package="WE-SI_744135">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744135pdf"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="5.1A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="31mm"/>
<attribute name="LR" value="95uH"/>
<attribute name="PART-NUMBER" value=" 744135 "/>
<attribute name="RDC-MAX" value="0.063Ohm"/>
<attribute name="VALUE" value="157uH"/>
<attribute name="W" value="13.5mm"/>
</technology>
</technologies>
</device>
<device name="_744136" package="WE-SI_744136">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744136pdf"/>
<attribute name="FRES" value="3.3MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="L" value="31mm"/>
<attribute name="LR" value="215uH"/>
<attribute name="PART-NUMBER" value=" 744136 "/>
<attribute name="RDC-MAX" value="0.14Ohm"/>
<attribute name="VALUE" value="346uH"/>
<attribute name="W" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_744137" package="WE-SI_744137">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744137pdf"/>
<attribute name="FRES" value="1.5MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="31mm"/>
<attribute name="LR" value="380uH"/>
<attribute name="PART-NUMBER" value=" 744137 "/>
<attribute name="RDC-MAX" value="0.175Ohm"/>
<attribute name="VALUE" value="630uH"/>
<attribute name="W" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_744138" package="WE-SI_744138">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744138pdf"/>
<attribute name="FRES" value="1.8MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="L" value="43mm"/>
<attribute name="LR" value="440uH"/>
<attribute name="PART-NUMBER" value=" 744138 "/>
<attribute name="RDC-MAX" value="0.24Ohm"/>
<attribute name="VALUE" value="727uH"/>
<attribute name="W" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_744139" package="WE-SI_744139">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744139pdf"/>
<attribute name="FRES" value="0.65MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="L" value="44mm"/>
<attribute name="LR" value="680uH"/>
<attribute name="PART-NUMBER" value=" 744139 "/>
<attribute name="RDC-MAX" value="0.28Ohm"/>
<attribute name="VALUE" value="1124uH"/>
<attribute name="W" value="18.5mm"/>
</technology>
</technologies>
</device>
<device name="_744150" package="WE-SI_744150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744150pdf"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="10.3A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="L" value="28.5mm"/>
<attribute name="LR" value="16uH"/>
<attribute name="PART-NUMBER" value=" 744150 "/>
<attribute name="RDC-MAX" value="0.015Ohm"/>
<attribute name="VALUE" value="26uH"/>
<attribute name="W" value="14.5mm"/>
</technology>
</technologies>
</device>
<device name="_7441501" package="WE-SI_7441501">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/7441501pdf"/>
<attribute name="FRES" value="44.6MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="14.5A"/>
<attribute name="ISAT" value="6.9A"/>
<attribute name="L" value="28.5mm"/>
<attribute name="LR" value="7uH"/>
<attribute name="PART-NUMBER" value=" 7441501 "/>
<attribute name="RDC-MAX" value="0.008Ohm"/>
<attribute name="VALUE" value="12uH"/>
<attribute name="W" value="14.5mm"/>
</technology>
</technologies>
</device>
<device name="_744151" package="WE-SI_744151">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744151pdf"/>
<attribute name="FRES" value="13.6MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="8.1A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L" value="30mm"/>
<attribute name="LR" value="32uH"/>
<attribute name="PART-NUMBER" value=" 744151 "/>
<attribute name="RDC-MAX" value="0.025Ohm"/>
<attribute name="VALUE" value="48uH"/>
<attribute name="W" value="12mm"/>
</technology>
</technologies>
</device>
<device name="_744152" package="WE-SI_744152">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744152pdf"/>
<attribute name="FRES" value="5.4MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="7.7A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="L" value="28mm"/>
<attribute name="LR" value="39uH"/>
<attribute name="PART-NUMBER" value=" 744152 "/>
<attribute name="RDC-MAX" value="0.03Ohm"/>
<attribute name="VALUE" value="82uH"/>
<attribute name="W" value="12mm"/>
</technology>
</technologies>
</device>
<device name="_744153" package="WE-SI_744153">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744153pdf"/>
<attribute name="FRES" value="6.4MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="32mm"/>
<attribute name="LR" value="78uH"/>
<attribute name="PART-NUMBER" value=" 744153 "/>
<attribute name="RDC-MAX" value="0.05Ohm"/>
<attribute name="VALUE" value="137uH"/>
<attribute name="W" value="15.5mm"/>
</technology>
</technologies>
</device>
<device name="_744154" package="WE-SI_744154">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744154pdf"/>
<attribute name="FRES" value="3.1MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="6.5A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="32mm"/>
<attribute name="LR" value="85uH"/>
<attribute name="PART-NUMBER" value=" 744154 "/>
<attribute name="RDC-MAX" value="0.055Ohm"/>
<attribute name="VALUE" value="172uH"/>
<attribute name="W" value="16.5mm"/>
</technology>
</technologies>
</device>
<device name="_744155" package="WE-SI_744155">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744155pdf"/>
<attribute name="FRES" value="4.7MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="7.1A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="43mm"/>
<attribute name="LR" value="120uH"/>
<attribute name="PART-NUMBER" value=" 744155 "/>
<attribute name="RDC-MAX" value="0.06Ohm"/>
<attribute name="VALUE" value="220uH"/>
<attribute name="W" value="15mm"/>
</technology>
</technologies>
</device>
<device name="_744156" package="WE-SI_744156">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744156pdf"/>
<attribute name="FRES" value="1.5MHz"/>
<attribute name="H" value="12mm"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L" value="44mm"/>
<attribute name="LR" value="200uH"/>
<attribute name="PART-NUMBER" value=" 744156 "/>
<attribute name="RDC-MAX" value="0.07Ohm"/>
<attribute name="VALUE" value="380uH"/>
<attribute name="W" value="15.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
