<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Low Voltage and Data Lines - WE-SL&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-08-05&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-SL">
<description>&lt;b&gt;WE-SL SMT Common Mode Line Filter&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;WE-SL</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H">
<description>&lt;b&gt;WE-CMBH&lt;br&gt;
Common Mode Power Line Choke</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
<symbol name="WE-SL_4WIN">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-SL_4WINDING" prefix="L">
<description>&lt;b&gt;WE-SL SMT Common Mode Line Filter
&lt;br&gt;&lt;br&gt;Characteristics&lt;br&gt;

&lt;/b&gt;&lt;br&gt;Two or four winding configuration
&lt;br&gt;Core material: NiZn/MnZn
&lt;br&gt;Rated voltage: 80 VDC (42 VAC)
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category 40/125/21



&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications
&lt;br&gt; 
&lt;/b&gt;&lt;br&gt;Current compensated choke for data and signal lines
&lt;br&gt;Power supply system
&lt;br&gt;Signal and sensor lines
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;ISDN-Bus
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14850v209%20Family_WE-SL_7442017.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14850v209%20Family_WE-SL_7442017.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="http://katalog.we-online.de/en/pbs/WE-SL?"&gt;http://katalog.we-online.de/en/pbs/WE-SL?&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2020-08-05&lt;br&gt;
&lt;/b&gt;2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SL_4WIN"/>
</gates>
<devices>
<device name="" package="WE-SL">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="3"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="1"/>
<connect gate="G$1" pin="5" pad="8"/>
<connect gate="G$1" pin="6" pad="7"/>
<connect gate="G$1" pin="7" pad="6"/>
<connect gate="G$1" pin="8" pad="5"/>
</connects>
<technologies>
<technology name="_744201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744201.pdf"/>
<attribute name="IR" value="200mA"/>
<attribute name="LS" value="290nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744201 "/>
<attribute name="RDC" value="0.85Ohm"/>
<attribute name="VALUE" value="4700uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="14000Ohm"/>
</technology>
<technology name="_744202">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744202.pdf"/>
<attribute name="IR" value="350mA"/>
<attribute name="LS" value="170nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744202 "/>
<attribute name="RDC" value="0.4Ohm"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="5000Ohm"/>
</technology>
<technology name="_744203">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744203.pdf"/>
<attribute name="IR" value="400mA"/>
<attribute name="LS" value="140nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744203 "/>
<attribute name="RDC" value="0.3Ohm"/>
<attribute name="VALUE" value="500uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="3000Ohm"/>
</technology>
<technology name="_744204">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744204.pdf"/>
<attribute name="IR" value="600mA"/>
<attribute name="LS" value="110nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744204 "/>
<attribute name="RDC" value="0.12Ohm"/>
<attribute name="VALUE" value="250uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="1400Ohm"/>
</technology>
<technology name="_744205">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744205.pdf"/>
<attribute name="IR" value="700mA"/>
<attribute name="LS" value="92nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744205 "/>
<attribute name="RDC" value="0.1Ohm"/>
<attribute name="VALUE" value="100uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="900Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SL_2WINDING" prefix="L">
<description>&lt;b&gt;WE-SL SMT Common Mode Line Filter
&lt;br&gt;&lt;br&gt;Characteristics&lt;br&gt;

&lt;/b&gt;&lt;br&gt;Two or four winding configuration
&lt;br&gt;Core material: NiZn/MnZn
&lt;br&gt;Rated voltage: 80 VDC (42 VAC)
&lt;br&gt;Flammability corresponding to UL 94 V-0
&lt;br&gt;Climatic category 40/125/21



&lt;b&gt;&lt;br&gt;&lt;br&gt;Applications
&lt;br&gt; 
&lt;/b&gt;&lt;br&gt;Current compensated choke for data and signal lines
&lt;br&gt;Power supply system
&lt;br&gt;Signal and sensor lines
&lt;br&gt;Suppression of common mode noise
&lt;br&gt;ISDN-Bus
&lt;br&gt;


&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14850v209%20Family_WE-SL_7442017.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14850v209%20Family_WE-SL_7442017.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-SL"&gt;https://katalog.we-online.com/en/pbs/WE-SL&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2020-08-05&lt;br&gt;
&lt;/b&gt;2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-SL">
<connects>
<connect gate="G$1" pin="1" pad="4"/>
<connect gate="G$1" pin="2" pad="5"/>
<connect gate="G$1" pin="3" pad="8"/>
<connect gate="G$1" pin="4" pad="1"/>
</connects>
<technologies>
<technology name="_744206">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744206.pdf"/>
<attribute name="IR" value="2000mA"/>
<attribute name="LS" value="86nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744206 "/>
<attribute name="RDC" value="0.065Ohm"/>
<attribute name="VALUE" value="60uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="1600Ohm"/>
</technology>
<technology name="_744207">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744207.pdf"/>
<attribute name="IR" value="2700mA"/>
<attribute name="LS" value="63nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744207 "/>
<attribute name="RDC" value="0.035Ohm"/>
<attribute name="VALUE" value="35uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="1100Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
