<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - EMC Components - Common Mode Chokes for Low Voltage and Data Lines - WE-SL2&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-06-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-SL2">
<description>&lt;b&gt;WE-SL2 SMT Common Mode Line Filter&lt;/b&gt;</description>
</package>
</packages>
<symbols>
<symbol name="CM2W-H">
<description>&lt;b&gt;WE-CMBH&lt;br&gt;
Common Mode Power Line Choke</description>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-SL2" prefix="L">
<description>&lt;b&gt;WE-SL2 SMT Common Mode Line Filter
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;Characteristics 
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Common Mode Choke
&lt;br&gt;Ring core with the core materials of NiZn and MnZn
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;Operating voltage: 80 VDC (42 VAC)
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Current compensated choke for data and signal lines
&lt;br&gt;Power supply systems
&lt;br&gt;Signal and sensor lines
&lt;br&gt;CAN
&lt;br&gt;Suppression for common mode noise
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14852v209%20Family_WE-SL2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14852v209%20Family_WE-SL2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-SL2/"&gt;https://www.we-online.com/catalog/en/WE-SL2/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Ella Wu  2020-06-18&lt;br&gt;
&lt;/b&gt;2020 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="CM2W-H"/>
</gates>
<devices>
<device name="" package="WE-SL2">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="2"/>
</connects>
<technologies>
<technology name="_744220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744220.pdf"/>
<attribute name="IR" value="500mA"/>
<attribute name="LS" value="180nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744220"/>
<attribute name="RDC" value="0.75Ohm"/>
<attribute name="VALUE" value="4700uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="20000Ohm"/>
</technology>
<technology name="_744220103">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744220103.pdf"/>
<attribute name="IR" value="350mA"/>
<attribute name="LS" value="320nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744220103"/>
<attribute name="RDC" value="1.2Ohm"/>
<attribute name="VALUE" value="10000uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="25000Ohm"/>
</technology>
<technology name="_744220203">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744220203.pdf"/>
<attribute name="IR" value="200mA"/>
<attribute name="LS" value="490nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744220203"/>
<attribute name="RDC" value="2.6Ohm"/>
<attribute name="VALUE" value="20000uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="50000Ohm"/>
</technology>
<technology name="_744221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744221.pdf"/>
<attribute name="IR" value="600mA"/>
<attribute name="LS" value="130nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744221"/>
<attribute name="RDC" value="0.42Ohm"/>
<attribute name="VALUE" value="2000uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="9200Ohm"/>
</technology>
<technology name="_744222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744222.pdf"/>
<attribute name="IR" value="800mA"/>
<attribute name="LS" value="90nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744222"/>
<attribute name="RDC" value="0.207Ohm"/>
<attribute name="VALUE" value="1000uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="6000Ohm"/>
</technology>
<technology name="_744223">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744223.pdf"/>
<attribute name="IR" value="1000mA"/>
<attribute name="LS" value="75nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744223"/>
<attribute name="RDC" value="0.15Ohm"/>
<attribute name="VALUE" value="500uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="3300Ohm"/>
</technology>
<technology name="_744224">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744224.pdf"/>
<attribute name="IR" value="1200mA"/>
<attribute name="LS" value="60nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744224"/>
<attribute name="RDC" value="0.13Ohm"/>
<attribute name="VALUE" value="250uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="1800Ohm"/>
</technology>
<technology name="_744225">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744225.pdf"/>
<attribute name="IR" value="900mA"/>
<attribute name="LS" value="80nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744225"/>
<attribute name="RDC" value="0.25Ohm"/>
<attribute name="VALUE" value="40uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="3100Ohm"/>
</technology>
<technology name="_744225S">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744225S.pdf"/>
<attribute name="IR" value="900mA"/>
<attribute name="LS" value="2250nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744225S"/>
<attribute name="RDC" value="0.25Ohm"/>
<attribute name="VALUE" value="40uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="3100Ohm"/>
</technology>
<technology name="_744226">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744226.pdf"/>
<attribute name="IR" value="1600mA"/>
<attribute name="LS" value="55nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744226"/>
<attribute name="RDC" value="0.08Ohm"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="920Ohm"/>
</technology>
<technology name="_744226S">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744226S.pdf"/>
<attribute name="IR" value="1600mA"/>
<attribute name="LS" value="850nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744226S"/>
<attribute name="RDC" value="0.08Ohm"/>
<attribute name="VALUE" value="10uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="920Ohm"/>
</technology>
<technology name="_744227">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744227.pdf"/>
<attribute name="IR" value="1000mA"/>
<attribute name="LS" value="85nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744227"/>
<attribute name="RDC" value="0.16Ohm"/>
<attribute name="VALUE" value="51uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="5500Ohm"/>
</technology>
<technology name="_744227S">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744227S.pdf"/>
<attribute name="IR" value="1000mA"/>
<attribute name="LS" value="3150nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744227S"/>
<attribute name="RDC" value="0.16Ohm"/>
<attribute name="VALUE" value="51uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="5500Ohm"/>
</technology>
<technology name="_744228">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744228.pdf"/>
<attribute name="IR" value="1000mA"/>
<attribute name="LS" value="60nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744228"/>
<attribute name="RDC" value="0.12Ohm"/>
<attribute name="VALUE" value="25uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="2800Ohm"/>
</technology>
<technology name="_744228S">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744228S.pdf"/>
<attribute name="IR" value="1000mA"/>
<attribute name="LS" value="1500nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744228S"/>
<attribute name="RDC" value="0.12Ohm"/>
<attribute name="VALUE" value="25uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="2800Ohm"/>
</technology>
<technology name="_744229">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/744229.pdf"/>
<attribute name="IR" value="400mA"/>
<attribute name="LS" value="280nH"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="744229"/>
<attribute name="RDC" value="0.95Ohm"/>
<attribute name="VALUE" value="6500uH"/>
<attribute name="VR" value="80V"/>
<attribute name="VT" value="500  V (AC) "/>
<attribute name="ZMAX" value="18400Ohm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
