<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Shielded Power Inductors - WE-SPC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023a, 2023-02-20&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-SPC_4828">
<description>&lt;b&gt;WE-SPC SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4828, SMT, 2pins
&lt;br&gt;LXWXH=4.8X4.8X2.8mm</description>
</package>
<package name="WE-SPC_4838">
<description>&lt;b&gt;WE-SPC SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4838, SMT, 2pins
&lt;br&gt;LXWXH=4.8X4.8X3.8mm</description>
</package>
<package name="WE-SPC_4818">
<description>&lt;b&gt;WE-SPC SMD Power Inductor&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4818, SMT, 2pins
&lt;br&gt;LXWXH=4.8X4.8X1.8mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-SPC_4818" prefix="L">
<description>&lt;b&gt;WE-SPC SMT Power Inductor
&lt;br&gt;Shielded&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely small size
&lt;br&gt;High saturation current, up to 13 A
&lt;br&gt;Magnetic shielded, which results in a low leakage field
&lt;br&gt;High self resonance frequency
&lt;br&gt;Low self-losses
&lt;br&gt;Optimize solderability characteristics
&lt;br&gt;Constant saturation characteristics
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C up to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power devices
&lt;br&gt;DC/DC converter
&lt;br&gt;PCMCIA card
&lt;br&gt;Smart phone
&lt;br&gt;PDA
&lt;br&gt;Digital camera
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14857v209%20Family_WE-SPC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14857v209%20Family_WE-SPC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-SPC"&gt;www.we-online.com/en/components/products/WE-SPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-SPC_4818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744089410022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089410022?ae"/>
<attribute name="FRES" value="230MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089410022 "/>
<attribute name="RDC-MAX" value="0.015ohm"/>
<attribute name="RDC-TYP" value="0.0127ohm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744089410043">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089410043?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089410043 "/>
<attribute name="RDC-MAX" value="0.0176ohm"/>
<attribute name="RDC-TYP" value="0.015ohm"/>
<attribute name="VALUE" value="0.43uH"/>
</technology>
<technology name="_744089410068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089410068?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089410068 "/>
<attribute name="RDC-MAX" value="0.0221ohm"/>
<attribute name="RDC-TYP" value="0.0187ohm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74408941010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941010?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="5.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941010 "/>
<attribute name="RDC-MAX" value="0.0295ohm"/>
<attribute name="RDC-TYP" value="0.025ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74408941022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941022?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941022 "/>
<attribute name="RDC-MAX" value="0.066ohm"/>
<attribute name="RDC-TYP" value="0.056ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74408941029">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941029?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941029 "/>
<attribute name="RDC-MAX" value="0.101ohm"/>
<attribute name="RDC-TYP" value="0.085ohm"/>
<attribute name="VALUE" value="2.9uH"/>
</technology>
<technology name="_74408941035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941035?ae"/>
<attribute name="FRES" value="52MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941035 "/>
<attribute name="RDC-MAX" value="0.113ohm"/>
<attribute name="RDC-TYP" value="0.095ohm"/>
<attribute name="VALUE" value="3.5uH"/>
</technology>
<technology name="_74408941050">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941050?ae"/>
<attribute name="FRES" value="43MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941050 "/>
<attribute name="RDC-MAX" value="0.14ohm"/>
<attribute name="RDC-TYP" value="0.117ohm"/>
<attribute name="VALUE" value="5uH"/>
</technology>
<technology name="_74408941068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941068?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941068 "/>
<attribute name="RDC-MAX" value="0.19ohm"/>
<attribute name="RDC-TYP" value="0.16ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74408941078">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941078?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.05A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941078 "/>
<attribute name="RDC-MAX" value="0.23ohm"/>
<attribute name="RDC-TYP" value="0.195ohm"/>
<attribute name="VALUE" value="7.8uH"/>
</technology>
<technology name="_74408941089">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941089?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941089 "/>
<attribute name="RDC-MAX" value="0.24ohm"/>
<attribute name="RDC-TYP" value="0.203ohm"/>
<attribute name="VALUE" value="8.9uH"/>
</technology>
<technology name="_74408941100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941100?ae"/>
<attribute name="FRES" value="33MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941100 "/>
<attribute name="RDC-MAX" value="0.248ohm"/>
<attribute name="RDC-TYP" value="0.21ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74408941150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941150?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941150 "/>
<attribute name="RDC-MAX" value="0.43ohm"/>
<attribute name="RDC-TYP" value="0.365ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74408941220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941220?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.65A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941220 "/>
<attribute name="RDC-MAX" value="0.549ohm"/>
<attribute name="RDC-TYP" value="0.465ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74408941330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941330?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941330 "/>
<attribute name="RDC-MAX" value="1.015ohm"/>
<attribute name="RDC-TYP" value="0.86ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74408941470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408941470?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408941470 "/>
<attribute name="RDC-MAX" value="1.133ohm"/>
<attribute name="RDC-TYP" value="0.96ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPC_4838" prefix="L">
<description>&lt;b&gt;WE-SPC SMT Power Inductor
&lt;br&gt;Shielded&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely small size
&lt;br&gt;High saturation current, up to 13 A
&lt;br&gt;Magnetic shielded, which results in a low leakage field
&lt;br&gt;High self resonance frequency
&lt;br&gt;Low self-losses
&lt;br&gt;Optimize solderability characteristics
&lt;br&gt;Constant saturation characteristics
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C up to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power devices
&lt;br&gt;DC/DC converter
&lt;br&gt;PCMCIA card
&lt;br&gt;Smart phone
&lt;br&gt;PDA
&lt;br&gt;Digital camera
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14857v209%20Family_WE-SPC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14857v209%20Family_WE-SPC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-SPC"&gt;www.we-online.com/en/components/products/WE-SPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-SPC_4818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744089430022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089430022?ae"/>
<attribute name="FRES" value="250MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="13A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089430022 "/>
<attribute name="RDC-MAX" value="0.014ohm"/>
<attribute name="RDC-TYP" value="0.012ohm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744089430039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089430039?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="9.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089430039 "/>
<attribute name="RDC-MAX" value="0.016ohm"/>
<attribute name="RDC-TYP" value="0.0135ohm"/>
<attribute name="VALUE" value="0.39uH"/>
</technology>
<technology name="_744089430056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089430056?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="8.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089430056 "/>
<attribute name="RDC-MAX" value="0.017ohm"/>
<attribute name="RDC-TYP" value="0.015ohm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744089430082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089430082?ae"/>
<attribute name="FRES" value="108MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="7.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089430082 "/>
<attribute name="RDC-MAX" value="0.02ohm"/>
<attribute name="RDC-TYP" value="0.017ohm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74408943010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943010?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943010 "/>
<attribute name="RDC-MAX" value="0.022ohm"/>
<attribute name="RDC-TYP" value="0.019ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74408943022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943022?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943022 "/>
<attribute name="RDC-MAX" value="0.03ohm"/>
<attribute name="RDC-TYP" value="0.026ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74408943033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943033?ae"/>
<attribute name="FRES" value="64MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943033 "/>
<attribute name="RDC-MAX" value="0.036ohm"/>
<attribute name="RDC-TYP" value="0.031ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74408943047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943047?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943047 "/>
<attribute name="RDC-MAX" value="0.052ohm"/>
<attribute name="RDC-TYP" value="0.045ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74408943068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943068?ae"/>
<attribute name="FRES" value="34MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943068 "/>
<attribute name="RDC-MAX" value="0.059ohm"/>
<attribute name="RDC-TYP" value="0.051ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74408943082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943082?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943082 "/>
<attribute name="RDC-MAX" value="0.081ohm"/>
<attribute name="RDC-TYP" value="0.07ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74408943100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943100?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943100 "/>
<attribute name="RDC-MAX" value="0.094ohm"/>
<attribute name="RDC-TYP" value="0.082ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74408943101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943101?ae"/>
<attribute name="FRES" value="7.8MHz"/>
<attribute name="IR" value="0.52A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943101 "/>
<attribute name="RDC-MAX" value="0.85ohm"/>
<attribute name="RDC-TYP" value="0.77ohm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_74408943150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943150?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943150 "/>
<attribute name="RDC-MAX" value="0.136ohm"/>
<attribute name="RDC-TYP" value="0.118ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74408943220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943220?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943220 "/>
<attribute name="RDC-MAX" value="0.213ohm"/>
<attribute name="RDC-TYP" value="0.185ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74408943330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943330?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943330 "/>
<attribute name="RDC-MAX" value="0.298ohm"/>
<attribute name="RDC-TYP" value="0.259ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74408943470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943470?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943470 "/>
<attribute name="RDC-MAX" value="0.351ohm"/>
<attribute name="RDC-TYP" value="0.305ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74408943560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943560?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943560 "/>
<attribute name="RDC-MAX" value="0.481ohm"/>
<attribute name="RDC-TYP" value="0.418ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_74408943680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943680?ae"/>
<attribute name="FRES" value="9.5MHz"/>
<attribute name="IR" value="0.6A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943680 "/>
<attribute name="RDC-MAX" value="0.7ohm"/>
<attribute name="RDC-TYP" value="0.608ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_74408943820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408943820?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.58A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408943820 "/>
<attribute name="RDC-MAX" value="0.75ohm"/>
<attribute name="RDC-TYP" value="0.689ohm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPC_4828" prefix="L">
<description>&lt;b&gt;WE-SPC SMT Power Inductor
&lt;br&gt;Shielded&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely small size
&lt;br&gt;High saturation current, up to 13 A
&lt;br&gt;Magnetic shielded, which results in a low leakage field
&lt;br&gt;High self resonance frequency
&lt;br&gt;Low self-losses
&lt;br&gt;Optimize solderability characteristics
&lt;br&gt;Constant saturation characteristics
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C up to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power devices
&lt;br&gt;DC/DC converter
&lt;br&gt;PCMCIA card
&lt;br&gt;Smart phone
&lt;br&gt;PDA
&lt;br&gt;Digital camera
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14857v209%20Family_WE-SPC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14857v209%20Family_WE-SPC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-SPC"&gt;www.we-online.com/en/components/products/WE-SPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-SPC_4818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744089420022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089420022?ae"/>
<attribute name="FRES" value="220MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="13.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089420022 "/>
<attribute name="RDC-MAX" value="0.0144ohm"/>
<attribute name="RDC-TYP" value="0.0122ohm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_744089420039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089420039?ae"/>
<attribute name="FRES" value="160MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="10.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089420039 "/>
<attribute name="RDC-MAX" value="0.0177ohm"/>
<attribute name="RDC-TYP" value="0.015ohm"/>
<attribute name="VALUE" value="0.39uH"/>
</technology>
<technology name="_744089420056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089420056?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="8.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089420056 "/>
<attribute name="RDC-MAX" value="0.0184ohm"/>
<attribute name="RDC-TYP" value="0.0156ohm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744089420082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744089420082?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="6.7A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 744089420082 "/>
<attribute name="RDC-MAX" value="0.0248ohm"/>
<attribute name="RDC-TYP" value="0.021ohm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74408942012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942012?ae"/>
<attribute name="FRES" value="82MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942012 "/>
<attribute name="RDC-MAX" value="0.026ohm"/>
<attribute name="RDC-TYP" value="0.022ohm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74408942022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942022?ae"/>
<attribute name="FRES" value="54MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942022 "/>
<attribute name="RDC-MAX" value="0.045ohm"/>
<attribute name="RDC-TYP" value="0.038ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74408942033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942033?ae"/>
<attribute name="FRES" value="44MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942033 "/>
<attribute name="RDC-MAX" value="0.057ohm"/>
<attribute name="RDC-TYP" value="0.0483ohm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_74408942047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942047?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="2.9A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942047 "/>
<attribute name="RDC-MAX" value="0.103ohm"/>
<attribute name="RDC-TYP" value="0.0868ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74408942068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942068?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942068 "/>
<attribute name="RDC-MAX" value="0.13ohm"/>
<attribute name="RDC-TYP" value="0.11ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74408942082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942082?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942082 "/>
<attribute name="RDC-MAX" value="0.134ohm"/>
<attribute name="RDC-TYP" value="0.113ohm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_74408942100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942100?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.38A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942100 "/>
<attribute name="RDC-MAX" value="0.148ohm"/>
<attribute name="RDC-TYP" value="0.125ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74408942150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942150?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942150 "/>
<attribute name="RDC-MAX" value="0.245ohm"/>
<attribute name="RDC-TYP" value="0.207ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74408942220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942220?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942220 "/>
<attribute name="RDC-MAX" value="0.354ohm"/>
<attribute name="RDC-TYP" value="0.3ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_74408942330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942330?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942330 "/>
<attribute name="RDC-MAX" value="0.5ohm"/>
<attribute name="RDC-TYP" value="0.424ohm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_74408942470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942470?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.66A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942470 "/>
<attribute name="RDC-MAX" value="0.608ohm"/>
<attribute name="RDC-TYP" value="0.515ohm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_74408942560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942560?ae"/>
<attribute name="FRES" value="9.5MHz"/>
<attribute name="IR" value="0.51A"/>
<attribute name="ISAT" value="0.82A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942560 "/>
<attribute name="RDC-MAX" value="0.92ohm"/>
<attribute name="RDC-TYP" value="0.78ohm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_74408942680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942680?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="0.49A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942680 "/>
<attribute name="RDC-MAX" value="1.02ohm"/>
<attribute name="RDC-TYP" value="0.864ohm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_74408942820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74408942820?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.46A"/>
<attribute name="ISAT" value="0.68A"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value=" 74408942820 "/>
<attribute name="RDC-MAX" value="1.11ohm"/>
<attribute name="RDC-TYP" value="0.94ohm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
