<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Quartz Crystals &amp; Oscillators - WE-SPXO&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-07&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-SPXO_CFPS-9">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-9 
&lt;br&gt;L X W X H = 5.0mm X 3.2mm X 1.3mm</description>
</package>
<package name="WE-SPXO_IQXO-540">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-540
&lt;br&gt;L X W X H = 2.0mm X 1.6mm X 0.8mm</description>
</package>
<package name="WE-SPXO_IQXO-404">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-404
&lt;br&gt;L X W X H = 2mm X 1.6mm X 0.8mm</description>
</package>
<package name="WE-SPXO_IQXO-623">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-623
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.1mm</description>
</package>
<package name="WE-SPXO_CFPS-102">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-102
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.2mm</description>
</package>
<package name="WE-SPXO_IQXO-624">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-623
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.1mm</description>
</package>
<package name="WE-SPXO_IQXO-402">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-402
&lt;br&gt;L X W X H = 2mm X 1.6mm X 0.8mm</description>
</package>
<package name="WE-SPXO_IQXO-794">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-794
&lt;br&gt;L X W X H = 2.5mm X 2.0mm X 1.0mm</description>
</package>
<package name="WE-SPXO_CFPS-107">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-107
&lt;br&gt;L X W X H = 2.5mm X 2mm X 0.95mm</description>
</package>
<package name="WE-SPXO_IQXO-542">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-542
&lt;br&gt;L X W X H = 2.0mm X 1.6mm X 0.8mm</description>
</package>
<package name="WE-SPXO_CFPS-39">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-39 
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.2mm</description>
</package>
<package name="WE-SPXO_IQXO-618-33">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-618-33
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.1mm</description>
</package>
<package name="WE-SPXO_CFPS-104">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-104
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.2mm</description>
</package>
<package name="WE-SPXO_CFPS-109">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-109
&lt;br&gt;L X W X H = 2.5mm X 2mm X 0.95mm</description>
</package>
<package name="WE-SPXO_IQXO-951-2520">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-951 2520
&lt;br&gt;L X W X H = 2.5mm X 2mm X 0.95mm</description>
</package>
<package name="WE-SPXO_IQXO-618-25">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-618-25
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.1mm</description>
</package>
<package name="WE-SPXO_IQXO-951-3225">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-951 3225
&lt;br&gt;L X W X H = 3.2mm X 2.5mm X 1.2mm</description>
</package>
<package name="WE-SPXO_IQXO-951-2016">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-951 2016
&lt;br&gt;L X W X H = 2mm X 1.6mm X 0.8mm</description>
</package>
<package name="WE-SPXO_CFPS-73">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-73 
&lt;br&gt;L X W X H = 7.0mm X 5.0mm X 1.8mm</description>
</package>
<package name="WE-SPXO_CFPS-72">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;CFPS-72
&lt;br&gt;L X W X H = 7.0mm X 5.0mm X 1.8mm</description>
</package>
<package name="WE-SPXO_IQXO-791">
<description>&lt;B&gt;WE-SPXO Simple Packaged Quartz Oscillator
&lt;br&gt;&lt;br&gt;Size : &lt;/b&gt;IQXO-791
&lt;br&gt;L X W X H = 2.5mm X 2.0mm X 1.0mm</description>
</package>
</packages>
<symbols>
<symbol name="WE-SPXO_CFPS-E/D">
<pin name="E/D" direction="pas"/>
<pin name="+VS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="WE-SPXO_CFPS-E/D_6PINS">
<pin name="E/D" direction="pas"/>
<pin name="+VS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT+" direction="pas"/>
<pin name="OUT-" direction="pas"/>
<pin name="NC" direction="pas"/>
</symbol>
<symbol name="WE-SPXO_CFPS-SO">
<pin name="SO" direction="pas"/>
<pin name="+VS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="pas"/>
</symbol>
<symbol name="WE-SPXO_CFPS-TR">
<pin name="TRI" direction="pas"/>
<pin name="+VS" direction="pas"/>
<pin name="GND" direction="pas"/>
<pin name="OUT" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-SPXO_CFPS-9" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-9">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_831024589">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831024589?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831024589"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_831024807">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831024807?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831024807"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_831024880">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831024880?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831024880"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_831024957">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831024957?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831024957"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_831024978">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831024978?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831024978"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_831024986">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831024986?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831024986"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_831026068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831026068?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831026068"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
<technology name="_831026152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831026152?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.3mm"/>
<attribute name="LENGTH" value="5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831026152"/>
<attribute name="SIZE" value="CFPS-9"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="3.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-540" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-540">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_830208214609">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208214609?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208214609"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208214709">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208214709?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208214709"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208214809">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208214809?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208214809"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208214909">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208214909?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208214909"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215009?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215009"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215109">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215109?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215109"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215209">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215209?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215209"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215309">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215309?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215309"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215409">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215409?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215409"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215509?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215509"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215609">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215609?ae"/>
<attribute name="FREQUENCY" value="32.768 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215609"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208215809">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208215809?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208215809"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831054046">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831054046?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831054046"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056237">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056237?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056237"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056238">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056238?ae"/>
<attribute name="FREQUENCY" value="13 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056238"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="13 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056239">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056239?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056239"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056240">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056240?ae"/>
<attribute name="FREQUENCY" value="19.44 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056240"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="19.44 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056241">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056241?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056241"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056242">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056242?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056242"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056243">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056243?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056243"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056244">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056244?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056244"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056245">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056245?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056245"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056246">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056246?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056246"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056247">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056247?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056247"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056248">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056248?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056248"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056249">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056249?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056249"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831066629">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831066629?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831066629"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831068242">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831068242?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831068242"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831068248">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831068248?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831068248"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831068250">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831068250?ae"/>
<attribute name="FREQUENCY" value="38.4 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831068250"/>
<attribute name="SIZE" value="IQXO-540"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="38.4 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-404" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-404">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_830207370601">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207370601?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207370601"/>
<attribute name="SIZE" value="IQXO-404"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830207370701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207370701?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207370701"/>
<attribute name="SIZE" value="IQXO-404"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-623" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D_6PINS"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-623">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="4"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
</connects>
<technologies>
<technology name="_830208332501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208332501?ae"/>
<attribute name="FREQUENCY" value="100 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVPECL"/>
<attribute name="PART-NUMBER" value="830208332501"/>
<attribute name="SIZE" value="IQXO-623"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="2.5 V"/>
<attribute name="VALUE" value="100 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208332601">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208332601?ae"/>
<attribute name="FREQUENCY" value="125 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVPECL"/>
<attribute name="PART-NUMBER" value="830208332601"/>
<attribute name="SIZE" value="IQXO-623"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="2.5 V"/>
<attribute name="VALUE" value="125 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208332701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208332701?ae"/>
<attribute name="FREQUENCY" value="156.25 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVPECL"/>
<attribute name="PART-NUMBER" value="830208332701"/>
<attribute name="SIZE" value="IQXO-623"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="2.5 V"/>
<attribute name="VALUE" value="156.25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-624" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D_6PINS"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-624">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="4"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
</connects>
<technologies>
<technology name="_830208334301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208334301?ae"/>
<attribute name="FREQUENCY" value="100 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVPECL"/>
<attribute name="PART-NUMBER" value="830208334301"/>
<attribute name="SIZE" value="IQXO-624"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="100 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208334501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208334501?ae"/>
<attribute name="FREQUENCY" value="125 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVPECL"/>
<attribute name="PART-NUMBER" value="830208334501"/>
<attribute name="SIZE" value="IQXO-624"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="125 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208334601">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208334601?ae"/>
<attribute name="FREQUENCY" value="156.25 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVPECL"/>
<attribute name="PART-NUMBER" value="830208334601"/>
<attribute name="SIZE" value="IQXO-624"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="156.25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_CFPS-102" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-SO"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-102">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SO" pad="1"/>
</connects>
<technologies>
<technology name="_830205297709">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205297709?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205297709"/>
<attribute name="SIZE" value="CFPS-102"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208228309">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208228309?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208228309"/>
<attribute name="SIZE" value="CFPS-102"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-402" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-402">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_830207370001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207370001?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207370001"/>
<attribute name="SIZE" value="IQXO-402"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830207370101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207370101?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207370101"/>
<attribute name="SIZE" value="IQXO-402"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-794" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-SO"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-794">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SO" pad="1"/>
</connects>
<technologies>
<technology name="_830206924301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830206924301?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830206924301"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208221801">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208221801?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208221801"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208221901">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208221901?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208221901"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222001?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222001"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222101?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222101"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222201?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222201"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222301?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222301"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222401">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222401?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222401"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222501?ae"/>
<attribute name="FREQUENCY" value="32.768 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222501"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222601">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222601?ae"/>
<attribute name="FREQUENCY" value="33.3333 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222601"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="33.3333 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222701?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222701"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208222901">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208222901?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208222901"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056262">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056262?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056262"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056263">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056263?ae"/>
<attribute name="FREQUENCY" value="13 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056263"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="13 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056264">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056264?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056264"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056266">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056266?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056266"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056267">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056267?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056267"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056268">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056268?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056268"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056269">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056269?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056269"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056270?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056270"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056271">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056271?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056271"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056272">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056272?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056272"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056273">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056273?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056273"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056274">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056274?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056274"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831066658">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831066658?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831066658"/>
<attribute name="SIZE" value="IQXO-794"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-542" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-542">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_830208216409">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208216409?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208216409"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208216609">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208216609?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208216609"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208216709">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208216709?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208216709"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208216809">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208216809?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208216809"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208217009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208217009?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208217009"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208217109">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208217109?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208217109"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208217409">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208217409?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208217409"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208217609">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208217609?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208217609"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208217809">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208217809?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208217809"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208217909">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208217909?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208217909"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208218109">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208218109?ae"/>
<attribute name="FREQUENCY" value="32.768 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208218109"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_830208218209">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208218209?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208218209"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056168">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056168?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056168"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056169">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056169?ae"/>
<attribute name="FREQUENCY" value="13 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056169"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="13 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056188">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056188?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056188"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056214">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056214?ae"/>
<attribute name="FREQUENCY" value="19.44 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056214"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="19.44 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056215">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056215?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056215"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056216">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056216?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056216"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056217">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056217?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056217"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056218">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056218?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056218"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056219">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056219?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056219"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056220?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056220"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056221?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056221"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056222">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056222?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056222"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_831056223">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056223?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056223"/>
<attribute name="SIZE" value="IQXO-542"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-618-33" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D_6PINS"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-618-33">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="4"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
</connects>
<technologies>
<technology name="_830208331709">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208331709?ae"/>
<attribute name="FREQUENCY" value="100 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVDS"/>
<attribute name="PART-NUMBER" value="830208331709"/>
<attribute name="SIZE" value="IQXO-618-33"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="100 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208331909">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208331909?ae"/>
<attribute name="FREQUENCY" value="125 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVDS"/>
<attribute name="PART-NUMBER" value="830208331909"/>
<attribute name="SIZE" value="IQXO-618-33"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="125 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208332009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208332009?ae"/>
<attribute name="FREQUENCY" value="156.25 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVDS"/>
<attribute name="PART-NUMBER" value="830208332009"/>
<attribute name="SIZE" value="IQXO-618-33"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="156.25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_CFPS-107" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-TR"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-107">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRI" pad="1"/>
</connects>
<technologies>
<technology name="_830206385009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830206385009?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830206385009"/>
<attribute name="SIZE" value="CFPS-107"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208229109">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208229109?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208229109"/>
<attribute name="SIZE" value="CFPS-107"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="1.8 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_CFPS-39" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-39">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_830205075709">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205075709?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205075709"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830205312509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205312509?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205312509"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830205530509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205530509?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205530509"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830205530709">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205530709?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205530709"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830205889709">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205889709?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205889709"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830205896509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205896509?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205896509"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207044109">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207044109?ae"/>
<attribute name="FREQUENCY" value="100 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207044109"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="100 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207192009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207192009?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207192009"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207245309">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207245309?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207245309"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207647309">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207647309?ae"/>
<attribute name="FREQUENCY" value="11.0592 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207647309"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="11.0592 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207658809">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207658809?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207658809"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207659009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207659009?ae"/>
<attribute name="FREQUENCY" value="22.5792 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207659009"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="22.5792 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207659209">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207659209?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207659209"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207659609">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207659609?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207659609"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207670409">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207670409?ae"/>
<attribute name="FREQUENCY" value="54 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207670409"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="54 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207670609">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207670609?ae"/>
<attribute name="FREQUENCY" value="80 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207670609"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="80 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830207670909">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207670909?ae"/>
<attribute name="FREQUENCY" value="125 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207670909"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="125 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208197509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208197509?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208197509"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025019">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025019?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025019"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025165">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025165?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025165"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025166">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025166?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025166"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025492">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025492?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025492"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025493">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025493?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025493"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025494">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025494?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025494"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025495">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025495?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025495"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025496">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025496?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025496"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025497">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025497?ae"/>
<attribute name="FREQUENCY" value="30 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025497"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="30 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025558">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025558?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025558"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025559">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025559?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025559"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831025560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831025560?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831025560"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831026368">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831026368?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831026368"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831027167">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831027167?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831027167"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831055678">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831055678?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831055678"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831055872">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831055872?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831055872"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831059271">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831059271?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831059271"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_831063343">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831063343?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831063343"/>
<attribute name="SIZE" value="CFPS-39"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_CFPS-104" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-SO"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-104">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SO" pad="1"/>
</connects>
<technologies>
<technology name="_830205028309">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830205028309?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830205028309"/>
<attribute name="SIZE" value="CFPS-104"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208228609">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208228609?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208228609"/>
<attribute name="SIZE" value="CFPS-104"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_CFPS-109" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-TR"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-109">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="TRI" pad="1"/>
</connects>
<technologies>
<technology name="_830207390509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207390509?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830207390509"/>
<attribute name="SIZE" value="CFPS-109"/>
<attribute name="STABILITY" value="30ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208229409">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208229409?ae"/>
<attribute name="FREQUENCY" value="32.768 kHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +125 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208229409"/>
<attribute name="SIZE" value="CFPS-109"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 kHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-618-25" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D_6PINS"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-618-25">
<connects>
<connect gate="G$1" pin="+VS" pad="6"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="3"/>
<connect gate="G$1" pin="NC" pad="2"/>
<connect gate="G$1" pin="OUT+" pad="4"/>
<connect gate="G$1" pin="OUT-" pad="5"/>
</connects>
<technologies>
<technology name="_830207511509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830207511509?ae"/>
<attribute name="FREQUENCY" value="125 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVDS"/>
<attribute name="PART-NUMBER" value="830207511509"/>
<attribute name="SIZE" value="IQXO-618-25"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="2.5 V"/>
<attribute name="VALUE" value="125 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208332209">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208332209?ae"/>
<attribute name="FREQUENCY" value="100 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVDS"/>
<attribute name="PART-NUMBER" value="830208332209"/>
<attribute name="SIZE" value="IQXO-618-25"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="2.5 V"/>
<attribute name="VALUE" value="100 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_830208332309">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208332309?ae"/>
<attribute name="FREQUENCY" value="156.25 MHz"/>
<attribute name="HEIGHT" value="1.1mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="LVDS"/>
<attribute name="PART-NUMBER" value="830208332309"/>
<attribute name="SIZE" value="IQXO-618-25"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="2.5 V"/>
<attribute name="VALUE" value="156.25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-951-3225" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-SO"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-951-3225">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SO" pad="1"/>
</connects>
<technologies>
<technology name="_8302091564">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091564?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091564"/>
<attribute name="SIZE" value="IQXO-951 3225"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_8302091565">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091565?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091565"/>
<attribute name="SIZE" value="IQXO-951 3225"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_8302091566">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091566?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091566"/>
<attribute name="SIZE" value="IQXO-951 3225"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_8302091567">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091567?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091567"/>
<attribute name="SIZE" value="IQXO-951 3225"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_8302091568">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091568?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091568"/>
<attribute name="SIZE" value="IQXO-951 3225"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_8302091569">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091569?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091569"/>
<attribute name="SIZE" value="IQXO-951 3225"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
<technology name="_8302091570">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091570?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1.2mm"/>
<attribute name="LENGTH" value="3.2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091570"/>
<attribute name="SIZE" value="IQXO-951 3225"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-951-2520" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-SO"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-951-2520">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SO" pad="1"/>
</connects>
<technologies>
<technology name="_830208483509">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208483509?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208483509"/>
<attribute name="SIZE" value="IQXO-951 2520"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208544409">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208544409?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208544409"/>
<attribute name="SIZE" value="IQXO-951 2520"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8302091571">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091571?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091571"/>
<attribute name="SIZE" value="IQXO-951 2520"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8302091572">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091572?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091572"/>
<attribute name="SIZE" value="IQXO-951 2520"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8302091573">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091573?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091573"/>
<attribute name="SIZE" value="IQXO-951 2520"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8302091574">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091574?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091574"/>
<attribute name="SIZE" value="IQXO-951 2520"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_8302091578">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091578?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.95mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091578"/>
<attribute name="SIZE" value="IQXO-951 2520"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-951-2016" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-951-2016">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_830208445309">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208445309?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208445309"/>
<attribute name="SIZE" value="IQXO-951 2016"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_8302091579">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091579?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091579"/>
<attribute name="SIZE" value="IQXO-951 2016"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_8302091580">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091580?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091580"/>
<attribute name="SIZE" value="IQXO-951 2016"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_8302091581">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091581?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091581"/>
<attribute name="SIZE" value="IQXO-951 2016"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_8302091582">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091582?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091582"/>
<attribute name="SIZE" value="IQXO-951 2016"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_8302091583">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091583?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091583"/>
<attribute name="SIZE" value="IQXO-951 2016"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
<technology name="_8302091585">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/8302091585?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="0.8mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +105 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="8302091585"/>
<attribute name="SIZE" value="IQXO-951 2016"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="1.62 V to 3.63 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_CFPS-73" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-SO"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-73">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SO" pad="1"/>
</connects>
<technologies>
<technology name="_831009437">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831009437?ae"/>
<attribute name="FREQUENCY" value="100 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831009437"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="100 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831009440">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831009440?ae"/>
<attribute name="FREQUENCY" value="125 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831009440"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="125 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831009441">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831009441?ae"/>
<attribute name="FREQUENCY" value="80 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831009441"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="80 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831017885">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831017885?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831017885"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018036">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018036?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018036"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018037">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018037?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018037"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018038">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018038?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018038"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018039?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018039"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018040">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018040?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018040"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018041">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018041?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018041"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018042">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018042?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018042"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018043">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018043?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018043"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018044">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018044?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018044"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018045">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018045?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018045"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018077">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018077?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018077"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018287">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018287?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018287"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018379">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018379?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018379"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018534">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018534?ae"/>
<attribute name="FREQUENCY" value="6 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018534"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="6 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018538">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018538?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018538"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018541">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018541?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018541"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018545">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018545?ae"/>
<attribute name="FREQUENCY" value="60 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018545"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="60 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018577">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018577?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018577"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018610">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018610?ae"/>
<attribute name="FREQUENCY" value="3.6864 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018610"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="3.6864 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018785">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018785?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018785"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019170">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019170?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019170"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019203">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019203?ae"/>
<attribute name="FREQUENCY" value="32.768 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019203"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019710">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019710?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019710"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019870">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019870?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019870"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019928">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019928?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019928"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019966">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019966?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019966"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019987">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019987?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019987"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019992">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019992?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019992"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831020184">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831020184?ae"/>
<attribute name="FREQUENCY" value="14.31818 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831020184"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="14.31818 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831020392">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831020392?ae"/>
<attribute name="FREQUENCY" value="18.432 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831020392"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="18.432 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831020465">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831020465?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831020465"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831020466">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831020466?ae"/>
<attribute name="FREQUENCY" value="16.384 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831020466"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16.384 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831021270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831021270?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831021270"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831021890">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831021890?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831021890"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831022731">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831022731?ae"/>
<attribute name="FREQUENCY" value="100 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831022731"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="100 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831022825">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831022825?ae"/>
<attribute name="FREQUENCY" value="125 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831022825"/>
<attribute name="SIZE" value="CFPS-73"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="125 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_IQXO-791" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-E/D"/>
</gates>
<devices>
<device name="" package="WE-SPXO_IQXO-791">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="E/D" pad="1"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
</connects>
<technologies>
<technology name="_830206415701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830206415701?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830206415701"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830206415801">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830206415801?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830206415801"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208219901">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208219901?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208219901"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220001?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220001"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220101?ae"/>
<attribute name="FREQUENCY" value="12.288 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220101"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12.288 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220201?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220201"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220301?ae"/>
<attribute name="FREQUENCY" value="19.2 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220301"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="19.2 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220401">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220401?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220401"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220501?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220501"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220601">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220601?ae"/>
<attribute name="FREQUENCY" value="32.768 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220601"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="32.768 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220701?ae"/>
<attribute name="FREQUENCY" value="33.3333 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220701"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="33.3333 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_830208220901">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830208220901?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-20 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830208220901"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056289">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056289?ae"/>
<attribute name="FREQUENCY" value="12 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056289"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="12 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056290">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056290?ae"/>
<attribute name="FREQUENCY" value="13 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056290"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="13 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056293">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056293?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056293"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056294">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056294?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056294"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056295">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056295?ae"/>
<attribute name="FREQUENCY" value="24.576 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056295"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="24.576 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056296">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056296?ae"/>
<attribute name="FREQUENCY" value="25 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056296"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="25 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056297">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056297?ae"/>
<attribute name="FREQUENCY" value="26 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056297"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="26 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056298">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056298?ae"/>
<attribute name="FREQUENCY" value="27 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056298"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="27 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056299">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056299?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056299"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056300">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056300?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056300"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831056301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831056301?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831056301"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831061624">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831061624?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831061624"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831066657">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831066657?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831066657"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
<technology name="_831072801">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831072801?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="2.5mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831072801"/>
<attribute name="SIZE" value="IQXO-791"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="3.3 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-SPXO_CFPS-72" prefix="Y">
<description>&lt;b&gt;WE-SPXO Simple Packaged Quartz Oscillator&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Characteristics&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; SMT models
&lt;br&gt;Hermetically sealed
&lt;br&gt;Frequencies between 3.6864 MHz and 156.25 MHz plus 32.768 kHz
&lt;br&gt;Maximum operating temperatures range: -40 °C to 125 °C
&lt;br&gt;Stabilities down to ±25 ppm available
&lt;br&gt;Available supply voltages: 1.8 V; 2.5 V; 3.3 V; 5 V and 1.62 V to 3.63 V
&lt;br&gt;Available output signal types: CMOS; LVDS; LVPECL
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;
&lt;br&gt;
&lt;br&gt; Microprocessor
&lt;br&gt;Wireless Communication Devices
&lt;br&gt;Industrial Devices
&lt;br&gt;Real Time Clocks
&lt;br&gt;Wired Communication (e.g. Ethernet and USB)
&lt;br&gt;IoT
&lt;br&gt;Optical Network
&lt;br&gt;Audio and Multimedia Devices
&lt;br&gt;Test and Measurement Equipment
&lt;br&gt;Navigation and Locators
&lt;br&gt;&lt;br&gt; 

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o135918v209%20WE%20SPXO%20Group.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-SPXO/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-SPXO&lt;/a&gt;
&lt;br&gt;
&lt;br&gt;Updated by Ella 2025-03-07&lt;br&gt;
2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-SPXO_CFPS-SO"/>
</gates>
<devices>
<device name="" package="WE-SPXO_CFPS-72">
<connects>
<connect gate="G$1" pin="+VS" pad="4"/>
<connect gate="G$1" pin="GND" pad="2"/>
<connect gate="G$1" pin="OUT" pad="3"/>
<connect gate="G$1" pin="SO" pad="1"/>
</connects>
<technologies>
<technology name="_830201878701">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830201878701?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830201878701"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830202129201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830202129201?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830202129201"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_830202536501">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/830202536501?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="830202536501"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="25ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831009443">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831009443?ae"/>
<attribute name="FREQUENCY" value="80 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831009443"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="80 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831017735">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831017735?ae"/>
<attribute name="FREQUENCY" value="10 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831017735"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="10 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018032">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018032?ae"/>
<attribute name="FREQUENCY" value="20 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018032"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="20 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018033?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018033"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018034">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018034?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018034"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018035?ae"/>
<attribute name="FREQUENCY" value="50 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018035"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="50 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018739">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018739?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018739"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831018871">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831018871?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831018871"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="100ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019079">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019079?ae"/>
<attribute name="FREQUENCY" value="8 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019079"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="8 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019082?ae"/>
<attribute name="FREQUENCY" value="24 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019082"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="24 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019083">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019083?ae"/>
<attribute name="FREQUENCY" value="32 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019083"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="32 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019137">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019137?ae"/>
<attribute name="FREQUENCY" value="40 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019137"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="40 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019275">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019275?ae"/>
<attribute name="FREQUENCY" value="16 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019275"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="16 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019805">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019805?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019805"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831019884">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831019884?ae"/>
<attribute name="FREQUENCY" value="48 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="0 °C up to +70 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831019884"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="48 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
<technology name="_831020502">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/831020502?ae"/>
<attribute name="FREQUENCY" value="4 MHz"/>
<attribute name="HEIGHT" value="1.8mm"/>
<attribute name="LENGTH" value="7mm"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="OPERATING-TEMPERATURE" value="-40 °C up to +85 °C"/>
<attribute name="OUTPUT-LOGIC" value="CMOS"/>
<attribute name="PART-NUMBER" value="831020502"/>
<attribute name="SIZE" value="CFPS-72"/>
<attribute name="STABILITY" value="50ppm"/>
<attribute name="V-SUPPLY" value="5 V"/>
<attribute name="VALUE" value="4 MHz"/>
<attribute name="WIDTH" value="5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
