<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Dual Coil Power Inductors - WE-TDC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-TDC_8038">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-TDC SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;8038</description>
</package>
<package name="WE-TDC_8018">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-TDC SMD Shielded Coupled Inductor&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;8018</description>
</package>
</packages>
<symbols>
<symbol name="WE-TDC">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="4" direction="pas"/>
<pin name="3" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-TDC_8038" prefix="L">
<description>&lt;b&gt;WE-TDC SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt;Low profile
&lt;br&gt;Magnetical shielded which results in a low leakage field
&lt;br&gt;8x8 mm case
&lt;br&gt;Operating temperature range -40 up to 125°C
&lt;br&gt;1:1 transformer
&lt;br&gt;Low self-losses
&lt;br&gt;Higher Self Resonant Frequency
&lt;br&gt;Low leakage inductance
&lt;br&gt;Coupled inductor with two identical windings
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-Isolated Flyback Converter
&lt;br&gt;Buck or Boost with auxiliary winding
&lt;br&gt;BUCK-BOOST, SEPIC, ZETA &amp; CUK Converter
&lt;br&gt;Switching regulators with secound, unregulated output voltage
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14862v209%20Family_WE-TDC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14862v209%20Family_WE-TDC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-TDC"&gt;https://katalog.we-online.com/en/pbs/WE-TDC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Yingchun, Shan 2019-08-14&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TDC"/>
</gates>
<devices>
<device name="" package="WE-TDC_8038">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name="_744894400039">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744894400039.pdf"/>
<attribute name="FRE" value="210MHz"/>
<attribute name="IR1" value="4.5A"/>
<attribute name="IR2" value="4.5A"/>
<attribute name="ISAT" value="14A"/>
<attribute name="L2" value="0.39uH"/>
<attribute name="PART-NUMBER" value="744894400039"/>
<attribute name="RDC1-MAX" value="0.0145Ohm"/>
<attribute name="RDC1-TYP" value="0.0116Ohm"/>
<attribute name="RDC2-MAX" value="0.0145Ohm"/>
<attribute name="RDC2-TYP" value="0.0116Ohm"/>
<attribute name="VALUE" value="0.39uH"/>
</technology>
<technology name="_744894400082">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744894400082.pdf"/>
<attribute name="FRE" value="140MHz"/>
<attribute name="IR1" value="3.7A"/>
<attribute name="IR2" value="3.7A"/>
<attribute name="ISAT" value="9.6A"/>
<attribute name="L2" value="0.82uH"/>
<attribute name="PART-NUMBER" value="744894400082"/>
<attribute name="RDC1-MAX" value="0.02Ohm"/>
<attribute name="RDC1-TYP" value="0.0159Ohm"/>
<attribute name="RDC2-MAX" value="0.02Ohm"/>
<attribute name="RDC2-TYP" value="0.0159Ohm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_74489440012">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440012.pdf"/>
<attribute name="FRE" value="90MHz"/>
<attribute name="IR1" value="3.05A"/>
<attribute name="IR2" value="3.05A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="L2" value="1.2uH"/>
<attribute name="PART-NUMBER" value=" 74489440012 "/>
<attribute name="RDC1-MAX" value="0.026Ohm"/>
<attribute name="RDC1-TYP" value="0.0202Ohm"/>
<attribute name="RDC2-MAX" value="0.026Ohm"/>
<attribute name="RDC2-TYP" value="0.0202Ohm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_74489440018">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440018.pdf"/>
<attribute name="FRE" value="60MHz"/>
<attribute name="IR1" value="2.85A"/>
<attribute name="IR2" value="2.85A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="L2" value="1.8uH"/>
<attribute name="PART-NUMBER" value=" 74489440018 "/>
<attribute name="RDC1-MAX" value="0.031Ohm"/>
<attribute name="RDC1-TYP" value="0.0255Ohm"/>
<attribute name="RDC2-MAX" value="0.031Ohm"/>
<attribute name="RDC2-TYP" value="0.0255Ohm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_74489440027">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440027.pdf"/>
<attribute name="FRE" value="55MHz"/>
<attribute name="IR1" value="2.5A"/>
<attribute name="IR2" value="2.5A"/>
<attribute name="ISAT" value="5.1A"/>
<attribute name="L2" value="2.7uH"/>
<attribute name="PART-NUMBER" value=" 74489440027 "/>
<attribute name="RDC1-MAX" value="0.04Ohm"/>
<attribute name="RDC1-TYP" value="0.0345Ohm"/>
<attribute name="RDC2-MAX" value="0.04Ohm"/>
<attribute name="RDC2-TYP" value="0.0345Ohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_74489440036">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440036.pdf"/>
<attribute name="FRE" value="45MHz"/>
<attribute name="IR1" value="2.3A"/>
<attribute name="IR2" value="2.3A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="L2" value="3.6uH"/>
<attribute name="PART-NUMBER" value=" 74489440036 "/>
<attribute name="RDC1-MAX" value="0.053Ohm"/>
<attribute name="RDC1-TYP" value="0.047Ohm"/>
<attribute name="RDC2-MAX" value="0.053Ohm"/>
<attribute name="RDC2-TYP" value="0.047Ohm"/>
<attribute name="VALUE" value="3.6uH"/>
</technology>
<technology name="_74489440047">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440047.pdf"/>
<attribute name="FRE" value="30MHz"/>
<attribute name="IR1" value="1.85A"/>
<attribute name="IR2" value="1.85A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="L2" value="4.7uH"/>
<attribute name="PART-NUMBER" value=" 74489440047 "/>
<attribute name="RDC1-MAX" value="0.064Ohm"/>
<attribute name="RDC1-TYP" value="0.0545Ohm"/>
<attribute name="RDC2-MAX" value="0.064Ohm"/>
<attribute name="RDC2-TYP" value="0.0545Ohm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_74489440068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440068.pdf"/>
<attribute name="FRE" value="25MHz"/>
<attribute name="IR1" value="1.45A"/>
<attribute name="IR2" value="1.45A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 74489440068 "/>
<attribute name="RDC1-MAX" value="0.1Ohm"/>
<attribute name="RDC1-TYP" value="0.088Ohm"/>
<attribute name="RDC2-MAX" value="0.1Ohm"/>
<attribute name="RDC2-TYP" value="0.088Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74489440100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440100.pdf"/>
<attribute name="FRE" value="23MHz"/>
<attribute name="IR1" value="1.35A"/>
<attribute name="IR2" value="1.35A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 74489440100 "/>
<attribute name="RDC1-MAX" value="0.128Ohm"/>
<attribute name="RDC1-TYP" value="0.113Ohm"/>
<attribute name="RDC2-MAX" value="0.128Ohm"/>
<attribute name="RDC2-TYP" value="0.113Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74489440120">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440120.pdf"/>
<attribute name="FRE" value="20MHz"/>
<attribute name="IR1" value="1.3A"/>
<attribute name="IR2" value="1.3A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="L2" value="12uH"/>
<attribute name="PART-NUMBER" value=" 74489440120 "/>
<attribute name="RDC1-MAX" value="0.132Ohm"/>
<attribute name="RDC1-TYP" value="0.117Ohm"/>
<attribute name="RDC2-MAX" value="0.132Ohm"/>
<attribute name="RDC2-TYP" value="0.117Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_74489440150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440150.pdf"/>
<attribute name="FRE" value="17MHz"/>
<attribute name="IR1" value="1.1A"/>
<attribute name="IR2" value="1.1A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="L2" value="15uH"/>
<attribute name="PART-NUMBER" value=" 74489440150 "/>
<attribute name="RDC1-MAX" value="0.185Ohm"/>
<attribute name="RDC1-TYP" value="0.165Ohm"/>
<attribute name="RDC2-MAX" value="0.185Ohm"/>
<attribute name="RDC2-TYP" value="0.165Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74489440180">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440180.pdf"/>
<attribute name="FRE" value="15MHz"/>
<attribute name="IR1" value="1.05A"/>
<attribute name="IR2" value="1.05A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="L2" value="18uH"/>
<attribute name="PART-NUMBER" value=" 74489440180 "/>
<attribute name="RDC1-MAX" value="0.201Ohm"/>
<attribute name="RDC1-TYP" value="0.179Ohm"/>
<attribute name="RDC2-MAX" value="0.201Ohm"/>
<attribute name="RDC2-TYP" value="0.179Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_74489440220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489440220.pdf"/>
<attribute name="FRE" value="14MHz"/>
<attribute name="IR1" value="1A"/>
<attribute name="IR2" value="1A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 74489440220 "/>
<attribute name="RDC1-MAX" value="0.228Ohm"/>
<attribute name="RDC1-TYP" value="0.203Ohm"/>
<attribute name="RDC2-MAX" value="0.228Ohm"/>
<attribute name="RDC2-TYP" value="0.203Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TDC_8018" prefix="L">
<description>&lt;b&gt;WE-TDC SMD Shielded Coupled Inductor
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Core material: NiZn
&lt;br&gt;Low profile
&lt;br&gt;Magnetical shielded which results in a low leakage field
&lt;br&gt;8x8 mm case
&lt;br&gt;Operating temperature range -40 up to 125°C
&lt;br&gt;1:1 transformer
&lt;br&gt;Low self-losses
&lt;br&gt;Higher Self Resonant Frequency
&lt;br&gt;Low leakage inductance
&lt;br&gt;Coupled inductor with two identical windings
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Non-Isolated Flyback Converter
&lt;br&gt;Buck or Boost with auxiliary winding
&lt;br&gt;BUCK-BOOST, SEPIC, ZETA &amp; CUK Converter
&lt;br&gt;Switching regulators with secound, unregulated output voltage
&lt;br&gt;
&lt;br&gt;&lt;br&gt;&lt;br&gt;&lt;b&gt; Note: The "VALUE"shown in the symbol and packaging is the Inductance for L1,L2=L1&lt;br&gt;&lt;/b&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14862v209%20Family_WE-TDC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14862v209%20Family_WE-TDC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-TDC"&gt;https://katalog.we-online.com/en/pbs/WE-TDC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated  by  Yingchun, Shan 2019-08-14&lt;br&gt;
&lt;/b&gt;2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-TDC"/>
</gates>
<devices>
<device name="" package="WE-TDC_8018">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="4"/>
<connect gate="G$1" pin="3" pad="2"/>
<connect gate="G$1" pin="4" pad="3"/>
</connects>
<technologies>
<technology name="_744894300033">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744894300033.pdf"/>
<attribute name="FRE" value="280MHz"/>
<attribute name="IR1" value="4A"/>
<attribute name="IR2" value="4A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="L2" value="0.33uH"/>
<attribute name="PART-NUMBER" value="744894300033"/>
<attribute name="RDC1-MAX" value="0.015Ohm"/>
<attribute name="RDC1-TYP" value="0.0111Ohm"/>
<attribute name="RDC2-MAX" value="0.015Ohm"/>
<attribute name="RDC2-TYP" value="0.0111Ohm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_744894300068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/744894300068.pdf"/>
<attribute name="FRE" value="190MHz"/>
<attribute name="IR1" value="3.3A"/>
<attribute name="IR2" value="3.3A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="L2" value="0.68uH"/>
<attribute name="PART-NUMBER" value="744894300068"/>
<attribute name="RDC1-MAX" value="0.021Ohm"/>
<attribute name="RDC1-TYP" value="0.0163Ohm"/>
<attribute name="RDC2-MAX" value="0.021Ohm"/>
<attribute name="RDC2-TYP" value="0.0163Ohm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
<technology name="_74489430010">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430010.pdf"/>
<attribute name="FRE" value="136MHz"/>
<attribute name="IR1" value="2.85A"/>
<attribute name="IR2" value="2.85A"/>
<attribute name="ISAT" value="5.1A"/>
<attribute name="L2" value="1uH"/>
<attribute name="PART-NUMBER" value=" 74489430010 "/>
<attribute name="RDC1-MAX" value="0.028Ohm"/>
<attribute name="RDC1-TYP" value="0.0222Ohm"/>
<attribute name="RDC2-MAX" value="0.028Ohm"/>
<attribute name="RDC2-TYP" value="0.0222Ohm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_74489430022">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430022.pdf"/>
<attribute name="FRE" value="85MHz"/>
<attribute name="IR1" value="1.9A"/>
<attribute name="IR2" value="1.9A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="L2" value="2.2uH"/>
<attribute name="PART-NUMBER" value=" 74489430022 "/>
<attribute name="RDC1-MAX" value="0.058Ohm"/>
<attribute name="RDC1-TYP" value="0.0495Ohm"/>
<attribute name="RDC2-MAX" value="0.058Ohm"/>
<attribute name="RDC2-TYP" value="0.0495Ohm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_74489430027">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430027.pdf"/>
<attribute name="FRE" value="65MHz"/>
<attribute name="IR1" value="1.85A"/>
<attribute name="IR2" value="1.85A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="L2" value="2.7uH"/>
<attribute name="PART-NUMBER" value=" 74489430027 "/>
<attribute name="RDC1-MAX" value="0.805Ohm"/>
<attribute name="RDC1-TYP" value="0.0695Ohm"/>
<attribute name="RDC2-MAX" value="0.805Ohm"/>
<attribute name="RDC2-TYP" value="0.0695Ohm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_74489430039">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430039.pdf"/>
<attribute name="FRE" value="60MHz"/>
<attribute name="IR1" value="1.6A"/>
<attribute name="IR2" value="1.6A"/>
<attribute name="ISAT" value="2.55A"/>
<attribute name="L2" value="3.9uH"/>
<attribute name="PART-NUMBER" value=" 74489430039 "/>
<attribute name="RDC1-MAX" value="0.094Ohm"/>
<attribute name="RDC1-TYP" value="0.082Ohm"/>
<attribute name="RDC2-MAX" value="0.094Ohm"/>
<attribute name="RDC2-TYP" value="0.082Ohm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_74489430056">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430056.pdf"/>
<attribute name="FRE" value="50MHz"/>
<attribute name="IR1" value="1.45A"/>
<attribute name="IR2" value="1.45A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="L2" value="5.6uH"/>
<attribute name="PART-NUMBER" value=" 74489430056 "/>
<attribute name="RDC1-MAX" value="0.131Ohm"/>
<attribute name="RDC1-TYP" value="0.114Ohm"/>
<attribute name="RDC2-MAX" value="0.131Ohm"/>
<attribute name="RDC2-TYP" value="0.114Ohm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_74489430068">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430068.pdf"/>
<attribute name="FRE" value="46MHz"/>
<attribute name="IR1" value="1.25A"/>
<attribute name="IR2" value="1.25A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="L2" value="6.8uH"/>
<attribute name="PART-NUMBER" value=" 74489430068 "/>
<attribute name="RDC1-MAX" value="0.146Ohm"/>
<attribute name="RDC1-TYP" value="0.128Ohm"/>
<attribute name="RDC2-MAX" value="0.146Ohm"/>
<attribute name="RDC2-TYP" value="0.128Ohm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_74489430100">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430100.pdf"/>
<attribute name="FRE" value="35MHz"/>
<attribute name="IR1" value="1A"/>
<attribute name="IR2" value="1A"/>
<attribute name="ISAT" value="1.65A"/>
<attribute name="L2" value="10uH"/>
<attribute name="PART-NUMBER" value=" 74489430100 "/>
<attribute name="RDC1-MAX" value="0.215Ohm"/>
<attribute name="RDC1-TYP" value="0.19Ohm"/>
<attribute name="RDC2-MAX" value="0.215Ohm"/>
<attribute name="RDC2-TYP" value="0.19Ohm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_74489430120">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430120.pdf"/>
<attribute name="FRE" value="33MHz"/>
<attribute name="IR1" value="0.95A"/>
<attribute name="IR2" value="0.95A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="L2" value="12uH"/>
<attribute name="PART-NUMBER" value=" 74489430120 "/>
<attribute name="RDC1-MAX" value="0.227Ohm"/>
<attribute name="RDC1-TYP" value="0.202Ohm"/>
<attribute name="RDC2-MAX" value="0.227Ohm"/>
<attribute name="RDC2-TYP" value="0.202Ohm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_74489430150">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430150.pdf"/>
<attribute name="FRE" value="29MHz"/>
<attribute name="IR1" value="0.85A"/>
<attribute name="IR2" value="0.85A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="L2" value="15uH"/>
<attribute name="PART-NUMBER" value=" 74489430150 "/>
<attribute name="RDC1-MAX" value="0.308Ohm"/>
<attribute name="RDC1-TYP" value="0.275Ohm"/>
<attribute name="RDC2-MAX" value="0.308Ohm"/>
<attribute name="RDC2-TYP" value="0.275Ohm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_74489430180">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430180.pdf"/>
<attribute name="FRE" value="27MHz"/>
<attribute name="IR1" value="0.8A"/>
<attribute name="IR2" value="0.8A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="L2" value="18uH"/>
<attribute name="PART-NUMBER" value=" 74489430180 "/>
<attribute name="RDC1-MAX" value="0.38Ohm"/>
<attribute name="RDC1-TYP" value="0.345Ohm"/>
<attribute name="RDC2-MAX" value="0.38Ohm"/>
<attribute name="RDC2-TYP" value="0.345Ohm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_74489430220">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/74489430220.pdf"/>
<attribute name="FRE" value="17MHz"/>
<attribute name="IR1" value="0.7A"/>
<attribute name="IR2" value="0.7A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="L2" value="22uH"/>
<attribute name="PART-NUMBER" value=" 74489430220 "/>
<attribute name="RDC1-MAX" value="0.48Ohm"/>
<attribute name="RDC1-TYP" value="0.435Ohm"/>
<attribute name="RDC2-MAX" value="0.48Ohm"/>
<attribute name="RDC2-TYP" value="0.435Ohm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
