<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Single Coil Power Inductors - WE-TIF&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-TIF_1016">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1016</description>
</package>
<package name="WE-TIF_1018">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1018</description>
</package>
<package name="WE-TIF_1014">
<description>&lt;b&gt; &lt;br&gt;&lt;b&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;br&gt;&lt;/b&gt;
&lt;pre&gt; &lt;b&gt;&lt;font size="4"&gt;Size: &lt;/b&gt;1014</description>
</package>
</packages>
<symbols>
<symbol name="L-POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-TIF_1016" prefix="L">
<description>&lt;B&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Radial through-hole inductor &lt;br&gt;
High saturation core material&lt;br&gt;
 Maximum current up to 3.1 A &lt;br&gt;
2 additional pins for high mechanical stability&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Signal filtering &lt;br&gt;
EMI and power supply filter&lt;br&gt;
 DC/DC converters &lt;br&gt;
Switching power&lt;br&gt;
 Supplies for small and medium voltage&lt;br&gt; 
Power supply for LED &lt;br&gt;
Nearfield applications &lt;br&gt;



&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14866v209%20Family_WE-TIF_E.jpgg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14866v209%20Family_WE-TIF_E.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-TIF"&gt;https://katalog.we-online.com/en/pbs/WE-TIF&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun,Shan 2019-08-13&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-POINT"/>
</gates>
<devices>
<device name="" package="WE-TIF_1016">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447221101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="2.45A"/>
<attribute name="ISAT" value="2.75A"/>
<attribute name="PART-NUMBER" value=" 7447221101 "/>
<attribute name="RDC-MAX" value="100Ohm"/>
<attribute name="RDC-TYP" value="85mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_7447221102">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 7447221102 "/>
<attribute name="RDC-MAX" value="980Ohm"/>
<attribute name="RDC-TYP" value="850mOhm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_7447221103">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.26MHz"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.29A"/>
<attribute name="PART-NUMBER" value=" 7447221103 "/>
<attribute name="RDC-MAX" value="9700Ohm"/>
<attribute name="RDC-TYP" value="8400mOhm"/>
<attribute name="VALUE" value="10000uH"/>
</technology>
<technology name="_7447221221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 7447221221 "/>
<attribute name="RDC-MAX" value="220Ohm"/>
<attribute name="RDC-TYP" value="190mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_7447221222">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.65MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.61A"/>
<attribute name="PART-NUMBER" value=" 7447221222 "/>
<attribute name="RDC-MAX" value="2100Ohm"/>
<attribute name="RDC-TYP" value="1850mOhm"/>
<attribute name="VALUE" value="2200uH"/>
</technology>
<technology name="_7447221331">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="PART-NUMBER" value=" 7447221331 "/>
<attribute name="RDC-MAX" value="320Ohm"/>
<attribute name="RDC-TYP" value="280mOhm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_7447221332">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.5MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 7447221332 "/>
<attribute name="RDC-MAX" value="3200Ohm"/>
<attribute name="RDC-TYP" value="2800mOhm"/>
<attribute name="VALUE" value="3300uH"/>
</technology>
<technology name="_7447221471">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.6MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 7447221471 "/>
<attribute name="RDC-MAX" value="460Ohm"/>
<attribute name="RDC-TYP" value="400mOhm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_7447221472">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.41MHz"/>
<attribute name="IR" value="0.34A"/>
<attribute name="ISAT" value="0.42A"/>
<attribute name="PART-NUMBER" value=" 7447221472 "/>
<attribute name="RDC-MAX" value="4600Ohm"/>
<attribute name="RDC-TYP" value="4000mOhm"/>
<attribute name="VALUE" value="4700uH"/>
</technology>
<technology name="_7447221681">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.3MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7447221681 "/>
<attribute name="RDC-MAX" value="670Ohm"/>
<attribute name="RDC-TYP" value="580mOhm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_7447221682">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.33MHz"/>
<attribute name="IR" value="0.28A"/>
<attribute name="ISAT" value="0.35A"/>
<attribute name="PART-NUMBER" value=" 7447221682 "/>
<attribute name="RDC-MAX" value="6600Ohm"/>
<attribute name="RDC-TYP" value="5700mOhm"/>
<attribute name="VALUE" value="6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIF_1018" prefix="L">
<description>&lt;B&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Radial through-hole inductor &lt;br&gt;
High saturation core material&lt;br&gt;
 Maximum current up to 3.1 A &lt;br&gt;
2 additional pins for high mechanical stability&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Signal filtering &lt;br&gt;
EMI and power supply filter&lt;br&gt;
 DC/DC converters &lt;br&gt;
Switching power&lt;br&gt;
 Supplies for small and medium voltage&lt;br&gt; 
Power supply for LED &lt;br&gt;
Nearfield applications &lt;br&gt;



&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14866v209%20Family_WE-TIF_E.jpgg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14866v209%20Family_WE-TIF_E.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-TIF"&gt;https://katalog.we-online.com/en/pbs/WE-TIF&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun,Shan 2019-08-13&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-POINT"/>
</gates>
<devices>
<device name="" package="WE-TIF_1018">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447231101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="3.6MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="3.1A"/>
<attribute name="PART-NUMBER" value=" 7447231101 "/>
<attribute name="RDC-MAX" value="90Ohm"/>
<attribute name="RDC-TYP" value="75mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_7447231102">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.1MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 7447231102 "/>
<attribute name="RDC-MAX" value="860Ohm"/>
<attribute name="RDC-TYP" value="750mOhm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_7447231103">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.32MHz"/>
<attribute name="IR" value="0.25A"/>
<attribute name="ISAT" value="0.32A"/>
<attribute name="PART-NUMBER" value=" 7447231103 "/>
<attribute name="RDC-MAX" value="8500Ohm"/>
<attribute name="RDC-TYP" value="7400mOhm"/>
<attribute name="VALUE" value="10000uH"/>
</technology>
<technology name="_7447231221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="2.4MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="PART-NUMBER" value=" 7447231221 "/>
<attribute name="RDC-MAX" value="200mOhm"/>
<attribute name="RDC-TYP" value="170mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_7447231222">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.72MHz"/>
<attribute name="IR" value="0.54A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 7447231222 "/>
<attribute name="RDC-MAX" value="1900Ohm"/>
<attribute name="RDC-TYP" value="1650mOhm"/>
<attribute name="VALUE" value="2200uH"/>
</technology>
<technology name="_7447231331">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.9MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.75A"/>
<attribute name="PART-NUMBER" value=" 7447231331 "/>
<attribute name="RDC-MAX" value="290mOhm"/>
<attribute name="RDC-TYP" value="250mOhm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_7447231332">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.58MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="PART-NUMBER" value=" 7447231332 "/>
<attribute name="RDC-MAX" value="2800Ohm"/>
<attribute name="RDC-TYP" value="2450mOhm"/>
<attribute name="VALUE" value="3300uH"/>
</technology>
<technology name="_7447231471">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.6MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 7447231471 "/>
<attribute name="RDC-MAX" value="410mOhm"/>
<attribute name="RDC-TYP" value="360mOhm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_7447231472">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.48MHz"/>
<attribute name="IR" value="0.36A"/>
<attribute name="ISAT" value="0.47A"/>
<attribute name="PART-NUMBER" value=" 7447231472 "/>
<attribute name="RDC-MAX" value="4000Ohm"/>
<attribute name="RDC-TYP" value="3500mOhm"/>
<attribute name="VALUE" value="4700uH"/>
</technology>
<technology name="_7447231681">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.3MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value=" 1.2 "/>
<attribute name="PART-NUMBER" value=" 7447231681 "/>
<attribute name="RDC-MAX" value="590mOhm"/>
<attribute name="RDC-TYP" value="510mOhm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_7447231682">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.4MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.39A"/>
<attribute name="PART-NUMBER" value=" 7447231682 "/>
<attribute name="RDC-MAX" value="5750Ohm"/>
<attribute name="RDC-TYP" value="5000mOhm"/>
<attribute name="VALUE" value="6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TIF_1014" prefix="L">
<description>&lt;B&gt;WE-TIF Radial Leaded Wire Wound Inductor with 4 Pins&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;
&lt;B&gt;Characteristics&lt;br&gt;&lt;/b&gt;&lt;br&gt;
Radial through-hole inductor &lt;br&gt;
High saturation core material&lt;br&gt;
 Maximum current up to 3.1 A &lt;br&gt;
2 additional pins for high mechanical stability&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Application&lt;/b&gt;&lt;br&gt;
&lt;br&gt;
Signal filtering &lt;br&gt;
EMI and power supply filter&lt;br&gt;
 DC/DC converters &lt;br&gt;
Switching power&lt;br&gt;
 Supplies for small and medium voltage&lt;br&gt; 
Power supply for LED &lt;br&gt;
Nearfield applications &lt;br&gt;



&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14866v209%20Family_WE-TIF_E.jpgg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14866v209%20Family_WE-TIF_E.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-TIF"&gt;https://katalog.we-online.com/en/pbs/WE-TIF&lt;/a&gt;&lt;p&gt;

Updated by  Yingchun,Shan 2019-08-13&lt;br&gt;
2019(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-POINT"/>
</gates>
<devices>
<device name="" package="WE-TIF_1014">
<connects>
<connect gate="G$1" pin="1" pad="3"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7447211101">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="PART-NUMBER" value=" 7447211101 "/>
<attribute name="RDC-MAX" value="115Ohm"/>
<attribute name="RDC-TYP" value="100mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_7447211102">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1MHz"/>
<attribute name="IR" value="0.68A"/>
<attribute name="ISAT" value="0.92A"/>
<attribute name="PART-NUMBER" value=" 7447211102 "/>
<attribute name="RDC-MAX" value="1100Ohm"/>
<attribute name="RDC-TYP" value="960mOhm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_7447211103">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.26MHz"/>
<attribute name="IR" value="0.21A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="PART-NUMBER" value=" 7447211103 "/>
<attribute name="RDC-MAX" value="10700Ohm"/>
<attribute name="RDC-TYP" value="9300mOhm"/>
<attribute name="VALUE" value="10000uH"/>
</technology>
<technology name="_7447211221">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="2.5MHz"/>
<attribute name="IR" value="1.47A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 7447211221 "/>
<attribute name="RDC-MAX" value="250Ohm"/>
<attribute name="RDC-TYP" value="220mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_7447211222">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.65MHz"/>
<attribute name="IR" value="0.46A"/>
<attribute name="ISAT" value="0.63A"/>
<attribute name="PART-NUMBER" value=" 7447211222 "/>
<attribute name="RDC-MAX" value="2400Ohm"/>
<attribute name="RDC-TYP" value="2100mOhm"/>
<attribute name="VALUE" value="2200uH"/>
</technology>
<technology name="_7447211331">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="PART-NUMBER" value=" 7447211331 "/>
<attribute name="RDC-MAX" value="370Ohm"/>
<attribute name="RDC-TYP" value="320mOhm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_7447211332">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.5MHz"/>
<attribute name="IR" value="0.37A"/>
<attribute name="ISAT" value="0.52A"/>
<attribute name="PART-NUMBER" value=" 7447211332 "/>
<attribute name="RDC-MAX" value="3600Ohm"/>
<attribute name="RDC-TYP" value="3100mOhm"/>
<attribute name="VALUE" value="3300uH"/>
</technology>
<technology name="_7447211471">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.6MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="PART-NUMBER" value=" 7447211471 "/>
<attribute name="RDC-MAX" value="530Ohm"/>
<attribute name="RDC-TYP" value="460mOhm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_7447211472">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.41MHz"/>
<attribute name="IR" value="0.31A"/>
<attribute name="ISAT" value="0.43A"/>
<attribute name="PART-NUMBER" value=" 7447211472 "/>
<attribute name="RDC-MAX" value="5100Ohm"/>
<attribute name="RDC-TYP" value="4400mOhm"/>
<attribute name="VALUE" value="4700uH"/>
</technology>
<technology name="_7447211681">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="1.3MHz"/>
<attribute name="IR" value="0.83A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7447211681 "/>
<attribute name="RDC-MAX" value="760Ohm"/>
<attribute name="RDC-TYP" value="660mOhm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
<technology name="_7447211682">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/.pdf"/>
<attribute name="FRES" value="0.33MHz"/>
<attribute name="IR" value="0.26A"/>
<attribute name="ISAT" value="0.36A"/>
<attribute name="PART-NUMBER" value=" 7447211682 "/>
<attribute name="RDC-MAX" value="7400Ohm"/>
<attribute name="RDC-TYP" value="6400mOhm"/>
<attribute name="VALUE" value="6800uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
