<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - PFC Chokes - WE-TORPFC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-02-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-TORPFC_T50_76080X202">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T37_76080X403">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T50_76080X201">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T50_76080X203">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T43_76080X122">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T43_76080X101">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T37_76080X401">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T75_76080X3X1">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
<package name="WE-TORPFC_T43_76080X102">
<description>&lt;b&gt;WE-TORPFC Toroidal PFC Chokes</description>
</package>
</packages>
<symbols>
<symbol name="L">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-TORPFC_T50" prefix="L">
<description>&lt;b&gt; WE-TORPFC Toroidal PFC Chokes
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Typical topology Boost CCM
&lt;br&gt;Offline working voltage
&lt;br&gt;Flat Wire windings, low DCR and allow better cooling
&lt;br&gt;Operating Temperature Range -40ºC to +155ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Fixed chargers on streets and garages (EV charger)
&lt;br&gt;Solar Inverters
&lt;br&gt;Industrial or Medical AC-DC
&lt;br&gt;Telecom PSU
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TORPFC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-TORPFC&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
&lt;/b&gt;Created by Ella Wu 2023-06-21&lt;br&gt;
&lt;/b&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_76080X201" package="WE-TORPFC_T50_76080X201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800201?ae"/>
<attribute name="DIAMETER" value="72mm"/>
<attribute name="HEIGHT" value="31mm"/>
<attribute name="IR" value="12.4A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="L" value="194uH"/>
<attribute name="PART-NUMBER" value="760800201"/>
<attribute name="RDC-MAX" value="40mOhm"/>
<attribute name="SIZE" value="T50"/>
<attribute name="VALUE" value="194uH"/>
</technology>
<technology name="_760801201">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801201?ae"/>
<attribute name="DIAMETER" value="72mm"/>
<attribute name="HEIGHT" value="31mm"/>
<attribute name="IR" value="12.4A"/>
<attribute name="ISAT" value="37A"/>
<attribute name="L" value="194uH"/>
<attribute name="PART-NUMBER" value="760801201"/>
<attribute name="RDC-MAX" value="40mOhm"/>
<attribute name="SIZE" value="T50"/>
<attribute name="VALUE" value="194uH"/>
</technology>
</technologies>
</device>
<device name="_76080X202" package="WE-TORPFC_T50_76080X202">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800202">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800202?ae"/>
<attribute name="DIAMETER" value="72mm"/>
<attribute name="HEIGHT" value="45mm"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="L" value="389uH"/>
<attribute name="PART-NUMBER" value="760800202"/>
<attribute name="RDC-MAX" value="50mOhm"/>
<attribute name="SIZE" value="T50"/>
<attribute name="VALUE" value="389uH"/>
</technology>
<technology name="_760801202">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801202?ae"/>
<attribute name="DIAMETER" value="72mm"/>
<attribute name="HEIGHT" value="45mm"/>
<attribute name="IR" value="11.5A"/>
<attribute name="ISAT" value="37A"/>
<attribute name="L" value="389uH"/>
<attribute name="PART-NUMBER" value="760801202"/>
<attribute name="RDC-MAX" value="50mOhm"/>
<attribute name="SIZE" value="T50"/>
<attribute name="VALUE" value="389uH"/>
</technology>
</technologies>
</device>
<device name="_76080X203" package="WE-TORPFC_T50_76080X203">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800203">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800203?ae"/>
<attribute name="DIAMETER" value="72mm"/>
<attribute name="HEIGHT" value="60mm"/>
<attribute name="IR" value="11.7A"/>
<attribute name="ISAT" value="19A"/>
<attribute name="L" value="584uH"/>
<attribute name="PART-NUMBER" value="760800203"/>
<attribute name="RDC-MAX" value="65mOhm"/>
<attribute name="SIZE" value="T50"/>
<attribute name="VALUE" value="584uH"/>
</technology>
<technology name="_760801203">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801203?ae"/>
<attribute name="DIAMETER" value="72mm"/>
<attribute name="HEIGHT" value="60mm"/>
<attribute name="IR" value="11.7A"/>
<attribute name="ISAT" value="37A"/>
<attribute name="L" value="584uH"/>
<attribute name="PART-NUMBER" value="760801203"/>
<attribute name="RDC-MAX" value="65mOhm"/>
<attribute name="SIZE" value="T50"/>
<attribute name="VALUE" value="584uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TORPFC_T37" prefix="L">
<description>&lt;b&gt; WE-TORPFC Toroidal PFC Chokes
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Typical topology Boost CCM
&lt;br&gt;Offline working voltage
&lt;br&gt;Flat Wire windings, low DCR and allow better cooling
&lt;br&gt;Operating Temperature Range -40ºC to +155ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Fixed chargers on streets and garages (EV charger)
&lt;br&gt;Solar Inverters
&lt;br&gt;Industrial or Medical AC-DC
&lt;br&gt;Telecom PSU
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TORPFC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-TORPFC&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
&lt;/b&gt;Created by Ella Wu 2023-06-21&lt;br&gt;
&lt;/b&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_76080X401" package="WE-TORPFC_T37_76080X401">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800401">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800401?ae"/>
<attribute name="DIAMETER" value="53mm"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="IR" value="13.9A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="L" value="118uH"/>
<attribute name="PART-NUMBER" value="760800401"/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value="T37"/>
<attribute name="VALUE" value="118uH"/>
</technology>
<technology name="_760801401">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801401?ae"/>
<attribute name="DIAMETER" value="53mm"/>
<attribute name="HEIGHT" value="28mm"/>
<attribute name="IR" value="13.9A"/>
<attribute name="ISAT" value="23A"/>
<attribute name="L" value="118uH"/>
<attribute name="PART-NUMBER" value="760801401"/>
<attribute name="RDC-MAX" value="22mOhm"/>
<attribute name="SIZE" value="T37"/>
<attribute name="VALUE" value="118uH"/>
</technology>
</technologies>
</device>
<device name="_76080X403" package="WE-TORPFC_T37_76080X403">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800403">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800403?ae"/>
<attribute name="DIAMETER" value="53mm"/>
<attribute name="HEIGHT" value="50mm"/>
<attribute name="IR" value="12.3A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="L" value="355uH"/>
<attribute name="PART-NUMBER" value="760800403"/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="SIZE" value="T37"/>
<attribute name="VALUE" value="355uH"/>
</technology>
<technology name="_760801403">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801403?ae"/>
<attribute name="DIAMETER" value="53mm"/>
<attribute name="HEIGHT" value="50mm"/>
<attribute name="IR" value="12.3A"/>
<attribute name="ISAT" value="23A"/>
<attribute name="L" value="355uH"/>
<attribute name="PART-NUMBER" value="760801403"/>
<attribute name="RDC-MAX" value="35mOhm"/>
<attribute name="SIZE" value="T37"/>
<attribute name="VALUE" value="355uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TORPFC_T75" prefix="L">
<description>&lt;b&gt; WE-TORPFC Toroidal PFC Chokes
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Typical topology Boost CCM
&lt;br&gt;Offline working voltage
&lt;br&gt;Flat Wire windings, low DCR and allow better cooling
&lt;br&gt;Operating Temperature Range -40ºC to +155ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Fixed chargers on streets and garages (EV charger)
&lt;br&gt;Solar Inverters
&lt;br&gt;Industrial or Medical AC-DC
&lt;br&gt;Telecom PSU
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TORPFC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-TORPFC&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
&lt;/b&gt;Created by Ella Wu 2023-06-21&lt;br&gt;
&lt;/b&gt;2023 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_76080X3X1" package="WE-TORPFC_T75_76080X3X1">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800301?ae"/>
<attribute name="DIAMETER" value="99mm"/>
<attribute name="HEIGHT" value="62mm"/>
<attribute name="IR" value="24.5A"/>
<attribute name="ISAT" value="43A"/>
<attribute name="L" value="180uH"/>
<attribute name="PART-NUMBER" value="760800301"/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="SIZE" value="T75"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_760801301">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801301?ae"/>
<attribute name="DIAMETER" value="99mm"/>
<attribute name="HEIGHT" value="62mm"/>
<attribute name="IR" value="24.5A"/>
<attribute name="ISAT" value="105A"/>
<attribute name="L" value="180uH"/>
<attribute name="PART-NUMBER" value="760801301"/>
<attribute name="RDC-MAX" value="20mOhm"/>
<attribute name="SIZE" value="T75"/>
<attribute name="VALUE" value="180uH"/>
</technology>
<technology name="_760801321">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801321?ae"/>
<attribute name="DIAMETER" value="99mm"/>
<attribute name="HEIGHT" value="62mm"/>
<attribute name="IR" value="17.2A"/>
<attribute name="ISAT" value="38A"/>
<attribute name="L" value="720uH"/>
<attribute name="PART-NUMBER" value="760801321"/>
<attribute name="RDC-MAX" value="42mOhm"/>
<attribute name="SIZE" value="T75"/>
<attribute name="VALUE" value="720uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TORPFC_T43" prefix="L">
<description>&lt;b&gt; WE-TORPFC Toroidal PFC Chokes
&lt;br&gt;
&lt;br&gt;Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Typical topology Boost CCM
&lt;br&gt;Offline working voltage
&lt;br&gt;Flat Wire windings, low DCR and allow better cooling
&lt;br&gt;Operating Temperature Range -40ºC to +155ºC
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Fixed chargers on streets and garages (EV charger)
&lt;br&gt;Solar Inverters
&lt;br&gt;Industrial or Medical AC-DC
&lt;br&gt;Telecom PSU
&lt;br&gt;
&lt;br&gt;
&lt;/b&gt;&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o719897v209%20Family-WE-PFC-76080XXXX.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-TORPFC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-TORPFC&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
&lt;/b&gt;Updated by Ella Wu 2025-02-24&lt;br&gt;
&lt;/b&gt;2025 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L"/>
</gates>
<devices>
<device name="_76080X101" package="WE-TORPFC_T43_76080X101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800101?ae"/>
<attribute name="DIAMETER" value="60mm"/>
<attribute name="HEIGHT" value="34mm"/>
<attribute name="IR" value="11.2A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="L" value="255uH"/>
<attribute name="PART-NUMBER" value="760800101"/>
<attribute name="RDC-MAX" value="36mOhm"/>
<attribute name="SIZE" value="T43"/>
<attribute name="VALUE" value="255uH"/>
</technology>
<technology name="_760801101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801101?ae"/>
<attribute name="DIAMETER" value="60mm"/>
<attribute name="HEIGHT" value="34mm"/>
<attribute name="IR" value="11.2A"/>
<attribute name="ISAT" value="24A"/>
<attribute name="L" value="255uH"/>
<attribute name="PART-NUMBER" value="760801101"/>
<attribute name="RDC-MAX" value="36mOhm"/>
<attribute name="SIZE" value="T43"/>
<attribute name="VALUE" value="255uH"/>
</technology>
</technologies>
</device>
<device name="_76080X102" package="WE-TORPFC_T43_76080X102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760800102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760800102?ae"/>
<attribute name="DIAMETER" value="60mm"/>
<attribute name="HEIGHT" value="54.5mm"/>
<attribute name="IR" value="9.8A"/>
<attribute name="ISAT" value="10.5A"/>
<attribute name="L" value="510uH"/>
<attribute name="PART-NUMBER" value="760800102"/>
<attribute name="RDC-MAX" value="55mOhm"/>
<attribute name="SIZE" value="T43"/>
<attribute name="VALUE" value="510uH"/>
</technology>
<technology name="_760801102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801102?ae"/>
<attribute name="DIAMETER" value="60mm"/>
<attribute name="HEIGHT" value="54.5mm"/>
<attribute name="IR" value="9.8A"/>
<attribute name="ISAT" value="24A"/>
<attribute name="L" value="510uH"/>
<attribute name="PART-NUMBER" value="760801102"/>
<attribute name="RDC-MAX" value="55mOhm"/>
<attribute name="SIZE" value="T43"/>
<attribute name="VALUE" value="510uH"/>
</technology>
</technologies>
</device>
<device name="_76080X122" package="WE-TORPFC_T43_76080X122">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_760801122">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760801122?ae"/>
<attribute name="DIAMETER" value="60mm"/>
<attribute name="HEIGHT" value="54.5mm"/>
<attribute name="IR" value="25.3A"/>
<attribute name="ISAT" value="45A"/>
<attribute name="L" value="132.75uH"/>
<attribute name="PART-NUMBER" value="760801122"/>
<attribute name="RDC-MAX" value="14mOhm"/>
<attribute name="SIZE" value="T43"/>
<attribute name="VALUE" value="132.75uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
