<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Single Coil Power Inductors - WE-TPC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2023b, 2023-05-15&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-TPC_8043">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8043, SMT, 4pins
&lt;br&gt;LXWXH=8X8X4.3mm</description>
</package>
<package name="WE-TPC_8015">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8015, SMT, 4pins
&lt;br&gt;LXWXH=8X8X1.35mm</description>
</package>
<package name="WE-TPC_1028">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1028, SMT, 2pins
&lt;br&gt;LXWXH=10X10X2.8mm</description>
</package>
<package name="WE-TPC_1038">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 1038, SMT, 2pins
&lt;br&gt;LXWXH=10X10X3.8mm</description>
</package>
<package name="WE-TPC_4828">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4828, SMT, 2pins
&lt;br&gt;LXWXH=4.8X4.8X2.8mm</description>
</package>
<package name="WE-TPC_5828">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 5828, SMT, 2pins
&lt;br&gt;LXWXH=5.8X5.8X2.8mm</description>
</package>
<package name="WE-TPC_4818">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 4818, SMT, 2pins
&lt;br&gt;LXWXH=4.8X4.8X1.8mm</description>
</package>
<package name="WE-TPC_2811">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2811, SMT, 2pins
&lt;br&gt;LXWXH=2.78X2.8X1.1mm</description>
</package>
<package name="WE-TPC_8020">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8020, SMT, 4pins
&lt;br&gt;LXWXH=8X8X1.8mm</description>
</package>
<package name="WE-TPC_2828">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2828, SMT, 2pins
&lt;br&gt;LXWXH=2.8X2.8X2.8mm</description>
</package>
<package name="WE-TPC_3816">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 3816, SMT, 2pins
&lt;br&gt;LXWXH=3.8X3.8X1.65mm</description>
</package>
<package name="WE-TPC_8012">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 8012, SMT, 4pins
&lt;br&gt;LXWXH=8X8X1.1mm</description>
</package>
<package name="WE-TPC_5818">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 5818, SMT, 2pins
&lt;br&gt;LXWXH=5.8X5.8X1.8mm</description>
</package>
<package name="WE-TPC_3510">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 3510, SMT, 2pins
&lt;br&gt;LXWXH=2.78X2.78X1.35mm</description>
</package>
<package name="WE-TPC_6823">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 6823, SMT, 2pins
&lt;br&gt;LXWXH=6.8X6.8X2.3mm</description>
</package>
<package name="WE-TPC_2813">
<description>&lt;b&gt;WE-TPC SMD Tiny Power Inductorr&lt;br&gt;&lt;/b&gt;
&lt;br&gt;Size: 2813, SMT, 2pins
&lt;br&gt;LXWXH=2.78X2.78X1.35mm</description>
</package>
</packages>
<symbols>
<symbol name="L_GAP">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L_GAP_POINT">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L_GAP_PADNAME">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-TPC_1028" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-TPC_1028">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744065001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065001?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="ISAT" value="9.5A"/>
<attribute name="PART-NUMBER" value=" 744065001 "/>
<attribute name="RDC" value="4.9mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7440650015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440650015?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="7.2A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="PART-NUMBER" value=" 7440650015 "/>
<attribute name="RDC" value="7.3mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7440650022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440650022?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="5.9A"/>
<attribute name="PART-NUMBER" value=" 7440650022 "/>
<attribute name="RDC" value="11mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7440650033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440650033?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="PART-NUMBER" value=" 7440650033 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7440650047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440650047?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="PART-NUMBER" value=" 7440650047 "/>
<attribute name="RDC" value="16.5mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7440650068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440650068?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="4.2A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="PART-NUMBER" value=" 7440650068 "/>
<attribute name="RDC" value="25mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7440650082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440650082?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="PART-NUMBER" value=" 7440650082 "/>
<attribute name="RDC" value="28.5mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744065100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065100?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="PART-NUMBER" value=" 744065100 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744065101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065101?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 744065101 "/>
<attribute name="RDC" value="365mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744065121">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065121?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="PART-NUMBER" value=" 744065121 "/>
<attribute name="RDC" value="428mOhm"/>
<attribute name="VALUE" value="120uH"/>
</technology>
<technology name="_744065150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065150?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.25A"/>
<attribute name="PART-NUMBER" value=" 744065150 "/>
<attribute name="RDC" value="69mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744065151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065151?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="PART-NUMBER" value=" 744065151 "/>
<attribute name="RDC" value="530mOhm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744065220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065220?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 744065220 "/>
<attribute name="RDC" value="104mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744065221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065221?ae"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="PART-NUMBER" value=" 744065221 "/>
<attribute name="RDC" value="750mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744065330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065330?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 744065330 "/>
<attribute name="RDC" value="139mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744065470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065470?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="PART-NUMBER" value=" 744065470 "/>
<attribute name="RDC" value="167mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744065560">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065560?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744065560 "/>
<attribute name="RDC" value="208mOhm"/>
<attribute name="VALUE" value="56uH"/>
</technology>
<technology name="_744065680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065680?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="PART-NUMBER" value=" 744065680 "/>
<attribute name="RDC" value="232mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_744065820">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744065820?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 744065820 "/>
<attribute name="RDC" value="323mOhm"/>
<attribute name="VALUE" value="82uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_1038" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-TPC_1038">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7440660015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440660015?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="9.6A"/>
<attribute name="ISAT" value="10A"/>
<attribute name="PART-NUMBER" value=" 7440660015 "/>
<attribute name="RDC" value="6.6mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_7440660022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440660022?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="8.8A"/>
<attribute name="ISAT" value="6.8A"/>
<attribute name="PART-NUMBER" value=" 7440660022 "/>
<attribute name="RDC" value="8.2mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7440660035">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440660035?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="6.6A"/>
<attribute name="ISAT" value="6.4A"/>
<attribute name="PART-NUMBER" value=" 7440660035 "/>
<attribute name="RDC" value="13mOhm"/>
<attribute name="VALUE" value="3.5uH"/>
</technology>
<technology name="_744066005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066005?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="5.3A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="PART-NUMBER" value=" 744066005 "/>
<attribute name="RDC" value="16.8mOhm"/>
<attribute name="VALUE" value="5uH"/>
</technology>
<technology name="_7440660062">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440660062?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="PART-NUMBER" value=" 7440660062 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_744066100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066100?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 744066100 "/>
<attribute name="RDC" value="27mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744066101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066101?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="PART-NUMBER" value=" 744066101 "/>
<attribute name="RDC" value="265mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744066150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066150?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="3.25A"/>
<attribute name="PART-NUMBER" value=" 744066150 "/>
<attribute name="RDC" value="45mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744066151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066151?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744066151 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744066180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066180?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="2.95A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 744066180 "/>
<attribute name="RDC" value="48mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744066220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066220?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="PART-NUMBER" value=" 744066220 "/>
<attribute name="RDC" value="63mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744066221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066221?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="PART-NUMBER" value=" 744066221 "/>
<attribute name="RDC" value="505mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744066330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066330?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 744066330 "/>
<attribute name="RDC" value="92mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744066331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066331?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 744066331 "/>
<attribute name="RDC" value="750mOhm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_744066470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066470?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.85A"/>
<attribute name="PART-NUMBER" value=" 744066470 "/>
<attribute name="RDC" value="138mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744066680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066680?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 744066680 "/>
<attribute name="RDC" value="155mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
<technology name="_744066681">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744066681?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="IR" value="0.46A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744066681 "/>
<attribute name="RDC" value="1750mOhm"/>
<attribute name="VALUE" value="680uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_4828" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-TPC_4828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404300033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74404300033?ae"/>
<attribute name="FRES" value="400MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value=" 74404300033 "/>
<attribute name="RDC" value="8mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_74404300047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74404300047?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="5A"/>
<attribute name="PART-NUMBER" value=" 74404300047 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74404300082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74404300082?ae"/>
<attribute name="FRES" value="170MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="ISAT" value="3.7A"/>
<attribute name="PART-NUMBER" value=" 74404300082 "/>
<attribute name="RDC" value="14mOhm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_7440430012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440430012?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="PART-NUMBER" value=" 7440430012 "/>
<attribute name="RDC" value="17mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_7440430018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440430018?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="2.45A"/>
<attribute name="PART-NUMBER" value=" 7440430018 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_7440430022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440430022?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.35A"/>
<attribute name="PART-NUMBER" value=" 7440430022 "/>
<attribute name="RDC" value="27mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7440430027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440430027?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="2.35A"/>
<attribute name="ISAT" value="1.95A"/>
<attribute name="PART-NUMBER" value=" 7440430027 "/>
<attribute name="RDC" value="25mOhm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_744043003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043003?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="2.15A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 744043003 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7440430039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440430039?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="1.72A"/>
<attribute name="ISAT" value="1.65A"/>
<attribute name="PART-NUMBER" value=" 7440430039 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_744043004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043004?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="PART-NUMBER" value=" 744043004 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744043005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043005?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="1.38A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 744043005 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744043006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043006?ae"/>
<attribute name="FRES" value="57MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 744043006 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744043008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043008?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 744043008 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744043100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043100?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.19A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 744043100 "/>
<attribute name="RDC" value="95mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744043101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043101?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="0.51A"/>
<attribute name="ISAT" value="0.29A"/>
<attribute name="PART-NUMBER" value=" 744043101 "/>
<attribute name="RDC" value="550mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744043102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043102?ae"/>
<attribute name="FRES" value="2.3MHz"/>
<attribute name="IR" value="0.14A"/>
<attribute name="ISAT" value="0.08A"/>
<attribute name="PART-NUMBER" value=" 744043102 "/>
<attribute name="RDC" value="5400mOhm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_744043120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043120?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1.12A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="PART-NUMBER" value=" 744043120 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744043150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043150?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.03A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="PART-NUMBER" value=" 744043150 "/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744043151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043151?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="0.22A"/>
<attribute name="PART-NUMBER" value=" 744043151 "/>
<attribute name="RDC" value="770mOhm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744043152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043152?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="IR" value="0.09A"/>
<attribute name="ISAT" value="0.05A"/>
<attribute name="PART-NUMBER" value=" 744043152 "/>
<attribute name="RDC" value="6800mOhm"/>
<attribute name="VALUE" value="1500uH"/>
</technology>
<technology name="_744043180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043180?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="0.98A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 744043180 "/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744043220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043220?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.925A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 744043220 "/>
<attribute name="RDC" value="160mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744043221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043221?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.34A"/>
<attribute name="ISAT" value="0.2A"/>
<attribute name="PART-NUMBER" value=" 744043221 "/>
<attribute name="RDC" value="1008mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744043270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043270?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="0.89A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="PART-NUMBER" value=" 744043270 "/>
<attribute name="RDC" value="170mOhm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744043330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043330?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="PART-NUMBER" value=" 744043330 "/>
<attribute name="RDC" value="195mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744043331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043331?ae"/>
<attribute name="FRES" value="4.3MHz"/>
<attribute name="IR" value="0.285A"/>
<attribute name="ISAT" value="0.17A"/>
<attribute name="PART-NUMBER" value=" 744043331 "/>
<attribute name="RDC" value="1630mOhm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_744043390">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043390?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="0.795A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744043390 "/>
<attribute name="RDC" value="215mOhm"/>
<attribute name="VALUE" value="39uH"/>
</technology>
<technology name="_744043470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043470?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744043470 "/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744043471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043471?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.24A"/>
<attribute name="ISAT" value="0.125A"/>
<attribute name="PART-NUMBER" value=" 744043471 "/>
<attribute name="RDC" value="2128mOhm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_744043561">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043561?ae"/>
<attribute name="FRES" value="3MHz"/>
<attribute name="IR" value="0.22A"/>
<attribute name="ISAT" value="0.11A"/>
<attribute name="PART-NUMBER" value=" 744043561 "/>
<attribute name="RDC" value="2610mOhm"/>
<attribute name="VALUE" value="560uH"/>
</technology>
<technology name="_744043680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744043680?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="0.63A"/>
<attribute name="ISAT" value="0.4A"/>
<attribute name="PART-NUMBER" value=" 744043680 "/>
<attribute name="RDC" value="340mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_4818" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-TPC_4818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74404200056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74404200056?ae"/>
<attribute name="FRES" value="190MHz"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 74404200056 "/>
<attribute name="RDC" value="19mOhm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_744042001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042001?ae"/>
<attribute name="FRES" value="177MHz"/>
<attribute name="IR" value="2.7A"/>
<attribute name="ISAT" value="2.6A"/>
<attribute name="PART-NUMBER" value=" 744042001 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7440420018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440420018?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="2.35A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 7440420018 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_7440420027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440420027?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="2.03A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="PART-NUMBER" value=" 7440420027 "/>
<attribute name="RDC" value="47mOhm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_744042003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042003?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="1.95A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 744042003 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7440420039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440420039?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="1.82A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="PART-NUMBER" value=" 7440420039 "/>
<attribute name="RDC" value="60mOhm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_744042004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042004?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="1.72A"/>
<attribute name="ISAT" value="1.65A"/>
<attribute name="PART-NUMBER" value=" 744042004 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744042005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042005?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="1.64A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="PART-NUMBER" value=" 744042005 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744042006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042006?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 744042006 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744042008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042008?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744042008 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744042100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042100?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 744042100 "/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744042101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042101?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="PART-NUMBER" value=" 744042101 "/>
<attribute name="RDC" value="1170mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744042120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042120?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="PART-NUMBER" value=" 744042120 "/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744042150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042150?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.03A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="PART-NUMBER" value=" 744042150 "/>
<attribute name="RDC" value="190mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744042180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042180?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="0.92A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 744042180 "/>
<attribute name="RDC" value="270mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744042220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042220?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="0.88A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="PART-NUMBER" value=" 744042220 "/>
<attribute name="RDC" value="280mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744042221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042221?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.2A"/>
<attribute name="ISAT" value="0.16A"/>
<attribute name="PART-NUMBER" value=" 744042221 "/>
<attribute name="RDC" value="2880mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744042330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042330?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744042330 "/>
<attribute name="RDC" value="382mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744042331">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042331?ae"/>
<attribute name="FRES" value="5.5MHz"/>
<attribute name="IR" value="0.15A"/>
<attribute name="ISAT" value="0.13A"/>
<attribute name="PART-NUMBER" value=" 744042331 "/>
<attribute name="RDC" value="4100mOhm"/>
<attribute name="VALUE" value="330uH"/>
</technology>
<technology name="_744042470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042470?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.62A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="PART-NUMBER" value=" 744042470 "/>
<attribute name="RDC" value="540mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744042680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744042680?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.38A"/>
<attribute name="PART-NUMBER" value=" 744042680 "/>
<attribute name="RDC" value="715mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_5828">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-TPC_5828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744053002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053002?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="PART-NUMBER" value=" 744053002 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="2.6uH"/>
</technology>
<technology name="_744053003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053003?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="PART-NUMBER" value=" 744053003 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="3uH"/>
</technology>
<technology name="_744053004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053004?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="PART-NUMBER" value=" 744053004 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="4.2uH"/>
</technology>
<technology name="_7440530047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440530047?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="1.95A"/>
<attribute name="PART-NUMBER" value=" 7440530047 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744053005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053005?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 744053005 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="5.3uH"/>
</technology>
<technology name="_744053006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053006?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="PART-NUMBER" value=" 744053006 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_744053008">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053008?ae"/>
<attribute name="FRES" value="28MHz"/>
<attribute name="IR" value="2.1A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="PART-NUMBER" value=" 744053008 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_744053100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053100?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="PART-NUMBER" value=" 744053100 "/>
<attribute name="RDC" value="60mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744053101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053101?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="PART-NUMBER" value=" 744053101 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744053120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053120?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="1.46A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 744053120 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744053150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053150?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.38A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="PART-NUMBER" value=" 744053150 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744053180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053180?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744053180 "/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744053220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053220?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 744053220 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744053221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053221?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="0.3A"/>
<attribute name="ISAT" value="0.29A"/>
<attribute name="PART-NUMBER" value=" 744053221 "/>
<attribute name="RDC" value="1170mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744053270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053270?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="1.05A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 744053270 "/>
<attribute name="RDC" value="135mOhm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744053330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053330?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="PART-NUMBER" value=" 744053330 "/>
<attribute name="RDC" value="180mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744053470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053470?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="PART-NUMBER" value=" 744053470 "/>
<attribute name="RDC" value="220mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744053680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744053680?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="PART-NUMBER" value=" 744053680 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_2811" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-TPC_2811">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744028000056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744028000056?ae"/>
<attribute name="FRES" value="2000MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="6A"/>
<attribute name="PART-NUMBER" value="744028000056"/>
<attribute name="RDC" value="11.5mOhm"/>
<attribute name="VALUE" value="0.056uH"/>
</technology>
<technology name="_74402800015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402800015?ae"/>
<attribute name="FRES" value="800MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="3.6A"/>
<attribute name="PART-NUMBER" value=" 74402800015 "/>
<attribute name="RDC" value="18mOhm"/>
<attribute name="VALUE" value="0.15uH"/>
</technology>
<technology name="_74402800033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402800033?ae"/>
<attribute name="FRES" value="550MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 74402800033 "/>
<attribute name="RDC" value="27mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_74402800047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402800047?ae"/>
<attribute name="FRES" value="350MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="PART-NUMBER" value=" 74402800047 "/>
<attribute name="RDC" value="36mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74402800082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402800082?ae"/>
<attribute name="FRES" value="180MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="PART-NUMBER" value=" 74402800082 "/>
<attribute name="RDC" value="53mOhm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_744028001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744028001?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 744028001 "/>
<attribute name="RDC" value="65mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744028002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744028002?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 744028002 "/>
<attribute name="RDC" value="125mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744028003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744028003?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="0.85A"/>
<attribute name="PART-NUMBER" value=" 744028003 "/>
<attribute name="RDC" value="185mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744028004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744028004?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 744028004 "/>
<attribute name="RDC" value="265mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744028006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744028006?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="0.75A"/>
<attribute name="ISAT" value="0.55A"/>
<attribute name="PART-NUMBER" value=" 744028006 "/>
<attribute name="RDC" value="325mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8043" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_PADNAME"/>
</gates>
<devices>
<device name="" package="WE-TPC_8020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_7440710082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440710082?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="7.3A"/>
<attribute name="ISAT" value="8A"/>
<attribute name="PART-NUMBER" value=" 7440710082 "/>
<attribute name="RDC" value="7mOhm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_744071022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071022?ae"/>
<attribute name="FRES" value="62MHz"/>
<attribute name="IR" value="5.4A"/>
<attribute name="ISAT" value="6.3A"/>
<attribute name="PART-NUMBER" value=" 744071022 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744071039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071039?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="4.9A"/>
<attribute name="ISAT" value="4.5A"/>
<attribute name="PART-NUMBER" value=" 744071039 "/>
<attribute name="RDC" value="13mOhm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_744071047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071047?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="4.3A"/>
<attribute name="PART-NUMBER" value=" 744071047 "/>
<attribute name="RDC" value="17mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744071056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071056?ae"/>
<attribute name="FRES" value="31MHz"/>
<attribute name="IR" value="4A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 744071056 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_744071100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071100?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="2.8A"/>
<attribute name="PART-NUMBER" value=" 744071100 "/>
<attribute name="RDC" value="28mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744071101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071101?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 744071101 "/>
<attribute name="RDC" value="270mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744071102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071102?ae"/>
<attribute name="FRES" value="2.2MHz"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.34A"/>
<attribute name="PART-NUMBER" value=" 744071102 "/>
<attribute name="RDC" value="2985mOhm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_744071150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071150?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="PART-NUMBER" value=" 744071150 "/>
<attribute name="RDC" value="46mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744071220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071220?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="2.3A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 744071220 "/>
<attribute name="RDC" value="65mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744071221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071221?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="0.6A"/>
<attribute name="PART-NUMBER" value=" 744071221 "/>
<attribute name="RDC" value="510mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744071330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071330?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 744071330 "/>
<attribute name="RDC" value="95mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744071470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071470?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 744071470 "/>
<attribute name="RDC" value="120mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744071680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744071680?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744071680 "/>
<attribute name="RDC" value="185mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_2828" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-TPC_2828">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_74402500030">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402500030?ae"/>
<attribute name="FRES" value="440MHz"/>
<attribute name="IR" value="3.9A"/>
<attribute name="ISAT" value="5.7A"/>
<attribute name="PART-NUMBER" value=" 74402500030 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="0.3uH"/>
</technology>
<technology name="_74402500047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402500047?ae"/>
<attribute name="FRES" value="290MHz"/>
<attribute name="IR" value="3.3A"/>
<attribute name="ISAT" value="4.7A"/>
<attribute name="PART-NUMBER" value=" 74402500047 "/>
<attribute name="RDC" value="19mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74402500072">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402500072?ae"/>
<attribute name="FRES" value="210MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 74402500072 "/>
<attribute name="RDC" value="23.5mOhm"/>
<attribute name="VALUE" value="0.72uH"/>
</technology>
<technology name="_744025001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025001?ae"/>
<attribute name="FRES" value="180MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 744025001 "/>
<attribute name="RDC" value="36mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_744025002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025002?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 744025002 "/>
<attribute name="RDC" value="57mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744025003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025003?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 744025003 "/>
<attribute name="RDC" value="85mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744025004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025004?ae"/>
<attribute name="FRES" value="84MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="PART-NUMBER" value=" 744025004 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744025006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025006?ae"/>
<attribute name="FRES" value="59MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.3A"/>
<attribute name="PART-NUMBER" value=" 744025006 "/>
<attribute name="RDC" value="142mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744025100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025100?ae"/>
<attribute name="FRES" value="41MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744025100 "/>
<attribute name="RDC" value="170mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744025150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025150?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="0.72A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 744025150 "/>
<attribute name="RDC" value="356mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744025220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025220?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="0.5A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="PART-NUMBER" value=" 744025220 "/>
<attribute name="RDC" value="525mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744025270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025270?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="0.45A"/>
<attribute name="ISAT" value="0.67A"/>
<attribute name="PART-NUMBER" value=" 744025270 "/>
<attribute name="RDC" value="745mOhm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744025330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744025330?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.62A"/>
<attribute name="PART-NUMBER" value=" 744025330 "/>
<attribute name="RDC" value="840mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8020" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_PADNAME"/>
</gates>
<devices>
<device name="" package="WE-TPC_8020">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_74407000018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74407000018?ae"/>
<attribute name="FRES" value="600MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="ISAT" value="9A"/>
<attribute name="PART-NUMBER" value=" 74407000018 "/>
<attribute name="RDC" value="3.51mOhm"/>
<attribute name="VALUE" value="0.18uH"/>
</technology>
<technology name="_74407000047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74407000047?ae"/>
<attribute name="FRES" value="300MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="ISAT" value="6.5A"/>
<attribute name="PART-NUMBER" value=" 74407000047 "/>
<attribute name="RDC" value="5.8mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74407000082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74407000082?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="6.2A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="PART-NUMBER" value=" 74407000082 "/>
<attribute name="RDC" value="8.5mOhm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_7440700012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700012?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="4.2A"/>
<attribute name="PART-NUMBER" value=" 7440700012 "/>
<attribute name="RDC" value="12.5mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_7440700022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700022?ae"/>
<attribute name="FRES" value="115MHz"/>
<attribute name="IR" value="4.6A"/>
<attribute name="ISAT" value="3.2A"/>
<attribute name="PART-NUMBER" value=" 7440700022 "/>
<attribute name="RDC" value="17mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7440700033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700033?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="3.2A"/>
<attribute name="ISAT" value="2.55A"/>
<attribute name="PART-NUMBER" value=" 7440700033 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7440700047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700047?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="PART-NUMBER" value=" 7440700047 "/>
<attribute name="RDC" value="37mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7440700056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700056?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="PART-NUMBER" value=" 7440700056 "/>
<attribute name="RDC" value="47mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_7440700068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700068?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 7440700068 "/>
<attribute name="RDC" value="56mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7440700082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700082?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="1.7A"/>
<attribute name="PART-NUMBER" value=" 7440700082 "/>
<attribute name="RDC" value="70.5mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7440700100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700100?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="PART-NUMBER" value=" 7440700100 "/>
<attribute name="RDC" value="78mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7440700150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700150?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 7440700150 "/>
<attribute name="RDC" value="117mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7440700180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700180?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7440700180 "/>
<attribute name="RDC" value="135mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7440700220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440700220?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 7440700220 "/>
<attribute name="RDC" value="166mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_3816" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-TPC_3816">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744031001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031001?ae"/>
<attribute name="FRES" value="125MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="PART-NUMBER" value=" 744031001 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744031002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031002?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 744031002 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="2.5uH"/>
</technology>
<technology name="_744031003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031003?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="1.38A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744031003 "/>
<attribute name="RDC" value="66mOhm"/>
<attribute name="VALUE" value="3.6uH"/>
</technology>
<technology name="_744031004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031004?ae"/>
<attribute name="FRES" value="75MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 744031004 "/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7440310047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440310047?ae"/>
<attribute name="FRES" value="208MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="PART-NUMBER" value=" 7440310047 "/>
<attribute name="RDC" value="16mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744031006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031006?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="PART-NUMBER" value=" 744031006 "/>
<attribute name="RDC" value="135mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744031010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031010?ae"/>
<attribute name="FRES" value="144MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="PART-NUMBER" value=" 744031010 "/>
<attribute name="RDC" value="26mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744031100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031100?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="0.74A"/>
<attribute name="ISAT" value="0.56A"/>
<attribute name="PART-NUMBER" value=" 744031100 "/>
<attribute name="RDC" value="185mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744031101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031101?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.25A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="PART-NUMBER" value=" 744031101 "/>
<attribute name="RDC" value="1930mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744031150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031150?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="0.62A"/>
<attribute name="ISAT" value="0.45A"/>
<attribute name="PART-NUMBER" value=" 744031150 "/>
<attribute name="RDC" value="255mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744031220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031220?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="0.51A"/>
<attribute name="ISAT" value="0.36A"/>
<attribute name="PART-NUMBER" value=" 744031220 "/>
<attribute name="RDC" value="410mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744031330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031330?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="0.42A"/>
<attribute name="ISAT" value="0.32A"/>
<attribute name="PART-NUMBER" value=" 744031330 "/>
<attribute name="RDC" value="635mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744031470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031470?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.39A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="PART-NUMBER" value=" 744031470 "/>
<attribute name="RDC" value="940mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744031680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744031680?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.32A"/>
<attribute name="ISAT" value="0.22A"/>
<attribute name="PART-NUMBER" value=" 744031680 "/>
<attribute name="RDC" value="1150mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8012" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_PADNAME"/>
</gates>
<devices>
<device name="" package="WE-TPC_8012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_74406800024">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406800024?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="4.1A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="PART-NUMBER" value=" 74406800024 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="0.24uH"/>
</technology>
<technology name="_74406800056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406800056?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 74406800056 "/>
<attribute name="RDC" value="22mOhm"/>
<attribute name="VALUE" value="0.56uH"/>
</technology>
<technology name="_7440680010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680010?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="PART-NUMBER" value=" 7440680010 "/>
<attribute name="RDC" value="32mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7440680017">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680017?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 7440680017 "/>
<attribute name="RDC" value="41mOhm"/>
<attribute name="VALUE" value="1.7uH"/>
</technology>
<technology name="_7440680027">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680027?ae"/>
<attribute name="FRES" value="80MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="1.9A"/>
<attribute name="PART-NUMBER" value=" 7440680027 "/>
<attribute name="RDC" value="52mOhm"/>
<attribute name="VALUE" value="2.7uH"/>
</technology>
<technology name="_7440680033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680033?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 7440680033 "/>
<attribute name="RDC" value="61mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7440680047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680047?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="1.85A"/>
<attribute name="ISAT" value="1.55A"/>
<attribute name="PART-NUMBER" value=" 7440680047 "/>
<attribute name="RDC" value="72mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7440680056">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680056?ae"/>
<attribute name="FRES" value="48MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="PART-NUMBER" value=" 7440680056 "/>
<attribute name="RDC" value="110mOhm"/>
<attribute name="VALUE" value="5.6uH"/>
</technology>
<technology name="_7440680068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680068?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="1.4A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="PART-NUMBER" value=" 7440680068 "/>
<attribute name="RDC" value="127mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7440680082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680082?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7440680082 "/>
<attribute name="RDC" value="142mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7440680100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680100?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.2A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 7440680100 "/>
<attribute name="RDC" value="177mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7440680120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680120?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="1.15A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="PART-NUMBER" value=" 7440680120 "/>
<attribute name="RDC" value="195mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_7440680150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680150?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 7440680150 "/>
<attribute name="RDC" value="213mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7440680180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680180?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="0.75A"/>
<attribute name="PART-NUMBER" value=" 7440680180 "/>
<attribute name="RDC" value="302mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7440680220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440680220?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.85A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 7440680220 "/>
<attribute name="RDC" value="350mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_8015" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_PADNAME"/>
</gates>
<devices>
<device name="" package="WE-TPC_8012">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="3"/>
</connects>
<technologies>
<technology name="_74406900022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406900022?ae"/>
<attribute name="FRES" value="400MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="ISAT" value="7.5A"/>
<attribute name="PART-NUMBER" value=" 74406900022 "/>
<attribute name="RDC" value="9mOhm"/>
<attribute name="VALUE" value="0.22uH"/>
</technology>
<technology name="_74406900052">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74406900052?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="5.8A"/>
<attribute name="PART-NUMBER" value=" 74406900052 "/>
<attribute name="RDC" value="15mOhm"/>
<attribute name="VALUE" value="0.52uH"/>
</technology>
<technology name="_7440690010">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690010?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="3.6A"/>
<attribute name="ISAT" value="3.8A"/>
<attribute name="PART-NUMBER" value=" 7440690010 "/>
<attribute name="RDC" value="21mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7440690016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690016?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="3.3A"/>
<attribute name="PART-NUMBER" value=" 7440690016 "/>
<attribute name="RDC" value="29mOhm"/>
<attribute name="VALUE" value="1.6uH"/>
</technology>
<technology name="_7440690022">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690022?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.85A"/>
<attribute name="PART-NUMBER" value=" 7440690022 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_7440690033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690033?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="2.55A"/>
<attribute name="ISAT" value="2.3A"/>
<attribute name="PART-NUMBER" value=" 7440690033 "/>
<attribute name="RDC" value="42mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_7440690047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690047?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 7440690047 "/>
<attribute name="RDC" value="56mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7440690068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690068?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="1.75A"/>
<attribute name="ISAT" value="1.65A"/>
<attribute name="PART-NUMBER" value=" 7440690068 "/>
<attribute name="RDC" value="88mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7440690082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690082?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 7440690082 "/>
<attribute name="RDC" value="99mOhm"/>
<attribute name="VALUE" value="8.2uH"/>
</technology>
<technology name="_7440690100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690100?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 7440690100 "/>
<attribute name="RDC" value="112mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_7440690120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690120?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.2A"/>
<attribute name="PART-NUMBER" value=" 7440690120 "/>
<attribute name="RDC" value="148mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_7440690150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690150?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 7440690150 "/>
<attribute name="RDC" value="179mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_7440690180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690180?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.05A"/>
<attribute name="PART-NUMBER" value=" 7440690180 "/>
<attribute name="RDC" value="225mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_7440690220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440690220?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 7440690220 "/>
<attribute name="RDC" value="272mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_5818" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-TPC_5818">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_7440520012">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440520012?ae"/>
<attribute name="FRES" value="120MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="ISAT" value="3.5A"/>
<attribute name="PART-NUMBER" value=" 7440520012 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_7440520018">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440520018?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="2.6A"/>
<attribute name="ISAT" value="3A"/>
<attribute name="PART-NUMBER" value=" 7440520018 "/>
<attribute name="RDC" value="24mOhm"/>
<attribute name="VALUE" value="1.8uH"/>
</technology>
<technology name="_744052002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052002?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="PART-NUMBER" value=" 744052002 "/>
<attribute name="RDC" value="30mOhm"/>
<attribute name="VALUE" value="2.5uH"/>
</technology>
<technology name="_744052003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052003?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="2.4A"/>
<attribute name="PART-NUMBER" value=" 744052003 "/>
<attribute name="RDC" value="35mOhm"/>
<attribute name="VALUE" value="3uH"/>
</technology>
<technology name="_7440520039">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440520039?ae"/>
<attribute name="FRES" value="60MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="ISAT" value="2.1A"/>
<attribute name="PART-NUMBER" value=" 7440520039 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="3.9uH"/>
</technology>
<technology name="_744052005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052005?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="1.65A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 744052005 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="5uH"/>
</technology>
<technology name="_744052006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052006?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="PART-NUMBER" value=" 744052006 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_744052007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052007?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="1.35A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 744052007 "/>
<attribute name="RDC" value="70mOhm"/>
<attribute name="VALUE" value="7.5uH"/>
</technology>
<technology name="_744052009">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052009?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="1.35A"/>
<attribute name="PART-NUMBER" value=" 744052009 "/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="VALUE" value="9uH"/>
</technology>
<technology name="_744052100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052100?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 744052100 "/>
<attribute name="RDC" value="105mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744052101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052101?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.35A"/>
<attribute name="ISAT" value="0.42A"/>
<attribute name="PART-NUMBER" value=" 744052101 "/>
<attribute name="RDC" value="815mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744052120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052120?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="PART-NUMBER" value=" 744052120 "/>
<attribute name="RDC" value="130mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744052150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052150?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="0.95A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744052150 "/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744052180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052180?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="0.9A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 744052180 "/>
<attribute name="RDC" value="185mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744052220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052220?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="ISAT" value="0.9A"/>
<attribute name="PART-NUMBER" value=" 744052220 "/>
<attribute name="RDC" value="240mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744052221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052221?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.23A"/>
<attribute name="ISAT" value="0.3A"/>
<attribute name="PART-NUMBER" value=" 744052221 "/>
<attribute name="RDC" value="1890mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744052270">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052270?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="0.78A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 744052270 "/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="VALUE" value="27uH"/>
</technology>
<technology name="_744052470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052470?ae"/>
<attribute name="FRES" value="18MHz"/>
<attribute name="IR" value="0.77A"/>
<attribute name="ISAT" value="0.7A"/>
<attribute name="PART-NUMBER" value=" 744052470 "/>
<attribute name="RDC" value="530mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744052471">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052471?ae"/>
<attribute name="FRES" value="4MHz"/>
<attribute name="IR" value="0.14A"/>
<attribute name="ISAT" value="0.18A"/>
<attribute name="PART-NUMBER" value=" 744052471 "/>
<attribute name="RDC" value="4175mOhm"/>
<attribute name="VALUE" value="470uH"/>
</technology>
<technology name="_744052680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744052680?ae"/>
<attribute name="FRES" value="14MHz"/>
<attribute name="IR" value="0.64A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744052680 "/>
<attribute name="RDC" value="840mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_3510" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_PADNAME"/>
</gates>
<devices>
<device name="" package="WE-TPC_3510">
<connects>
<connect gate="G$1" pin="1" pad="2"/>
<connect gate="G$1" pin="2" pad="4"/>
</connects>
<technologies>
<technology name="_744030001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744030001?ae"/>
<attribute name="FRES" value="210MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744030001 "/>
<attribute name="RDC" value="95mOhm"/>
<attribute name="VALUE" value="1.2uH"/>
</technology>
<technology name="_744030002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744030002?ae"/>
<attribute name="FRES" value="140MHz"/>
<attribute name="IR" value="0.74A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 744030002 "/>
<attribute name="RDC" value="140mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744030003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744030003?ae"/>
<attribute name="FRES" value="130MHz"/>
<attribute name="IR" value="0.65A"/>
<attribute name="ISAT" value="0.72A"/>
<attribute name="PART-NUMBER" value=" 744030003 "/>
<attribute name="RDC" value="198mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744030004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744030004?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="0.48A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744030004 "/>
<attribute name="RDC" value="252mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_7440300047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440300047?ae"/>
<attribute name="FRES" value="270MHz"/>
<attribute name="IR" value="1.45A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 7440300047 "/>
<attribute name="RDC" value="48mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_744030006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744030006?ae"/>
<attribute name="FRES" value="85MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="ISAT" value="0.43A"/>
<attribute name="PART-NUMBER" value=" 744030006 "/>
<attribute name="RDC" value="400mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_7440300068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440300068?ae"/>
<attribute name="FRES" value="230MHz"/>
<attribute name="IR" value="1.3A"/>
<attribute name="ISAT" value="1.5A"/>
<attribute name="PART-NUMBER" value=" 7440300068 "/>
<attribute name="RDC" value="60mOhm"/>
<attribute name="VALUE" value="0.68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_2813" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP"/>
</gates>
<devices>
<device name="" package="WE-TPC_2813">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744029000068">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744029000068?ae"/>
<attribute name="FRES" value="1000MHz"/>
<attribute name="IR" value="4.5A"/>
<attribute name="ISAT" value="5.5A"/>
<attribute name="PART-NUMBER" value="744029000068"/>
<attribute name="RDC" value="10.5mOhm"/>
<attribute name="VALUE" value="0.068uH"/>
</technology>
<technology name="_74402900016">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402900016?ae"/>
<attribute name="FRES" value="800MHz"/>
<attribute name="IR" value="3.8A"/>
<attribute name="ISAT" value="3.9A"/>
<attribute name="PART-NUMBER" value=" 74402900016 "/>
<attribute name="RDC" value="16mOhm"/>
<attribute name="VALUE" value="0.16uH"/>
</technology>
<technology name="_74402900033">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402900033?ae"/>
<attribute name="FRES" value="500MHz"/>
<attribute name="IR" value="3.1A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="PART-NUMBER" value=" 74402900033 "/>
<attribute name="RDC" value="23mOhm"/>
<attribute name="VALUE" value="0.33uH"/>
</technology>
<technology name="_74402900047">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402900047?ae"/>
<attribute name="FRES" value="350MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.2A"/>
<attribute name="PART-NUMBER" value=" 74402900047 "/>
<attribute name="RDC" value="29mOhm"/>
<attribute name="VALUE" value="0.47uH"/>
</technology>
<technology name="_74402900082">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/74402900082?ae"/>
<attribute name="FRES" value="200MHz"/>
<attribute name="IR" value="2.4A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 74402900082 "/>
<attribute name="RDC" value="36mOhm"/>
<attribute name="VALUE" value="0.82uH"/>
</technology>
<technology name="_744029001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744029001?ae"/>
<attribute name="FRES" value="150MHz"/>
<attribute name="IR" value="2.2A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="PART-NUMBER" value=" 744029001 "/>
<attribute name="RDC" value="45mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_744029002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744029002?ae"/>
<attribute name="FRES" value="90MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="ISAT" value="1.15A"/>
<attribute name="PART-NUMBER" value=" 744029002 "/>
<attribute name="RDC" value="88mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744029003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744029003?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="1.25A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="PART-NUMBER" value=" 744029003 "/>
<attribute name="RDC" value="110mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744029004">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744029004?ae"/>
<attribute name="FRES" value="65MHz"/>
<attribute name="IR" value="1A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="PART-NUMBER" value=" 744029004 "/>
<attribute name="RDC" value="170mOhm"/>
<attribute name="VALUE" value="4.7uH"/>
</technology>
<technology name="_744029006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744029006?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="0.82A"/>
<attribute name="ISAT" value="0.65A"/>
<attribute name="PART-NUMBER" value=" 744029006 "/>
<attribute name="RDC" value="250mOhm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
<technology name="_744029100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744029100?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="0.65A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744029100 "/>
<attribute name="RDC" value="390mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-TPC_6823" prefix="L">
<description>&lt;b&gt;WE-TPC SMT Tiny Power Inductor
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Extremely flat power inductor
&lt;br&gt;High current capability
&lt;br&gt;Magnetically shielded which results in a low leakage field
&lt;br&gt;Recommended solder profile: Reflow
&lt;br&gt;Operating temperature: –40 °C to +125 °C
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Portable power like PDA, digital camera, PCMCIA cards and displays
&lt;br&gt;DC/DC converter
&lt;br&gt;Embedded PC
&lt;br&gt;Mobile data gathering, telemetric
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o14870v209%20WE-TPC_Gruppe_2.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/en/components/products/WE-TPC"&gt;www.we-online.com/en/components/products/WE-TPC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2023-02-20&lt;br&gt;
&lt;/b&gt;2023(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="L_GAP_POINT"/>
</gates>
<devices>
<device name="" package="WE-TPC_6823">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="_744062001">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062001?ae"/>
<attribute name="FRES" value="110MHz"/>
<attribute name="IR" value="4.8A"/>
<attribute name="ISAT" value="4.6A"/>
<attribute name="PART-NUMBER" value=" 744062001 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="1uH"/>
</technology>
<technology name="_7440620015">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/7440620015?ae"/>
<attribute name="FRES" value="100MHz"/>
<attribute name="IR" value="4.3A"/>
<attribute name="ISAT" value="4A"/>
<attribute name="PART-NUMBER" value=" 7440620015 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="1.5uH"/>
</technology>
<technology name="_744062002">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062002?ae"/>
<attribute name="FRES" value="70MHz"/>
<attribute name="IR" value="3.4A"/>
<attribute name="ISAT" value="2.7A"/>
<attribute name="PART-NUMBER" value=" 744062002 "/>
<attribute name="RDC" value="10mOhm"/>
<attribute name="VALUE" value="2.2uH"/>
</technology>
<technology name="_744062003">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062003?ae"/>
<attribute name="FRES" value="55MHz"/>
<attribute name="IR" value="2.8A"/>
<attribute name="ISAT" value="2.5A"/>
<attribute name="PART-NUMBER" value=" 744062003 "/>
<attribute name="RDC" value="20mOhm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
<technology name="_744062005">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062005?ae"/>
<attribute name="FRES" value="50MHz"/>
<attribute name="IR" value="2.15A"/>
<attribute name="ISAT" value="2A"/>
<attribute name="PART-NUMBER" value=" 744062005 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="VALUE" value="5uH"/>
</technology>
<technology name="_744062006">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062006?ae"/>
<attribute name="FRES" value="45MHz"/>
<attribute name="IR" value="1.9A"/>
<attribute name="ISAT" value="1.8A"/>
<attribute name="PART-NUMBER" value=" 744062006 "/>
<attribute name="RDC" value="40mOhm"/>
<attribute name="VALUE" value="6.2uH"/>
</technology>
<technology name="_744062007">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062007?ae"/>
<attribute name="FRES" value="40MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="ISAT" value="1.6A"/>
<attribute name="PART-NUMBER" value=" 744062007 "/>
<attribute name="RDC" value="50mOhm"/>
<attribute name="VALUE" value="7.5uH"/>
</technology>
<technology name="_744062100">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062100?ae"/>
<attribute name="FRES" value="35MHz"/>
<attribute name="IR" value="1.6A"/>
<attribute name="ISAT" value="1.4A"/>
<attribute name="PART-NUMBER" value=" 744062100 "/>
<attribute name="RDC" value="53mOhm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
<technology name="_744062101">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062101?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.55A"/>
<attribute name="ISAT" value="0.47A"/>
<attribute name="PART-NUMBER" value=" 744062101 "/>
<attribute name="RDC" value="440mOhm"/>
<attribute name="VALUE" value="100uH"/>
</technology>
<technology name="_744062102">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062102?ae"/>
<attribute name="FRES" value="2MHz"/>
<attribute name="IR" value="0.16A"/>
<attribute name="ISAT" value="0.13A"/>
<attribute name="PART-NUMBER" value=" 744062102 "/>
<attribute name="RDC" value="3820mOhm"/>
<attribute name="VALUE" value="1000uH"/>
</technology>
<technology name="_744062120">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062120?ae"/>
<attribute name="FRES" value="30MHz"/>
<attribute name="IR" value="1.43A"/>
<attribute name="ISAT" value="1.25A"/>
<attribute name="PART-NUMBER" value=" 744062120 "/>
<attribute name="RDC" value="60mOhm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
<technology name="_744062150">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062150?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.31A"/>
<attribute name="ISAT" value="1.1A"/>
<attribute name="PART-NUMBER" value=" 744062150 "/>
<attribute name="RDC" value="80mOhm"/>
<attribute name="VALUE" value="15uH"/>
</technology>
<technology name="_744062151">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062151?ae"/>
<attribute name="FRES" value="9MHz"/>
<attribute name="IR" value="0.43A"/>
<attribute name="ISAT" value="0.36A"/>
<attribute name="PART-NUMBER" value=" 744062151 "/>
<attribute name="RDC" value="605mOhm"/>
<attribute name="VALUE" value="150uH"/>
</technology>
<technology name="_744062152">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062152?ae"/>
<attribute name="FRES" value="1.5MHz"/>
<attribute name="IR" value="0.08A"/>
<attribute name="ISAT" value="0.11A"/>
<attribute name="PART-NUMBER" value=" 744062152 "/>
<attribute name="RDC" value="7000mOhm"/>
<attribute name="VALUE" value="1500uH"/>
</technology>
<technology name="_744062180">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062180?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.28A"/>
<attribute name="ISAT" value="1A"/>
<attribute name="PART-NUMBER" value=" 744062180 "/>
<attribute name="RDC" value="90mOhm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
<technology name="_744062220">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062220?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="1.22A"/>
<attribute name="ISAT" value="0.95A"/>
<attribute name="PART-NUMBER" value=" 744062220 "/>
<attribute name="RDC" value="100mOhm"/>
<attribute name="VALUE" value="22uH"/>
</technology>
<technology name="_744062221">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062221?ae"/>
<attribute name="FRES" value="7MHz"/>
<attribute name="IR" value="0.36A"/>
<attribute name="ISAT" value="0.25A"/>
<attribute name="PART-NUMBER" value=" 744062221 "/>
<attribute name="RDC" value="1010mOhm"/>
<attribute name="VALUE" value="220uH"/>
</technology>
<technology name="_744062330">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062330?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="0.93A"/>
<attribute name="ISAT" value="0.78A"/>
<attribute name="PART-NUMBER" value=" 744062330 "/>
<attribute name="RDC" value="150mOhm"/>
<attribute name="VALUE" value="33uH"/>
</technology>
<technology name="_744062470">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062470?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.73A"/>
<attribute name="ISAT" value="0.62A"/>
<attribute name="PART-NUMBER" value=" 744062470 "/>
<attribute name="RDC" value="260mOhm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
<technology name="_744062680">
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/744062680?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="0.64A"/>
<attribute name="ISAT" value="0.5A"/>
<attribute name="PART-NUMBER" value=" 744062680 "/>
<attribute name="RDC" value="300mOhm"/>
<attribute name="VALUE" value="68uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
