<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Power Magnetics - Transformers For AC/DC Converter - WE-UOST&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2019a, 2019-09-26&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-UOST">
<description>&lt;B&gt;WE-UOST Universal Offline Standard Transformers&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;EE16/8/5 THT12 Pin</description>
</package>
</packages>
<symbols>
<symbol name="WE-UOST">
<pin name="1" direction="pas"/>
<pin name="8" direction="pas"/>
<pin name="7" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-UOST_EE/16/8/5" prefix="T">
<description>&lt;b&gt; WE-UOST Universal Offline Standard Transformer
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt; &lt;/b&gt;&lt;/b&gt; Input voltage range 85–265 VAC (125–375 VDC)
&lt;br&gt; Output power 12–16 W
&lt;br&gt; Designed to comply with EN61558-2-16: Reinforced insulation
&lt;br&gt; Creepage and clearance distance &gt;6.5 mm
&lt;br&gt; Insulation test voltage 4 kVAC
&lt;br&gt; For SMD assembly
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; SMPS with power up to 16 W
&lt;br&gt; Auxiliary power supplies
&lt;br&gt; Usable with all low power AC/DC ICs like LT3798/99, UCC28610, ViPER &amp; Tiny/Link Switch
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://katalog.we-online.com/media/images/v2/o14889v209%20Family_WE-UOST_Universal.jpg" title="Enlarge picture"&gt;
&lt;img src="https://katalog.we-online.com/media/images/v2/o14889v209%20Family_WE-UOST_Universal.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://katalog.we-online.com/en/pbs/WE-UOST"&gt;https://katalog.we-online.com/en/pbs/WE-UOST&lt;/a&gt;&lt;p&gt;

Updated  by  Yingchun,Shan 2019-08-26&lt;br&gt;
2019 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WE-UOST"/>
</gates>
<devices>
<device name="_SCH1" package="WE-UOST">
<connects>
<connect gate="G$1" pin="1" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="6"/>
<connect gate="G$1" pin="6" pad="3"/>
<connect gate="G$1" pin="7" pad="4"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="_760871113">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760871113.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="1.25A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1310uH"/>
<attribute name="LSMIN" value="40uH"/>
<attribute name="N" value="140 : 6 : 6 : 16"/>
<attribute name="PART-NUMBER" value=" 760871113 "/>
<attribute name="RDC1" value="3000mOhm"/>
<attribute name="RDC2" value="25mOhm"/>
<attribute name="RDC3" value="25mOhm"/>
<attribute name="RDC4" value="450mOhm"/>
<attribute name="VALUE" value="5V  1.25A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VO2" value="5V"/>
</technology>
<technology name="_760871135">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760871135.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="0.55A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1250uH"/>
<attribute name="LSMIN" value="53uH"/>
<attribute name="N" value="136 : 13 : 13 : 15"/>
<attribute name="PART-NUMBER" value=" 760871135 "/>
<attribute name="RDC1" value="2920mOhm"/>
<attribute name="RDC2" value="92mOhm"/>
<attribute name="RDC3" value="92mOhm"/>
<attribute name="RDC4" value="400mOhm"/>
<attribute name="VALUE" value="12V 0.55A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VO2" value="12V"/>
</technology>
<technology name="_760871142">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760871142.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="0.28A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1250uH"/>
<attribute name="LSMIN" value="40uH"/>
<attribute name="N" value="140 : 27 : 27 : 16"/>
<attribute name="PART-NUMBER" value=" 760871142 "/>
<attribute name="RDC1" value="3000mOhm"/>
<attribute name="RDC2" value="620mOhm"/>
<attribute name="RDC3" value="620mOhm"/>
<attribute name="RDC4" value="450mOhm"/>
<attribute name="VALUE" value="24V 0.28A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VO2" value="24V"/>
</technology>
<technology name="_760875112">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760875112.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="1.5A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1500uH"/>
<attribute name="LSMIN" value="50uH"/>
<attribute name="N" value="160 : 7 : 7 : 18"/>
<attribute name="PART-NUMBER" value=" 760875112 "/>
<attribute name="RDC1" value="4200mOhm"/>
<attribute name="RDC2" value="33.5mOhm"/>
<attribute name="RDC3" value="33.5mOhm"/>
<attribute name="RDC4" value="400mOhm"/>
<attribute name="VALUE" value="5V 1.5A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="195-265V(AC)"/>
<attribute name="VO2" value="5V"/>
</technology>
<technology name="_760875131">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760875131.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="0.65A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1500uH"/>
<attribute name="LSMIN" value="60uH"/>
<attribute name="N" value="160 : 14 : 14 : 16"/>
<attribute name="PART-NUMBER" value=" 760875131 "/>
<attribute name="RDC1" value="4200mOhm"/>
<attribute name="RDC2" value="140mOhm"/>
<attribute name="RDC3" value="140mOhm"/>
<attribute name="RDC4" value="450mOhm"/>
<attribute name="VALUE" value="12V 0.65A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VO2" value="12V"/>
</technology>
</technologies>
</device>
<device name="_SCH2" package="WE-UOST">
<connects>
<connect gate="G$1" pin="1" pad="9"/>
<connect gate="G$1" pin="2" pad="7"/>
<connect gate="G$1" pin="3" pad="12"/>
<connect gate="G$1" pin="4" pad="11"/>
<connect gate="G$1" pin="5" pad="5 6"/>
<connect gate="G$1" pin="6" pad="3 4"/>
<connect gate="G$1" pin="7" pad="2"/>
<connect gate="G$1" pin="8" pad="1"/>
</connects>
<technologies>
<technology name="_760871534">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760871534.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="1.25A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1250uH"/>
<attribute name="LSMIN" value="35uH"/>
<attribute name="N" value="140 : 9 : 7 : 18"/>
<attribute name="PART-NUMBER" value=" 760871534 "/>
<attribute name="RDC1" value="3000mOhm"/>
<attribute name="RDC2" value="190mOhm"/>
<attribute name="RDC3" value="30mOhm"/>
<attribute name="RDC4" value="400mOhm"/>
<attribute name="VALUE" value="12V 0.55A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VO2" value="5V"/>
</technology>
<technology name="_760871543">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760871543.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="1.15A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1310uH"/>
<attribute name="LSMIN" value="35uH"/>
<attribute name="N" value="140 : 22 : 6 : 16"/>
<attribute name="PART-NUMBER" value=" 760871543 "/>
<attribute name="RDC1" value="3000mOhm"/>
<attribute name="RDC2" value="450mOhm"/>
<attribute name="RDC3" value="25mOhm"/>
<attribute name="RDC4" value="400mOhm"/>
<attribute name="VALUE" value="24V 0.3A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VO2" value="5V"/>
</technology>
<technology name="_760875532">
<attribute name="DATASHEET-URL" value="https://katalog.we-online.com/pbs/datasheet/760875532.pdf"/>
<attribute name="FSWITCH" value="60-150kHz"/>
<attribute name="IO2" value="1.36A"/>
<attribute name="ISAT" value="0.8A"/>
<attribute name="L" value="1500uH"/>
<attribute name="LSMIN" value="60uH"/>
<attribute name="N" value="160 : 10 : 7 : 16"/>
<attribute name="PART-NUMBER" value=" 760875532 "/>
<attribute name="RDC1" value="6500mOhm"/>
<attribute name="RDC2" value="86mOhm"/>
<attribute name="RDC3" value="24mOhm"/>
<attribute name="RDC4" value="370mOhm"/>
<attribute name="VALUE" value="12V 0.7A"/>
<attribute name="VAUX" value="14V"/>
<attribute name="VI" value="85-265V(AC)"/>
<attribute name="VO2" value="5V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
