<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Passive Components - Power Magnetics - Wireless Power Transmission - WE-WPCC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-07-24&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WE-WPCC_TX_760308101312">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;
&lt;BR&gt; Size: Ø 54 x 4 mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101150">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:Ø 65 x 3.5 mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_ARRAY_760308103148">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;A28 two-coil array</description>
</package>
<package name="WE-WPCC_RX_760308102210">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 3737&lt;br&gt;</description>
</package>
<package name="WE-WPCC_ARRAY_760308104119">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Qi - A19  two-coil array</description>
</package>
<package name="WE-WPCC_RX_760308103204">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 3830&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101214">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:Φ19mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308102213">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 2929&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103202">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 4832&lt;br&gt; &lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103206">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 2815&lt;br&gt; &lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103307">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 4027&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308102306">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 4444&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103305">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 4544&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103205">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 3426&lt;br&gt; &lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308102207">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 4040&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103211">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 4636&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101220">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ17mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101219">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ15mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101208">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:Φ10mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101303">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Size:Φ26mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101216">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Φ6mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103215">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 4832&lt;br&gt; &lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101221">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:Φ6mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308105214">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:Φ19mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308105309">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:Φ26mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101309">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt; Size:Φ26mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308102212">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
type 2929&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101217">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:Φ10mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308101208A">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:Φ10mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101104">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size：ø 20mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_RX_760308103203">
<description>&lt;b&gt;Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
Size 4832&lt;br&gt; &lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308100110">
<description>&lt;B&gt;WE-WPCC Wireless Power Transfer Transmitter Coil&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Size: Ø 50</description>
</package>
<package name="WE-WPCC_RX_760308201">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Receiver Coil&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Size:3737&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308111">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308104113">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:6052&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101411">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;
&lt;BR&gt; Size:Ø 50 x 2.8 mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101304">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:ø 47mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101103">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size:ø 30mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101311">
<description>&lt;b&gt;WE-WPCC Wireless Power Transfer Transmitter Coil&lt;/b&gt;&lt;br&gt;
Size : Ø 70 x 8.5 mm&lt;br&gt;</description>
</package>
<package name="WE-WPCC_ARRAY_760308104120">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Qi - A28  3-coil array</description>
</package>
<package name="WE-WPCC_TX_760308101310">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:Ø 75 x 3.3 mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_ARRAY_760308106">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Qi - A6  3-coil array</description>
</package>
<package name="WE-WPCC_ARRAY_760308103113">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Qi - MP-A13 3-coil array</description>
</package>
<package name="WE-WPCC_ARRAY_760308103145">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Qi - MP-A6  3-coil array</description>
</package>
<package name="WE-WPCC_ARRAY_760308103149">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Qi - MP-A9 3-coil array</description>
</package>
<package name="WE-WPCC_ARRAY_760308103147">
<description>&lt;b&gt;WE-WPCC Wireless Power Array&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;MP-A8 3-coil array</description>
</package>
<package name="WE-WPCC_TX_760308100111">
<description>&lt;B&gt;WE-WPCC Wireless Power Transfer Transmitter Coil&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Size: Ø 50</description>
</package>
<package name="WE-WPCC_TX_760308100143">
<description>&lt;B&gt;WE-WPCC Wireless Power Transfer Transmitter Coil&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Size: Ø 50</description>
</package>
<package name="WE-WPCC_TX_760308141">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308103102">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308105">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101106">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size：ø 20mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101107">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size：ø 20mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101302">
<description>&lt;B&gt;WE-WPCC Wireless Power Transfer Transmitter Coil&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Size: Ø 50</description>
</package>
<package name="WE-WPCC_TX_760308102144">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308103109">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5751&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101141">
<description>&lt;B&gt;WE-WPCC Wireless Power Transfer Transmitter Coil&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Size: Ø 50</description>
</package>
<package name="WE-WPCC_TX_760308102308">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5030&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308102142">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101105">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;Size：ø 20mm &lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308100141">
<description>&lt;B&gt;WE-WPCC Wireless Power Transfer Transmitter Coil&lt;/B&gt;&lt;BR&gt;
&lt;BR&gt;Size: Ø 50</description>
</package>
<package name="WE-WPCC_TX_760308103146">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5547&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308110">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt; Size:5353&lt;br&gt;</description>
</package>
<package name="WE-WPCC_TX_760308101410">
<description>&lt;b&gt;WE-WPCC Wireless Power Charging Transmitter Coil&lt;/b&gt;
&lt;BR&gt; Size:Ø 50 x 3.1 mm&lt;br&gt;</description>
</package>
</packages>
<symbols>
<symbol name="L-2W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
<symbol name="L-1W">
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
</symbol>
<symbol name="L-3W">
<description>&lt;B&gt;WE-MLS mULTILINE emi Suppression Ferrite&lt;/b&gt;&lt;br&gt;
3 WAYS</description>
<pin name="6" direction="pas"/>
<pin name="3" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="2" direction="pas"/>
<pin name="5" direction="pas"/>
<pin name="4" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WE-WPCC_TX_2COILS" prefix="L">
<description>&lt;b&gt;WE-WPCC WPT/NFC Combination Coil&lt;/b&gt;&lt;br&gt;
&lt;BR&gt;&lt;b&gt;Characteristics &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Combination of WPT and NFC in one component
&lt;br&gt;Space-saving design
&lt;br&gt;Double-sided adhesive tape at the bottom for attachment
&lt;br&gt;Applicable for Qi (5 W &amp; 15 W), Air Fuel Alliance, NFC and proprietary solutions with high power levels, where data transfer is needed
&lt;br&gt;High permeability ferrite shielding focuses magnetic flux and protects sensitive electronics
&lt;br&gt;Litz wire and high quality ferrite for high Q and maximum power transfer efficiency
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Applications where wireless power transfer with high power levels and data communication with high data rates are necessary
&lt;br&gt;Wireless charging of sensors, smartphones, wearables, handhelds, cameras, smart watches, tablets, etc.
&lt;br&gt;Wireless power charging and payment services in one component
&lt;br&gt;Peer-to-peer communication and wireless power charging of mobile devices
&lt;br&gt;Support for your development: Use the Wireless Power 15W Kit
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o168180v209%20Family_WE-WPCC_Combination%20Coils.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o168180v209%20Family_WE-WPCC_Combination%20Coils.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WE-WPCC_COMBINATION_COILS"&gt;https://www.we-online.com/catalog/en/WE-WPCC_COMBINATION_COILS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2023-01-09&lt;br&gt;
2023 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-2W"/>
</gates>
<devices>
<device name="_760308101312" package="WE-WPCC_TX_760308101312">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance - NFC"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101312?ae"/>
<attribute name="FRES" value="7MHz/63MHz"/>
<attribute name="IR" value="6A/13A"/>
<attribute name="L" value="24uH/0.7uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308101312"/>
<attribute name="Q" value="125%/30%"/>
<attribute name="RDC-MAX" value="90ohm/30ohm"/>
<attribute name="SIZE" value="D54 x 4 mm"/>
<attribute name="VALUE" value="24uH/0.7uH"/>
</technology>
</technologies>
</device>
<device name="_760308101150" package="WE-WPCC_TX_760308101150">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance - NFC"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101150?ae"/>
<attribute name="FRES" value="20MHz/48MHz"/>
<attribute name="IR" value="7.5A/7A"/>
<attribute name="L" value="6.3uH/1.2uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308101150"/>
<attribute name="Q" value="100%/50%"/>
<attribute name="RDC-MAX" value="48ohm/55ohm"/>
<attribute name="SIZE" value="D65 x 3.5 mm"/>
<attribute name="VALUE" value="6.3uH/1.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_ARRAY_2COILS" prefix="L">
<description>&lt;b&gt;WE-WPCC Wireless Power Array
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Qi standard compliant
&lt;br&gt;Litzwire used - highest Q-value available on market
&lt;br&gt;Applicable for up to 15 W (up to 200 W outside the standards)
&lt;br&gt;High permeability shielding
&lt;br&gt;Cancels charging flux to be not coupled into sensitive components or batteries
&lt;br&gt;High reliable construction
&lt;br&gt;Mix and match your tool to find the perfect coil combination: Mix and Match
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Portable devices used in a clean area, where connectors pose a risk of polluting e.g. medical facilities, (industrial) clean &lt;br&gt;rooms, mining industry
&lt;br&gt;Devices with a large number of mating cycles to avoid connector damage: e.g. Smart watches, fitness tracker...
&lt;br&gt;Consumer products: e.g. Digital cameras, baby phone, remote control, smartphone sleeves, watertight products
&lt;br&gt;Explosion sensitive area where the use of a physical connection is hazardous
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107360v209%20WPCC_Grupp_Array.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o107360v209%20WPCC_Grupp_Array.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;br&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-WPCC-ARRAY/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-WPCC-ARRAY&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
Updated by Ella Wu 2022-03-31&lt;br&gt;
&lt;/b&gt;2022(C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L-2W"/>
</gates>
<devices>
<device name="_760308103148" package="WE-WPCC_ARRAY_760308103148">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="A28 two-coil array"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103148?ae"/>
<attribute name="FRES" value="15MHz/19MHz"/>
<attribute name="IR" value="8.5A/8.5A"/>
<attribute name="L" value="6.9uH/6.4uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308103148"/>
<attribute name="Q" value="120/115"/>
<attribute name="RDC-MAX" value="52ohm/52ohm"/>
<attribute name="SIZE" value="71 x 61 x 4 mm"/>
<attribute name="VALUE" value="6.9uH/6.4uH"/>
</technology>
</technologies>
</device>
<device name="_760308104119" package="WE-WPCC_ARRAY_760308104119">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A19"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308104119?ae"/>
<attribute name="FRES" value="12MHz/12MHz"/>
<attribute name="IR" value="8A/8A"/>
<attribute name="L" value="12uH/11.5uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308104119"/>
<attribute name="Q" value="130/130"/>
<attribute name="RDC-MAX" value="68ohm/68ohm"/>
<attribute name="SIZE" value="88 x 52 x 3.5 mm"/>
<attribute name="VALUE" value="12uH/11.5uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_RX_2COILS" prefix="L">
<description>&lt;b&gt;WE-WPCC WPT/NFC Combination Coil&lt;/b&gt;&lt;br&gt;

&lt;BR&gt;&lt;b&gt;Characteristics &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Combination of WPT and NFC in one component
&lt;br&gt;Space-saving design
&lt;br&gt;Double-sided adhesive tape at the bottom for attachment
&lt;br&gt;Applicable for Qi (5 W &amp; 15 W), Air Fuel Alliance, NFC and proprietary solutions with high power levels, where data transfer is needed
&lt;br&gt;High permeability ferrite shielding focuses magnetic flux and protects sensitive electronics
&lt;br&gt;Litz wire and high quality ferrite for high Q and maximum power transfer efficiency
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Applications where wireless power transfer with high power levels and data communication with high data rates are necessary
&lt;br&gt;Wireless charging of sensors, smartphones, wearables, handhelds, cameras, smart watches, tablets, etc.
&lt;br&gt;Wireless power charging and payment services in one component
&lt;br&gt;Peer-to-peer communication and wireless power charging of mobile devices
&lt;br&gt;Support for your development: Use the Wireless Power 15W Kit
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o168180v209%20Family_WE-WPCC_Combination%20Coils.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o168180v209%20Family_WE-WPCC_Combination%20Coils.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-WPCC_COMBINATION_COILS/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-WPCC_COMBINATION_COILS&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2022-03-31&lt;br&gt;
2022 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-2W"/>
</gates>
<devices>
<device name="_760308102306" package="WE-WPCC_RX_760308102306">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance - NFC"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102306?ae"/>
<attribute name="FRES" value="17.5MHz/50MHz"/>
<attribute name="IR" value="2A/5A"/>
<attribute name="L" value="8uH/1.4uH"/>
<attribute name="P" value="40W"/>
<attribute name="PART-NUMBER" value="760308102306"/>
<attribute name="Q" value="19%/47%"/>
<attribute name="RDC-MAX" value="400ohm/100ohm"/>
<attribute name="SIZE" value="44 x 44 x 1 mm"/>
<attribute name="VALUE" value="8uH/1.4uH"/>
</technology>
</technologies>
</device>
<device name="_760308103305" package="WE-WPCC_RX_760308103305">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance - NFC"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103305?ae"/>
<attribute name="FRES" value="22MHz/50MHz"/>
<attribute name="IR" value="2.6A/5A"/>
<attribute name="L" value="8.8uH/1.4uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308103305"/>
<attribute name="Q" value="30%/47%"/>
<attribute name="RDC-MAX" value="220ohm/100ohm"/>
<attribute name="SIZE" value="45 x 44 x 0.7 mm"/>
<attribute name="VALUE" value="8.8uH/1.4uH"/>
</technology>
</technologies>
</device>
<device name="_760308103307" package="WE-WPCC_RX_760308103307">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance - NFC"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103307?ae"/>
<attribute name="FRES" value="22MHz/54MHz"/>
<attribute name="IR" value="1.5A/4A"/>
<attribute name="L" value="8uH/1.6uH"/>
<attribute name="P" value="30W"/>
<attribute name="PART-NUMBER" value="760308103307"/>
<attribute name="Q" value="19%/47%"/>
<attribute name="RDC-MAX" value="350ohm/100ohm"/>
<attribute name="SIZE" value="40 x 27 x 1 mm"/>
<attribute name="VALUE" value="8uH/1.6uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_RX_1COIL" prefix="L">
<description>&lt;b&gt;WE-WPCC Wireless Power Transfer Receiver Coil&lt;/b&gt;&lt;br&gt;

&lt;BR&gt;&lt;b&gt;Characteristics &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Qi standard compliant
&lt;br&gt;highest Q-value available on market
&lt;br&gt;Today there are two inductive wireless power standards; the Qi standard of WPC and the PMA standard of Power Matters &lt;br&gt;Alliance. We offer a dual standard receiver coil - 760308102210. The advantage of this high quality coil with litz wire and ferrite &lt;br&gt;fortification in the center is that devices using this solution can be charged on charging stations of both standards.
&lt;br&gt;Mix and match your tool to find the perfect coil combination: Mix and Match
&lt;br&gt;
&lt;br&gt;

&lt;b&gt;Applications &lt;/b&gt;&lt;br&gt;
&lt;br&gt;Cell phones/ smartphones/ hand-held devices
&lt;br&gt;Portable devices used in a clean area, where connectors pose a risk of polluting e.g. medical facilities and (industrial) clean rooms
&lt;br&gt;Devices with a large number of mating cycles to avoid connector damage
&lt;br&gt;Headsets
&lt;br&gt;Portable media players 
&lt;br&gt;

&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107339v209%20WE-WPCC_Receiver_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107339v209%20WE-WPCC_Receiver_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-WPCC-RECEIVER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-WPCC-RECEIVER&lt;/a&gt;&lt;p&gt;

Updated by Ella Wu 2025-07-24&lt;br&gt;
2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_760308102210" package="WE-WPCC_RX_760308102210">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102210?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="7.5uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308102210"/>
<attribute name="Q" value="45%"/>
<attribute name="RDC-MAX" value="180ohm"/>
<attribute name="SIZE" value="37 x 37 x 1.8 mm"/>
<attribute name="VALUE" value="7.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308103204" package="WE-WPCC_RX_760308103204">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103204?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="16.7uH"/>
<attribute name="P" value="30W"/>
<attribute name="PART-NUMBER" value="760308103204"/>
<attribute name="Q" value="32%"/>
<attribute name="RDC-MAX" value="430ohm"/>
<attribute name="SIZE" value="38 x 30 x 0.8 mm"/>
<attribute name="VALUE" value="16.7uH"/>
</technology>
</technologies>
</device>
<device name="_760308103202" package="WE-WPCC_RX_760308103202">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103202?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="12uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308103202"/>
<attribute name="Q" value="33%"/>
<attribute name="RDC-MAX" value="200ohm"/>
<attribute name="SIZE" value="48 x 32 x 0.9 mm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
</technologies>
</device>
<device name="_760308102213" package="WE-WPCC_RX_760308102213">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102213?ae"/>
<attribute name="FRES" value="21MHz"/>
<attribute name="IR" value="1.7A"/>
<attribute name="L" value="7.9uH"/>
<attribute name="P" value="30W"/>
<attribute name="PART-NUMBER" value="760308102213"/>
<attribute name="Q" value="18%"/>
<attribute name="RDC-MAX" value="330ohm"/>
<attribute name="SIZE" value="29 x 29 x 0.6 mm"/>
<attribute name="VALUE" value="7.9uH"/>
</technology>
</technologies>
</device>
<device name="_760308101214" package="WE-WPCC_RX_760308101214">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101214?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="L" value="26uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308101214"/>
<attribute name="Q" value="25%"/>
<attribute name="RDC-MAX" value="520ohm"/>
<attribute name="SIZE" value="D19 x 0.8 mm"/>
<attribute name="VALUE" value="26uH"/>
</technology>
</technologies>
</device>
<device name="_760308103206" package="WE-WPCC_RX_760308103206">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103206?ae"/>
<attribute name="FRES" value="23MHz"/>
<attribute name="IR" value="1.55A"/>
<attribute name="L" value="7.5uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308103206"/>
<attribute name="Q" value="16%"/>
<attribute name="RDC-MAX" value="380ohm"/>
<attribute name="SIZE" value="28,9 x 15,7 x 0,76 mm"/>
<attribute name="VALUE" value="7.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308103205" package="WE-WPCC_RX_760308103205">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103205?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="L" value="11uH"/>
<attribute name="P" value="40W"/>
<attribute name="PART-NUMBER" value="760308103205"/>
<attribute name="Q" value="30%"/>
<attribute name="RDC-MAX" value="200ohm"/>
<attribute name="SIZE" value="34 x 26 x 0.9 mm"/>
<attribute name="VALUE" value="11uH"/>
</technology>
</technologies>
</device>
<device name="_760308102207" package="WE-WPCC_RX_760308102207">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102207?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="5A"/>
<attribute name="L" value="8uH"/>
<attribute name="P" value="80W"/>
<attribute name="PART-NUMBER" value="760308102207"/>
<attribute name="Q" value="30%"/>
<attribute name="RDC-MAX" value="80ohm"/>
<attribute name="SIZE" value="40 x 40 x 1.2 mm"/>
<attribute name="VALUE" value="8uH"/>
</technology>
</technologies>
</device>
<device name="_760308103211" package="WE-WPCC_RX_760308103211">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - Airfuel Alliance"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103211?ae"/>
<attribute name="FRES" value="12.7MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="L" value="7.3uH"/>
<attribute name="P" value="40W"/>
<attribute name="PART-NUMBER" value="760308103211"/>
<attribute name="Q" value="28%"/>
<attribute name="RDC-MAX" value="200ohm"/>
<attribute name="SIZE" value="46 x 36 x 0.5 mm"/>
<attribute name="VALUE" value="7.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308101208" package="WE-WPCC_RX_760308101208">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101208?ae"/>
<attribute name="FRES" value="26MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="L" value="13uH"/>
<attribute name="P" value="15W"/>
<attribute name="PART-NUMBER" value="760308101208"/>
<attribute name="Q" value="17%"/>
<attribute name="RDC-MAX" value="500ohm"/>
<attribute name="SIZE" value="D10 x 1.6 mm"/>
<attribute name="VALUE" value="13uH"/>
</technology>
</technologies>
</device>
<device name="_760308101216" package="WE-WPCC_RX_760308101216">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101216?ae"/>
<attribute name="FRES" value="32MHz"/>
<attribute name="IR" value="0.8A"/>
<attribute name="L" value="7.2uH"/>
<attribute name="P" value="5W"/>
<attribute name="PART-NUMBER" value="760308101216"/>
<attribute name="Q" value="10%"/>
<attribute name="RDC-MAX" value="450ohm"/>
<attribute name="SIZE" value="D6 x 2 mm"/>
<attribute name="VALUE" value="7.2uH"/>
</technology>
</technologies>
</device>
<device name="_760308101219" package="WE-WPCC_RX_760308101219">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101219?ae"/>
<attribute name="FRES" value="22MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="L" value="11.8uH"/>
<attribute name="P" value="5W"/>
<attribute name="PART-NUMBER" value="760308101219"/>
<attribute name="Q" value="13%"/>
<attribute name="RDC-MAX" value="750ohm"/>
<attribute name="SIZE" value="D15 x 0.6 mm"/>
<attribute name="VALUE" value="11.8uH"/>
</technology>
</technologies>
</device>
<device name="_760308101220" package="WE-WPCC_RX_760308101220">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101220?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.1A"/>
<attribute name="L" value="12.6uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308101220"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="360ohm"/>
<attribute name="SIZE" value="D17 x 0.8 mm"/>
<attribute name="VALUE" value="12.6uH"/>
</technology>
</technologies>
</device>
<device name="_760308101303" package="WE-WPCC_RX_760308101303">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101303?ae"/>
<attribute name="FRES" value="8MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="L" value="47uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308101303"/>
<attribute name="Q" value="25%"/>
<attribute name="RDC-MAX" value="500ohm"/>
<attribute name="SIZE" value="D26 x 1.3 mm"/>
<attribute name="VALUE" value="47uH"/>
</technology>
</technologies>
</device>
<device name="_760308103215" package="WE-WPCC_RX_760308103215">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103215?ae"/>
<attribute name="FRES" value="8.8MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="14.3uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308103215"/>
<attribute name="Q" value="40%"/>
<attribute name="RDC-MAX" value="190ohm"/>
<attribute name="SIZE" value="48 x 32 x 1 mm"/>
<attribute name="VALUE" value="14.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308101221" package="WE-WPCC_RX_760308101221">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101221?ae"/>
<attribute name="FRES" value="10MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="L" value="24uH"/>
<attribute name="P" value="5W"/>
<attribute name="PART-NUMBER" value="760308101221"/>
<attribute name="Q" value="16%"/>
<attribute name="RDC-MAX" value="1150ohm"/>
<attribute name="SIZE" value="D6 x 4.3 mm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
</technologies>
</device>
<device name="_760308105214" package="WE-WPCC_RX_760308105214">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308105214?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="L" value="6.3uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308105214"/>
<attribute name="Q" value="15%"/>
<attribute name="RDC-MAX" value="350ohm"/>
<attribute name="SIZE" value="D19 x 0.8 mm"/>
<attribute name="VALUE" value="6.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308105309" package="WE-WPCC_RX_760308105309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308105309?ae"/>
<attribute name="FRES" value="18.5MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="L" value="10.5uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308105309"/>
<attribute name="Q" value="19%"/>
<attribute name="RDC-MAX" value="450ohm"/>
<attribute name="SIZE" value="D26 x 0.5 mm"/>
<attribute name="VALUE" value="10.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308101309" package="WE-WPCC_RX_760308101309">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101309?ae"/>
<attribute name="FRES" value="19MHz"/>
<attribute name="IR" value="1.5A"/>
<attribute name="L" value="10uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308101309"/>
<attribute name="Q" value="20%"/>
<attribute name="RDC-MAX" value="450ohm"/>
<attribute name="SIZE" value="D26 x 0.5 mm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_760308101208A" package="WE-WPCC_RX_760308101208A">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101208A?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="0.7A"/>
<attribute name="L" value="18uH"/>
<attribute name="P" value="15W"/>
<attribute name="PART-NUMBER" value="760308101208A"/>
<attribute name="Q" value="18%"/>
<attribute name="RDC-MAX" value="650ohm"/>
<attribute name="SIZE" value="D10 x 1.6 mm"/>
<attribute name="VALUE" value="18uH"/>
</technology>
</technologies>
</device>
<device name="_760308101217" package="WE-WPCC_RX_760308101217">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101217?ae"/>
<attribute name="FRES" value="17.5MHz"/>
<attribute name="IR" value="0.4A"/>
<attribute name="L" value="24.2uH"/>
<attribute name="P" value="5W"/>
<attribute name="PART-NUMBER" value="760308101217"/>
<attribute name="Q" value="13%"/>
<attribute name="RDC-MAX" value="1400ohm"/>
<attribute name="SIZE" value="D10 x 1.8 mm"/>
<attribute name="VALUE" value="24.2uH"/>
</technology>
</technologies>
</device>
<device name="_760308103203" package="WE-WPCC_RX_760308103203">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103203?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="1.8A"/>
<attribute name="L" value="12uH"/>
<attribute name="P" value="20W"/>
<attribute name="PART-NUMBER" value="760308103203"/>
<attribute name="Q" value="21%"/>
<attribute name="RDC-MAX" value="360ohm"/>
<attribute name="SIZE" value="48 x 32 x 0.8 mm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
</technologies>
</device>
<device name="_760308201" package="WE-WPCC_RX_760308201">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308201?ae"/>
<attribute name="FRES" value="15MHz"/>
<attribute name="IR" value="3.5A"/>
<attribute name="L" value="10uH"/>
<attribute name="P" value="60W"/>
<attribute name="PART-NUMBER" value="760308201"/>
<attribute name="Q" value="50%"/>
<attribute name="RDC-MAX" value="200ohm"/>
<attribute name="SIZE" value="37 x 37 x 1.8 mm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_760308102212" package="WE-WPCC_RX_760308102212">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Rx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102212?ae"/>
<attribute name="FRES" value="25MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="5.4uH"/>
<attribute name="P" value="30W"/>
<attribute name="PART-NUMBER" value="760308102212"/>
<attribute name="Q" value="18%"/>
<attribute name="RDC-MAX" value="240ohm"/>
<attribute name="SIZE" value="29 x 29 x 0.6 mm"/>
<attribute name="VALUE" value="5.4uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_ARRAY_3COILS" prefix="L">
<description>&lt;b&gt;WE-WPCC Wireless Power Array
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Qi standard compliant
&lt;br&gt;Litzwire used - highest Q-value available on market
&lt;br&gt;Applicable for up to 15 W (up to 200 W outside the standards)
&lt;br&gt;High permeability shielding
&lt;br&gt;Cancels charging flux to be not coupled into sensitive components or batteries
&lt;br&gt;High reliable construction
&lt;br&gt;Mix and match your tool to find the perfect coil combination: Mix and Match
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Portable devices used in a clean area, where connectors pose a risk of polluting e.g. medical facilities, (industrial) clean &lt;br&gt;rooms, mining industry
&lt;br&gt;Devices with a large number of mating cycles to avoid connector damage: e.g. Smart watches, fitness tracker...
&lt;br&gt;Consumer products: e.g. Digital cameras, baby phone, remote control, smartphone sleeves, watertight products
&lt;br&gt;Explosion sensitive area where the use of a physical connection is hazardous
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107360v209%20WPCC_Grupp_Array.jpg"&gt;
&lt;img src="https://www.we-online.com/components/media/o107360v209%20WPCC_Grupp_Array.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;&lt;br&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-WPCC-ARRAY/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/components/products/WE-WPCC-ARRAY&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;
Updated by Ella Wu 2022-03-31&lt;br&gt;
&lt;/b&gt;2022(C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L-3W"/>
</gates>
<devices>
<device name="_760308104120" package="WE-WPCC_ARRAY_760308104120">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A28"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308104120?ae"/>
<attribute name="FRES" value="15MHz/15MHz/15MHz"/>
<attribute name="IR" value="9A/9A/9A"/>
<attribute name="L" value="6.9uH/6.4uH/6.9uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308104120"/>
<attribute name="Q" value="100/100/100"/>
<attribute name="RDC-MAX" value="45ohm/45ohm/45ohm"/>
<attribute name="SIZE" value="92 x 50 x 5.5 mm"/>
<attribute name="VALUE" value="6.9uH/6.4uH/6.9uH"/>
</technology>
</technologies>
</device>
<device name="_760308106" package="WE-WPCC_ARRAY_760308106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A6"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308106?ae"/>
<attribute name="FRES" value="14MHz/14MHz/14MHz"/>
<attribute name="IR" value="9A/9A/9A"/>
<attribute name="L" value="12.5uH/11.5uH/12.5uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308106"/>
<attribute name="Q" value="125/125/125"/>
<attribute name="RDC-MAX" value="65ohm/65ohm/65ohm"/>
<attribute name="SIZE" value="130 x 55 x 8 mm"/>
<attribute name="VALUE" value="12.5uH/11.5uH/12.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308103145" package="WE-WPCC_ARRAY_760308103145">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - MP-A6"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103145?ae"/>
<attribute name="FRES" value="10MHz/10MHz/10MHz"/>
<attribute name="IR" value="8.5A/8.5A/8.5A"/>
<attribute name="L" value="11.3uH/11.3uH/11.3uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308103145"/>
<attribute name="Q" value="150/150/145"/>
<attribute name="RDC-MAX" value="83ohm/83ohm/83ohm"/>
<attribute name="SIZE" value="109 x 56 x 5.2 mm"/>
<attribute name="VALUE" value="11.3uH/11.3uH/11.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308103147" package="WE-WPCC_ARRAY_760308103147">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="MP-A8 3-coil array"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103147?ae"/>
<attribute name="FRES" value="11MHz/11MHz/11MHz"/>
<attribute name="IR" value="9A/10A/9A"/>
<attribute name="L" value="8.5uH/7.5uH/8.5uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308103147"/>
<attribute name="Q" value="145/130/145"/>
<attribute name="RDC-MAX" value="56ohm/56ohm/56ohm"/>
<attribute name="SIZE" value="100 x 55 x 5.2 mm"/>
<attribute name="VALUE" value="8.5uH/7.5uH/8.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308103113" package="WE-WPCC_ARRAY_760308103113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - MP-A13 3-coil array"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103113?ae"/>
<attribute name="FRES" value="14MHz/14MHz/14MHz"/>
<attribute name="IR" value="9A/9A/9A"/>
<attribute name="L" value="12.5uH/11.5uH/12.5uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308103113"/>
<attribute name="Q" value="125/115/125"/>
<attribute name="RDC-MAX" value="65ohm/65ohm/65ohm"/>
<attribute name="SIZE" value="100 x 55 x 4.5 mm"/>
<attribute name="VALUE" value="12.5uH/11.5uH/12.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308103149" package="WE-WPCC_ARRAY_760308103149">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="4" pad="4"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="6" pad="6"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - MP-A9 3-coil array"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103149?ae"/>
<attribute name="FRES" value="8MHz/8MHz/8MHz"/>
<attribute name="IR" value="9A/9A/9A"/>
<attribute name="L" value="10.2uH/9.8uH/10.2uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308103149"/>
<attribute name="Q" value="135/130/135"/>
<attribute name="RDC-MAX" value="55ohm/55ohm/55ohm"/>
<attribute name="SIZE" value="106 x 57 x 4.2 mm"/>
<attribute name="VALUE" value="10.2uH/9.8uH/10.2uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WE-WPCC_TX_1COIL" prefix="L">
<description>&lt;b&gt;WE-WPCC Wireless Power Transfer Transmitter Coil
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Qi standard compliant
&lt;br&gt;Litzwire used - highest Q-value available on market
&lt;br&gt;Applicable for up to 15 W (up to 300 W outside the standards)
&lt;br&gt;High permeability shielding
&lt;br&gt;Cancels charging flux to be not coupled into sensitive components or batteries
&lt;br&gt;High reliable construction
&lt;br&gt;Pot core construction limits the stray field in the design
&lt;br&gt;
&lt;br&gt; &lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Portable devices used in a clean area, where connectors pose a risk of polluting e.g. medical facilities, (industrial) clean &lt;br&gt;rooms, mining industry
&lt;br&gt;Devices with a large number of mating cycles to avoid connector damage: e.g. Smart watches, fitness tracker...
&lt;br&gt;Consumer products: e.g. Digital cameras, baby phone, remote control, smartphone sleeves, watertight products
&lt;br&gt;Explosion sensitive area where the use of a physical connection is hazardous
&lt;br&gt;Smart sensors
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o107327v209%20WE-WPCC_Transmitter_102142_101104_101141_103146.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o107327v209%20WE-WPCC_Transmitter_102142_101104_101141_103146.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WE-WPCC-TRANSMITTER/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WE-WPCC-TRANSMITTER&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;

Updated by Ella Wu 2024-03-15&lt;br&gt;
&lt;/b&gt;2024(C) Würth Elektronik&lt;br&gt;</description>
<gates>
<gate name="G$1" symbol="L-1W"/>
</gates>
<devices>
<device name="_760308101104" package="WE-WPCC_TX_760308101104">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101104?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="L" value="6.8uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308101104"/>
<attribute name="Q" value="42%"/>
<attribute name="RDC-MAX" value="130ohm"/>
<attribute name="SIZE" value="D20 x 2.8 mm"/>
<attribute name="VALUE" value="6.8uH"/>
</technology>
</technologies>
</device>
<device name="_760308100110" package="WE-WPCC_TX_760308100110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A10; MP-A1/A7"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308100110?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="L" value="24uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308100110"/>
<attribute name="Q" value="180%"/>
<attribute name="RDC-MAX" value="100ohm"/>
<attribute name="SIZE" value="D50 x 6 mm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
</technologies>
</device>
<device name="_760308111" package="WE-WPCC_TX_760308111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A11; MP-A11"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308111?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="13A"/>
<attribute name="L" value="6.3uH"/>
<attribute name="P" value="200W"/>
<attribute name="PART-NUMBER" value="760308111"/>
<attribute name="Q" value="80%"/>
<attribute name="RDC-MAX" value="25ohm"/>
<attribute name="SIZE" value="53 x 53 x 6 mm"/>
<attribute name="VALUE" value="6.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308104113" package="WE-WPCC_TX_760308104113">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A13"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308104113?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="L" value="12uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308104113"/>
<attribute name="Q" value="120%"/>
<attribute name="RDC-MAX" value="72ohm"/>
<attribute name="SIZE" value="60 x 52 x 4 mm"/>
<attribute name="VALUE" value="12uH"/>
</technology>
</technologies>
</device>
<device name="_760308101103" package="WE-WPCC_TX_760308101103">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101103?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="6.5uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308101103"/>
<attribute name="Q" value="35%"/>
<attribute name="RDC-MAX" value="200ohm"/>
<attribute name="SIZE" value="D30 x 1.9 mm"/>
<attribute name="VALUE" value="6.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308101304" package="WE-WPCC_TX_760308101304">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi-A11; MP-A11"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101304?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="L" value="6.3uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308101304"/>
<attribute name="Q" value="115%"/>
<attribute name="RDC-MAX" value="48ohm"/>
<attribute name="SIZE" value="D48 x 3 mm"/>
<attribute name="VALUE" value="6.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308141" package="WE-WPCC_TX_760308141">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A29; MP-A5"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308141?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="L" value="10uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308141"/>
<attribute name="Q" value="200%"/>
<attribute name="RDC-MAX" value="30ohm"/>
<attribute name="SIZE" value="53 x 53 x 6 mm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_760308102142" package="WE-WPCC_TX_760308102142">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102142?ae"/>
<attribute name="FRES" value="12MHz"/>
<attribute name="IR" value="18A"/>
<attribute name="L" value="5.8uH"/>
<attribute name="P" value="300W"/>
<attribute name="PART-NUMBER" value="760308102142"/>
<attribute name="Q" value="100%"/>
<attribute name="RDC-MAX" value="12ohm"/>
<attribute name="SIZE" value="53 x 53 x 6.5 mm"/>
<attribute name="VALUE" value="5.8uH"/>
</technology>
</technologies>
</device>
<device name="_760308103102" package="WE-WPCC_TX_760308103102">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - MP-A2"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103102?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="7A"/>
<attribute name="L" value="10uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308103102"/>
<attribute name="Q" value="130%"/>
<attribute name="RDC-MAX" value="55ohm"/>
<attribute name="SIZE" value="53 x 53 x 4.5 mm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_760308100111" package="WE-WPCC_TX_760308100111">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A11; MP-A11"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308100111?ae"/>
<attribute name="FRES" value="24MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="L" value="6.3uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308100111"/>
<attribute name="Q" value="120%"/>
<attribute name="RDC-MAX" value="51ohm"/>
<attribute name="SIZE" value="D50 x 6 mm"/>
<attribute name="VALUE" value="6.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308100143" package="WE-WPCC_TX_760308100143">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308100143?ae"/>
<attribute name="FRES" value="16MHz"/>
<attribute name="IR" value="12A"/>
<attribute name="L" value="6uH"/>
<attribute name="P" value="200W"/>
<attribute name="PART-NUMBER" value="760308100143"/>
<attribute name="Q" value="180%"/>
<attribute name="RDC-MAX" value="18ohm"/>
<attribute name="SIZE" value="D50 x 6.7 mm"/>
<attribute name="VALUE" value="6uH"/>
</technology>
</technologies>
</device>
<device name="_760308100141" package="WE-WPCC_TX_760308100141">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A29; MP-A5"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308100141?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="L" value="10uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308100141"/>
<attribute name="Q" value="180%"/>
<attribute name="RDC-MAX" value="30ohm"/>
<attribute name="SIZE" value="D50 x 6 mm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_760308101302" package="WE-WPCC_TX_760308101302">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101302?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="L" value="5.3uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308101302"/>
<attribute name="Q" value="100%"/>
<attribute name="RDC-MAX" value="35ohm"/>
<attribute name="SIZE" value="D50 x 4.7 mm"/>
<attribute name="VALUE" value="5.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308102144" package="WE-WPCC_TX_760308102144">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102144?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="9.5A"/>
<attribute name="L" value="19.5uH"/>
<attribute name="P" value="200W"/>
<attribute name="PART-NUMBER" value="760308102144"/>
<attribute name="Q" value="220%"/>
<attribute name="RDC-MAX" value="45ohm"/>
<attribute name="SIZE" value="53 x 53 x 7 mm"/>
<attribute name="VALUE" value="19.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308102308" package="WE-WPCC_TX_760308102308">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308102308?ae"/>
<attribute name="FRES" value="27MHz"/>
<attribute name="IR" value="8.5A"/>
<attribute name="L" value="3uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308102308"/>
<attribute name="Q" value="60%"/>
<attribute name="RDC-MAX" value="35ohm"/>
<attribute name="SIZE" value="50 x 30 x 2.4 mm"/>
<attribute name="VALUE" value="3uH"/>
</technology>
</technologies>
</device>
<device name="_760308101141" package="WE-WPCC_TX_760308101141">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A29; MP-A5"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101141?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="L" value="10uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308101141"/>
<attribute name="Q" value="220%"/>
<attribute name="RDC-MAX" value="30ohm"/>
<attribute name="SIZE" value="D50 x 5 mm"/>
<attribute name="VALUE" value="10uH"/>
</technology>
</technologies>
</device>
<device name="_760308101106" package="WE-WPCC_TX_760308101106">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101106?ae"/>
<attribute name="FRES" value="38MHz"/>
<attribute name="IR" value="2.5A"/>
<attribute name="L" value="2.5uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308101106"/>
<attribute name="Q" value="30%"/>
<attribute name="RDC-MAX" value="90ohm"/>
<attribute name="SIZE" value="D20 x 2.8 mm"/>
<attribute name="VALUE" value="2.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308101107" package="WE-WPCC_TX_760308101107">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101107?ae"/>
<attribute name="FRES" value="7.5MHz"/>
<attribute name="IR" value="2A"/>
<attribute name="L" value="24uH"/>
<attribute name="P" value="40W"/>
<attribute name="PART-NUMBER" value="760308101107"/>
<attribute name="Q" value="55%"/>
<attribute name="RDC-MAX" value="315ohm"/>
<attribute name="SIZE" value="D31 x 2.8 mm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
</technologies>
</device>
<device name="_760308101105" package="WE-WPCC_TX_760308101105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101105?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="3A"/>
<attribute name="L" value="3.3uH"/>
<attribute name="P" value="50W"/>
<attribute name="PART-NUMBER" value="760308101105"/>
<attribute name="Q" value="30%"/>
<attribute name="RDC-MAX" value="90ohm"/>
<attribute name="SIZE" value="D20 x 2.8 mm"/>
<attribute name="VALUE" value="3.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308101" package="WE-WPCC_TX_760308101">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A1"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="L" value="24uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308101"/>
<attribute name="Q" value="90%"/>
<attribute name="RDC-MAX" value="100ohm"/>
<attribute name="SIZE" value="53 x 53 x 6 mm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
</technologies>
</device>
<device name="_760308110" package="WE-WPCC_TX_760308110">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A10; MP-A1/A7"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308110?ae"/>
<attribute name="FRES" value="5MHz"/>
<attribute name="IR" value="6A"/>
<attribute name="L" value="24uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308110"/>
<attribute name="Q" value="180%"/>
<attribute name="RDC-MAX" value="100ohm"/>
<attribute name="SIZE" value="53 x 53 x 6 mm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
</technologies>
</device>
<device name="_760308105" package="WE-WPCC_TX_760308105">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - A5"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308105?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="13A"/>
<attribute name="L" value="6.3uH"/>
<attribute name="P" value="200W"/>
<attribute name="PART-NUMBER" value="760308105"/>
<attribute name="Q" value="55%"/>
<attribute name="RDC-MAX" value="25ohm"/>
<attribute name="SIZE" value="53 x 53 x 6 mm"/>
<attribute name="VALUE" value="6.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308103146" package="WE-WPCC_TX_760308103146">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - MP-A8"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103146?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="8A"/>
<attribute name="L" value="8.5uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308103146"/>
<attribute name="Q" value="140%"/>
<attribute name="RDC-MAX" value="56ohm"/>
<attribute name="SIZE" value="55 x 47 x 4.5 mm"/>
<attribute name="VALUE" value="8.5uH"/>
</technology>
</technologies>
</device>
<device name="_760308103109" package="WE-WPCC_TX_760308103109">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="Qi - MP - A9"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308103109?ae"/>
<attribute name="FRES" value="11MHz"/>
<attribute name="IR" value="9A"/>
<attribute name="L" value="10.2uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308103109"/>
<attribute name="Q" value="130%"/>
<attribute name="RDC-MAX" value="50ohm"/>
<attribute name="SIZE" value="57 x 51 x 4.2 mm"/>
<attribute name="VALUE" value="10.2uH"/>
</technology>
</technologies>
</device>
<device name="_760308101410" package="WE-WPCC_TX_760308101410">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101410?ae"/>
<attribute name="FRES" value="6MHz"/>
<attribute name="IR" value="5.5A"/>
<attribute name="L" value="24uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308101410"/>
<attribute name="Q" value="170%"/>
<attribute name="RDC-MAX" value="100ohm"/>
<attribute name="SIZE" value="D50 x 3.1 mm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
</technologies>
</device>
<device name="_760308101411" package="WE-WPCC_TX_760308101411">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101411?ae"/>
<attribute name="FRES" value="20MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="L" value="6.3uH"/>
<attribute name="P" value="150W"/>
<attribute name="PART-NUMBER" value="760308101411"/>
<attribute name="Q" value="110%"/>
<attribute name="RDC-MAX" value="48ohm"/>
<attribute name="SIZE" value="D50 x 2.8 mm"/>
<attribute name="VALUE" value="6.3uH"/>
</technology>
</technologies>
</device>
<device name="_760308101311" package="WE-WPCC_TX_760308101311">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101311?ae"/>
<attribute name="FRES" value="13MHz"/>
<attribute name="IR" value="21A"/>
<attribute name="L" value="5.8uH"/>
<attribute name="P" value="400W"/>
<attribute name="PART-NUMBER" value="760308101311"/>
<attribute name="Q" value="220%"/>
<attribute name="RDC-MAX" value="14ohm"/>
<attribute name="SIZE" value="D70 x 8.5 mm"/>
<attribute name="VALUE" value="5.8uH"/>
</technology>
</technologies>
</device>
<device name="_760308101310" package="WE-WPCC_TX_760308101310">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="2" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="COMPLIANCE" value="works with Qi Tx ICs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/760308101310?ae"/>
<attribute name="FRES" value="7.7MHz"/>
<attribute name="IR" value="7.5A"/>
<attribute name="L" value="24uH"/>
<attribute name="P" value="100W"/>
<attribute name="PART-NUMBER" value="760308101310"/>
<attribute name="Q" value="155%"/>
<attribute name="RDC-MAX" value="110ohm"/>
<attribute name="SIZE" value="D75 x 3.3 mm"/>
<attribute name="VALUE" value="24uH"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
