<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - LEDs - Singnal LEDs - Clip LED - WL-SBCC&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-18&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SBCC_0603">
<description>&lt;B&gt;WL-SBCC&lt;/B&gt; &lt;BR&gt;SMT Bi-color Chip LED Compact ,Size:0603,1.6x0.8x0.4mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SBCC_0603">
<description>&lt;b&gt;WL-SBCC_0603&lt;/b&gt;</description>
<pin name="V-" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="R+" direction="pas"/>
<pin name="V+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SBCC_0603" prefix="D" uservalue="yes">
<description>&lt;br&gt; &lt;B&gt;WL-SBCC SMT Bi-color Chip LED Compact
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Two chips in one packaging 
&lt;br&gt;Small size 
&lt;br&gt;Industry standard footprint 
&lt;br&gt;High efficiency 
&lt;br&gt;Low power consumption 
&lt;br&gt;Wide viewing angle 
&lt;br&gt;Small package for exceptional brightness 
&lt;br&gt;Packaged in standard tape and reel 7" 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;&lt;br&gt;&lt;/b&gt;Backlighting applications 
&lt;br&gt;Status indicator 
&lt;br&gt;Front panel indicators 
&lt;br&gt;Push button backlighting 
&lt;br&gt;Symbol and switch backlighting 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o136122v209%20Family_WC-SBCC.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o136122v209%20Family_WC-SBCC.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SBCC/"&gt;https://www.we-online.com/catalog/en/WL-SBCC/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Created by Yingchun, Shan 2020-03-18&lt;br&gt;
&lt;/b&gt;2020(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SBCC_0603"/>
</gates>
<devices>
<device name="" package="WL-SBCC_0603">
<connects>
<connect gate="G$1" pin="R+" pad="3"/>
<connect gate="G$1" pin="R-" pad="2"/>
<connect gate="G$1" pin="V+" pad="4"/>
<connect gate="G$1" pin="V-" pad="1"/>
</connects>
<technologies>
<technology name="_150060RV75240">
<attribute name="ABSTRAHLWINKEL" value="140°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP "/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150060RV75240.pdf"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Bright Green "/>
<attribute name="I-V-R-TYP" value="230mcd"/>
<attribute name="I-V-V-TYP" value="90mcd"/>
<attribute name="LAMDA-DOM-R-TYP" value="625nm"/>
<attribute name="LAMDA-DOM-V-TYP" value="570nm"/>
<attribute name="LAMDA-PEAK-R-TYP" value="630nm"/>
<attribute name="LAMDA-PEAK-V-TYP" value="572nm"/>
<attribute name="PART-NUMBER" value="150060RV75240"/>
<attribute name="V-F-R-TYP" value="2V"/>
<attribute name="V-F-V-TYP" value="2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
