<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - LEDs - Singnal LEDs - Clip LED - WL-SBCW&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-03-31&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SBCW_0606">
<description>&lt;B&gt;WL-SBCW SMT Bi-color Chip LED Waterclear
&lt;/B&gt; &lt;BR&gt;&lt;BR&gt;Size 0606,SMT, 4pins
&lt;BR&gt;1.6x1.6x0.7mm(LXWXH)</description>
</package>
<package name="WL-SBCW_1210">
<description>&lt;B&gt;WL-SBCW SMT Bi-color Chip LED Waterclear
&lt;/B&gt; &lt;BR&gt;&lt;BR&gt;Size 0606, SMT, 4pins
&lt;BR&gt;3.2x2.7x0.7mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SBCW">
<description>Dual LED</description>
<pin name="V-" direction="pas"/>
<pin name="V+" direction="pas"/>
<pin name="S-" direction="pas"/>
<pin name="S+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SBCW_0606" prefix="D">
<description>&lt;b&gt; WL-SBCW SMD Bi-color Chip LED Waterclear
&lt;br&gt;
&lt;br&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;

&lt;br&gt;Two chips in one package
&lt;br&gt;Small size
&lt;br&gt;Industry standard footprint
&lt;br&gt;High efficiency
&lt;br&gt;Low power consumption
&lt;br&gt;Wide viewing angle
&lt;br&gt;Small LED package for exceptional brightness
&lt;br&gt;Packaged in standard tape and reel 7"
&lt;br&gt;Compatible with automatic placement machine
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Backlighting applications
&lt;br&gt;Status indicator
&lt;br&gt;Front panel indicators
&lt;br&gt;Push button backlighting
&lt;br&gt;Symbol and switch backlighting
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14901v209%20Family_WL_SBCW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14901v209%20Family_WL_SBCW.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SBCW"&gt;https://www.we-online.com/catalog/en/WL-SBCW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-03-31&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SBCW"/>
</gates>
<devices>
<device name="" package="WL-SBCW_0606">
<connects>
<connect gate="G$1" pin="S+" pad="4"/>
<connect gate="G$1" pin="S-" pad="1"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="_150066RG74000">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150066RG74000.pdf"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red / 520nm@Green"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red / 3.2V@Green"/>
<attribute name="LUMINOUS-INTENSITY" value="300mcd@Red / 560mcd@Green"/>
<attribute name="PART-NUMBER" value="150066RG74000"/>
<attribute name="PEAK-WAVELENGTH" value="630nm@Red / 515nm@Green"/>
<attribute name="VALUE" value="150066RG74000"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
<technology name="_150066SV74000">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150066SV74000.pdf"/>
<attribute name="DOMINANT-WAVELENGTH" value="630nm@SuperRed / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Super Red &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@SuperRed / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="55mcd@SuperRed / 30mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150066SV74000"/>
<attribute name="PEAK-WAVELENGTH" value="645nm@SuperRed / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150066SV74000"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
<technology name="_150066YV74000">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150066YV74000.pdf"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm@Yellow / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Yellow &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Yellow / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="120mcd@Yellow / 30mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150066YV74000"/>
<attribute name="PEAK-WAVELENGTH" value="595nm@Yellow / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150066YV74000"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SBCW_1210" prefix="D">
<description>&lt;b&gt; WL-SBCW SMD Bi-color Chip LED Waterclear
&lt;br&gt;
&lt;br&gt; Characteristics

&lt;br&gt;&lt;br&gt;&lt;/b&gt;&lt;

&lt;br&gt;Two chips in one package
&lt;br&gt;Small size
&lt;br&gt;Industry standard footprint
&lt;br&gt;High efficiency
&lt;br&gt;Low power consumption
&lt;br&gt;Wide viewing angle
&lt;br&gt;Small LED package for exceptional brightness
&lt;br&gt;Packaged in standard tape and reel 7"
&lt;br&gt;Compatible with automatic placement machine
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Backlighting applications
&lt;br&gt;Status indicator
&lt;br&gt;Front panel indicators
&lt;br&gt;Push button backlighting
&lt;br&gt;Symbol and switch backlighting
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14901v209%20Family_WL_SBCW.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14901v209%20Family_WL_SBCW.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SBCW"&gt;https://www.we-online.com/catalog/en/WL-SBCW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-03-31&lt;br&gt;
&lt;/b&gt;2022(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SBCW"/>
</gates>
<devices>
<device name="" package="WL-SBCW_1210">
<connects>
<connect gate="G$1" pin="S+" pad="4"/>
<connect gate="G$1" pin="S-" pad="1"/>
<connect gate="G$1" pin="V+" pad="3"/>
<connect gate="G$1" pin="V-" pad="2"/>
</connects>
<technologies>
<technology name="_150121SV74000">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150121SV74000.pdf"/>
<attribute name="DOMINANT-WAVELENGTH" value="630nm@SuperRed / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Super Red &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@SuperRed / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="55mcd@SuperRed / 30mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150121SV74000"/>
<attribute name="PEAK-WAVELENGTH" value="645nm@SuperRed / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150121SV74000"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
<technology name="_150121YV74000">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150121YV74000.pdf"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm@Yellow / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Yellow &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Yellow / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="120mcd@Yellow / 40mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150121YV74000"/>
<attribute name="PEAK-WAVELENGTH" value="595nm@Yellow / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150121YV74000"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
