<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - LEDs - Singnal LEDs - TOP LED - WL-SBTW&lt;br&gt;&lt;Hr&gt;
&lt;BR&gt;&lt;BR&gt;

&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2022a, 2022-06-17&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SBTW_3528">
<description>&lt;B&gt;WL-SBTW SMT Bi-color TOP LED Waterclear&lt;BR&gt;

&lt;/B&gt;&lt;BR&gt;Size:3528, SMT, 4pins
&lt;BR&gt;3.5x2.8x1.9mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SBTW_150141XX73100">
<pin name="C2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="A1" direction="pas"/>
</symbol>
<symbol name="WL-SBTW_150141XX73110">
<pin name="C2" direction="pas"/>
<pin name="A2" direction="pas"/>
<pin name="C1" direction="pas"/>
<pin name="A1" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SBTW_3528_150141XX73110" prefix="D">
<description>&lt;b&gt;WL-SBTW SMT Bi-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;None diffused lens 
&lt;br&gt;LED with Black surface 
&lt;br&gt;Compact package outline e
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Decorative lighting
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14902v209%20WL-SBTW_150352RY73100.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14902v209%20WL-SBTW_150352RY73100.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SBTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SBTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-06-17&lt;br&gt;
&lt;/b&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SBTW_150141XX73110"/>
</gates>
<devices>
<device name="" package="WL-SBTW_3528">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="4"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="2"/>
</connects>
<technologies>
<technology name="_150141RY73110">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141RY73110?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red / 590nm@Yellow"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Yellow"/>
<attribute name="FORWARD-VOLTAGE" value="@Red / 2V@Yellow"/>
<attribute name="LUMINOUS-INTENSITY" value="150mcd@Red / 230mcd@Yellow"/>
<attribute name="PART-NUMBER" value="150141RY73110"/>
<attribute name="PEAK-WAVELENGTH" value="630nm@Red / 592nm@Yellow"/>
<attribute name="VALUE" value="150141RY73110"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141SV73110">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141SV73110?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="630nm@SuperRed / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Super Red &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@SuperRed / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="60mcd@SuperRed / 40mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150141SV73110"/>
<attribute name="PEAK-WAVELENGTH" value="645nm@SuperRed / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150141SV73110"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141YV73110">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141YV73110?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm@Yellow / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Yellow &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Yellow / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="230mcd@Yellow / 40mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150141YV73110"/>
<attribute name="PEAK-WAVELENGTH" value="592nm@Yellow / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150141YV73110"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SBTW_3528_150141XX73100" prefix="D">
<description>&lt;b&gt;WL-SBTW SMT Bi-color TOP LED Waterclear
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt;Low energy consumption 
&lt;br&gt;High reliability 
&lt;br&gt;Low current requirement 
&lt;br&gt;Fast switching 
&lt;br&gt;No UV/IR radiation 
&lt;br&gt;None diffused lens 
&lt;br&gt;LED with Black surface 
&lt;br&gt;Compact package outline e
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Flat backlight for LCDs, switches and symbols 
&lt;br&gt;Decorative lighting
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o14902v209%20WL-SBTW_150352RY73100.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o14902v209%20WL-SBTW_150352RY73100.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SBTW/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/catalog/WL-SBTW&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2022-06-17&lt;br&gt;
&lt;/b&gt;2022 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SBTW_150141XX73100"/>
</gates>
<devices>
<device name="" package="WL-SBTW_3528">
<connects>
<connect gate="G$1" pin="A1" pad="1"/>
<connect gate="G$1" pin="A2" pad="2"/>
<connect gate="G$1" pin="C1" pad="3"/>
<connect gate="G$1" pin="C2" pad="4"/>
</connects>
<technologies>
<technology name="_150141RB73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141RB73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red / 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red / 3.2V@Blue"/>
<attribute name="LUMINOUS-INTENSITY" value="260mcd@Red / 240mcd@Blue"/>
<attribute name="PART-NUMBER" value="150141RB73100"/>
<attribute name="PEAK-WAVELENGTH" value="630nm@Red / 465nm@Blue"/>
<attribute name="VALUE" value="150141RB73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141RV73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141RV73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="250mcd@Red / 60mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150141RV73100"/>
<attribute name="PEAK-WAVELENGTH" value="630nm@Red / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150141RV73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141YB73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141YB73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm@Yellow / 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Yellow &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Yellow / 3.2V@Blue"/>
<attribute name="LUMINOUS-INTENSITY" value="240mcd@Yellow / 220mcd@Blue"/>
<attribute name="PART-NUMBER" value="150141YB73100"/>
<attribute name="PEAK-WAVELENGTH" value="592nm@Yellow / 465nm@Blue"/>
<attribute name="VALUE" value="150141YB73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
<technology name="_150141YV73100">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150141YV73100?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="590nm@Yellow / 570nm@BrightGreen"/>
<attribute name="EMITTING-COLOR" value="Yellow &amp; Bright Green"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Yellow / 2V@BrightGreen"/>
<attribute name="LUMINOUS-INTENSITY" value="220mcd@Yellow / 60mcd@BrightGreen"/>
<attribute name="PART-NUMBER" value="150141YV73100"/>
<attribute name="PEAK-WAVELENGTH" value="592nm@Yellow / 572nm@BrightGreen"/>
<attribute name="VALUE" value="150141YV73100"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
