<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - LEDs - Signal LEDs - Chip LED - WL-SFCC&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-04-25&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="150044M155220">
<description>&lt;b&gt;WL-SFCC SMT Full-color Chip LED Compact&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size0404, SMT, 4pins
&lt;br&gt;0.95x0.95x0.25mm(LXWXH)</description>
</package>
<package name="150044M155260">
<description>&lt;b&gt;WL-SFCC SMT Full-color Chip LED Compact&lt;br&gt;
&lt;/b&gt;&lt;br&gt;Size0404, SMT, 4pins
&lt;br&gt;1x1x0.65mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="150044M155220">
<pin name="+" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
</symbol>
<symbol name="150044M155260">
<pin name="+" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="150044M155220" prefix="D">
<description>&lt;b&gt;WL-SFCC SMT Full-color Chip LED Compact
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Anti-reflection surface 
&lt;br&gt;Smallest RGB package 
&lt;br&gt;Very wide viewing angle 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Full-color display 
&lt;br&gt;Indoor video walls 
&lt;br&gt;Backlighting 
&lt;br&gt;Indicator 
&lt;br&gt;Front panel indicator 
&lt;br&gt;Home and smart appliances 
&lt;br&gt;Wearable and portable devices 
&lt;br&gt;Healthcare applications 
&lt;br&gt;Signal control system 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o710465v209%20150044M155220_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o710465v209%20150044M155220_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SFCC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SFCC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-25&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="150044M155220"/>
</gates>
<devices>
<device name="" package="150044M155220">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="B-" pad="3"/>
<connect gate="G$1" pin="G-" pad="4"/>
<connect gate="G$1" pin="R-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150044M155220?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="623nm@Red &amp; 525nm@Green &amp; 465nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red &amp; 3V@Green &amp; 3V@Blue"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="LUMINOUS-INTENSITY" value="200nm@Red &amp; 500nm@Green &amp; 110nm@Blue"/>
<attribute name="MOUNT" value="1mm"/>
<attribute name="PART-NUMBER" value="150044M155220"/>
<attribute name="PEAK-WAVELENGTH" value="630nm@Red &amp; 520nm@Green &amp; 460nm@Blue"/>
<attribute name="SIZE" value="0404 Super Flat"/>
<attribute name="VALUE" value="150044M155220"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="150044M155260" prefix="D">
<description>&lt;b&gt;WL-SFCC SMT Full-color Chip LED Compact
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; Anti-reflection surface 
&lt;br&gt;Smallest RGB package 
&lt;br&gt;Very wide viewing angle 
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Full-color display 
&lt;br&gt;Indoor video walls 
&lt;br&gt;Backlighting 
&lt;br&gt;Indicator 
&lt;br&gt;Front panel indicator 
&lt;br&gt;Home and smart appliances 
&lt;br&gt;Wearable and portable devices 
&lt;br&gt;Healthcare applications 
&lt;br&gt;Signal control system 
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/components/media/o710465v209%20150044M155220_multi-parts.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/components/media/o710465v209%20150044M155220_multi-parts.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SFCC/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SFCC&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella 2025-04-25&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="150044M155260"/>
</gates>
<devices>
<device name="" package="150044M155260">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="B-" pad="4"/>
<connect gate="G$1" pin="G-" pad="3"/>
<connect gate="G$1" pin="R-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150044M155260?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="621nm@Red &amp; 530nm@Green &amp; 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red &amp; 2.7V@Green &amp; 2.8V@Blue"/>
<attribute name="HEIGHT" value="1mm"/>
<attribute name="LENGTH" value="1mm"/>
<attribute name="LUMINOUS-INTENSITY" value="80nm@Red &amp; 180nm@Green &amp; 50nm@Blue"/>
<attribute name="MOUNT" value="1mm"/>
<attribute name="PART-NUMBER" value="150044M155260"/>
<attribute name="PEAK-WAVELENGTH" value="625nm@Red &amp; 522nm@Green &amp; 465nm@Blue"/>
<attribute name="SIZE" value="0404"/>
<attribute name="VALUE" value="150044M155260"/>
<attribute name="VIEWING-ANGLE" value="140°"/>
<attribute name="WIDTH" value="1mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
