<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.0.1">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - LEDs - Singnal LEDs - Clip LED - WL-SFCD&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2020a, 2020-03-19&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SFCD_0805">
<description>&lt;B&gt;WL-SFCD &lt;/B&gt;&lt;BR&gt;SMT Full-color Chip LED Diffused ,Size:0805,2x1.3x0.5mm(LXWXH)</description>
</package>
<package name="WL-SFCD_1210">
<description>&lt;B&gt;WL-SFCD &lt;/B&gt;&lt;BR&gt;SMT Full-color Chip LED Diffused ,Size:1210,2.7x3.2x1.1mm(LXWXH)</description>
</package>
<package name="WL-SFCD_0606">
<description>&lt;B&gt;WL-SFCD &lt;/B&gt;&lt;BR&gt;SMT Full-color Chip LED Diffused ,Size:0606,1.6x1.6x0.4mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SFCD_0805">
<pin name="+" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
</symbol>
<symbol name="WL-SFCD">
<pin name="+" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SFCD_0805" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SFCD SMT Full-color Chip LED Diffused 
&lt;br&gt;
&lt;br&gt;

Characteristics&lt;/b&gt;
&lt;br&gt;&lt;br&gt;High efficiency 
&lt;br&gt;Low power consumption 
&lt;br&gt;Diffused optics LED 
&lt;br&gt;Red/Green/Blue color combination 
&lt;br&gt;Compatible with reflow soldering 
&lt;br&gt;Industry standard footprint 
&lt;br&gt;RGB 
&lt;br&gt;Compatible with automatic placement machine 
&lt;br&gt;Wide viewing angle 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Backlighting 
&lt;br&gt;Status indicator 
&lt;br&gt;Front panel indicator 
&lt;br&gt;Office automation, home appliances, industrial equipment 
&lt;br&gt;Backlighting for keypad, symbol and switch button 
&lt;br&gt;Indicator 
&lt;br&gt;Consumer electronics 
&lt;br&gt;Safety and security 
&lt;br&gt;General LED lighting 
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106333v209%20Family_WL-SFCD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106333v209%20Family_WL-SFCD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SFCD/"&gt;https://www.we-online.com/catalog/en/WL-SFCD/&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;Updated By Yingchun,Shan,2020-03-19&lt;br&gt;
&lt;/b&gt;2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SFCD_0805"/>
</gates>
<devices>
<device name="" package="WL-SFCD_0805">
<connects>
<connect gate="G$1" pin="+" pad="4"/>
<connect gate="G$1" pin="B-" pad="3"/>
<connect gate="G$1" pin="G-" pad="2"/>
<connect gate="G$1" pin="R-" pad="1"/>
</connects>
<technologies>
<technology name="_150080M153000">
<attribute name="ABSTRAHLWINKEL" value="120°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150080M153000.pdf"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="I-V-B-TYP" value="70mcd"/>
<attribute name="I-V-G-TYP" value="285mcd"/>
<attribute name="I-V-R-TYP" value="112mcd"/>
<attribute name="LAMDA-DOM-B-TYP" value="470nm"/>
<attribute name="LAMDA-DOM-G-TYP" value="525nm"/>
<attribute name="LAMDA-DOM-R-TYP" value="624nm"/>
<attribute name="LAMDA-PEAK-B-TYP" value="468nm"/>
<attribute name="LAMDA-PEAK-G-TYP" value="520nm"/>
<attribute name="LAMDA-PEAK-R-TYP" value="632nm"/>
<attribute name="PART-NUMBER" value="150080M153000"/>
<attribute name="V-F-B-TYP" value="3.3V"/>
<attribute name="V-F-G-TYP" value="3.3V"/>
<attribute name="V-F-R-TYP" value="2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SFCD_1210" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SFCD SMT Full-color Chip LED Diffused 
&lt;br&gt;
&lt;br&gt;

Characteristics&lt;/b&gt;
&lt;br&gt;&lt;br&gt;High efficiency 
&lt;br&gt;Low power consumption 
&lt;br&gt;Diffused optics LED 
&lt;br&gt;Red/Green/Blue color combination 
&lt;br&gt;Compatible with reflow soldering 
&lt;br&gt;Industry standard footprint 
&lt;br&gt;RGB 
&lt;br&gt;Compatible with automatic placement machine 
&lt;br&gt;Wide viewing angle 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Backlighting 
&lt;br&gt;Status indicator 
&lt;br&gt;Front panel indicator 
&lt;br&gt;Office automation, home appliances, industrial equipment 
&lt;br&gt;Backlighting for keypad, symbol and switch button 
&lt;br&gt;Indicator 
&lt;br&gt;Consumer electronics 
&lt;br&gt;Safety and security 
&lt;br&gt;General LED lighting 
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106333v209%20Family_WL-SFCD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106333v209%20Family_WL-SFCD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SFCD/"&gt;https://www.we-online.com/catalog/en/WL-SFCD/&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;Updated By Yingchun,Shan,2020-03-19&lt;br&gt;
&lt;/b&gt;2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SFCD"/>
</gates>
<devices>
<device name="" package="WL-SFCD_1210">
<connects>
<connect gate="G$1" pin="+" pad="4"/>
<connect gate="G$1" pin="B-" pad="3"/>
<connect gate="G$1" pin="G-" pad="2"/>
<connect gate="G$1" pin="R-" pad="1"/>
</connects>
<technologies>
<technology name="_150121M153000">
<attribute name="ABSTRAHLWINKEL" value="120°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150121M153000.pdf"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="I-V-B-TYP" value="80mcd"/>
<attribute name="I-V-G-TYP" value="180mcd"/>
<attribute name="I-V-R-TYP" value="70mcd"/>
<attribute name="LAMDA-DOM-B-TYP" value="470nm"/>
<attribute name="LAMDA-DOM-G-TYP" value="525nm"/>
<attribute name="LAMDA-DOM-R-TYP" value="624nm"/>
<attribute name="LAMDA-PEAK-B-TYP" value="468nm"/>
<attribute name="LAMDA-PEAK-G-TYP" value="520nm"/>
<attribute name="LAMDA-PEAK-R-TYP" value="632nm"/>
<attribute name="PART-NUMBER" value="150121M153000"/>
<attribute name="V-F-B-TYP" value="3.3V"/>
<attribute name="V-F-G-TYP" value="3.3V"/>
<attribute name="V-F-R-TYP" value="2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SFCD_0606" prefix="D" uservalue="yes">
<description>&lt;b&gt;WL-SFCD SMT Full-color Chip LED Diffused 
&lt;br&gt;
&lt;br&gt;

Characteristics&lt;/b&gt;
&lt;br&gt;&lt;br&gt;High efficiency 
&lt;br&gt;Low power consumption 
&lt;br&gt;Diffused optics LED 
&lt;br&gt;Red/Green/Blue color combination 
&lt;br&gt;Compatible with reflow soldering 
&lt;br&gt;Industry standard footprint 
&lt;br&gt;RGB 
&lt;br&gt;Compatible with automatic placement machine 
&lt;br&gt;Wide viewing angle 
&lt;br&gt;
&lt;br&gt;
&lt;b&gt;Applications&lt;/b&gt;&lt;br&gt;
&lt;br&gt;Backlighting 
&lt;br&gt;Status indicator 
&lt;br&gt;Front panel indicator 
&lt;br&gt;Office automation, home appliances, industrial equipment 
&lt;br&gt;Backlighting for keypad, symbol and switch button 
&lt;br&gt;Indicator 
&lt;br&gt;Consumer electronics 
&lt;br&gt;Safety and security 
&lt;br&gt;General LED lighting 
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o106333v209%20Family_WL-SFCD.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o106333v209%20Family_WL-SFCD.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SFCD/"&gt;https://www.we-online.com/catalog/en/WL-SFCD/&lt;/a&gt;&lt;p&gt;
&lt;/b&gt;Updated By Yingchun,Shan,2020-03-19&lt;br&gt;
&lt;/b&gt;2020 (C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SFCD"/>
</gates>
<devices>
<device name="" package="WL-SFCD_0606">
<connects>
<connect gate="G$1" pin="+" pad="4"/>
<connect gate="G$1" pin="B-" pad="3"/>
<connect gate="G$1" pin="G-" pad="2"/>
<connect gate="G$1" pin="R-" pad="1"/>
</connects>
<technologies>
<technology name="_150066M153000">
<attribute name="ABSTRAHLWINKEL" value="120°"/>
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + InGaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/150066M153000.pdf"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="I-V-B-TYP" value="180mcd"/>
<attribute name="I-V-G-TYP" value="900mcd"/>
<attribute name="I-V-R-TYP" value="285mcd"/>
<attribute name="LAMDA-DOM-B-TYP" value="470nm"/>
<attribute name="LAMDA-DOM-G-TYP" value="525nm"/>
<attribute name="LAMDA-DOM-R-TYP" value="624nm"/>
<attribute name="LAMDA-PEAK-B-TYP" value="468nm"/>
<attribute name="LAMDA-PEAK-G-TYP" value="520nm"/>
<attribute name="LAMDA-PEAK-R-TYP" value="632nm"/>
<attribute name="PART-NUMBER" value="150066M153000"/>
<attribute name="V-F-B-TYP" value="3.3V"/>
<attribute name="V-F-G-TYP" value="3.3V"/>
<attribute name="V-F-R-TYP" value="2V"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
