<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.6.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Optoelectronic Components - LEDs - Signal LEDs - TOP LED - WL-SFTD&lt;br&gt;
&lt;Hr&gt;
&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Disclaimer: While Würth Elektronik eiSos has made every reasonable effort to ensure the accuracy of the PCB layout models provided, &lt;br&gt;
Würth Elektronik eiSos does not guarantee the exemption of error on the PCB layout models, nor does Würth Elektronik eiSos guarantee that the PCB layout model is current. &lt;br&gt;
Würth Elektronik eiSos reserves the right to make any adjustments at any time without notice. &lt;br&gt;
Würth Elektronik eiSos expressly disclaims all implied warranties regarding this PCB layout model. &lt;br&gt;
 &lt;br&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2025a, 2025-03-14&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="150161M153130">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;/b&gt;&lt;br&gt;Size : 1616, SMT, 4pins

&lt;br&gt;&lt;br&gt;1.6X1.6X1.6mm(LXWXH)</description>
</package>
<package name="150282M167310">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;/b&gt;&lt;br&gt;Size: 2828, SMT, 6pins

&lt;br&gt;&lt;br&gt;2.8X2.7X3mm(LXWXH)</description>
</package>
<package name="150353M153300">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;/b&gt;&lt;br&gt;Size: 3535, SMT, 6pins

&lt;br&gt;&lt;br&gt;3.7X3.5X2.8mm(LXWXH)</description>
</package>
<package name="150282M153310">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;/b&gt;&lt;br&gt;Size: 2828, SMT, 6pins

&lt;br&gt;&lt;br&gt;2.8X2.8X2.5mm(LXWXH)</description>
</package>
<package name="150202M153130">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;/b&gt;&lt;br&gt;Size : 2020, SMT, 4pins

&lt;br&gt;&lt;br&gt;2X2.2X1.9mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="150161M153130">
<pin name="+" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
</symbol>
<symbol name="150353M153300">
<pin name="3" direction="pas"/>
<pin name="B" direction="pas"/>
<pin name="G" direction="pas"/>
<pin name="R" direction="pas"/>
<pin name="1" direction="pas"/>
<pin name="5" direction="pas"/>
</symbol>
<symbol name="150282M167310">
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
<pin name="B+" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="R+" direction="pas"/>
</symbol>
<symbol name="150282M153310">
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
<pin name="B+" direction="pas"/>
<pin name="G+" direction="pas"/>
<pin name="R+" direction="pas"/>
</symbol>
<symbol name="150202M153130">
<pin name="+" direction="pas"/>
<pin name="R-" direction="pas"/>
<pin name="G-" direction="pas"/>
<pin name="B-" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="150161M153130" prefix="D">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Industry standard size 3535
&lt;br&gt;Matte and non-reflective surface
&lt;br&gt;High reliability 
&lt;br&gt;Low energy consumtion
&lt;br&gt;Low current requirement
&lt;br&gt;MSL 5a
&lt;br&gt;Water-resistant IPx6
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Outdoor Full-Color Video Screen
&lt;br&gt;Decorative lighting
&lt;br&gt;Entertainment
&lt;br&gt;LED display screen
&lt;br&gt;Indicator
&lt;br&gt;Backlight

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SFTD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SFTD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-03-14&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="150161M153130"/>
</gates>
<devices>
<device name="" package="150161M153130">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="B-" pad="4"/>
<connect gate="G$1" pin="G-" pad="3"/>
<connect gate="G$1" pin="R-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150161M153130?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red &amp; 520nm@Green &amp; 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red &amp; 3.2V@Green &amp; 3.2V@Blue"/>
<attribute name="HEIGHT" value="1.6mm"/>
<attribute name="LENGTH" value="1.6mm"/>
<attribute name="LUMINOUS-INTENSITY" value="200nm@Red &amp; 400nm@Green &amp; 60nm@Blue"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150161M153130"/>
<attribute name="PEAK-WAVELENGTH" value="635nm@Red &amp; 515nm@Green &amp; 465nm@Blue"/>
<attribute name="SIZE" value="1616"/>
<attribute name="VALUE" value="150161M153130"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
<attribute name="WIDTH" value="1.6mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="150282M167310" prefix="D">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Industry standard size 3535
&lt;br&gt;Matte and non-reflective surface
&lt;br&gt;High reliability 
&lt;br&gt;Low energy consumtion
&lt;br&gt;Low current requirement
&lt;br&gt;MSL 5a
&lt;br&gt;Water-resistant IPx6
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Outdoor Full-Color Video Screen
&lt;br&gt;Decorative lighting
&lt;br&gt;Entertainment
&lt;br&gt;LED display screen
&lt;br&gt;Indicator
&lt;br&gt;Backlight

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SFTD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SFTD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-03-14&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="150282M167310"/>
</gates>
<devices>
<device name="" package="150282M167310">
<connects>
<connect gate="G$1" pin="B+" pad="6"/>
<connect gate="G$1" pin="B-" pad="1"/>
<connect gate="G$1" pin="G+" pad="5"/>
<connect gate="G$1" pin="G-" pad="2"/>
<connect gate="G$1" pin="R+" pad="4"/>
<connect gate="G$1" pin="R-" pad="3"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150282M167310?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="620nm@Red &amp; 530nm@Green &amp; 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red &amp; 3.2V@Green &amp; 3.2V@Blue"/>
<attribute name="HEIGHT" value="3mm"/>
<attribute name="LENGTH" value="2.8mm"/>
<attribute name="LUMINOUS-INTENSITY" value="1200nm@Red &amp; 3000nm@Green &amp; 600nm@Blue"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150282M167310"/>
<attribute name="PEAK-WAVELENGTH" value="635nm@Red &amp; 515nm@Green &amp; 465nm@Blue"/>
<attribute name="SIZE" value="2828"/>
<attribute name="VALUE" value="150282M167310"/>
<attribute name="VIEWING-ANGLE" value="70°"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="150353M153300" prefix="D">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Industry standard size 3535
&lt;br&gt;Matte and non-reflective surface
&lt;br&gt;High reliability 
&lt;br&gt;Low energy consumtion
&lt;br&gt;Low current requirement
&lt;br&gt;MSL 5a
&lt;br&gt;Water-resistant IPx6
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Outdoor Full-Color Video Screen
&lt;br&gt;Decorative lighting
&lt;br&gt;Entertainment
&lt;br&gt;LED display screen
&lt;br&gt;Indicator
&lt;br&gt;Backlight

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SFTD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SFTD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-03-14&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="150353M153300"/>
</gates>
<devices>
<device name="" package="150353M153300">
<connects>
<connect gate="G$1" pin="1" pad="1"/>
<connect gate="G$1" pin="3" pad="3"/>
<connect gate="G$1" pin="5" pad="5"/>
<connect gate="G$1" pin="B" pad="6"/>
<connect gate="G$1" pin="G" pad="4"/>
<connect gate="G$1" pin="R" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150353M153300?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red &amp; 520nm@Green &amp; 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red &amp; 3.2V@Green &amp; 3.2V@Blue"/>
<attribute name="HEIGHT" value="2.8mm"/>
<attribute name="LENGTH" value="3.7mm"/>
<attribute name="LUMINOUS-INTENSITY" value="800nm@Red &amp; 1900nm@Green &amp; 400nm@Blue"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150353M153300"/>
<attribute name="PEAK-WAVELENGTH" value="635nm@Red &amp; 515nm@Green &amp; 465nm@Blue"/>
<attribute name="SIZE" value="3535"/>
<attribute name="VALUE" value="150353M153300"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
<attribute name="WIDTH" value="3.5mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="150282M153310" prefix="D">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Industry standard size 3535
&lt;br&gt;Matte and non-reflective surface
&lt;br&gt;High reliability 
&lt;br&gt;Low energy consumtion
&lt;br&gt;Low current requirement
&lt;br&gt;MSL 5a
&lt;br&gt;Water-resistant IPx6
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Outdoor Full-Color Video Screen
&lt;br&gt;Decorative lighting
&lt;br&gt;Entertainment
&lt;br&gt;LED display screen
&lt;br&gt;Indicator
&lt;br&gt;Backlight

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SFTD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SFTD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-03-14&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="150282M153310"/>
</gates>
<devices>
<device name="" package="150282M153310">
<connects>
<connect gate="G$1" pin="B+" pad="4"/>
<connect gate="G$1" pin="B-" pad="3"/>
<connect gate="G$1" pin="G+" pad="5"/>
<connect gate="G$1" pin="G-" pad="2"/>
<connect gate="G$1" pin="R+" pad="6"/>
<connect gate="G$1" pin="R-" pad="1"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150282M153310?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red &amp; 520nm@Green &amp; 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red &amp; 3.2V@Green &amp; 3.2V@Blue"/>
<attribute name="HEIGHT" value="2.5mm"/>
<attribute name="LENGTH" value="2.8mm"/>
<attribute name="LUMINOUS-INTENSITY" value="800nm@Red &amp; 1900nm@Green &amp; 400nm@Blue"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150282M153310"/>
<attribute name="PEAK-WAVELENGTH" value="635nm@Red &amp; 515nm@Green &amp; 465nm@Blue"/>
<attribute name="SIZE" value="2828"/>
<attribute name="VALUE" value="150282M153310"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
<attribute name="WIDTH" value="2.8mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="150202M153130" prefix="D">
<description>&lt;b&gt;WL-SFTD SMT Full-color Top LED Diffused
&lt;br&gt;
&lt;br&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt; Industry standard size 3535
&lt;br&gt;Matte and non-reflective surface
&lt;br&gt;High reliability 
&lt;br&gt;Low energy consumtion
&lt;br&gt;Low current requirement
&lt;br&gt;MSL 5a
&lt;br&gt;Water-resistant IPx6
&lt;br&gt;
&lt;br&gt;&lt;b&gt;Applications &lt;/b&gt;
&lt;br&gt;
&lt;br&gt;Outdoor Full-Color Video Screen
&lt;br&gt;Decorative lighting
&lt;br&gt;Entertainment
&lt;br&gt;LED display screen
&lt;br&gt;Indicator
&lt;br&gt;Backlight

&lt;br&gt;
&lt;br&gt;
&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o135756v209%20Gruppe_WL-SFTD_1616_2022_2828_2828.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="www.we-online.com/catalog/WL-SFTD/?utm_source=eagle_model&amp;utm_medium=description_link&amp;utm_campaign=eisos_eagle"&gt;www.we-online.com/en/components/products/WL-SFTD&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu 2025-03-14&lt;br&gt;
&lt;/b&gt;2025 (C) Würth Elektronik</description>
<gates>
<gate name="G$1" symbol="150202M153130"/>
</gates>
<devices>
<device name="" package="150202M153130">
<connects>
<connect gate="G$1" pin="+" pad="1"/>
<connect gate="G$1" pin="B-" pad="4"/>
<connect gate="G$1" pin="G-" pad="3"/>
<connect gate="G$1" pin="R-" pad="2"/>
</connects>
<technologies>
<technology name="">
<attribute name="CHIP-TECHNOLOGY" value="AlInGaP + GaN"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/redexpert/spec/150202M153130?ae"/>
<attribute name="DOMINANT-WAVELENGTH" value="625nm@Red &amp; 520nm@Green &amp; 470nm@Blue"/>
<attribute name="EMITTING-COLOR" value="Red &amp; Green &amp; Blue"/>
<attribute name="FORWARD-VOLTAGE" value="2V@Red &amp; 3.2V@Green &amp; 3.2V@Blue"/>
<attribute name="HEIGHT" value="1.9mm"/>
<attribute name="LENGTH" value="2mm"/>
<attribute name="LUMINOUS-INTENSITY" value="350nm@Red &amp; 750nm@Green &amp; 120nm@Blue"/>
<attribute name="MOUNT" value="SMT"/>
<attribute name="PART-NUMBER" value="150202M153130"/>
<attribute name="PEAK-WAVELENGTH" value="635nm@Red &amp; 515nm@Green &amp; 465nm@Blue"/>
<attribute name="SIZE" value="2022"/>
<attribute name="VALUE" value="150202M153130"/>
<attribute name="VIEWING-ANGLE" value="120°"/>
<attribute name="WIDTH" value="2.2mm"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
