<?xml version="1.0" encoding="utf-8"?>
<!DOCTYPE eagle SYSTEM "eagle.dtd">
<eagle version="9.5.2">
<drawing>
<library>
<description>&lt;BR&gt;Wurth Elektronik - Infrared - Infrared LEDs - WL-SIMW&lt;br&gt;&lt;Hr&gt;

&lt;BR&gt;
&lt;TABLE BORDER=0 CELLSPACING=0 CELLPADDING=0&gt;
&lt;TR&gt;   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;&lt;br&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;
      -----&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt; &lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------------------------&lt;BR&gt;
&lt;B&gt;&lt;I&gt;&lt;span style='font-size:26pt;
  color:#FF6600;'&gt;WE &lt;/span&gt;&lt;/i&gt;&lt;/b&gt;
&lt;BR&gt;
      ---------------------------&lt;BR&gt;&lt;b&gt;Würth Elektronik&lt;/b&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
    &lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;br&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;
      ----O--------&lt;BR&gt;
      ---------O---&lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
   
&lt;TD BGCOLOR="#cccccc" ALIGN=CENTER&gt;&lt;FONT FACE=ARIAL SIZE=3&gt;&lt;BR&gt;
      &amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp; &amp;nbsp;&lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;
       &lt;BR&gt;&lt;BR&gt;&lt;/FONT&gt;
    &lt;/TD&gt;
  &lt;/TR&gt;

  &lt;TR&gt;
    &lt;TD COLSPAN=7&gt;&amp;nbsp;
    &lt;/TD&gt;
  &lt;/TR&gt;
  
&lt;/TABLE&gt;
&lt;B&gt;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;&amp;nbsp;More than you expect&lt;BR&gt;&lt;BR&gt;&lt;BR&gt;&lt;/B&gt;

&lt;HR&gt;&lt;BR&gt;
&lt;b&gt;Würth Elektronik eiSos GmbH &amp; Co. KG&lt;/b&gt;&lt;br&gt;
EMC &amp; Inductive Solutions&lt;br&gt;

Max-Eyth-Str.1&lt;br&gt;
D-74638 Waldenburg&lt;br&gt;
&lt;br&gt;
Tel: +49 (0)7942-945-0&lt;br&gt;
Fax:+49 (0)7942-945-5000&lt;br&gt;
&lt;br&gt;
&lt;a href="http://www.we-online.com/web/en/electronic_components/produkte_pb/bauteilebibliotheken/eagle_4.php"&gt;www.we-online.com/eagle&lt;/a&gt;&lt;br&gt;
&lt;a href="mailto:libraries@we-online.com"&gt;libraries@we-online.com&lt;/a&gt; &lt;BR&gt;&lt;BR&gt;
&lt;br&gt;&lt;HR&gt;&lt;BR&gt;
Neither Autodesk nor Würth Elektronik eiSos does warrant that this library is error-free or &lt;br&gt;
that it meets your specific requirements.&lt;br&gt;&lt;BR&gt;
Please contact us for more information.&lt;br&gt;
&lt;HR&gt;
&lt;br&gt;Eagle Version 9, Library Revision 2021a, 2021-11-04&lt;br&gt;
&lt;HR&gt;
Copyright: Würth Elektronik</description>
<packages>
<package name="WL-SIMW_3535_154353XXAA350">
<description>&lt;b&gt;WL-SIMW&lt;/b&gt;&lt;br&gt; SMT Infrared Ceramic Waterclear,Size 3535:3.45x3.45x2.1mm(LXWXH)</description>
</package>
<package name="WL-SIMW_3535_154353XXA9050">
<description>&lt;b&gt;WL-SIMW&lt;/b&gt;&lt;br&gt; SMT Infrared Ceramic Waterclear,Size 3535:3.45x3.45x2.65mm(LXWXH)</description>
</package>
</packages>
<symbols>
<symbol name="WL-SIMW">
<pin name="-" direction="pas"/>
<pin name="+" direction="pas"/>
</symbol>
</symbols>
<devicesets>
<deviceset name="WL-SIMW_3535_154353XXAA350" prefix="D">
<description>&lt;b&gt;WL-SIMW SMT Infrared Ceramic Waterclear 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High power output IR LEDs 
&lt;br&gt;Low thermal resistance 
&lt;br&gt;Peak wavelengths: 850, 940 nm 
&lt;br&gt;High ESD withstand voltage: 8 kV (HBM) 
&lt;br&gt;Viewing Angle: 90°, 130° 
&lt;br&gt;Standard soldering pad footprint 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Infrared/ Night Vision/ Security cameras 
&lt;br&gt;Machine vision systems 
&lt;br&gt;Gesture recognition systems
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78430v209%20WL-SIMW_IR_90Grad_130Grad_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78430v209%20WL-SIMW_IR_90Grad_130Grad_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SIMW/"&gt;https://www.we-online.com/catalog/en/WL-SIMW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu, 2021-11-04&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SIMW"/>
</gates>
<devices>
<device name="" package="WL-SIMW_3535_154353XXAA350">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15435385AA350">
<attribute name="CENTROID-WAVELENGTH" value="850nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15435385AA350.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="PART-NUMBER" value="15435385AA350"/>
<attribute name="PEAK-WAVELENGTH" value="855nm"/>
<attribute name="RADIANT-INTENSITY" value="250mW/sr"/>
<attribute name="VALUE" value="15435385AA350"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
<technology name="_15435394AA350">
<attribute name="CENTROID-WAVELENGTH" value="940nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15435394AA350.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="1.9V"/>
<attribute name="PART-NUMBER" value="15435394AA350"/>
<attribute name="PEAK-WAVELENGTH" value="945nm"/>
<attribute name="RADIANT-INTENSITY" value="220mW/sr"/>
<attribute name="VALUE" value="15435394AA350"/>
<attribute name="VIEWING-ANGLE" value="130°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
<deviceset name="WL-SIMW_3535_154353XXA9050" prefix="D">
<description>&lt;b&gt;WL-SIMW SMT Infrared Ceramic Waterclear 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Characteristics
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;&lt;/b&gt; High power output IR LEDs 
&lt;br&gt;Low thermal resistance 
&lt;br&gt;Peak wavelengths: 850, 940 nm 
&lt;br&gt;High ESD withstand voltage: 8 kV (HBM) 
&lt;br&gt;Viewing Angle: 90°, 130° 
&lt;br&gt;Standard soldering pad footprint 
&lt;br&gt;
&lt;br&gt;&lt;b&gt; Applications
&lt;br&gt;
&lt;br&gt;&lt;/b&gt;Infrared/ Night Vision/ Security cameras 
&lt;br&gt;Machine vision systems 
&lt;br&gt;Gesture recognition systems
&lt;br&gt;&lt;br&gt;
&lt;br&gt;&lt;a href="https://www.we-online.com/catalog/media/o78430v209%20WL-SIMW_IR_90Grad_130Grad_4C.jpg" title="Enlarge picture"&gt;
&lt;img src="https://www.we-online.com/catalog/media/o78430v209%20WL-SIMW_IR_90Grad_130Grad_4C.jpg" width="320"&gt;&lt;/a&gt;&lt;p&gt;
Details see: &lt;a href="https://www.we-online.com/catalog/en/WL-SIMW/"&gt;https://www.we-online.com/catalog/en/WL-SIMW/&lt;/a&gt;&lt;p&gt;

&lt;/b&gt;Updated by Ella Wu, 2021-11-04&lt;br&gt;
&lt;/b&gt;2021(C) Wurth Elektronik</description>
<gates>
<gate name="G$1" symbol="WL-SIMW"/>
</gates>
<devices>
<device name="" package="WL-SIMW_3535_154353XXA9050">
<connects>
<connect gate="G$1" pin="+" pad="2"/>
<connect gate="G$1" pin="-" pad="1"/>
</connects>
<technologies>
<technology name="_15435385A9050">
<attribute name="CENTROID-WAVELENGTH" value="850nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15435385A9050.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="2V"/>
<attribute name="PART-NUMBER" value="15435385A9050"/>
<attribute name="PEAK-WAVELENGTH" value="855nm"/>
<attribute name="RADIANT-INTENSITY" value="350mW/sr"/>
<attribute name="VALUE" value="15435385A9050"/>
<attribute name="VIEWING-ANGLE" value="90°"/>
</technology>
<technology name="_15435394A9050">
<attribute name="CENTROID-WAVELENGTH" value="940nm"/>
<attribute name="CHIP-TECHNOLOGY" value="AlGaAs"/>
<attribute name="DATASHEET-URL" value="https://www.we-online.com/catalog/datasheet/15435394A9050.pdf"/>
<attribute name="EMITTING-COLOR" value="Infrared"/>
<attribute name="FORWARD-VOLTAGE" value="1.9V"/>
<attribute name="PART-NUMBER" value="15435394A9050"/>
<attribute name="PEAK-WAVELENGTH" value="945nm"/>
<attribute name="RADIANT-INTENSITY" value="300mW/sr"/>
<attribute name="VALUE" value="15435394A9050"/>
<attribute name="VIEWING-ANGLE" value="90°"/>
</technology>
</technologies>
</device>
</devices>
</deviceset>
</devicesets>
</library>
</drawing>
</eagle>
